Copyright 1999-2001 ARM Limited
Copyright 1999-2001 Wind River Systems, Inc.
Copyright 2003-2004 Agere Systems Inc.
Copy
tNetFlashUp
spawn netFlashUp task in Tftp_FlashUp
 enter usrAppInit and call Main_Start
 1:*:WifiPhone:ANY:128:128:*:*:*:*:0:0:1
# i?
 Can't use dynamic address %s without DHCP.
Unable to verify assigned DHCP address.
(::%lx:%lx
:%x:%lx:%lx
(Warning: DHCP over backplane might require proxy arp.
Error in initializing dhcpcLib
(Negotiation Required,
Negotiation Not Required,
Local:%sNegotiable:
Local:%sNot Negotiable:%s
Remote:%sNegotiable:
Remote:%sNot Negotiable:%s
 SYS_PPP
usrBasicPPPFrameworkInit:Could not create PPP framework
 pppSysProfile
pppSysProfileCreate:Could not create base profile
_add_static_PPP_LCP
lcp_echoRequestSendInterval
lcp_authProtocol
Local:Negotiation Required,Negotiable:c223
Local:Alternate:c023
vxTarget
vxPPPClient
Remote:Negotiation Not Required,Not Negotiable:c223
Remote:Alternate:c023
lcp_magicNumber
Remote:Negotiation Not Required,Negotiable
lcp_PFCompression
lcp_ACFCompression
Remote:Negotiation Not Required,Not Negotiable:1
Remote:Range:1,4294967295,0
lcp_fcsAlternatives
Remote:Alternate:2
_add_dynamic_PPP_CHAP
chap_localUserName
chap_challengeInterval
_add_dynamic_PPP_PAP
pap_localUserName
ipcp_ipAddr
Local:Negotiation Required,Not Negotiable:90.0.0.1
Remote:Negotiation Required,Not Negotiable:90.0.0.2
ipcp_vjcParams
Local:Negotiation Not Required,Not Negotiable:002d0f01
Remote:Negotiation Not Required,Not Negotiable:002d0f01
_add_dynamic_VJC
_add_static_ASYNC_FRAMING
sio_channelNum
sio_baudRate
19200
sio_maxSendQSize
_add_static_PPP_VS_END
 pppOeSysProfile
_remove_SIO_ADAPTER
_remove_ASYNC_FRAMING
muxDevName
muxDevUnit
muxSvcType
0x8864:0x8863
lcp_MRU
Local:Negotiation Required,Negotiable:1492
Local:Range:576,1492,0
Remote:Negotiation Required,Not Negotiable:1492
Remote:Range:576,1492,0
pppOE_connectionMode
pppOE_svcName
gold
Local
Local:Negotiation Required,Negotiable:
Remote:Negotiation Required,Negotiable:
 pppBasicLinkProfile
usrBasicPPPProfileInit:Could not create base profile
lcp_maxUnAckedEchoRequests
%s%s
Remote:Range:
1,4294967295,0
_add_static_PPP_IPCP
 wvlan(0,0)host:/vxWorks h=192.168.1.1 e=192.168.1.100 u=u tn=t
 0@-
Error: invalid netmask in boot field "%s".
Error: invalid inet address in boot field "%s".
 bootHost
Host Name: %s 
Target Name: %s 
target
User: %s 
StartUp Script: %s 
Other: %s 
(scsi
tffs
(addGateway: malloc failed
addGateway: can't create a routing socket
addGateway: can't write to routing socket
 netIoctl: failed to create a socket
 usrNetBootConfig: Invalid Argument
%s%d
usrNetBootConfig: Failed SIOCSIFNETMASK for %s
usrNetBootConfig: Failed SIOCSIFADDR for %s
usrNetBootConfig: failed to create a socket
usrNetBootConfig: ioctl (SIOCGIFFLAGS)
usrNetBootConfig: ioctl (SIOCSIFFLAGS)
0.0.0.0
usrNetBootConfig: Failed addGateway
(usrNetBsdSocket: failed sockLibAdd for AF_INET
usrNetBsdSocket: failed sockLibAdd for PF_ROUTE
kern.ipc.maxsockbuf
kern.ipc.maxsockets
kern.ipc.sockbuf_waste_factor
kern.ipc.somaxconn
 0@-
(muxDevLoad failed for device entry %d!
muxDevStart failed for entry %d!
(usrNetEther: can't register ADDR_RES_FUNC
usrNetEther: can't register IF_OUTPUT_FUNC
usrNetEther: can't register MULTI_ADDR_RES_FUNC
net.link.ether.inet.prune_intvl
net.link.ether.inet.max_age
net.link.ether.inet.host_down_time
net.link.ether.inet.maxtries
net.link.ether.inet.useloopback
net.link.ether.inet.proxyall
net.link.ether.inet.log_arp_wrong_iface
$ L2
$ x2
 usrNetGtfInit: netTaskSemId not initialized
usrNetGtfInit: failed to create GTF_TIMER_MANAGER
(localhost
127.0.0.1
 usrNetIpv4: wrong value for ICMPERRORLEN (0-488) 
net.inet.icmp.maskrepl
net.inet.icmp.drop_redirect
net.inet.icmp.log_redirect
net.inet.icmp.icmplim
net.inet.icmp.bmcastecho
net.inet.icmp.icmpErrorLen
usrNetInit: memory size too big
usrNetInit: unaligned memory
usrNetInit: invalid hostname
(Failed to attach to device %s%d
Attached %s interface to %s unit %d
(kern.ipc.max_linkhdr
kern.ipc.max_protohdr
kern.ipc.max_hdr
net.inet.ip.portrange.lowfirst
net.inet.ip.ipport_lowlastauto
net.inet.ip.ipport_firstauto
net.inet.ip.ipport_lastauto
net.inet.ip.ipport_hifirstauto
net.inet.ip.ipport_hilastauto
net.inet.ip.forwarding
net.inet.ip.redirect
net.inet.ip.ttl
net.inet.ip.sourceroute
net.inet.ip.accept_sourceroute
net.inet.ip.maxfragpackets
net.inet.ip.check_interface
net.inet.ip.rtexpire
net.inet.ip.rtminexpire
net.inet.ip.rtmaxcache
net.inet.ip.subnets_are_local
 Attaching interface lo0... 
usrNetLoopback: DS_MALLOC failed
usrNetLoopback: loopattach failed
usrNetLoopback: usrNetBootConfig failed
done
(net.inet.raw.maxdgram
net.inet.raw.recvspace
 %s:
" \h
! DH
(net.inet.tcp.mssdflt
net.inet.tcp.rfc1323
net.inet.tcp.rfc1644
net.inet.tcp.do_tcpdrain
net.inet.tcp.icmp_may_rst
net.inet.tcp.tcp_seq_genscheme
net.inet.tcp.keepinit
net.inet.tcp.keepidle
net.inet.tcp.keepintvl
net.inet.tcp.delacktime
net.inet.tcp.msl
net.inet.tcp.always_keepalive
net.inet.tcp.sendspace
net.inet.tcp.recvspace
net.inet.tcp.log_in_vain
net.inet.tcp.blackhole
net.inet.tcp.delayed_ack
net.inet.tcp.tcp_lq_overflow
net.inet.tcp.path_mtu_discovery
net.inet.tcp.slowstart_flightsize
net.inet.tcp.local_slowstart_flightsize
net.inet.tcp.newreno
 net.inet.udp.checksum
net.inet.udp.log_in_vain
net.inet.udp.blackhole
net.inet.udp.maxdgram
net.inet.udp.recvspace
(usrRoot: MMU configuration failed, errno = %#x
 utstar
bQbbezcRQS
 gfff/tyCo/
Adding %ld symbols for standalone.
IPv4
 L6!  u
/null
(0@-
(p@-
(sysFlashWriteEx: sector %d base error
sysFlashWriteEx: ERROR writing to flash: pF=%08X, len=%d, off=%08X
 get the flash base in sysFlashGet
get the sector number of nvram in sysFlashGet
get the base addr of the nvram sector in sysFlashGet
(0@-
tShell
sysRestoreConsole: ERROR resuming shell task
tLogTask
sysRestoreConsole: ERROR resuming log task
 sysFlashTaskCleanup: ERROR deleting FlashTask
sysReadHeader: ERROR reading size
sysReadHeader: ERROR reading addr
 into FlashTask
sysFlashTask: FIOGETNAME ioctl failed
sysFlashTask: ERROR opening console port %s
sysFlashTask: ERROR closing console port %s
sysFlashTask: ERROR getting shell task id
sysFlashTask: tShell task can not be suspended
sysFlashTask: ERROR getting log task id
sysFlashTask: tLogTask task can not be suspended
sysFlashTask: flashSectorAddr failed
sysFlashTask: ERROR reading
sysFlashTask SECTOR_SIZE_CMD: ERROR bad size
sysFlashTask SECTOR_SIZE_CMD: Address(0x%x) out of range
sysFlashTask SECTOR_SIZE_CMD: Bad Sector
sysFlashTask READ_CMD: Address(0x%x) out of range
sysFlashTask READ_CMD: ERROR bad size
sysFlashTask WRITE_CMD: Address(0x%x) out of range
sysFlashTask WRITE_CMD: ERROR bad size
sysFlashTask WRITE_CMD: ERROR reading data
sysFlashTask WRITE_CMD: FlashWrite Failed
sysFlashTask FLASHTASK_SW_VERSION_CMD: read SW version Failed
sysFlashTask FLASHTASK_INIT_DEFAULT_CMD:saveNamePsw Failed
sysFlashTask FLASHTASK_INIT_DEFAULT_CMD:_Load_MMI_Tbl or setDefaultParam Failed
sysFlashTask FLASHTASK_READ_PSID_CMD:_GetPSID Failed
sysFlashTask FLASHTASK_READ_ADMINPSW_CMD:TftpGetDefaultValue Failed
sysFlashTask FLASHTASK_READ_ENCKEY_CMD:TftpGetDefaultValue Failed
sysFlashTask FLASHTASK_READ_HASHDIR_CMD:TftpGetDefaultValue Failed
sysFlashTask FLASHTASK_READ_TFTP_DOMAIN_CMD:TFTPConfigGet Failed
sysFlashTask: Unknown command(0x%x)
sysFlashTask: exiting
 ERROR: SO Writer state is not set by MMI !
tsysFTask
ERROR: taskSpawn(sysFTInit) failed
(p@-
(0@-
(0@-
(sysRtcGet: RTC Clock not running
sysRtcGet: RTC Clock not enabled
sysRtcGet: mktime() error
RTC date: %s
 sysRtcSet: RTC Clock not running
sysRtcSet: RTC Clock not enabled
sysRtcSet: mktime(2k) error
sysRtcSet: mktime() error
sysRtcSet: secs %d
sysRtcSet: secs2k %ld
sysRtcSet: can't set time before 1 JAN 2004
RTC_Ptr->SECONDS_COUNTER: %d
(p@-
(0@-
(0@-
CVUUU0@-
rtc_set_test: RTC Clock not running
rtc_set_test: RTC Clock not enabled
RTC_Ptr->SECONDS_COUNTER: %#x
rtc_set_test SET OK!
(p@-
(pllInit: NO RTC Clock - can't switch
pllInit: Unsupported clock frequency (%lu)
start hwFeedWDT process
 wdStart feed_timer failed
after hwWatchDogReset TIMER_Ptr->CONTROL &=~0x100 is 0x%x
hwWatchDogReset  TIMER_Ptr->WT_COUNT is 0x%x
hwWatchDogReset  TIMER_Ptr->COUNT_RATE is 0x%x
hwWatchDogInit TIMER_Ptr->INT_ENABLE is 0x%x
(k%u P 
 go into kpd_long_press,g_key_press_flag is %d
(unknown key pressed
unknown keynum
 660-820 mAh Battery
(0@-
(gfffx
(/dev/psc: *** Ringer Stopped in ringer_ctrl***
/dev/psc: *** Ringer Started in ringer_ctrl***
/dev/psc: SET_LED_BRIGHTNESS %u in psc_ioctl
/dev/psc: SET_BACKLIGHT %u in psc_ioctl
(0@-
(`h	(`~
(Current handset Charging Current are following:
g_pscChgCurrent[%d] is %d ;   
Current handset Battery volume are following:
g_pscBatVol[%d] is %d ;   
Current handset Battery and Charging param are following:
Current battery_charging is %d:
Current wart_connected is %d:
Current charging_allowed is %d:
Current g_Power_State is %d:
Current charge_timeout_stopped is %d:
Current overcharge_timer_started is %d:
Current handset Battery voltage is %d:
 0@-
(0@-
(0@-
`h	(Charging temperature exception
ADC_AUX2 is %d,battery is missing
ADC_AUX2 is %d,battery is missing or temperatrue abnormal
 battery volume is %d,
(enter into in Bat_low_process,step 2
IsBatteryNormal: wdCreate Battery_low_lcd_timer failed
multikey should be g_multikey_state is %x 
(RPCM_Ptr->RESET_STATUS  is 0x%x
is_watchdog_reset is 0x%x
after RPCM_Ptr->RESET_STATUS  is 0x%x
after is_watchdog_reset is 0x%x
(/dev/psc
(Lithium Ion Battery Table
--- Table Entry %2u --------------------------------------
 Lithium Ion Type: %u
 Description: "%s"
 End of Charge Current: %u.%03uv
 Min Temp for Charge:   %u.%03uv
 Max Temp for Charge:   %u.%03uv
---------------------------------------------------------
Battery In Use: Table Entry %u
 pscSetBatteryCurrent: illegal table entry
Battery Entry %u: End of Charge Current ADC value set to %u
Hornet VoWifi, ARM946ES (LE) Factory Firmware
 1.2/0
 Enable RTC interrupts
(0@-
(Copy
Error getting MAC address
NOTICE: Your system will reboot after the MAC address is successfully changed
Old MAC address = 
%02x:
%02x
Enter new MAC address (separated by ':') > 
Error: Multicast/Broadcast MAC address entered (must be unicast)
Updating MAC Address in EEPROM.  Please wait ...
Error in writing to EEPROM
Rebooting now
Invalid MAC address len
wlcEnable ERROR, wlcCardInserted() failed
(IDCode                 = %08x
CacheType              = %08x
ControlReg             = %08x
DataCacheable          = %08x
InstructionCacheable   = %08x
WriteBufControl        = %08x
DataProtection         = %08x
InstructionProtection  = %08x
Protection region %2u   = %08x
 Enter Date (MM/DD/YYYY): 
Invalid Date
Enter Time (HH:MM:SS):   
Invalid Time
 sys date: %s
Usage: date ["YYMMDDhhmmss"][1][-1]
(DSP awake
 DSP asleep
(sysPause: RTC Clock not running - can't pause
sysPause: semBCreate failed
enter into new sys pause mode
charging go into sleep, keyInt is %d,
( **** System shutdown requested ****
 **** System power on ****
sysWrite: ERROR writing
 sysRead: ERROR reading from console
 sysReadExact: ERROR reading exact
 charging is %d in charge_sleep
enter into charge_sys_pause 1
enter into syspause if( charging ) change the UART baud to match the clock
resync time when we return from pause
 flashUp: WatchDog timeout - FlashUpdate aborted
 flashUp: PROGRAM Addr ERROR: Abs Address %08X
flashUp: PROGRAM Sector ERROR: Sector #%3u, Abs Address %08X
flashUp: PROGRAM: Sector #%3u, Abs Address %08X
 0@-
(flashUp: ERASE Addr ERROR: Abs Address %08X
flashUp: ERASE Sector ERROR: Sector #%3u, Abs Address %08X
flashUp: ERASE Addr ERROR: Sector #%3u, Abs Address %08X
flashUp: malloc error
flashUp1: ERASE: Sector #%3u, Abs Address %08X
flashUp: ERASE ERROR: Sector #%3u, Abs Address %08X
flashUp: PROGRAM ERROR: Sector #%3u, Abs Address %08X
 DoThisFLASH 
flashUp: LOGIN occurred
 flashUp: LOGOUT occurred
 flashUp: Rebooting ... 
 flashUp2: ERASE: Image could not erase sector %u
flashUp3: ERASE: Sector #%3u, Abs Address %08X
flashUp: ERROR erasing Sector #%3u, Abs Address %08X
flashUp: ERASE_end: Sector #%3u, Abs Address %08X
 flashUp: PROGRAM: Image could not fit into FLASH
flashUp: PROGRAM Addr ERROR: Sector #%3u, Abs Address %08X
flashup: ERROR programming addr %08X, offset %08X, len %d
(Comparing checksums: total bytes received=%d
flashup: ERROR! checksum does not match. Computed from TCP: 0x%08X, Computed from flash:0x%08X
 recv_exact: peer sock shutdown
ERROR receiving data from socket
 netFlashUp: semBCreate flashUpdateSem failed
netFlashUp: wdCreate flashUpdateWdog failed
tNetFlashInfo
netFlashUp: Unable to create socket
netFlashUp: Unable to bind socket
netFlashUp: Unable to listen on socket
netFlashUp:before accept sockt
netFlashUp: Unable to accept on socket
netFlashUp:after accept sockt
netFlashUp: Receive data from socket failed
netFlashUp: peer sock shutdown
netFlashUp: LogoutOccurred and return top loop
netFlashUp: netMessageHandler failed
netFlashUp: Finish from above loop and will continue accept client's request
 handleNetLoginMessages: recv error
(p@-
(ERROR: base sector number for program image wrong
ERROR: erasing sector %d, addr=%08X
Erased sector %d, addr=%08X
(ERROR program offset=%08X, length=%d
flashup: PROGRAM: Sector %d, Sector Base %08X
(Please send your info
netDiscoverMessage: Password mismatch
 wvlan0
wvlan
Get MAC address failed
WARNING: Can not get cookie to wvlan0
ERROR sending DISCOVER RESPONSE to requestor
DISCOVER RESPONSE sent out successfully
 flashEraseImage: semBCreate flashUpdateSem failed
flashEraseImage: wdCreate flashUpdateWdog failed
ERROR getting flashUpdateSem
TFTP process exit by user in flashEraseImage 
flashUp4: ERASE: Sector #%3u, Abs Address %08X
flashUp4: ERASE_end: Sector #%3u, Abs Address %08X
flashup: ERROR erasing sector %d, base addr: %08X
Begin decompressing...
flashup: Image size info error (0x%08X)
flashUp:sec_end = %d, flashsecnum = 0x%x.
Begin decompressing3...
ERROR erasing working image
ERROR: Can not allocate enough memory for inflate
1.1.4
%s error: %d
inflateInit
total_out = 0x%x
flashup: ERROR writing to flash.
inflate
 NOT DEFINED ERR: err = %d.
total_out = 0x%x.
inflateEnd
Begin decompressing5...
 flashUp: PROGRAM: Sector #%3u, Base %08X, offset=%08X, numBytes=%d
flashup: SUCCESS writing to flash.
_EraseAllFlashDataSection is error
 0@-
Beyond the range when _GetRamFsData
_GetRamFsData ERROR!!!!!
Get _GetRamFsData 0x%08X error is %d in _GetRamFsData
 Beyond the range when _WriteRamFsData
_WriteRamFsData ERROR!!!!!
Write RamFsData 0x%08X error in _WriteRamFsData
_WriteRamFsData OK!
_WriteRamFsData %d in RecordAddress 0x%08X   in _WriteRamFsData
Get Rtc error in _GetRtc
Get Hour format error in _GetRtc
 p@-
 Set Rtc error in _SetRtc
MsgQMAIN = msgQCreate is error
(send Battery_Send2MainMsgQ is error
send Battery_Send2MainMsgQ is ok
 send Ate_Send2MainMsgQ is error
send Ate_Send2MainMsgQ is ok
 send PwrOn_Send2MainMsgQ is error
send PwrOn_Send2MainMsgQ is ok
 send Charge_Send2MainMsgQ is error
send Charge_Send2MainMsgQ is ok
 send KeyMsg is error
send KeyMsg is ok
 **********the system boot type is: %d************
enter  Main_Process bloop ok
enter loop, receive msg error, 
enter loop,after receive , newMsg.type is %d
after fuzhi , main_evtType is %d
enter switch , main_evtType is %d
get msg battery buff is %s,
get msg battery volume is %d,
get msg POWERON_MAIN,
Factory mode
g_Power_State is %d
tApp
get msg CHARGE_MAIN,
tDds
tPause
(enter into Main_Start
Main_initMsgq is error
maintaskInit
create maintaskInit is error , Task_Main_id is %d
tPscInit
create pscInit is error , Task_pscinit_id is %d
creating task pscinit is ok
 dumpdata
Exception Dump:
---------------------------------------------------------------
Task Name  : %s
Task ID    : 0x%x
Vector Num : 0x%x
Timestamp  : %d:%d:%d %d-%d-%d
0x%08x %-15s+%-3x: 
unknown
0x%08x %s (
0x%x
0x%08x %s
----------------------------------------------------------------
No Exception Dump Data
 <%s> pc=0x%x  return_pc=0x%x  nagrs=%d
log_dump
<%s> level=%d over range
<%s> tid=0x%x
exception_dump
<%s> tid=0x%x does not suspend
 ramfilesystem003
Fail to read ramFs flag from flash!
 Fail to save ram file system to flash!
 Fail to invalidate flash ram fs flag!
 Fail to load ram file system from flash!
P?(<%s> Load from flash OK!
ram_fs_flash_init
<%s> ReInit flash disk at 0x%x...
<%s> ramDevCreate Fail!
<%s> ramDevCreate OK!
flash
<%s> dosFSDevCreate failed! status=%d
<%s> dosFsDevCreate OK
<%s> ram_fs_read_from_flash fail!
<%s> Create flash disk at 0x%x...
<%s> dosfsVolFormat failed! status=%d
<%s> dosfsVolFormat OK
 <%s> Can't create ram block device!
ram_fs_ram_init
<%s> Create ram disk device OK!
<%s> dosFSDevCreate OK
 flashcan not be checked or could not be repaired
%d, status: %d, count: %d 
 t_Sec_timer_task
create Task_Sec_Timer_id is error , Task_Main_id is %d
(Delay timer is full,g_Delay_num is %d 
 g_SecTimer[%d] is Started Failure
SecTimer Queue is full, g_Timer_num is %d
SecTimerDelete is error, g_Timer_num is %d, TimerID is %d
 Alert the cb is NULL, %d
 0@-
(VxWorks
5.5.1
VxWorks5.5.1
Jun 19 2006, 16:08:57
unknown compression method
invalid window size
incorrect header check
need dictionary
incorrect data check
incompatible version
buffer error
insufficient memory
data error
stream error
file error
stream end
need dictionary
1.1.4
invalid block type
invalid stored block lengths
too many length or distance symbols
invalid bit length repeat
PC2,0
PC2,
PC2,0
 0@-
invalid literal/length code
invalid distance code
C2,0
C2,0
C2,0
C2,0
invalid distance code
invalid literal/length code
  inflate 1.1.4 Copyright 1995-2002 Mark Adler 
oversubscribed dynamic bit lengths tree
incomplete dynamic bit lengths tree
 oversubscribed literal/length tree
incomplete literal/length tree
oversubscribed distance tree
incomplete distance tree
empty distance tree with lengths
-12:00
-11:00
-10:00
-09:00
-08:00
-07:00
-06:00
-05:00
-04:00
-03:30
-03:00
-02:00
-01:00
00:00
+01:00
+02:00
+03:00
+04:00
+04:30
+05:00
+05:30
+05:45
+06:00
+06:30
+07:00
+08:00
+09:00
+09:30
+10:00
+11:00
+12:00
+13:00
the authentiaction flag check failure use default value,  0x%x
(network Config menu
SIP Config menu
RTP&VoiceMail Config menu
NAT Config menu
DSP Config menu
Jitter Buffer menu
Wireless&PPPoE  menu
SSID&KEP menu
Vendor menu
Misc  menu
call feature
Ctrl Parameters 1
syslog&TFTP Ctrl parameters
SIP timer & stun Ctrl parameters
Ctrl Parameters 2
Save and exit
Exit
Use current settings
Use default settings
Modify current settings
0123456789
 %u.
 -0123456789
.0123456789
 80[
 TFTP three default parameters invalid, need reset 
Before TFTP three default parameters reset 
After TFTP three default parameters reset 
? (1=Yes)
 (%ld to %ld)
? (1=Yes,0=No)
[%s]
Alert the time zone string is NULL!!
 [%s]
[NULL menu id]:
[NULL item id]
 **UNACCEPTABLE ****  :%s
NULL
"%s"
[NULL item data]
 Unable to save configuration settings to NVRAM; values valid this session only
Saved configuration settings to NVRAM
No values have been changed
 Unable to clear NVRAM configuration settings
Cleared NVRAM configuration settings; session settings unchanged
 **********Session configuration settings**********
<DemoInitPhoneParam> the boot parameters error, set them to empty and reboot now
<DemoInitPhoneParam> the boot parameters is OK
size of phone parameter: %d
read from RAM failed!
time zone %d
-500
Replaced %d unacceptable items with defaults. and save all the config data to flash
error: item %d, lenght :%d, content %s,
SAVE data ok!
65535
-128
-32768
32767
 set DemoCfg to zero.....
reading from FLASH....
(<FindAP>take net search semaphore failure
<FindAP> exit DDS mode
<FindAP>cann't find AP reset the WiFi module and find again
<FindAP> enter DDS mode
<FindAP> wifi duration: %d
have been initialize...
cann't create a binary semphone
 call back to pm for registring
call back to pm for connecting fail
call back to pm for connecting
set: %d, read : %d
 test_gmt
hi, this is the %d times test
this,function will change the nike name
Write a value to flash need: %d msecond
(IP: %s
gate way: %s
IP Mask: %s
DNS IP : %s
 code_order is %d,%d,%d,%d
*( K
 Error getting MAC address
%02x-
%02x
.txt
<SetSelectParamDefault> failure, don't change the parameters in flash
<SetSelectParamDefault> OK, set %d items to default value
 tryConn2AP
 can't save user name
can't save user password
WIFI setting: can't save data to flash..
WIFI setting: save data ok..
 DHCP work mode
Reserved Parameter
tftp.config.com
0.0.0.0
tftp file
tftp encKey
Terminal IP Address
Terminal subnet mask
255.255.255.0
Terminal Gatewate IP address
Primary DNS Server IP Address
Second DNS Server IP Address
DNS Server IP address source
Exit this menu
SIP terminal use outbound proxy
SIP terminal use register
sipserver.com
SIP proxy Domain Name
sipproxy.com
SIP proxy IP address
SIP proxy port
5060
SIP register Domain Name
sip.register.com
SIP register IP address
SIP register port
SIP terminal user name
username
SIP terminal pass word
password
SIP terminal port
SIP terminal use Null packet
SIP terminal use DNS
Terminal audio RTP port
10010
Terminal audio Packetize time
Jitter buffer compensate size
Mail access num
Mail box num
Mai box psw
www.nat.server.com
8000
use STUN
g711u
g711a
g726
g729a
Reserved Codec
Max Connections
Max buffer size packets
Max latency packets
Max hold threshold %
Min buffer size packets
Min stable events
HWM grow rate %
HWM shrink rate %
Silence timer
Wifi work mode
AP1 PSK
UTStarcom
AP2 PSK
AP3 PSK
AP4 PSK
www.pppoeserver.com
SSID1
SSID2
SSID3
SSID4
WEPKey11(5Btyes)
WEPKey12(13Btyes)
WEPKey21(5Btyes)
WEPKey22(13Btyes)
WEPKey31(5Btyes)
WEPKey32(13Btyes)
WEPKey41(5Btyes)
WEPKey42(13Btyes)
Vendor Name
Enterprise Code
Product ID
F1000
Model Name
Wifi parameters data structure Version
Display Name
Set Repeat Dial on busy flag
Set Reject Anonymous flag
Set Call Waiting flag
Set Caller ID block flag
Set Registration duration
Set Call Transfer
Wepkey select 
00001111
3way flag
Auto scan interval
Primary NTP Server Domain name
ntp.nasa.gov
Secondary NTP Server Domain name
Primary NTP Server IP
198.123.30.132
Secondary NTP Server IP
NTP server port
NTP Server DNS flag
Enable NTP
Time zone offset
NTP synchronize Interval
36000
Syslog server port
Syslog  duration
Syslog server Domain name
syslog.server.com
Syslog server IP address
Syslog Server name Flag
Syslog Level
TFTP Resync Period
Upgrade Error retry delay
Configuration Server FQDN
Configuration Path
F1000/
Config protocol
tftp
Encrypt Key
Firmware Upgrade Server FQDN
Firmware Upgrade Path
Firmware File name
vxworks_romresident.bin.z
Upgrade protocol
Administrator password
Factory reset password
Current Config Filename
Sip authentication string
authstring
Manually config SIP timer
4000
5000
TimerB
32000
TimerF
TimerH
TimerD
TimerJ
Stun server port
10000
Stun server
stun.server.net
Autosan flag
DST flag
Incoming call timer
DTMF transfer mode
Outgoing call timer
Set Repeat Dial on busy interval
Set Repeat Dial on busy counts
DNS Query type
HTTP authentication website
www.baidu.com
dump flag(debug only)
exit dds, cmd: 0x%x
alread exit dds
 enter dds, cmd: 0x%x
alread enter dds
(0.8.9.0
 Error getting MAC address
%02x
(cann't read  %d AP profile
WPA failure g_ssidIndex: %d
<AutoScan>can't connect to %s 
<AutoScan>user active AP- %d 
DHCP Success!
Get DHCP Parameter Success!
DHCP Failure!
Get DHCP Parameter Failure!
can't connect to AP stored in flash,try connect to open AP!
Connected to open AP failure !
Connected to an open AP success, start SIP stack!
Connected to AP that stored in flash, start SIP stack!
<ARP:AutoScan>arpResolve error,gate way: %s
 <SetSSIDAndWepKey> parameter error
SSID: %s, WepKey: %s,wep key index:%d,auth_mode:%d
<SetSSIDAndWepKey>: WLDesiredSSIDSet() error
<SetSSIDAndWepKey>: WLDefaultKeysSet() error
<SetSSIDAndWepKey>: WLTXKeyIdSet() error, key index: %
<SetSSIDAndWepKey>: WLEncryptionEnabledSet() error
AppInit: WLAuthenticationSet() error
Wifi encryption enabled
Wifi encryption disabled
<SetSSIDAndWepKey>: WLApply() error
<SetSSIDAndWepKey>: end 
 <ReadSSIDAndWepKey> num excess range %d
wepkeyselect string is %s, flag:%d,num:%d
(found  %d  open AP
oh,gee, can't connect to open AP %s
 <TryConnect2AP> user active AP-%d
connting fail
tPause
auto scan interval:%d sec
 ram/wpa.cfg
<AppInit> wpa config file name: %s
AppInit: wdCreate call_disconnect_timer failed
AppInit: Local Interface = %s
wvlan
wvlan0
AppInit(): Unable to create message queue
1. semaphore creation failed
AppInit: successfully hooked Wi-Fi notify
AppInit: WLAPModeSet() error
Wifi Station name='%s'
AppInit: WLOwnNameSet() error
Setting Wifi channel number to 0 (take default)
Use DHCP flag = %u
Setting Use DHCP = 1 (default)
Setting Use PPPoE = 0 (default)
AppInit: Unable to determine current IP address
AppInit: Unable to determine current IP subnet mask
%d.%d.%d.%d
AppInit: Unable to reset route
Successfully deleted old routes
AppInit: Unable to use given IP address; reverting to bootline
Successfully got IP mask='%s' = 0x%lx
AppInit: Unable to use IP subnet mask given in Phone Params, default to 0xFFFFFF00
AppInit: localIPAddr %s, IPMask %s
AppInit: Failed to set IP Mask for '%s'
AppInit: Failed to set IP Addr for '%s'
Attached TCP/IP interface to %s unit %u
AppInit: Could not get local IP address
0.0.0.0
-q delete -net 0.0.0.0
-n add -net 0.0.0.0 %s
AppInit: route,gate way ip addr %s
AppInit: Unable to add route to default IP gateway
Successfully set route to default IP gateway
AppInit: Unable to use Gateway IP address, no default route added
SIP DNS Resolver Init Failed
SIP DNS Resolver Init succeeded,current sip domain name is '%s',dns ip is '%s'
123456
AppInit: DSPAPI Manager configuration failure
AppInit: Error in creating DSPAPI decoder[%u]
AppInit: Error in creating DSPAPI encoder[%u]
 !!! DSP Software Version: %lx !!!
 Jb General configuaration failed
 JB Jitter configuartion failed
Wifi Authentication Type: Open System
Wifi Authentication Type: Shared Key
Error getting PPPoE Service Name
Error getting PPPoE User Name
Error getting PPPoE Password
Starting PPPoE
ERROR starting PPPoE
PPPoE FAILED
error reading LOCT_NET_DNS_IPAddr2 from flash
Second DNS Server IP (from flash) = '%s'
resolvParamsSet for second(+) DNS addr(s) FAILED
Local IP Number = %d.%d.%d.%d
tAPRoaming
StackMonitor
tSNTPClient
(AppInit: sntpcTimeGet() returned errno %d
AppInit: Unable to retrieve time from SNTP Server @ %s
 Waiting for WiFi connection to start PPPoE
Waiting for WiFi connection to do DHCP
Starting DHCP negotiation
ERROR Getting DHCP parameters, trying again
 ppp1
ifunit ERROR: Device named "%s" doesn't exist.
<GetDhcpParameters> before ifunit....
Calling dhcpcLeaseCleanup
Calling dhcpcInit
dhcpcInit ERROR: Unable to obtain DHCP lease
GetDhcp: Error reading Vendor Name
GetDhcp: Error reading Vendor Enterprise Code
GetDhcp: Error reading Vendor ProdCat Name
GetDhcp: Error reading Vendor Model Name
GetDhcp: Error reading Vendor Version number
dhcpcOptionSet _DHCP_DNS_SERVER_TAG FAILED
dhcpcOptionSet _DHCP_DNS_DOMAIN_TAG FAILED
dhcpcOptionSet _DHCP_ROUTER_TAG FAILED
dhcpcOptionSet _DHCP_VENDOR_SPEC_TAG FAILED
dhcpcOptionAdd _DHCP_CLASS_ID_TAG FAILED
GetDhcpParameters: Could not get PPPoE assigned local IP address
Using IP address of %s from PPPoE for DHCP INFORM
dhcpcInformGet returned ERROR=%d - errno=%d
ERROR Getting DHCP parameters, re-trying
GetDhcpParameters: Could not get PPPOE assigned IP subnet mask
Calling dhcpcBind...
after calling dhcpcBind, use %d s(tick),  %d (time)
dhcpcBind returned ERROR=%d - errno=%d
GetDhcpParameters: Could not get DHCP assigned local IP address
GetDhcpParameters: Could not get DHCP assigned IP subnet mask
Got parameters from DHCP server
localipaddr is %s 
Netmask from DHCP or PPPoE = %s
Got Option 43 parameters, decoding...
With Option43: Domain Name='%s'
Option43: DNS SERVER ADDR len (%d) != 4, INVALID!
%u.%u.%u.%u
Option43: DNS Server IP = '%s'
With Option43: DNS Resolver Init Failed,current dns_server_ip is '%s,dname is '%s''
FIELD_TYPE_CA_DOMAIN 
FIELD_TYPE_CA_ADDR 
Option43:SIP Proxy Domain Name='%s'
Option43:SIP Proxy IP ADDR len (%d) != 4, INVALID!
Option43:SIP Proxy IP ADDR = '%s'
Option43: SIP Proxy PORT len (%d) != 2, INVALID!
Option43: SIP Proxy PORT = %u
Option43: SIP Terminal PORT len (%d) != 2, INVALID!
Option43: SIP Terminal PORT = %u
Option43:SIP Registar Domain Name='%s'
Option43:SIP Registar IP ADDR len (%d) != 4, INVALID!
Option43:SIP Registar IP ADDR = '%s'
Option43: SIP Registar PORT len (%d) != 2, INVALID!
Option43: SIP Registar PORT = %u
Option43:SIP Redirect Domain Name='%s'
Option43:SIP Redirect IP ADDR len (%d) != 4, INVALID!
Option43:SIP Redirect IP ADDR = '%s'
Warning: Unknown Option43 type=%u skipped
dhcpcOptionGet _DHCP_VENDOR_SPEC_TAG FAILED, checking standard DHCP values
dhcpcOptionGet _DHCP_DNS_DOMAIN_TAG FAILED, using flash config value
GetDhcp: Error reading Domain Name from flash !
no option 43,SIP domain name is '%s'
DHCP domain name return is '%s'
dhcpcOptionGet _DHCP_DNS_SERVER_TAG FAILED, using flash config
GetDhcp: Error reading  DNS server ip address from flash !
no option 43,SIP dns server ip is '%s'
DNS SERVER len (%d) < 4, INVALID!
DNS Server IP = '%s'
no option 43,DNS Resolver Init Failed
Secondary DNS Server IP (from DHCP) = '%s'
error reading LOCT_NET_DNS_IPAddr1 from flash
Tertiary DNS Server IP (from flash) = '%s'
Fourth DNS Server IP (from flash) = '%s'
Tertiary DNS Server IP (from DHCP) = '%s'
Fourth DNS Server IP (from DHCP) = '%s'
dhcpcOptionGet _DHCP_ROUTER_TAG FAILED
ROUTER ADDR len (%d) < 4, INVALID!
Gateway IP Addr = '%s'
GetDhcpParameters: Unable to add route to default IP gateway
(recieve a disconnect event
 doing autoscan 
same subnet, continue wait for disconnected event
AP are roaming now, find available AP !
we are roaming now
 RestartPppoe: doing ifconfig wvlan0 down
wvlan0 down
RestartPppoe: ifconfig down error
RestartPppoe: doing ifconfig wvlan0 up
wvlan0 up
RestartPppoe: ifconfig up error
RestartPppoe: calling pppoeOpen
RestartPppoe: waiting for result of pppoeOpen (PppoeStatus)
PPPoE restart FAILED
ReStarting DHCP negotiation
DHCP not in use, checking WifiConn
Calling ATSendWifiConn
PPPoE complete, but No WiFiConn ???
Agere SIP Release %u.%u.%u
Agere SIP Release %u.%u
AppMain: Failure initializing application.
before taskSpawn sysPause
after taskSpawn sysPause
(dspPowerOff 
(ateDspPowerOff
(before dsp power on 
dsp power on 
 AppShutdown() was called
 AppBattery() was called
wf notify type: 0x%x
(wvlan%d) CFG_LINK_STAT.
WiFi Connected
WiFi Link Status : Connected
(wvlan%d) Link Status : Connected
WiFi Disconnected
WiFi Link Status : Disconnected
(wvlan%d) Link Status : Disconnected
WiFi Access Point Change
WiFi Link Status : Access Point Change
(wvlan%d) Link Status : Access Point Change,WiFiConn=%d
WiFi Access Point Out of Range
WiFi Link Status : Access Point Out of Range
(wvlan%d) Link Status : Access Point Out of Range,WiFiConn: %d
WiFi Access Point In Range
WiFi Link Status : Access Point In Range
(wvlan%d) Link Status : Access Point In Range,WiFiConn:%d
(wvlan%d) Link Status : UNKNOWN (0x%04x)
(wvlan%d) CFG_SECURITY_STAT.
(wvlan%d) Security Status : Dissassociate [AP]
(wvlan%d) Security Status : Deauthenticate [AP]
(wvlan%d) Security Status : Authenticate Fail [STA] or [AP]
(wvlan%d) Security Status : UNKNOWN (%u)
%02x:%02x:%02x:%02x:%02x:%02x
(wvlan%d) STA Address: %s
(wvlan%d) Reason : 0x%04x 
(wvlan%d) CFG_WMP.
(wvlan%d) CFG_NULL, mailbox empty.
Alert... SSID: %s, the lenght of it exceed: %d
%s has wepkey,discard it
cann't take net search semaphor
%s - WPA
ssid: %s signal: %d,encry_flag %d, recv num %d
Alert, the SSID table is full , received SSID: %s
probe rep length: %d
(wvlan%d) Unknown = 0x%04x.
 SendEventToApp: Could not get buffer.
 %s[%d]:Error in reading JB maximum connections
populate_jbGenCfg
%s[%d]:Error in reading JB maximum size
 %s[%d]:Error in reading Jitter max latency
populate_jbJitterCfg
%s[%d]:Error in reading Jitter max theshhold
%s[%d]:Error in reading Jitter buffer size
%s[%d]:Error in reading JB min stable time
%s[%d]:Error in reading JB grow rate
%s[%d]:Error in reading JB shrink rate
 Silence suppression[%d]
 %s:%s[%d]
Buffer allocation failed
y:/wfm10/02software/05code/ipphone/src/mgcpdemo/demomgcpat.cpp
endConn
Message Sending Failed
Unable to get the msg Bufer
Too few Arguments
 AppInit: Error reading DNS enable flag !
AppInit: Error reading  DNS server ip address !
AppInit: Error reading registar Domain Name !
AppInit: Error reading registar IP !
AppInit: Error reading proxy Domain Name !
AppInit: Error reading outband proxy usage !
AppInit: Error reading registar usage !
AppInit: Error reading SIP User  Name !
AppInit: Error reading SIP User  Password !
AppInit: Error reading Proxy Port !
AppInit: Error reading registrar Port !
AppInit: Error reading terminal Port !
AppInit: Error reading RTP Port !
AppInit: Error reading STUN server hostname !
AppInit: Error reading STUN enable flag !
AppInit: Error reading STUN service Port !
AppInit: Error reading Caller Id Flag !
123456789
AppInit: Error reading registar duration !
registar duration :%d
Flag of use TIMER configuration :%d
T1 :%d
T2 :%d
T4 :%d
Timer B :%d
Timer F :%d
Timer H :%d
Timer D :%d
Timer J :%d
 Error getting Comm Quality
MON COMM QUAL ERROR? comsQual=%d, strength=%d.
wifi strenght : %d
< MonitorWifiStrength> can't start wifi strenght monitor watch dog timer...
 dnsflag: %d,dns: %s, IP: %s
 Error, value of dns flag :%d
flag is %d
nikename: %s
out going CallerID_block_mode: %d
in comming CallerID_block_mode: %d
RTP packet size: %d
call waiting flag: %d
Authen name : %s
transfer flag: %d
set_sip_config finish...
 set_stun_params(...) stunServer = %s, stunPort = %d, stunflag =%d
set_stun_params finish...
(unloading SIP stack...
unload SIP stack success
 loading SIP stack...
fail to global_init!
fail to activate_stun_result, so, fail to load SIP stack!!!
load SIP stack success
 <RefleshDhcpParam> get DHCP error...
 tResetNetParam
 <ARP:demomgcpat>arpDelete ok
<ARP:demomgcpat>arpDelete error
<ARP:demomgcpat>%2x.%2x.%2x.%2x.%2x.%2x, arpResolve ok
<ARP:demomgcpat>arpResolve error
 arpResolve failure, localGwAddr:%s
(dhcpHandle is NULL!
DHCP current state: %d
the DHCP server don't response lease renew request, start auto scan process
push DHCP FSM in: %d s
 start push DHCP FSM in: %d s
 WEPKEY : %s
WLDefaultKeysSet() error
WLTXKeyIdSet() error
AppInit: WLEncryptionEnabledSet() error
WLReset() Error..
(wirelesslab2000
wirelesslab2001
wirelesslab2002
 utstarcom2000
 SSID: %s, WepKey: %s
<SetSSIDAndWepKey>: WLPortTypeSet() error
<SetSSIDAndWepKey>: WLCreateIBSSSet() error
<SetSSIDAndWepKey>: WLChannelSet() error
<SetSSIDAndWepKey>: WLTXKeyIdSet() error
<SetSSIDAndWepKey>: WLReset() error
GetDhcpParameters : %s
failure
 charge#$%
open wpa config file faliure: %s
network={
scan_ssid=0
ssid="%s"
auth_alg=OPEN
key_mgmt=NONE
auth_alg=SHARED
wep_key0=%s
wep_key1=%s
wep_key2=%s
wep_key3=%s
wep_key0="%s"
wep_key1="%s"
wep_key2="%s"
wep_key3="%s"
wep_tx_keyidx=%d
proto=WPA
pairwise=TKIP
group=WEP40 WEP104 TKIP
pairwise=CCMP
group=WEP40 WEP104 TKIP CCMP
key_mgmt=WPA-PSK
psk="%s"
psk=%s
psk length overflow (>64 or <8)
AP authentication mode error
hermes
<createDisk> error no memory
<createDisk> error creating RAM disk
<createDisk> error formatting RAM disk %s
 Primary Major    : %d
Primary Minor    : %d
Primary Variant  : %d
Primary Comp ID  : %d
Tertiary Major   : %d
Tertiary Minor   : %d
Tertiary Variant : %d
Tertiary Comp ID : %d
can open WPA configuration file %s
opening (and printing) WPA configuration file %s
WPACFG - %s
(break DHCP process
 <task1> take  the sem1
<task1>  take  the sem2
<task1>  release sem1
<task1>  release the sem2
 <task2>   take the sem2
<task2>  take the sem1
<task2>  release the sem2
<task2>  release the sem1
(gfff
InitDSP: Failure creating DSP manager.
(PlayTone() called:
DIAL TONE
BUSY TONE
RINGBACK TONE
ALERT TONE
OFF-HOOK TONE
CONGESTION TONE
RINGER TONE
Low Battery when Talking Alert Tone
PlayTone: Bad tone.
PlayTone: Setting input to HANDSET output to HANDSET
PlayTone: Setting input to HEADSET output to HEADSET
PlayTone: Setting input to HANDSET output to SPEAKERPHONE (wrong?)
calling dspMgr->playTone()
(StopTone() called
StopTone: Setting input to HANDSET output to HANDSET
StopTone: Setting input to HEADSET output to HEADSET
StopTone: Setting input to SPEAKERPHONE output to SPEAKERPHONE (wrong?)
( PlayDTMF: Bad tone.
Transmit dtmf by rfc2833.
Transmit dtmf in band.
Transmit dtmf out band.
tDtmf
PlayDtmf: Unable to spawn DtmfBurst
(tRinger
PlayRing: Unable to spawn CycleRinger
 StopRing() called
(dspLoopbackTask: dspMgr not initialized
dspLoopbackTask: dspApiDecoder[0] not initialized
dspLoopbackTask: dspApiEncoder[0] not initialized
dspLoopbackTask: starting
dspLoopbackTask: setCodecType(DSP_CODER_G711)
dspLoopbackTask: setAudioSource(DSP_INPUT_HANDSET)
dspLoopbackTask: setAudioOutput(DSP_AUDIO_TO_HANDSET)
dspLoopbackTask: setAudioSource(DSP_INPUT_MUTE)
dspLoopbackTask: setAudioOutput(DSP_AUDIO_TO_MUTE)
dspLoopbackTask: exiting
*** dspLoopback already stopped
*** dspLoopback already started
Usage: dspLoopback( n )
                    n: 0 = stop loopback
                       1 = start loopback
tDspLoop
 atedspLoopbackTask: ateDspMgr not initialized
ateDspLoopbackTask: dspAteDecoder not initialized
ateDspLoopbackTask: dspAteEncoder not initialized
ateDspLoopbackTask: starting
ateDspLoopbackTask: setCodecType(DSP_CODER_G711)
ateDspLoopbackTask: setAudioSource(DSP_INPUT_HEADSET)
dspLoopbackTask: setAudioOutput(DSP_INPUT_HEADSET)
ateDspLoopbackTask: setAudioSource(DSP_INPUT_HANDSET)
ateDspLoopbackTask: setAudioSource(DSP_INPUT_MUTE)
ateDspLoopbackTask: setAudioOutput(DSP_AUDIO_TO_MUTE)
ateDspLoopbackTask: exiting
*** ateDspLoopback already stopped
*** ateDspLoopback already started
Usage: ateDspLoopback( n )
tAteDspLoop
 ate_dsp_init: DSPATE Manager configuration failure
ate_dsp_init: Error in creating DSPATE decoder[%u]
ate_dsp_init: Error in creating DSPATE encoder[%u]
 dbgRingerDrv
 TURN ON RINGER HW 
 Ringer Driver Initialization Fail 
 Ringer Driver De Initialization Sucessful 
 TURN OFF RINGER HW 
++-- RINGER ON --++
++--  RINGER OFF --++
++--  RINGER Always OFF --++
 TURN ON VIBRATOR 
 Vibrator Driver Initialization Fail 
 Vibrator Driver De Initialization Sucessful 
 TURN OFF Vibrator HW 
++-- VIBRATOR ON --++
++-- VIBRATOR OFF --++
++--  VIBRATOR Always OFF --++
 Vibrator Driver Initialization Sucessful 
 Ringer Driver Initialization Sucessful 
+-- SWITCH ON RINGER --+
+-- SWITCH ON VIBRATOR --+
(dbgPlaymelody
*****dbgPlaymelody task not found, try to re create it!*****
*****Recreate dbgPlaymelody task failed, reboot now!*****
*****Restart task dbgPlaymelody failed, reboot now!*****
 VSpeakerSwitch: Unable to turn off Mic.
VSpeakerSwitch: Unable to turn on speaker.
headsetOn is %d,headsetSelect is %d in _VHandsetDSPSwitch
(headsetOn is %d,headsetSelect is %d in _VHeadDSPSwitch
pppoe stack add complete
StackAddComplete: calling pppConnectionOpen
(pppOe1StackAddErrorCallback: Error adding Stack 0x%x
(pppoe stack delete complete
(pppoe stack delete error
(pppoe open complete
(pppoe closed
Deleting secrets database
Deleting PPP stack
(pppOe1SysProfile
_remove_SIO_ADAPTER
_remove_ASYNC_FRAMING
lcp_ACCM
Local:
Remote:
lcp_ACFCompression
lcp_fcsAlternatives
lcp_PFCompression
ipcp_vjcParams
muxDevName
wvlan
muxDevUnit
muxSvcType
0x8864:0x8863
lcp_MRU
Local:Negotiation Required,Negotiable:1492
Remote:Negotiation Required,Not Negotiable:1492
Local:Range:576,1492,0
Remote:Range:576,1492,0
 pppOE_connectionMode
pppOE_svcName
lcp_authProtocol
Local
Remote
Remote:Negotiation Not Required,Not Negotiable:c223
Remote:Alternate:c023
chap_localUserName
pap_localUserName
ipcp_ipAddr
Local:Negotiation Required,Negotiable:
Remote:Negotiation Required,Negotiable:
pppOe1ClientConfig: failed to add the stack 
 calling pppConnectionClose
pppoe stack pointer is null, nothing to close
 pppoeOpen: checking PppoeCloseInProgress flag (=%d)
pppoeOpen: calling pfwStackAdd
pppoeOpen: failed to add the stack 
pppoeOpen: pfwStackAdd successful, stack should be starting PPPoE
(/dev/psc
pscGetVersion
 pscSetBacklight
 pscGetBacklightDelay
 pscSetBacklightDelay
 pscGetLedBrightness
 pscSetLedBrightness
 pscGetAccSupply
 pscSetAccSupply
 pscSetRinger open error
pscSetRinger ioctl error
 pscSetVibrator open error
pscSetVibrator ioctl error
 pscGetVibratorMotor
 pscSetVibratorMotor
 pscGetLidSwitch
 pscGetMainPwrSwitch
 pscGetADC
pscGetADC: VBAT=%0.3fv CHRG=%0.3fv AUX1=%0.3fv AUX2=%0.3fv
 pscRead
pscRead: 0x%lx 0x%04lx
 pscWrite
pscWrite: 0x%lx 0x%04lx
(KeypadMonitor: Failure to create message queue.
KeypadMonitor: Could not get buffer.
KeypadMonitor: Failure reading from KeypadQ.
KeypadTask: Digit 0 key event
KeypadTask: Digit 1 key event
KeypadTask: Digit 2 key event
KeypadTask: Digit 3 key event
KeypadTask: Digit 4 key event
KeypadTask: Digit 5 key event
KeypadTask: Digit 6 key event
KeypadTask: Digit 7 key event
KeypadTask: Digit 8 key event
KeypadTask: Digit 9 key event
KeypadTask: * key event
KeypadTask: # key event
KeypadTask: clear key event
KeypadTask: left key event
KeypadTask: right key event
KeypadTask: up key event
KeypadTask: down key event
KeypadTask: SEND key (old off hook) event
KeypadTask: S2 key == redial key event
KeypadTask: S3 key event
KeypadTask: S4 key event
KeypadTask: S5 key event
KeypadTask: S6 key event
KeypadTask: S7 key event
KeypadTask: END key (old on hook) event
KeypadTask: LID open event
KeypadTask: MAIN Power OFF event
KeypadTask: Volume up key event
KeypadTask: Volume down key event
KeypadTask: @ key event
KeypadTask: Phonebook key event
KeypadTask: Yes/Select key event
KeypadTask: Charging event
KeypadTask: LOW Battery event
Unhandled keycode=%u found in KeypadMonitor
KeypadTask: Charge complete event
KeypadTask: LID closed event
KeypadTask: MAIN Power ON event
KeypadMonitor: MQSend errno %d
KeypadMonitor: MQSend errno %d (loop=%d)
KeypadMonitor: Could not get buffer after 10 tries.
 Alert, mg_add_read_msgq() is called...  but this function isn't implement...
 Unable to get msg buff
Message sending failed 
Message sending succeded 
 Opt. Ringer
 !!! ERROR :-  RingerStart !!!
 !!! ERROR :-  VibratorStart !!!
 syslog: unknown facility/priority: %x
<%d>
[%s]
(tSyslog
(gfff
(gfff
(Create the local log message queue error,exit !!!
(tLocalLogTask
 %m/%d/%y %H:%M:%S
(port:%d, sessid: %d,dspGetTid: 0x%x,dspPutTid: 0x%x,socketReadTid: 0x%x
<saveRTPSession> Alert, rtp port :%d
<clearJb>: forget to close the RTP, close it now
 p@-
(p@-
%s[%d]:Failed in fetching connection Index
JbCntrlReq
(getJbConMask
(jbConReq: Max connections (%u) exceeded
jbConReq: jbConnCb buffer alloc failed
jbConReq: jBuff buffer allocation failed
jbConReq: buffer allocation failed
The capi buffer allocated = %d
The txcodec[%d]	rxCodec[%d]
The maxAlSduFrames[%d]
The Remote Ptime[%d]
tGetMgr%d
tPutMgr%d
tJbReadMgr%d
%s[%d]Unsupported payload type, %d 
codec2numframes
 JbConModReq
  TxPacketCount = %d; RxPacketCount = %d, RxDelayCount = %d ,
RxLostCount = %d , RxMaxDelay = %d 
 tRtp_Stat
Rtp Satistics Initialize Success!!!
(This call rtp packet statistics information :
 TxPacketCount = %d; RxPacketCount = %d, RxDelayCount = %d ,
   				 RxLostCount = %d , RxMaxDelay = %d 
jbReadSOcket is spawned
%s[%d]:Rfc2833 Event List initialization failed
jbReadSocket
%s[%d]:Memory allocation error
Rfc2833EventTimerQ
%s:%d:TIMER_COOKIE_NULL
%s[%d]: Invallid rtp fd context
proc_rcvd_messg
<<< (2) Buff Size Needed %d >>>>
<proc_rcvd_messg>  alert , receive a empty RTP packet, discard it!
****************************
%s[%d]:the numframes[%d] for the codec[%d]
jbDspGetManager
<jbDspGetManager> discard a zero RTP packet: nframe :%d, size:%d
 Unsupported Codec[%d]
%s:%d:Event List initialization failed
jbDspPutManager
LongSilenceTimerQ
%sProcessing received codec failed
 Connection no more exists
%s[%d]: Memory allocation failed
JbStartTimer
Error: Starting the timer failed
%s:NULL Context.
JbStopTimer
%s:The connection index is %u
jbProcessLongSilence
%s:%d:Error - non TIMER_EXPIRED message
LSTimerCallBack
%s:%d:Long silence timer message process failed
Case when CTS == LRTS
%s[%d]:Timer is already cancelled
process_rfc2833_event_pack
%s[%d]:The duartion now is %d
Error:Starting the timer failed
Case when CTS > LRTS
%s[%d]:Playing the rcvd DTMF digit,%d - DSP EVENT = %d
%s[%d]:The duartion is %d
%s[%d]:Unsupported RFC2833 Event
%s[%d]: DTMF timer expired
TeleEvTimerCallBack
%s[%d]: DTMF timer expired on the line %d
(0@-
(JbInsertPacket: buf truncated from %u to %u
 JbRemovePacket: buf cropped from %u to %u
(0@-
the next_port = %d
%s[%d]:RTCP Initialization failed
init_rtp
%s[%d]:canonical name is null.RTP process terminated
open_rtp_session
Malloc Failure
%s[%d]:udp ports creation failed
[%s]:The sesion id is %x
%s[%d]:session is already present
%s[%d]:rtp context is not allocated
(Unknown session id %d
Unknown session %d
 <close_rtp_session>: after get the sem!
close_rtp_session:send_rtcp_sesscmd() failied
/nclose_rtp_session:Msg sent to RTCP thread sucess
<close_rtp_session>: after unlock the sem!
<close_rtp_session>: 1!
<close_rtp_session>: 2!
<close_udp_ports>: rtpport is: %d!
<close_rtp_session>: 3!
 Invallid session, %x
======> Going to read RTP packet
%s[%d]:failed receiving RTP packet
parse_rtp_pack
Receive failed due to
RTP Header compr enabled fd = %d
%s[%d]:rtpevents updated sucessfully
%s[%d]:rtpevents parsing failed
%s[%d]:No telephony events included
Memory allocation failure
sockfd = %d, packsize = %d payload_len = %d
pack start = %p, payload start = %p, pack end = %p
v = %d, p = %d, x = %d, cc = %d, m = %d, pt = %d, seq = %d
ts = %0x
ssrc = %x
 Invallid Session %d
large payloadsize %d
Failed to send udp message, error = %d
 Memory allocation failure %d
 %s[%d]: packets sent for the session[%d] = %u
get_packcount_sent
 %s[%d]: octets sent for the session[%d] = %u
get_octetcount_sent
 %s[%d]: packets received for the session[%d] = %u
get_packcount_rcvd
 get_octetcount_rcvd
 get_jitter_val
 get_avtran_delay
%s[%d]:null pointer email addr
set_email_addr
%s[%d]:zero length string
%s[%d]:Memory allocation failed
%s[%d]:Email addr set sucessfully
%s[%d]:null pointer uname
set_uname
%s[%d]:user name set sucessfully
%s[%d]:null pointer phno
set_phno
%s[%d]:Phno set sucessfully
%s[%d]:null pointer location
set_location
%s[%d]:location set sucessfully
%s[%d]:RTP event pack size is 0
parse_rtpevents_pack
%s[%d]:Memory allocation failure
%s[%d]:Unsupported RTP event, %d
%s[%d]:No events to set
send_rtpteleph_events_pack
Memory Allocation Failure
%s[%d]:Memory Allocation Failure
%s[%d]:Unsupported RTP event 
RTP EVENTS PACK
===================
EVENT = %d
VOLUME = %d
EDGE = %d
RESERVED = %d
DURATION = %d
%s[%d]:Sent rtp event pack sucessfully
%s[%d]:Received RTP events pack freed sucessfully
clear_rtp_events_pack
 <create_udp_ports>: rtpfd is: %d, local port: %d!
RTPERROR
%s[%d]:Could not open RTP fd with port number %d
create_udp_ports
%s[%d]:Could not join the multicast group
%s[%d]:Failed in fetching interface ip addr
RTCPERROR
%s[%d]:Could not open RTCP fd with port number %d
h	(`
%s : Error : calloc fail.
reserve_port
%s : Index = %d
%s : Too short RTP port range.
 %s : port =  %d, Index = %d
release_port
%s :  Found used_port_p->port = %d
%s : Internal error : port not in use %d
 Failed to send udp message, error = %d
%s[%d]:Unsupported payload type
encap_rtp_payload
%s[%d]:Could not fetch ntptimestamp
start of the packet=0x%x	end of the packet=0x%x
sockfd = %d, packsize = %u payload_len = %d
pack start = %p, payload start = %p, pack end = %p
v = %d, p = %d, x = %d, cc = %d, m = %d, pt = %d, seq = 0x%xts = 0x%x
ssrc = 0x%x
%s[%d]: VALLID RTP EVENT, %d 
validate_rtp_event
%s[%d]: IN VALLID RTP EVENT
%s[%d]: Non vallid arguements
hash2getsessid
%s%u
 Sendto failed
full message not sent
 Invalid state parameters -- %s 
receive_udp_msg
========> Going to read UDP Packet
=======> I am not able to read UDP packet
recvfrom failed fd = %d
========> No of bytes read from socket  = %d
		 RTCP Thread start 
rtcp_timer_queue
rtcp_init:TIMER_COOKIE_NULL
%s[%d]:Timer API initialized sucessfully
proc_rtcp
timerqid = %d
 %s:%d:Error - non TIMER_EXPIRED message
rtcp_proc_timeout_event
proc_rtcp:Failed processing timer message
Timer message processing succeded
proc_rtcp: memory allocation failure
proc_rtcp:Failed in receiving message
Received RTCP message
proc_rtcp:Failed processing rtcp fd
RTCP fd processing succeded
h	(l=
 Bytes to read failed
proc_rtcp:memory allocation failure
Error : no message received
Awaiting for the incoming message
The received message length = %d
rcvd rtcp message processing failed
rcvd rtcp message processing succeded
%s[%d]:invallid session id
get_rtcp_fd
rtcp_msg_queue
<send_rtcp_sesscmd>: before MessageSendQueue!
send_rtcp_sesscmd:MessageSendQueue() failied
<send_rtcp_sesscmd>: after MessageSendQueue, FALSE!
<send_rtcp_sesscmd>: after MessageSendQueue!
send_rtcp_sesscmd:Message sent to RTCP thread sucessfully
%s[%d]: Message Queue creation failed
create_rtcp_msgq
RTCP Message queue is created sucessfully
RTCP Message queue ID is %d
%s[%d]:rtcp messageQ creation failed
rtcp_init
%s[%d]:RTCP initialized sucessfully
 tRtcp
Could not spawn RTCP thread
%s[%d]: ERROR: Exceeds the supported range for fd's (1 - 64)
set_rtcp_fds
remote source info initialization succeeded
updated remote source info sucessfully
remote source info updation failed
 check_req_sdes_items
%s:source descriptor is a null pointer
%s[%d]:Mandatory canonical name is not present
%s[%d]:Invallid RTCP packet
isvallid_rtcp
%s[%d]:Break the while
%s[%d]:RTCP packet is Vallid
%s[%d]:Failed in fetching local IP address
get_sessid
%s[%d]:rtcp session id = 0x%x
Received command message from RTP
%s[%d]:invallid session id
proc_rtcpfd
 RTCP FD is set
%s[%d]failed in processing rtcpfd
Error :No timer context exists
proc_time_out
%s[%d]failed in time out message
 RTCP timer cancelled sucessfully
RTCP RR build failed
RTCP RR
====================================================
=====================================================
RTCP BYE build failed
RTCP BYE
===========
=============================================
proc_rtcpfd_close
Send Failure: Could not send RTCP BYE
Sent RTCP BYE Sucessfully
%s[%d]:no sdes items
build_rtcp_pack
%s[%d]:Unknown packet type
%s[%d]:Memory allocation failure
%s[%d]:RTCP encapsulation failed
%s[%d]:RTCP build succeded
%s[%d]:bye buffer is null
print_rtcp_bye
ver = %d
padding = %d
source_count = %d
pack_type = %d
pack_len = %d
ssrc = %x
%s[%d]:rtcp buffer is null
print_rtcp_sr
ver = %d
padding = %d
remote_count = %d
pack_type = %d
pack_len = %0x
local_ssrc = %0x
ntp_ses = %0x
ntp_fra = %0x
rtp_ts = %0x
packet_sent = %0x
octetsent = %0x
---------Report Block - %d-----------
rem_ssrc = %0x
packets lost since last SR/RR = %d
packts lost from start = %0x
Last SeqNo = %0x
Jitter = %0x
lsr = %0x
dlsr = %0x
 print_rtcp_rr
pack_type = %d
pack_len = %d
local_ssrc = %0x
remote_ssrc = %0x
 print_rtcp_sdes
ver = %d
padding = %d
source_count = %d
Item No %d
item_type = %d
item_length = %d
data = %s
%s[%d]: memory allocation failure
concatinate_buffers
 rtcp_2char
%s[%d]:timer context is not allocated
fill_timer_context
Error: Starting the timer failed
RTCP SR build failed
RTCP SR
==================================================
================================================
=================================================
===============================================
RTCP SDES build failed
RTCP SDES
compute_rtcp_packet
%s[%d]:No sdes info available
=================================================
RTCP PACKET SENT SUCESSFULLY
%s[%d]:failed to fill timer context
%s[%d]:RTCP transmission interval timer Started
Remote port not set
Destination address/port not known
UDP FAILURE:
%s[%d]Failed to send udp message, error = %d
send_rtcp_pack
%s[%d]rtcp pack send failed
Sender report encapsulation failed
Receiver report encapsulation failed
sdes encapsulation failed
rtcp BYE encapsulation failed
 Not handled presently
 Unknown RTCP packet type
 encap_rtcp_rr
 encap_rtcp_sdes
%s[%d]:src descriptor is null
%s[%d]:Invallid length of sdes packet
%s[%d]:Invallid len of sdes pac
 encap_rtcp_bye
 encap_rtcp_sr
%s[%d]:remote source info is null
encap_report_block
%s[%d]Received RTCP message is NULL
proc_rcvd_rtcp
parsing the RTCP packet failed
parsing the RTCP packet succeeded
%s[%d]:Invallid RTCP packet
parse_incoming_rtcp
%s[%d]:RTCP SR packet rceived
%s[%d]:error in parsing RTCP sender report
%s[%d]:parsing RTCP sender report succeeded
%s[%d]:RTCP RR packet received
%s[%d]:error in parsing RTCP receiver report
%s[%d]:parsing RTCP receiver report succeeded
%s[%d]:RTCP SDES packet received
%s[%d]:error in parsing RTCP sdes
%s[%d]:parsing RTCP sdes succeeded
%s[%d]:RTCP BYE packet received
%s[%d]:error in parsing RTCP bye
%s[%d]:parsing RTCP bye succeeded
%s[%d]:RTCP packet APP received
%s[%d]:Unknown RTCP packet type
Memory allocation failure
The length is ZERO
Received RTCP SR information
====================================
========================================
The length is %u
---------Report Block-----------
ssrc = %0x
packts lost from start = %0x
Received RTCP RR information
======== RECEIVED RTCP SDES ========
pack_type = %d
pack_len = %d
remote_ssrc = %0x
%s[%d]:Failed to add the sdes info
parse_rtcp_sdes
============END OF SDES============
 add_sdes_item
==========CNAME=========
type = %d
length = %d
cname = %s
=========UNAME============
type = %d
length = %d
uname = %s
=========E-MAIL=============
type = %d
length = %d
email = %s
=========PHONENO============
type = %d
length = %d
phno = %s
=========LOCATION=========
type = %d
length = %d
location = %s
%s[%d]:Received unknown sdes item
====================================================
REVEIVED RTCP BYE from  ssrc = %x
======================================================
Could not start the timer
Started RTCP transmision interval timer sucessfully
 RTS: Hermes init failed
Error comparing ifw_section0 memory write at location %d
Error comparing ifw_section1 memory write at location %d
(RTS: base addr not set
ERROR downloading intermediate firmware
EepromRead failed
FillRecords failed
Update PDA failed
e	(P
Invalid Parameters
RTS - Failed getting RID 0xFD01
RTS - Not enough RAM buffer size
%d  %x, %x
 p@-
X	(NULL pointer
X	(** Failed Locate %x
 ** PDA_Append **
** PDA_Append() : Failed locating record
 p@-
** Record absent, append record
Append record failed !!
Different length in new and old record
PDA_Update(): Failed locating record
(%02x 
 base addr not set
wvlan0 not stopped
Error getting MAC address
NOTICE: Please reboot your device after the configurations are successfully updated
ERROR Channel List selection! (Values should be from 0 to 2
Error: Multicast/Broadcast MAC address entered (must be unicast)
Updating MAC Address in EEPROM.  Please wait ...
EEPROM update failed
EEPROM update successful
Finished updating entire EEPROM, please reboot your device
Invalid MAC address len
 DESC LIST ( seq = %d, port %d )
DESC LIST 0x%08x (%d bytes)
(0x%04x): 
%02x 
        
 MBLK ( seq = %d, port %d )
MBLK 0x%08x (%d bytes)
 >>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>>
PUT_LTV(wvlan%d)
GET_LTV(wvlan%d)
LEN          = 0x%04x
TYP          = 0x%04x
VAL (0x%04x) = 0x%04x
<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<
(ERROR (wvlanLoad): initString is equal to NULL
wvlan
ERROR (wvlanLoad): pBSP is equal to NULL
initString is %s
ERROR (wvlanLoad): wvlanParseInitString returned 0x%x
ERROR (wvlanLoad): params.hwType is unknown
ERROR (wvlanLoad): malloc pDev failed
%s%d
ERROR (wvlanLoad): semMCreate returns null for pDev->lock
ERROR (wvlanLoad): wvlanOorInitialize returned 0x%x
ERROR (wvlanLoad): wvlanNetMBlkInit returned 0x%x
ERROR (wvlanLoad): msf_connect returned 0x%x
ERROR (wvlanLoad): wvlanGo returned 0x%x
Agere Systems WaveLAN 802.11 END Driver v1.7.3.0003
ERROR (wvlanLoad): END_OBJ_INIT returned 0x%x
ERROR (wvlanLoad): END_MIB_INIT returned 0x%x
MCASTADDRDEL: %02X:%02X:%02X:%02X:%02X:%02X.
ERROR (wvlanMCastAddrDel): wvlanSetMCastAddr returned 0x%x
 ERROR (wvlanMCastAddrGet): etherMultiGet returned 0x%x
 MCASTADDRADD: %02X:%02X:%02X:%02X:%02X:%02X.
ERROR (wvlanMCastAddrAdd): etherMultiGet returned 0x%x
ERROR (wvlanStart): wvlanEnable returned 0x%x
(%s%d): wvlanIoctl(unknown or unhandled = 0x%x).
 0@-
 (wvlanInterruptHandler): pDev->rxF.mblk == NULL 
 !!!mBlkPktHdr.len (%d) > sizeof( data )!!!
DDS mode
ERROR (wvlanTx): hcf_send_msg returned 0x%x
ERROR (wvlanPollSendPort): WVLAN_MODE_POLLING or WVLAN_STARTED not set 
ERROR (wvlanPollSendPort): wvlanTx returned 0x%x
 ERROR (wvlanPollReceivePort): WVLAN_MODE_POLLING | WVLAN_STARTED not set
 ERROR (wvlanGo): dhf_download_fw returned 0x%x
ERROR (wvlanGo): hcf_get_info returned 0x%x
Hermes MAC Address of %02x:%02x:%02x:%02x:%02x:%02x
 p@-
(wvlan%d) Device ID 0x%02x
ERROR (wvlanGetPriRecords): hcf_get_info(CFG_FW_IDENTITY) returned 0x%x
(wvlan%d) Primary F/W Component ID %d, Variant %d, Version %d.%d
(wvlan%d) Tertiary F/W Component ID %d, Variant %d, Version %d.%d
ERROR (wvlanGetPriRecords): hcf_get_info(CFG_NIC_IDENTITY) returned 0x%x
(wvlan%d) NIC Component ID %d, Variant %d, Version %d.%d
 ANY
 ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_SYSTEM_SCALE) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_OWN_CHANNEL) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_MICRO_WAVE) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_MCAST_RATE) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_OWN_NAME) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_AUTHENTICATION) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_RTS_THRH) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_PORT_TYPE) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_TX_RATE_CNTL) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_PM_ENABLED) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_MCAST_RX) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_MAX_SLEEP_DURATION) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CREATE_IBSS) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_DESIRED_SSID) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_OWN_ATIM_WINDOW) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_HOLDOVER_DURATION) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_NIC_MAC_ADDR) returned 0x%x
ERROR (wvlanPutLtv): hcf_put_info(CFG_CNF_OWN_SSID) returned 0x%x
 ERROR (wvlanSetEncryption): hcf_put_info(CFG_CNF_ENCRYPTION) returned 0x%x
 ERROR (wvlanSetWep): hcf_put_info(CFG_TX_KEY_ID) returned 0x%x
ERROR (wvlanSetWep): hcf_put_info(CFG_DEFAULT_KEYS) returned 0x%x
 ERROR (wvlanSetMCastAddr): hcf_put_info(CFG_GROUP_ADDR) returned 0x%x
 0@-
ERROR (wvlanEnable): invalid port or driver mode
WARNING: %s, %d
Z:/wf10/02software/05code/wlandrv/src/wvlanend.c
 ERROR (wvlanDisable): invalid port or driver mode
	pDev address : 0x%x
disable port 0x%08x result is 0x%08x.
 ERROR (wvlanLock): semTake returned 0x%x
 ERROR (wvlanUnlock): semGive returned 0x%x
 ERROR (wvlanIntConnect): pRequestIsr returned 0x%x
 ERROR (wvlanIntDisconnect): pReleaseIsr returned 0x%x
 ERROR (wvlanNetMBlkInit): pDev->pTxList equal to NULL
ERROR (wvlanNetMBlkInit): mClBlkConfig.memArea equal to NULL
ERROR (wvlanNetMBlkInit): clDescTbl.memArea equal to NULL
ERROR (wvlanNetMBlkInit): netPoolInit returns 0x%x
 0@-
 ERROR (wvlanIoctlSetFlags): hcf_put_info(CFG_PROMISCUOUS_MODE) returned 0x%x
 ERROR (wvlanIoctlGetFlags): pFlags equals NULL
 ERROR (wvlanIoctlGetHdrLen): pHdrLen equals NULL
 ERROR (wvlanIoctlGetMib2): pMib2Tbl equals NULL
ERROR (wvlanIoctlGetMacAddr): pMacAddr equals NULL
 ERROR (wvlanIoctlSetMacAddr): pMacAddr equals NULL
ERROR (wvlanIoctlSetMacAddr): drvMode not equal to AP
===========================================================
Unit                 : %d (NOT LOADED!!!)
Unit                 : %d
END_OBJ *            : 0x%08x
IFBP                 : 0x%08x
HCF_TYPE             : 0x%08x
wvlanFlags           : 0x%08x
Chipset              : Hermes 1
Chipset              : Hermes 2
Chipset              : Hermes 2.5 (b only)
Chipset              : Hermes 2.5 (a/b/g)
Chipset              : UNKNOWN!!!
Hardware Bus         : PCI.
Hardware Bus         : PCMCIA.
Hardware Bus         : USB.
Hardware Bus         : UNKNOWN!!!
Driver Mode          : Station, no download.
Driver Mode          : Station.
Driver Mode          : Access Point.
Driver Mode          : UNKNOWN!!!
MAC Address          : %02x:%02x:%02x:%02x:%02x:%02x.
Network Name         : %s.
Station Name         : %s.
Num Tx Buffers       : %d.
Num Rx Buffers       : %d.
txFree               : %d
Encryption Enabled   : N.
Encryption Enabled   : Y.
%02X
WEP Key %d            : %s (%s)
TX Key               : %d.
Channel              : %d
Primary F/W          : %d.%02d
Primary F/W Comp ID  : %d
Primary F/W Variant  : %d
Tertiary F/W         : %d.%02d
Tertiary F/W Comp ID : %d
Tertiary F/W Variant : %d
NIC Component Version: %d.%02d
NIC Component ID     : %d
NIC Component Variant: %d
DDS Mode             : Entered
DDS Mode             : Not Entered
Coms   Quality       : %d
Signal Level         : %d
Noise  Level         : %d
BSSID                : %02x:%02x:%02x:%02x:%02x:%02x
numInts              : 0x%08x
numSkippedInts       : 0x%08x
numRecoveredInts     : 0x%08x
numFalseInts         : 0x%08x
maxIntsDpcdInaRow    : 0x%08x
IFB_IntOffCnt        : %d
numUsedAllFIDs       : %d
numTxFromIsrDpc      : %d
numTxFromSendPort    : 0x%08x
numNoTxFree          : 0x%08x
numEmergencyRx       : 0x%08x
numTxPktsTotal       : 0x%08x
numTxPktsVoice       : 0x%08x
maxTxFrags           : 0x%08x
WME Enabled          : %s
WME Status           : %s
 ERROR (wvlanUilAction): cannot initiate scan
(wvlanUilAction): UIL_ACT_RESET called
(wvlanUilAction): UIL_ACT_APPLY called
dbg---->sleep
dbg----->wakeup
 ERROR (wvlanUilSendDiagMsg): mBlk == NULL
 ERROR (wvlanUilGetInfo): wvlanValidateRIDMode(0x%04x) returns 0x%x
 ERROR (wvlanUilPutInfo): wvlanValidateRIDMode returns 0x%x
ERROR (wvlanUilPutInfo): WVLAN_DDS_ENTERED
dbg--set pm enabled value: 0x%x,  u.u16: 0x%x
(wvlanUilPutInfo): CFG_DRIVER_ENABLE set to %d
ERROR (wvlanKeyCheck): isxdigit failed
ERROR (wvlanKeyCheck): isxdigit+1 failed
 ERROR (msf_connect): IO Base Address equal to zero!!!
AP In Range --> Disconnected
dbg--lastLinkStat %d, IFB_LinkStat: %d, pmEnabled: 0x%x
 wvlanFlags: 0x%x
dbg--DDS flag %d 
dbg--wake up
wvlanUm(): ERROR getting BSSID for new Link
wvlanUm(): WME Status = 0x%04x
wvlanUm(): ERROR getting WME Status for new Link
wvlanUm() Waiting %d seconds for OOR connection
Calling wvlanApplyLight() from the scope of wvlanUm()
 ERROR (wvlanOorInitialize): wdCreate failed for tmrOorWaitForConnection
ERROR (wvlanOorInitialize): wdCreate failed for tmrOorWakeup
 p@-
dbg-- Entering DDS for %d 
fcnTimerOorWaitForConnection(): Entering DDS for %d seconds
fcnTimerOorWaitForConnection(): OOR wait time reset to %d seconds
 fcnTimerOorWakeup(): Issuing DDS wakeup
dbg--Waiting %d seconds for OOR connection
fcnTimerOorWakeup(): Waiting %d seconds for OOR connection
ERROR (wvlanProcessProbeResp): Number of Aps in SRT is %d.
ERROR (wvlanProcessProbeResp): too many APs in scan result table.
ERROR (wvlanProcessProbeResp): Exceeding maximum capacity in scan result table.
(wvlanProcessPMKIDRequest): REASSOC-REQ pending for %02X:%02X:%02X:%02X:%02X:%02X
wvlanProcessPMKIDRequest(): cannot remove PTK
wvlanProcessPMKIDRequest(): cannot remove GTK(%d)
wvlanProcessPMKIDRequest(): cannot remove WEP GTK(%d)
(wvlanProcessPMKIDRequest): ASSOC-REQ pending for %02X:%02X:%02X:%02X:%02X:%02X
ERROR: %s, %d
Z:/wf10/02software/05code/wlandrv/src/wvlanhornet.c
WVLAN sock %d out of range
WVLAN Card Unknown manufacturer/function ID
WVLAN Card incorrect product ID
 Found Hermes PCMCIA card at (%d:%d.%d), slot %d
PCMCIA card Product ID is 0x%04x
wvlan
 unit %d out of range
(wvlanPcmciaRequestISR:%d ERROR: intConnect() failed.
 wvlanPcmciaReleaseISR:%d ERROR: intConnect() failed.
 wvlan
ERROR: %s, %d
Z:/wf10/02software/05code/wlandrv/src/wvlanapi2.c
 0@-
 0@-
 p@-
 0@-
 p@-
 p@-
 p@-
 p@-
 0@-
 p@-
 0@-
 p@-
 0@-
 0@-
 p@-
 p@-
 p@-
(0@-
wvlan
 ERROR: %s, %d
Z:/wf10/02software/05code/wlandrv/src/cardbus/cis.c
(%d:%d.%d) Smart CIS Dump
(offset) is 0x%08x
(code) 0x%02x
(link) 0x%02x
(data) 0x%02x... %c
 (%d:%d.%d) COR  = 0x%04x
(%d:%d.%d) CSR  = 0x%04x
(%d:%d.%d) PRR  = 0x%04x
(0@-
(p@-
h_read: base addr not set
 h_write: base addr not set
 ioctlBatchRead: base addr not set, setting to wlcGetBaseIOAddress()
 ioctlBatchWrite: base addr not set, setting to wlcGetBaseIOAddress()
 RTS - hermes command (0x%04x) failed
RTS - SetBAP failed
RTS - GetRID : buffer len exceeded
RTS - Initialize command response failed
RTS - Initialize command failed
Hermes version: 0x%02x
	 0@-
	 0@-
H		 
8CdspPort
11CdspDecoder
11CdspEncoder
	 ,0
	 0@-
	 0@-
!!! ERROR: DSP16K DRIVER INSTALLATION FAILURE !!!
!!! ERROR: HEADSET INTERRUPT HANDLER FAILURE !!!
dspIsrTask
dspIsr2Task
tDspUdpServer
dspApi: DSP Bootloader Up & Running
	 dspJump: Jump Command Executed
(dspApi: DSP Image Download Complete
 DCC_DSP_WAKEUP Interupt from DSP 
(0@-
%	 p2	 
(|&	 
(0@-
11CdspManager
p2	 
H	 t3	 
3	 \4	 H
(P5	 
`8	 `8	 `8	 `8	 `8	 
8	 `8	 `8	 `8	 `8	 `8	 
|9	 
9	 $:	 
:	 $:	 
=	 p=	 
=	 p=	 
@	 LA	 
A	 H
(`B	 
`F	 `F	 `F	 `F	 `F	 
F	 `F	 `F	 `F	 `F	 `F	 
LJ	 
dI	 
,I	 
8CdspPort
15CdspRootDecoder
15CdspRootEncoder
H	 ,0
H	 0@-
H	 ,0
H	 0@-
H	 @0
H	 DSP Manager Error.
DSP Manager Error: Invalid audio destination.
DSP Manager Error: Invalid tone destination.
DSP Manager Error: Invalid DTMF.
DSP Manager Error: Invalid Tone.
DSP Manager Error: Invalid # of frames.
DSP Manager Error: Invalid buffer pointer.
DSP Manager Error: DSP driver not ready.
DSP Manager Error: Invalid coder type.
DSP Manager Error: Invalid tone direction.
L	 @M	 DSP Manager
M	 DN	 
N	 4O	 
M	 P
O	 dP	 
P	 DQ	 
R	 |S	 $T	 
T	 0@-
(<V	 
Y	 p@-
p`	 H_	 
_	 p`	 
(p@-
k	 Ll	 
l	 |m	 
n	 Do	 
o	 pp	 
p	 Pq	 
q	 0r	 
s	 `t	 
!!! ALERT: Report this message to msing5@agere.com 
Tu	 
(p@-
y	 (z	 (z	 (z	 (z	 (z	 (z	 (z	 (z	 (z	 (z	 (z	 (z	 (z	 
x	 (z	 (z	 (z	 (z	 (z	 (z	 (z	 8y	 (z	 
y	 (z	 xy	 
t{	 
{	 ,{	 
{	 P{	 
(p@-
	 p@-
15CdspRootManager
h	(p
	 \0
(p@-
(---Initializing TEST_APP!--- 
DSP Server: Error Creating data port
---TEST_APP:DSP buffer address table
  MSG-1   addrTbl[%d] = %4.4x
---TEST_APP:Error reading buffer address table from DSP
socket
bind
tsrvSendTask
	 ---Launching TEST_APP!--- 
---TEST APP--- Waiting for Requests
Socket error!!!
recvfrom
 MSG-2    addrTbl[%d] = %4.4x
---TEST_APP:Error reading buffer address table from the IPT_DSP
nBytes = %d
    word%d = %4.4x
sequenceNumber = %d!
Packet was duplicated!
(---TEST APP--- Sending Reply nr %d
---TEST APP--- Sending Reply Playload length %d
 Payload[%d] = 0x%2.2x
	 Processing RTT messages
Reloading Address Table
status=%d
        addrTbl[%d] = %x
---TEST APP---:  Processing Aquarium Requests!!!
---TEST APP---:  Invalid request!!!
Reload Address Table
Reset DSP
(p@-
(---TEST_APP:processRequest()---
command:TESTCMD_TEST_RESET_DSP
command:TEST_MODE_ON
command:TEST_MODE_OFF
command:PUT_BUFFER
    pRequest->length           = %x 
    pRequest->objectId         = %x 
command:GET_BUFFER
   (void *)&pReply->payload[0] = %x 
*ppRequestMsg= %x
*ppReplyMsg= %x
command:PUT_DATA_BUFFER
    address                    = %x 
    pRequest->payload[%d]      = %x 
    lenTbl[pRequest->objectId] = %x 
command:GET_DATA_BUFFER
    objectId                   = %4.4x 
    address                    = %4.4x 
command:POKE_MEM
     objId    = %2.2x 
     addr     = %8.8x 
     len      = %4.4x 
     HED_LEN  = %4.4x 
     dataPort = %8.8x 
command:PEEK_MEM
 After ADD *ppRequestMsg= %x    
 After ADD *ppReplyMsg  = %x    
command:TESTCMD_WRITE_DSP_IMAGE
     objId = %x 
     addr = %x 
     len = %x 
LENGTH ERROR! ---- pRequestMem->length = %x 
ID ERROR! ---- pRequestMem->objectId = %x 
command:TESTCMD_READ_DSP_IMAGE
command:CHANGE_DECODER
     objId                 = %x 
     len                   = %x 
     pRequest->payload[%d] = %x 
command: AIN SET
command: AOUT SET
command:Sec Audio Init
command:CHANGE_ENCODER
---TEST_APP:processRequest()---
    Invalid Command!!!
REPLY ERROR!!!!!!
 !!! ERROR: TcpLogInit - Could not create message queue !!!
TcpLogDaemon 
 !!! ERROR: TcpLogInit - Could not spawn task TcpLogDaemon !!!
TcpLogWriter 
 !!! ERROR: TcpLogInit - Could not spawn task TcpLogWriter !!!
TcpLogReader 
 !!! ERROR: TcpLogInit - Could not spawn task TcpLogReader !!!
(ganges
 !!! ERROR:TcpLogDaemon Error in opening Socket !!!
 !!! ERROR:TcpLogDaemon: Bind failed !!!
 !!! ERROR:TcpLogDaemon: Listen failed !!!
!!! ERROR:TcpLogDaemon: Accept failed !!!
Please enter a password 
Another telnet session is running. 
Entering a password will terminate the other session. 
Connected
Welcome to Debuging Zone
 !!! TcpLogDaemon - Session opened by another user will terminate this session !!!
Telnet session is terminated 
	 %c
!!! ERROR:tcpLogReader - Store Failure !!!
	 p@-
playtone
reboot
dccprint
 System Reboot 
tcpLogHexDump: dumping %d bytes: 
%0*X:  
	 0@-
7CModule
12CListElement
	 0@-
	 l0
5CList
10CMutexList
(p@-
(0@-
(dspWriteToDccControlMessage: WARNING paramBuffer addr (0x%lX) not 16-bit aligned
8CdspPort
16CdspRootDataPort
 0@-
(-----------------------------DNS------------------------------
SRV answer qdcount =%d,ancount = %d, nscount= %d,arcount =%d(%s,%d)
srv_getanswer
resolvDNExpand fail (%s,%d)
SRV answer Domain = %s,type = %d,ttl = %d,dlen=%d!!!(%s,%d)
This answer is %d  , not T_SRV(33)!!!(%s,%d)
SRV answer prority = %d ,weight =%d ,port =%d,target = %s!!!(%s,%d)
resp;vDNExpand fail (%s,%d)
Can't find relate target domain !!!(%s,%d)
SRV answer count = %d , target include ip count = %d(%s,%d)
 The input parameter is NULL !!!(%s,%d)
srvQuery
Start send query message!!!(%s,%d)
Havn't receive  answer packet len = %d!!!(%s,%d)
 The input buffer pointer pbuf is NULL!!!
Resolver begin query for name=%s, !!!
return for finding this alias cycle!!!
return for the alias length exceed the 128 byte!!!
return for exceeding the max query times!!!
Before Invoke the resolvGetHostbyName()!!!
Info  failover = %d, hp = %d ,name=%s!!!
alias[0]=%s,alias[1]=%s,alias[2]=%s,alias[3]=%s
Restart query by alias :%s!!!
resolve failure !!!
<resolv>: get one server ip from DNS srv: %s
The resolver have got the valid ip address for %s!!!
Resolve failure for %s!!!
The resolver is inverse query for %s!!!
(Take the resolver senmphore failure !!!
Begin SRV-Record query procedure !!!
_sip
_udp
SRV-Record query response have no IP Address!!!
SRV-Record query procedure failure!!!
Begin A-Record query procedure !!!
Have been queried the valid IP Address!!!
 ---------------------SRV Record---------------------
Target = %s, priority=%d , weight = %d, ttl = %d, port =%d,addr = %s
hp is : %x
<resolv>: the ttl is: %d.
error: host information for %s not found
 Entering name resolution thread.
<reslover_thread>:WiFiConn is False
Doing asynchronous name resolution.
Very strange transaction, aborting
REGISTER
<resolver_thread>: Register needn't resolv, continue use dest_back[%d].
failover is %d
<resolver_thread>: Request needn't resolv, continue use REGISTER's dest_back[%d].
INVITE
Could not send SIP req since there's no available SERVER IP in list!
<resolver_thread>: Request needn't resolv, continue use dest_back[%d].
<resolv_thread>:NULL osip_t, will continue.
<resolv_thread>: ICT found, resume operation!
<resolv_thread>:Previous ICT killed, will continue.
<resolv_thread>:Should not be here!.
Could not resolve %s.
Could not get the first via header.
DNS resolve success for %s
DNS resolve failed for %s
osipua resolver thread is exiting.
 gfff
retrans: %d, retry:%d, options:0x%x,nscount:%d
 maddr
received
rport
pcore's re_2xx is %u
(No dialog match for this ACK!
 0@-
(<osip_retransmissions_execute>: No ACK arrives, should terminate dialog!
application/sdp
 0@-
SdpHandler: ua is NULL
123456
654321
none
 You must not call sdp_handler_add_*_payload outside the write_offer callback
RTP/AVP
ptime
%i %s
rtpmap
fmtp
%i %i
 audio
 video
 Could not make sdp template!
(<sdp_handler_generate_answer>: remote_o_sess_version = %s ,last_remote_o_version =%s
sdp_handler >after set the last_remote_o_version: remote_o_sess_version = %s ,last_remote_o_version =%s
sdp_handler >after set the last_remote_o_session_id: remote_o_sess_id = %s ,last_remote_o_version =%s
telephone-event/8000
sdp_read _handler >after set the last_remote_o_version: remote_o_sess_version = %s ,last_remote_o_version =%s
sdp_read_handler >after set the last_remote_o_session_id: remote_o_sess_id = %s ,last_remote_o_version =%s
(Call failure code: %d and reason: %s
 anonymous
after process,displayname is %s
A new call, tel num: %s, displayname: %s,call type: %d, lineNum:%d
 The second call incoming, tel num: %s, displayname: %s,call type: %d, lineNum:%d
 Call to %s is accepted, linenumber is: %d.
 Call with %s ends.
<CallTerminatedNtfy>: Line number : %d
 Registering...
 Unregistering...
 registration successful!
unregistration successful!
 registration faillure!
 Please try the new contact: %s
 UDP listener failure!
Ring stops......
 <RingStartNtfy>: Ring starts...... Line number: %d
 Call from %s is rejected!
 Call to %s is canceled!
 Message successfully delivered to %s.
 Message is accepted, but can't guarantee end to end delivery!
 Incoming message from %s!
It saids: %s.
 <202forReferNtfy>: OK!
 <5XXforReferNtfy>: FAILURE!
 <4XXforReferNtfy>: FAILURE!
 <XFER_ReferReceived>: REFER received!: %d
 <XFERLineNumNtfy>: OK, New line number: %d
 <DTMFRecvNtfy>: DTMF received: %d!
fail to initialize webphonecore!
  !	(
T	(8`
 @!	(\X
sip:%s@%s:%d
<UA_Invite_peer>: Line full!
<UA_Invite_peer >: the call type  %d is incorrectly
 ?Replaces=%s%%3Bto-tag%%3D%s%%3Bfrom-tag%%3D%s
<UA_Refer_peer>: NO Session active!
at the end of the ua_refer_peer,szRpls = %s
 <UA_Blind_XFER>: already in refer prog!
<UA_Blind_XFER>: err hold peer!
 <UA_XFER_with_consult>: already in refer prog!
in UA_XFER_with_consult ,lc-szRfAddr = %s
<UA_XFER_with_consult>: err hold peer!
 <UA_XFER_with_consult_resume>: Not in XFER progress, can't continue!
<UA_XFER_with_consult_resume>: Strange scenario... can't continue!
(0@-
( for current call,back call is %x,call is %x,linenum is %x
terminate dialog wrongly
for back call 1,back call is %x,call is %x,linenum is %x
for back call 2,back call is %x,call is %x,linenum is %x
<UA_reject_peer>: NO CALL active!
 set the reg_ongoing flag 0 to 2
(sip:%s:%d
(p@-
(N-@
(p@-
(p@-
(p@-
(lc->ua  = NULL!!!!
sip:%s@%s:%i
update_contact_info_stun(), fail to contact_init!!!
Bad Contact address (%s).
update_contact_info_stun(), after set contact to ua.contact.host =%s
("%s"<sip:%s@%s>
<sip:%s@%s>
 "anonymous"<sip:%s@%s>
(AV profile
<set codec>: add PCMU!
<set codec>: add G726!
<set codec>: add G729A!
<set codec>: add PCMA!
<UA_message_peer>: There are calls in process!
(<UA_call_third_party>: line status not correct!
Set the state as "THREE_WAY_INVITING"
 when THREE_WAY_INVITED,unhold peer
 lc->ReferPhase = %d,linenum = %d,bhold = %d,bHoldStatus = %d
<UA_hold_cb>: bHoldStatus is 603!
<UA_hold_cb>: XFER_OUT,This console is on hold!
<UA_hold_cb>: XFER_BLIND,This console is on hold!
<UA_hold_cb>: XFER_CONSULT,This console is on hold!
<UA_hold_cb>: err in invite!
(gfff0@-
restart SIP stack failure
(The SIP stack task don't find , reboot now!
the task ID of SIP stack don't found now!!!!
SIP stack reset  :%d times
The SIP stack task crashed , restart now!
tResetSIP
Restart SIP stack task failed , reboot now!
maybe the memory is insufficient,can't reset SIP stack...
tResetSyslog
 0@-
(ResetSIP
 net_conf...
sel_if->ip4addr: %s
***********
ringstarted: %d,alert_ringstarted: %d,busy_ringstarted:%d 
address of audiostream: 0x%x,back_audiostream: 0x%x
address of ua: 0x%x,call: 0x%x,back_call: 0x%x
UA info:
UA fromtag: %s
,flags: 0x%x,
UA: dialog_count: %d,max_dialogs: %d,  call_list num: %d
host:%s,port:%d,presence_mode:%d
bInReferProg:%d,bReferMode:%d,ReferPhase:%d
szRfAddr %s
NULL
bCallWaiting:%d,bCallWaitingEnabled:%d,ThreeWayPhase:%d
address re_2xx: 0x%x,ack:0x%x
host: %s,port: %d, socket: %d
device_id: %s,LineInUse[0]:%d,LineInUse[1]:%d
address of RegRecord: 0x%x, ReqRecord: 0x%x
IncomingBlock: %d,bOutgoingBlock:%d
sip config.......
contact:%s
dispname:%s
username:%s
hostname:%s
localip:%s
sip_port: %d
reg_conf.registrar:%s
reg_conf.passwd:%s
reg_conf.addr_of_rec: %s
reg_conf.expires: %d
reg_conf.rtimer: %u
reg_conf.need_rereg: %d
reg_conf.use_registrar: %d
reg_conf.as_proxy: %d
*************
 td_id :0x%d
td_name: %s
td_priority: %d
td_status: %d
td_options:%d
td_entry: 0x%x
td_sp:0x%x
td_pStackBase:0x%x
td_pStackLimit:0x%x
td_pStackEnd:0x%x
td_stackSize:%d
td_stackCurrent:%d
td_stackHigh:%d
td_stackMargin:%d
td_errorStatus:%d
td_delay:%d
exception of SIP task:
vector address: 0x%x
PC: 0x%x
CPSR: 0x%x
NO EXCEPTION
get udp_thread.id TCB failure
td_entry: 0x%x
exception of resolve task:
Could not get destination for transaction: ctx_type=%i
 Could not set destination for transaction: ctx_type=%i
 INVITE
ICT transaction %d created,its call id %s
NULL
REGISTER
CANCEL
MESSAGE
OPTIONS
REFER
NOTIFY
error: dialog==NULL ! 
<ua_transaction_free>: Out dated transaction, delete it.
PING
 ua_transaction_execute: could not get dialog transaction.
<ua_transaction_execute>: BEFORE!
<ua_transaction_execute>: END!
 0@-
INVITE
 rport
received
(REGISTER
Message is REGISTER.
Message is BYE.
CANCEL
Message is CANCEL.
OPTIONS
Message is OPTIONS.
INFO
Message is INFO.
Message is INVITE.
Message is ACK
REFER
Message is REFER
NOTIFY
Message is NOTIFY
Message is %s
Message is NULL Packet.
 <in>REGISTER.
<in>BYE.
<in>CANCEL.
<in>OPTIONS.
<in>INFO.
<in>INVITE.
<in>ACK
<in>REFER
<in>NOTIFY
<in>%s
<in>NULL Packet.
<out>REGISTER.
<out>BYE.
<out>CANCEL.
<out>OPTIONS.
<out>INFO.
<out>INVITE.
<out>ACK
<out>REFER
<out>NOTIFY
<out>%s
<out>NULL Packet.
 OSIP_INFO1,Entering osipua thread.
errno: %d
the sem haven't created..
info: Receiving Message from %s:%u
after htons,sin_port is %d
UDP listener failed while receiving data!
The sip thread is exiting !!!
OSIP_INFO1,Exiting osipua thread.
Sending message to %s:%d:
OSIP_ERROR,error: destination is not an ip address:%s
OSIP_INFO1,warning: using default manager socket to send a message.
OSIP_ERROR,udp_send: could not send message using socket %i: %i
maddr
received
rport
Cannot send response because it has no via field
(0@-
 info: Name resolution requested.
 sip:
<sip:
<sip:%s
sip:%s
%s/%s
 %i %n
sdp has a strange a= line.
%i %i
(software\webphone
current host: %s
current ip %d by retrieve is: %s
 Could not get network interfaces !!
in webphonecore_init(), get_global_rtp_port()=%d
fail to query_stun_for_sipua()!!!
Can't init CAPI! So can't init RTP module!
at the begin of init, osip_t: %x
INVITE_ACCEPTED
FAILLURE
INVITE
INFORMATIVE
at the end of init, osip_t: %x
 can't delete SIP task
can't delete resolve task
delete task
Bad contact url: %s
(application/sdp
Calling < %s >...
Your call to < %s > fails!
webphone_core_invite: Strange scenario! line num & call status dismatch!
current state is INVITING AND set to busy
 Send message to < %s > fails!
Message sent successfully!
 Send option to < %s > fails!
Option sent successfully!
 No dialog to accept.
after osip_dialog_accept_invite!!
clear the prensence mode to ready for second call
after audio_stream_start!
it is a none sdp invite, so not start audio stream here , we should do it after recieve sdp in ack 
Call from < %s > is accepted.
 <webphone_core_terminate_dialog>: Called by AP, should lock mutex!
<webphone_core_terminate_dialog>: before webphone_core_lock!
<webphone_core_terminate_dialog>: after webphone_core_lock!
<webphone_core_terminate_dialog>: Called by AP, should unlock mutex!
before webphone_core_lock
call from %s is rejected!
Ring stops...
CALL is canceled!
<webphone_core_terminate_dialog>: Stop lc->audiostream, linenum: %d
<webphone_core_terminate_dialog>: Stop lc->back_audiostream, linenum: %d
after webphone_dialog_params_destroy!!
in webphone_core_terminate_dialog,after webphone_core_unlock
before osip_dialog_bye!!
after osip_dialog_bye!!
 	(d
Bad proxy or registrar url:%s
Bad address of record:%s
sip:%s@%s:%s
sip:%s@%s
(<webphone_core_hold>: No session active!
 <webphone_core_unhold>: No session active!
PCMU
PCMA
G729A
G726-32
G729AB
1016
H261
TSP0
1015
speex
G7231
telephone-event
AV profile
PCMA
PCMU
G729A
G729AB
1015
G726-32
speex
G7231
(0@-
(0@-
(0@-
(0@-
(sip:%s@%s
 sip:%s@%s:%i
--------------->In webphone_core_update_contact: %s
 127.0.0.1
the expiers is %d
unregistering...
Registrations with local loopback address are forbidden in linphone.
 0@-
 %s <sip:%s@%s>
%s <sip:%s>
sip:%s
A call-leg already exists for this transaction. (%x)
%s has called at %i.
username is %s
displayname is %s
anonymous
<osip_dialog_new_from_incoming_trn>: An anonymous call has been refused!
<osip_dialog_new_from_incoming_trn>: An call with no username or anonymouse username has been refused!
error: Requested user (%s) does not exist.
<osip_dialog_new_from_incoming_trn>: dialog count is %d.
INVITE
MESSAGE
OPTIONS
Unsupported new incoming request.
error - could not create a new dialog_t.
Unkown status code
SIP/2.0
 ACK
CANCEL
application/sdp
text/plain
identity
supported
REGISTER
REFER
PING
NOTIFY
INFO
<osip_dialog_generate_response_default>: no c_addr in offer!
0.0.0.0
<osip_dialog_generate_response_default>: set c_addr failed!
 error: SIP dialog does not exist.
error: could not find last invite incoming transaction
<<---------------OSIP_DIALOG_PING---------------------->>
 <<---------------OSIP_DIALOG_REGISTER---------------------->>
error: You have to specify a registrar.
error: Bad registrar address (%s).
 osip_dialog_register_with_authentification: no password, aborting
error: authen_username is NULL.
error: could not create authorization header.
error: could not build the proxy_authorization header.
Invalid sip address.
error: could not build sip message.
no message body is given!
 before generating_request_out_of_dialog
after generating_request 
after add_body_to_request 
after osip_dialog_send_request
 Replaces
no replaces in refer-to
have replaces in refer-to
origcallee is NULL
The 3way request message is NULL!
set replaces header failed
<osip_dialog_invite_3way>: error clone referred_by!
<osip_dialog_invite_3way>: NULL referred_by!
SIP/2.0/UDP %s:%i;rport;branch=z9hG4bK%u
No authentication header found in 407 to INVITE!
error: could not build the authorization header.
call_leg: %x, wa:%x, wa->auth_type:%x, wa->realm:%x, wa->nonce: %x.
<osip_dialog_invite_with_authentication>: ERROR proxy_authenticate_clone!
 could not build sip message.
 Could not msg_clone() %s
 <osip_dialog_bye>: Do not send CANCEL because we are not in the right ICT state.
<osip_dialog_bye>: current resolv_fifo size: %d!
<osip_dialog_bye>: One trn from resolv_fifo removed!
<osip_dialog_bye>: resolv_fifo size after remove: %d!
osip dialog bye, ict trn id is %d
in recv thread, ict trn id is %d
Could not generate BYE message.
<osip_dialog_bye>: ERROR! Return -1!
 <osip_dialog_hold>: dialog not established!
<osip_dialog_hold>: fail to generate re-INVITE!
<osip_dialog_hold>: no c_addr in offer!
<osip_dialog_hold>: set c_addr failed!
sendonly
 <osip_dialog_refer>: dialog not established!
<osip_dialog_refer>: Bad ReferTo string!
<osip_dialog_refer>: Could not generate REFER message.
<osip_dialog_refer>: fail to generate REFER!
<osip_dialog_refer>: error set refer-to!
 call is 0x%x and its status is %d
<osip_dialog_notify>: dialog not established!
<osip_dialog_notify>: Could not generate NOTIFY message.
<osip_dialog_notify>: fail to generate notify!
SIP/2.0 %d %s
SIP/2.0 %d Unkown status code
message/sipfrag
 caller free route.
 callee free route.
 <generate_ack>: before msg_setcall_id.
max-forwards
<osip_dialog_generate_request_within_dialog>: ERR in osip_create_proxy_authorization_header_indialog!
refer
UTSTARCOM F1000/Device ID-
,   version=
user-agent
 p@-
(not yet established !
 Ack or Cancel cseq does not match !!!!!!!!!!!!!
Request Cseq does not match !!!!!!!!!!!!!
Response Cseq does not match !!!!!!!!!!!!!
call-leg has been found!
WDJ:osip_dialog_respond fail osip_dialog_generate_response_default 
 <osip_dialog_ack>: before generate.
<osip_dialog_ack>: after generate.
  at the begin of generatint request
 prepare the request-line
WARNING: call_leg->from already contain a tag??? 
 before msg_setto
ERROR: callee address does not seems to be a sipurl: %s
o_proxy init error
 before route_free
 after route_free
 after route_set
1000
action
proxy
expires
 0@-
 There is no handler for %s
The handler for %s could not create a new context
 Could not create CANCEL transaction
error: you must not use osip_dialog_send_request() to send acks.
 Could not remove dialog from list.
Could not remove dialog from ua list.
Dialog is removed. It remains %i dialog(s) in the ua list.
Cannot add NULL body context to dialog.
ip_addr
 closing transaction : %x
 error: Failed to init mutex.
 end of manager_destroy
 port already listened
<osip_manager_add_udpport>: recv port differ with send port!
Failed to bind socket !
warning: port cannot be reused.
info: The table of scanned file descriptor is full.
 error: Could not close Udp Port.
 in start_resolver,resolver thread has been created!
 Could not to bind socket for sending messages.
port cannot be reused.
Starting osip stack and osipua layer.
info: Trying to bind on port (%i).
osip_ua_iniit---->SIP DNS INIT OK!
 Shutting down osip stack and osipua layer.
end of osip_global_free()
(You must call osipua_init() before creating a user agent !
 p@-
Could not parse registrar address.
 Could not parse proxy address.
Bad Contact address (%s).
Invalid port number %s.
Primary contact is not decimal ip address: %s !
 Could not remove ua from list.
 INVITE
INVITE_ACCEPTED
FAILLURE
INFORMATIVE
 Invalid alias sip address: %s
 Invalid alias sip address.
 0@-
osip_ua_find 1: %s <> %s 
127.0.0.1
osip_ua_find:  %s <>  %s 
183 stops the ring
 stop ringing.
The call to < %s > is accepted.
<INVITE_CB>: HERE
 Communicating with < %s > ends
bye_cb(),lc back_call is %x
bye_cb(),lc call is %x
(User is busy.
User is temporarily unavaillable.
%s. Retry after %i minute(s).
User does not want to be disturbed.
Call declined.
refuse to fulfill it.
User cannot be found at given address.
Remote user cannot support any of proposed codecs.
retry-after
Authentication failure!
REGISTER
failure cb,clear the reg_ongoing flag 2 to 0
received the 603 and clear the linenum
received the 403 and clear the linenum
Timeout. Remote host is not reachable.
Renewing STUN... Get_global_rtp_port()=%d
fail to query_stun_for_sipua()!!!
Fail to activate_stun_result!
INVITE
Remote host was found but refused connection.
faillure_cb: %s
<faillure_cb>: will do failover, the errnum is %d.
Next server IP addr is %s!
<faillure_cb>: i = %d. No additional IP address to do failover, will do new cycle of DNS lookup.
Clear blind refer flag to EMPTY for invite failure
three way status is %d
dialog linenum is %d,audiolinenum is %d
in failure cb,stop the audiostream
(application/sdp
Error during sdp negociation. Cannot accept incoming call.
Attention, you have a call from < %s >!
Attention, you have a call from unknown place!
(start ringing...
expires
expire
<2xx for registration>: No expire in 2xx!
<2xx for registration>: No CONTACT header in 2xx!
registration successful!
unregistration successful!
g_insleep = %d
after set,g_insleep = %d
No contact information !
User is not reachable, try the following:
< %s >
unsupported informative message.
  !	(
 PCMA/8000/1
GSM/8000/1
PCMU/8000/1
%s/8000
annexb=no
speex
telephone-event
telephone-event/8000
0-15
 MP4V-ES/90000
H263
 payload has no rtpmap.
 remote
Refusing codec %i (%s)
in accept_audio_offer , decide the port for audio , the port is %d
No dialog match for this ACK!
<on_other_invite>: compare session params:
                    prev_audio_params.localport: %d, audio_params->localport: %d.
                    prev_audio_params.pt: %d, audio_params->pt: %d
                    prev_audio_params.remoteport: %d, audio_params->reomteport: %d
                    prev_audio_params.remoteaddr: %s, audio_params->remoteaddr: %s
<analyze_ACK_4_body>: No need to modify session!
audio stream modified!
audio back stream modified!
after audio_stream_start_full!
<analyze_ACK_4_BODY>: Strange scenario, no sdp in this ACK!
 p@-
%s/%i/1
INVITE
OPTIONS
sdp_context_gen_out_req: unable to generate a sdp offer.
application/sdp
 sdp_context_notify_inc_resp: could not parse sdp msg.
 200
sdp_context_gen_out_resp: there is no sdp answer!
<gen_out_resp>: body is:
 sdp_context_notify_inc_req: Could not parse incoming sdp message:%s
<notify_inc_req>: body is:
sdp_context_notify_inc_req: negociation returned: %i
 p@-
md5-sess
 auth-int
auth
<calcResp>: goto authen_withqoponly!
 www_authenticate header is not acceptable.
digest
Authentication method not supported.authorization,current string is %s 
algorithm is %s
Authentication method not supported. (MD5 in creat authrization,current string is %s ).
allocation with authorization_init failed.
Digest
00000001
"0a4f113b"
authentication has qop: %s
"%s"
Unable to get a password: no registration context.
0a4f113b
Response in authorization |%s|
 Authentication method not supported. proxy header,current string is %s 
Authentication method not supported. (MD5 in proxy header).
Response in proxy_authorization |%s|
 wa:%x, wa->auth_type:%x, wa->realm:%x, wa->nonce: %x.
Authentication method not supported. proxy header in dialog,current string is%s
Authentication method not supported. (MD5 in proxy header indialog).
ICT Transaction %i killed. CSEQ: %s
 There is no content-type !
Found body %s
application/sdp
Could not find a body handler.
Creating a new body context.
 OnEvent_New_Incoming1xxResponse!
1xx response for an inexistant call leg! 
Shoud send out CANCEL...
get sdp for response info %d , so to connect audio stream! 
recieved 100 ok
recieved 180 ok
recieved 183 ok
 OnEvent_New_Incoming2xxResponse!
200 OK is probably incomplete!
<ict_2xx_received>: receive 2xx when DIALOG_TERMINATED!
in three_way_invited status
THREE_WAY_OUT,,new rtp port for unhold is %u
<ict_2xx_received>: lc->audiostream is null,after audio_stream_start!
,THREE_WAY_OUT,back_audio,new rtp port for unhold is %u
<ict_2xx_received>: after audio_stream_start!
INVITE
first get sdp in 200 OK , so to connect audio stream! 
<ict_2xx_received>: bNeedModify is: %d
ALERT:<ict_2xx_received>:audio_stream_start_full fail
The call to < %s > is accepted.
<ict_2xx_received>: 200 just inform ap for 183 has opened the audio
<ict_2xx_received>: ALERT never recieve sdp until 200 OK!
<ict_2xx_received>: no new sdp , call ap 
<2xxcb>: before ack.
Sending ACK!
callwaiting enabled so clear presence to 200ready
refer state is %d
lc call is 0x%x and status is %d,lc back call is 0x%x and status is %d
lc call linenum is %d
<ict_2xx_received>: err in osip_dialog_notify!
the call for notify has been byed
ict_2xx:Notify sent out and clear the refer status flag to EMPTY
200 OK for an inexistant call-leg !
 OnEvent_New_Incoming3xxResponse!
3xx response for an inexistant call leg! 
User has moved temporarily.
 OnEvent_New_Incoming4xxResponse!
4xx response for an inexistant dialog! 
User need to authenticate to INVITE!
ict_4xx_received(),407/401 when DIALOG_TERMINATED
<ict_4xx_received>: osip_dialog_invite_with_authentication ERROR!
Authentification aborted.
<ict_4xx_received>: err in osip_dialog_notify!
ict_4xx:Notify sent out and clear the refer status flag to EMPTY
 ict_5xx_received():
5xx response for an inexistant call leg! 
ict_5xx:Notify sent out and clear the refer status flag to EMPTY
 OnEvent_New_Incoming6xxResponse!
6xx response for an inexistant call leg! 
<ict_6xx_received>: err in osip_dialog_notify!
ict_6xx:Notify sent out and clear the refer status flag to EMPTY
ist Transaction %i killed.
 <on_first_invite>: Invitation from myself received!
INVITE for an inexistant dialog !
<on_first_invite> Sending 100 trying.
Retry-After
Error in contact url: %s
Could not create response for current status
There is no content-type !
Found body %s.
Could not find a body handler .
Creating a new body context.
it is a none SDP invite in first_invite!
on_first_invite: error - could not create a 180 Ringing.
on_first_invite: error - could not create a new dialog.
 receiving replaces invite for an existent park call-leg!
<on_replaces_invite> Sending 100 trying.
can not find replace INVITE ua!
on_replaces_invite: error - could not create a 180 Ringing.
<on_replaces_invite>: receive replaces INVITE when DIALOG_TERMINATED!
<on_replaces_invite>:receive replaces INVITE when DIALOG_ESTABLISHED!
in dialog_established state,and after terminate the replaced dialog
after send 200 ok.and start rtp stream.
refer-by not compatable 
it is 401 response,should require the authorized INVITE here.
<on_replaces_invite>:receive replaces INVITE when DIALOG_CONFIRMED!
early-tag
<on_replaces_invite> Shoud send out CANCEL...
<on_replaces_invite>:receive replaces INVITE when DIALOG_EARLY!
the dialog has not been replaced.
on replaces invite error:can not create the new dialog 
after audio_stream_start!
it is a none sdp invite, so not start audio stream here , we should do it after recieve sdp in ack 
 Receiving new invite for an existent call-leg!
<on_other_invite>: receive INVITE when DIALOG_TERMINATED!
audio
<on_other_invite>: no c_addr in offer! Will ignore.
<on_other_invite>: no audio section in offer! Will ignore.
application/sdp
ERROR: sdpctx is NULL!
DEBUG <on_other_invite>: receive INVITE with different o_version
local_o_version: %s, remote_o_version: %s!
<on_other_invite>: receive INVITE with different o_version
local_o_version: %s, remote_o_version: %s!
<on_other_invite>: receive INVITE when we are holding/unholding!
<on_other_invite> the remote_o_session_id = %s,sdp->o_sess_id = %s
Received an AUDIT INVITE, should return a dummy 200!
0.0.0.0
<on_other_invite>: receive INVITE when we are host of callwaiting/conference call!
<on_other_invite>: sdpctx == NULL!
WDJ before start audio_stream_start_full in on_other_invite , hold=1
<on_other_invite>: after audio_stream_start!
<on_other_invite>: compare session params:
                        prev_audio_params.localport: %d, audio_params->localport: %d.
                        prev_audio_params.pt: %d, audio_params->pt: %d
                        prev_audio_params.remoteport: %d, audio_params->reomteport: %d
                        prev_audio_params.remoteaddr: %s, audio_params->remoteaddr: %s
<on_other_invite>: No need to modify session!
<on_other_invite>: Audio stream modified!
it is a none SDP invite in other_invite!
 OnEvent_New_IncomingInvite!
<in replaces invite >received!
error = %d
before <on_replaces_invite> !
There are more than one replaced dialog matched.
there are no replaced dialog matched.
<ist_invite_received>: Receive INVITE that has been changed tags!
 in ist_invite_receive,error is %d
(OnEvent_New_IncomingAck!
Ack for an inexistant call-leg !
receive ack for a none sdp invite, so here try to parse sdp and start audio media 
 call body_context_notify_inc_response when receive sdp in ack
not receive sdp in invite and ack , so bye the peer 
receive sdp in ack for none sdp invite, so start audio stream 
ALERT lc->audiostream should be NULL 
ist_ack_received: dialog in bad state (%i)
NICT Transaction %i killed. CSEQ: %s
 OnEvent_New_Incoming1xxResponse!
1xx response for an inexistant call leg! 
 REGISTER
MESSAGE
Message successfully delivered to %s.
Message is accepted, but can't guarantee end to end delivery!
OPTIONS
200 for OPTION received!
REFER
2XX for REFER received!
NOTIFY
(nict_3xx_received(): not implemented
 OnEvent_New_Incoming4xxResponse!
4xx response for an inexistant call leg! 
User need to authenticate to REGISTER!
true
Authentification aborted.
User need to authenticate to BYE!
BYE Authentification aborted.
 Remote peer need authentication!
user need to authenticate to refer !
min-expires
min expires is %s
minexp value is %d,reg conf's exp is %d
reg auth count is %d
---->re initiate a register with new expire for 423 resp
Message deliver failure to %s.
 @!	(
 ict_5xx_received():
5xx response for an inexistant call leg! 
5xx for REFER received!
 OnEvent_New_Incoming6xxResponse!
6xx response for an inexistant call leg! 
NIST Transaction %i killed.
 nist_register_received: not fully implemented
(nist_bye_received():
Bye for an inexistant dialog !
(nist_cancel_received():
null invite request!
 nist_options_received(): not fully implemented.
nist_option_received: can not create new dialog
Retry-After
Error in contact url: %s
Could not create response for current status
 nist_message_received(): 
Sending 200 OK for MESSAGE req.
Response for MESSAGE sent..
Error in generating response for MESSAGE request!
There is no content-type !
text/plain
Incoming message from %s!
It saids: %s.
Unsupported content type in MESSAGE!
4	(|C
 nist_refer_received():
<nist_refer_received>: refer not in an established dialog!
<nist_refer_received>: LOCAL XFER MODE is NO_XFER, should return 487!
<nist_refer_received>: NULL refer-to!
<nist_refer_received>: ERROR refer-to!
<nist_refer_received>: webphone_core_invite failure!
Refer for an inexistant dialog !
( len is %d
$@ p is %s
messages-waiting
no messages-waiting header
voice-message
tmp is %s
vmnum is %d
NO voice mail
 nist_notify_received():
<nist_notify_received>: notify not for an established dialog!
<nist_notify_received>: notify without event header!
refer
<nist_notify_received>: event is not refer!
<nist_notify_received>: notify without content type!
message/sipfrag
<nist_notify_received>: content type is not sipfrag!
<nist_notify_received>: notify without body!
<nist_notify_received>: body content error!
<nist_notify_received>: webphone_core_terminate_dialog error!
Notify for an inexistant dialog !
application/simple-message-summary
<nist_notify_received>: content type is not simple-mesage-summary!
200 for NOTIFY(out-of-dialog) sent..
Error in generating response for NOTIFY request!
 nist_info_received():
INFO for an inexistant dialog !
Remote UA is not compliant: missing a contact in invite!
Remote UA is not compliant: missing a contact in response!
 tag
Remote UA is not compliant: missing a tag in response!
 p@-
 match failed
 INVITE
the replaces header only be contained in INVITE!
to-tag
the replaces header to-tag is not compatiable !
from-tag
the replaces header from-tag is not compatiable !
 p@-
Could not establish dialog!
 0@-
 allocating ICT context
(free ict ressource
 p@-
(0@-
 0@-
 0@-
allocating NICT context
(free nict ressource
 p@-
(p@-
(p@-
(p@-
(p@-
You are using a multithreaded application, but this method is not allowed! Use osip_find_transaction_add_add_event() instead.
 INVITE
(Cannot build a transction for this message!
1 Pending event already in transaction !
 p@-
(MESSAGE
 p@-
<osip_timers_init> the timers are:
t1: %d
t2: %d
t4: %d
timer_b: %d
timer_d: %d
timer_f: %d
timer_h: %d
timer_j: %d
too much traffic in fifo.
 0@-
 0@-
no element in fifo.
 0@-
 0@-
could not parse message
MESSAGE REC. CALLID:%s
 0@-
INVITE
 allocating transaction ressource %i %s
 free transaction ressource %i %s
transaction already removed from list %i!
 0@-
sipevent tr->transactionid: %i
sipevent tr->state: %i
sipevent evt->type: %i
sipevent evt->sip: %x
USELESS event!
sipevent evt: method called!
Remote UA is not compliant: missing a Via header!
branch
You created a transaction without any branch! THIS IS NOT ALLOWED
Remote UA is not compliant: missing a branch parameter header!
 z9hG4bK
sent-by
INVITE
 0@-
 0@-
;%s=%s
 0@-
username
realm
nonce
response
digest
algorithm
cnonce
opaque
 p@-
 username=
, realm=
, nonce=
, uri=
, response=
, digest=
, algorithm=
, cnonce=
, opaque=
, qop=
, nc=
 0@-
content-type
 p@-
 content-type: 
 0@-
%s@%s
%s/%s
;%s=%s
 0@-
%s %s
 0@-
;%s=%s
 0@-
%s <%s>
<%s>
;%s=%s
%s: %s
%s: 
%s <%s>
<%s>
;%s=%s
 SIP/%s/%s [%s]
SIP/%s/%s [%s]:%s
SIP/%s/%s %s
SIP/%s/%s %s:%s
;%s=%s
 (%s)
realm
domain
nonce
opaque
stale
algorithm
 p@-
 realm=
, domain=
, nonce=
, opaque=
, stale=
, algorithm=
, qop=
 0@-
(p@-
accept
accept-encoding
accept-language
alert-info
allow
authorization
call-id
call-info
contact
content-encoding
content-length
content-type
cseq
error-info
event
from
mime-version
proxy-authenticate
proxy-authorization
record-route
refer-to
referred-by
replaces
route
www-authenticate
allow-events
subscription-state
(No crlf found
 SIP/
Final CRLF is missing
 0@-
 Could not set header: "%s" %s
Could not set unknown header
 organization
from
call-id
cseq
subject
user-agent
server
www-authenticate
authentication-info
proxy-authenticate
proxy-authorization
proxy-authentication-info
authorization
replaces
refer-to
event
referred-by
 End of header Not found
SIP message does not end with CRLFCRLF
This code cannot be reached
boundary
--%s
 error in msg_startline_init()
error in msg_headers_parse()
error in msg_body_parse()
 rport
received
 Trying
Ringing
Call Is Being Forwarded
Queued
Session Progress
Accepted
Multiple Choices
Moved Permanently
Moved Temporarily
Use Proxy
Alternative Service
Bad Request
Unauthorized
Payment Required
Forbidden
Not Found
Method Not Allowed
Not Acceptable
Proxy Authentication Required
Request Timeout
Conflict
Gone
Length Required
Request Entity Too Large
Request-URI Too Large
Unsupported Media Type
Unsupported Uri Scheme
Bad Extension
Interval Too Short
Temporarily not available
Call Leg/Transaction Does Not Exist
Loop Detected
Too Many Hops
Address Incomplete
Ambiguous
Busy Here
Request Cancelled
Not Acceptable Here
Internal Server Error
Not Implemented
Bad Gateway
Service Unavailable
Gateway Time-out
SIP Version not supported
Busy Everywhere
Decline
Does not exist anywhere
 ERROR strtline->method has no value!
Via: 
Record-Route: 
Route: 
From: 
To: 
Call-ID: 
CSeq: 
Contact: 
Authorization: 
WWW-Authenticate: 
Proxy-Authenticate: 
Proxy-Authorization: 
Allow: 
Content-Type: 
Content-Encoding: 
Mime-Version: 
Call-Info: 
Alert-Info: 
Error-Info: 
Accept: 
Accept-Encoding: 
Accept-Language: 
Replaces: 
REFER
Refer_To: 
Refer-To: 
INVITE
Referred_By: 
Referred-By: 
Event: 
Content-Length: 
xxxxx
--++
--++--
%i     
sA {
|A${
[vA({
 0@-
The "s" parameter is mandatory, but this packet does not contain any! - anyway, we don't mind about it.
The rfc2327 says there should be at least an email or a phone header!- anyway, we don't mind about it.
 0@-
 0@-
sips
[%s]
;%s=%s
?%s=%s
&%s=%s
 p@-
%%%02X
 -_.!~*'()&=+$,;?/
(-_.!~*'()&=+$,
(-_.!~*'()[]/:&+$
(-_.!~*'()[]/?:+$
(%02X
 0@-
active
pending
terminated
deactivated
probation
rejected
timeout
giveup
noresource
 expires
;%s=%s
allocating IST context
(free ist ressource
(0@-
 0@-
maddr
received
rport
 0@-
 p@-
(0@-
 REGISTER
OPTIONS
INFO
CANCEL
NOTIFY
SUBSCRIBE
MESSAGE
REFER
 p@-
 allocating NIST context
(free nist ressource
 p@-
(0@-
 REGISTER
OPTIONS
INFO
CANCEL
NOTIFY
SUBSCRIBE
MESSAGE
REFER
maddr
received
rport
 0@-
;%s=%s
 0@-
Enter audio_stream_stop()...
<audio_stream_stop> result: %d
 Enter audio_stream_start_full()...  localIP:%s, local port:%d , remote ip %s ,  remote port %d ,  payload %d 
NO memory when create Audio stream!
audio stream started!
  paloadtype is 96,for G726_32
unsupported payload type!
Error in open_rtp_session!
error in set_session_remote!
Decoder setCodecType error!
encoder setCodecType error!
To start JbConReq:
sessID
<audio_stream_start_full>: set to headset!
<audio_stream_start_full>: set to handset!
The call state is mute , then set dsp mute !!!
Out of audio_stream_start_full(),result is %d
No session active
dur_msec = 0!
MemoryAllocation Error
Sending the DTMF event, %d.
Out of send_dtmf().
(ICFlush Failure at position 1
(PROTING
Malloc memory fail!size is 
MMI malloc memory fail!,will restart!
& $&
(	(Create timer is fail1! 
Create timer is fail2! 
Timer queue is full! 
Qgfff<~' D,
' p@-
(	(d
(	(<<PORTING>>
msgQSend has ERROR in ConnectTimerFunc!
MsgQMMI NOT INITIALIZED!
<<PORTING>> Timer id is:
<<PORTING>> MMI msg queue count is: 
 Rtc is invalid when power on!year>2019
 tmmi_task
tmmi_task_getrssi
4 t0
4 L/
, MMI msg queue is full,will restart!
(p@-
& %s:   %s    %s
%s:   %s
 PORTING
bNoRegCount changed!
Reboot wlan start
Reboot wlan end
bNoRegCount reset!
 enter 2 minutes if segment
send power key to mmi queue to auto return to idle
 i	((
 @U	(
- Send alarm message to MMI queue
( i	(0
&  i	(
- 0@-
(	(d
' Destroy MMI task  starting!
Destroy MMI task fail!
Destroy MMI task  OK!
+' 4g3 `
(@U	(
, H=
 Reset MMI task starting!
Reset MMI task fail1!
ResetMMI task fail2!
Reset MMI task OK!
4 t0
4 L/
 Porting:  Enabled timer id is %d
(	(L@
& p@-
Incoming call,dest number:
Incoming call,nick name:
Incoming call, line number:
<PM>
 sub_incoming_call m_malloc fail
& t&
& t&
 Alert signal, line number:
 sub_alert_info m_malloc fail
 Dest answer, line number:
 sub_accept_comu m_malloc fail
Send the _PM2MMI_CODE_INITCALL msg to MMI:
 DTMF signal received, line number:
 sub_DTMF_receive m_malloc fail
 Dest disconnect, line number:
 sub_disconnect_comu m_malloc fail
 link error, line number:
 sub_call_failure m_malloc fail
& tA
 Hold response, line number:
Hold response, status:
 sub_hold_res m_malloc fail
 UnHold response, line number:
UnHold response, status:
 sub_unhold_res m_malloc fail
 Hold incoming, line number:
Hold incoming, status:
 sub_incall_hold m_malloc fail
 UnHold incoming, line number:
UnHold incoming, status:
 sub_incall_unhold m_malloc fail
 sub_init_end m_malloc fail
 sip regist ok
 sub_rgst_ok m_malloc fail
  sub_rgst_failure m_malloc fail
 sub_vmail_receive m_malloc fail
& (4
  sub_sms_receive m_malloc fail
&  sub_sms_res m_malloc fail
 SendRSSI m_malloc fail
 sub_send_rssi_batt m_malloc fail
 SendBattLvl m_malloc fail
 Call transfer response, status:
sub_call_transfer_res m_malloc fail
 Call transfer linenum response, line number:
sub_transfer_linenum_res m_malloc fail
 Call transfer received
sub_call_transfer_received m_malloc fail
 call park response
sub_call_park_res m_malloc fail
& net service response
sub_netservice_res m_malloc fail
 net search response
sub_netsearch_res m_malloc fail
& tA
 0@-
 Call repace linenum incoming, line number:
sub_replace_linenum_inc m_malloc fail
 Got _PM2MMI_CODE_REG_SUCCESS msg from sip.
Got _PM2MMI_CODE_RGSTFAILURE msg from sip.
Got _PM2MMI_CODE_CNTING_SSID msg from sip.
Got _PM2MMI_CODE_CNTING_FAIL msg from sip.
Got _PM2MMI_CODE_REGISTING msg from sip.
Got _PM2MMI_CODE_VMAIL_IND msg from sip.
 PMDelSYSLineNumMsg msg receive error
,  PMSendSYSLineNumMsg msg send error
, <d
  PMGetSYSLineNumMsg msg receive error
( PMSendAPMsg que number:
, t3
  PMGetAPMsg Get error queue
PMGetAPMsg Get error message type : 
& t3
 PMSendRSSIMsg que number:
, t3
(Enter pm_init
tpm_task
(Call out starting, dest number:
Call out starting, call type:
3 WayCall out fail, dest number:
3 WayCall out fail, call type:
3 WayCall out Success, dest number:
3 WayCall out Success, call type:
3 WayCall out Success,line num:
Call out fail, dest number:
Call out fail, call type:
Call out Success, dest number:
Call out Success, call type:
Call out Success,line num:
 Disconnect starting,line number:
Disconnect fail,line number: PM_LINENUM_ERR
Disconnect fail,line number: 
Disconnect success,line number: 
 Answer starting,line number: 
Answer fail,line number: 
Answer Success,line number: 
 Hold starting,line number: 
Hold fail,line number: 
Hold Success,line number: 
 UnHold starting,line number: 
UnHold fail,line number: 
UnHold Success,line number: 
Send DTMF starting,dtmf number: 
Send DTMF fail,dtmf number: 
Send DTMF Success,dtmf number: 
 transfer starting,line number: 
transfer starting,number string: 
transfer fail,line number: 
transfer fail,number string: 
transfer success,line number: 
transfer success,number string: 
 transfer resume starting,line number: 
transfer resume fail,line number: 
transfer resume success,line number: 
 starting to idle 
success to idle 
Mix starting,line number: 
Mix fail,line number: 
Mix success,line number: 
 Do poweroff register starting...
Do poweroff register 
Call Waiting switch starting...
Call Waiting switch Success, switch: TRUE
Call Waiting switch Success, switch: FALSE
 callerid block switch starting...
callerid block switch Success, switch: TRUE
callerid block switch Success, switch: FALSE
 anonymous reject switch starting...
anonymous reject switch Success, switch: TRUE
anonymous reject switch Success, switch: FALSE
 set nick name starting...
set nick name Success
 switch call transfer starting...
switch call transfer fail
switch call transfer success
 set register duration starting...
set register duration fail
set register duration success
search net starting...
search net fail
search net success
Protocol get config starting,choice: 
Protocol get config fail,line choice: 
Protocol get config Success,choice: 
 Protocol set config starting,line choice: 
Protocol set config fail,line choice: 
Protocol set config Success,line choice: 
 Enter pm_main
Switch default enter
@U	(`
(0@-
(0@-
3 p@-
 p@-
&  E4 p@-
4 sys: compress phone number fail!
sys: j=0!
 SYS
Save outgoing call log start!
Save outgoing call log end!
Save incoming call log start!
Save incoming call log end!
Save missed call log start!
Save missed call log end!
 <SYS>
_SysPlayCallNotice Start play ring
 _SysStopCallNotice stop ring
(<l3 
 0@-
(_TlEnableSpeaker TRUE
_TlEnableSpeaker FALSE
 p@-
& p@-
(p@-
 0@-
(h4	(
 0@-
(0@-
 p@-
 0@-
3 `W	(
3 0@-
3 0@-
 p@-
 0@-
 0@-
& Tf
 0@-
 0@-
& Tf
 0@-
 0@-
& 0@-
 p@-
& p@-
 p@-
 p@-
 p@-
 0@-
 0@-
 0@-
 0@-
 0@-
  Sys; 
 timer _TM_CNT_CHARGE_ANIMATION started
(`W	(
3 p@-
3 <d
 0@-
4 p@-
 0@-
 0@-
4 0@-
4 _SysConnectedEntry 
 _SysVolumeEntry 
 _SysIncomingCallEntry 
k3 T
 _SysDisconnectEntry 
& t&
& T0
 0@-
 @U	(T
 p@-
 @U	(0
 0@-
 _SysAutoPowerOffProc after _SysSetPowerKeyUpStatus
@U	(0
 Battery increase and will stop warning ring
h3 <l3 
 p@-
 bNoRegCount reset!
 @U	(
& Tu
 0@-
 0@-
 0@-
 x`3 
 x`3 
  Received the  _PM2MMI_CODE_INITCALL msg from PM!
get _PM2MMI_CODE_REG_SUCCESS msg from PM!
get _PM2MMI_CODE_RGSTFAILURE msg from PM!
@U	(
 0@-
 p@-
 Battery event Start charge
Battery event Stop charge
 RSSI:
 FER
 0@-
`W	(
 0@-
 @U	(
&  _SysReturn2Idle 
Enter
g3  _SysCallOut 
start
 @U	(
 0@-
 0@-
 p@-
@U	(
 0@-
@U	(
 _SysCnting2ConnectedCn _GetPM2MMIInitCall before StopTone
 Get _PM2MMI_CODE_INITCALL event in connecting state 1!
 Get _PM2MMI_CODE_INITCALL event in connecting state 2!!!
_SysCnting2ConnectedCn _GetPM2MMIAlert before PlayTone
 p@-
(0@-
(<SYS> 
_SysConnecting2DiscCn before StopTone
 0@-
 p@-
 p@-
 0@-
 0@-
 0@-
 p@-
 p@-
 0@-
 0@-
 p@-
 0@-
@U	(
 0@-
 p@-
 p@-
 p@-
 0@-
  _SysCallWaitCnted2CWDisCn enter MENUID_SYS_DISCBACKCALL
 p@-
 _SysCallWaitingIncomingEntry before PlayTone
 _SysCallWaitingIncomingExit before StopTone
  _SysCallWaitingCntedEntry 
  _SysCallWaitingDisEntry 
  _SysCallWaitingDisExit 
  _Sys3WayEditEntry 
  _Sys3WayCntingEntry 
  _Sys3WayCntingExit 
  _Sys3WayCntedEntry 
  _Sys3WayMixEntry 
  _Sys3WayDropEntry 
  _Sys3WayDisEntry 
  _Sys3WayDisExit 
 0@-
 0@-
 0@-
Own number is: 
Out side number is: 
New call number is: 
New call number error! 
& (4
& tw
 p@-
 0@-
  _Sys3WayMix23WDropCn enter MENUID_SYS_DROP
 0@-
4  _SysRedialEntry
  _SysRedialExit
 SYS:
_SysConnecting2Cnting() sent a DTMF
(gfff
 0@-
(gfff
 x`3  _SysTransferEditEntry 
  _SysTransferEditExit 
  _SysTransferProceedingEntry 
  _SysTransferCntingEntry 
  _SysTransferCntingExit 
  _SysTransferCntedEntry 
  _SysTransferDisEntry
  _Sys3WayDisExit
Transfer number is: 
Transfer number error! 
& (4
& (4
 0@-
 h4	(4
(p@-
 _SysTransferCnting2TFCntedPMCn _GetPM2MMIInitCall before StopTone
_SysTransferCnting2TFCntedPMCn _GetPM2MMIAlert before PlayTone
 0@-
 0@-
 p@-
 0@-
 _SysPowerOffEntry star stop warning ring
_SysPowerOffEntry
  _SysStandByEntry
 @U	(
 p@-
( _SysConnectingEntry 
Start
+' P/
  _SysConnectingEntry1
 _SysConnectingEntry1 
  _SysStandByExit
@U	(
  _SysIncomingCallExit 
 <l3 @b
  _SysDisconnectExit 
 get TFTP TFTP_MMI_RESYNC or  TFTP_MMI_RETRY message
h3 06
(<l3 t
(@U	(
 0@-
& 0@-
4 tZ
4  r
4 8P
4 ,z
4 Hy
4 ,z
4 8P
 0@-
4 0{
4 8P
4 ,z
& df4 
4 @"	(
d3  0
	(@Y
(p@-
d3  
G4 8Y
d3 l
3 xh	(@
 	(HJ
+' $
 0@-
& p@-
 p@-
 p@-
"	(d
& p@-
 0@-
- ,z
"	(pF
 0@-
"	( I
"	(@I
 0@-
& pF
& pF
"	(x
& pF
"	(x
 p@-
& p@-
"	(0
& pF
(0@-
& 0@-
 p@-
& P*
(0@-
& @Y
4 HJ
+' l
& pC
4 @U	(l
4 @U	(l
4 @U	(l
4 @U	(l
4 @U	(l
4 @U	(l
4 @U	(l
4 @U	(l
4 @U	(l
& @Y
(p@-
 	(xh	(@
 0@-
(p@-
 	(pF
H4 p@-
(@"	(8
@"	(
(050309
 p@-
( E4 0@-
 	((
(0@-
 	(D
4 @U	(l
4 0@-
& D 
(@"	(
 \n4 8
xh	(@
 	(l
 0@-
 0@-
 0@-
 	(@Y
(0@-
(0@-
& p@-
& 4!
 	(0
(p@-
& p>
& P*
( E4 @U	(
(0@-
 	($N
(p@-
"	(@Y
 	(D
(p@-
 	(@Y
(0@-
 	(@%
(0@-
 	(@%
& p@-
& 4!
 	(0
 	(T/
<<<<PROFILE>>>>
_PlayMelody in Pro_PlayMelody
 p@-
 p@-
<l3 
 _PlayMelody in PlaySMSRing
 p@-
 p@-
V	((
4 @U	(l
4 @U	(l
V	()
4 X,
4 $7
(0@-
 0@-
 0@-
(0@-
(p@-
V	($7
4 p@-
(<l3 
4 0@-
 <l3 
 p@-
 0@-
 0@-
 0@-
4 0@-
(0@-
3 @3
(p@-
 0@-
 p@-
 0@-
p$	(D
(0@-
 0@-
(p$	(
(p$	(X
(p$	(X
(0@-
4 @U	(l
4 0@-
4 @U	(l
 	(H
$	(T
$	(D
p$	(X
 	(4
4 T/
  E4 
+' x
(0@-
4 0@-
& t&
Qgfffp@-
  E4 
  E4 
& h'
 	(hz
 	(hz
4 p@-
 0@-
p$	(
p$	(
p$	(
& l0
 p$	(D
- p$	(
 	(H
@U	(
 0@-
@U	(
& 0@-
& $;
 0@-
(p$	( 
(050309
& HA
  E4 
 0@-
& HA
 p$	($<
3 `Y
d3 T
3 <,
 p$	(
h	(h
3 P:
J4  
4 @U	(l
 p@-
4 x`3 
 p@-
4 x`3 
4 x`3 
4 x`3 
 0@-
T	(Z~
 0@-
4 x`3 
 p@-
4 x`3 
 p@-
 p@-
4 x`3 
4 x`3 
(p@-
4 x`3 
 : 0
T	(T:
T	(pi
T	(pi
T	(pi
T	(pi
(0@-
(0@-
(p@-
(0@-
T	(pi
T	(pi
T	(pi
& D4
& (b
(050309
4 x`3 
 p@-
  E4 
& D#
(p@-
4 x`3 
 0@-
h	(L
4 x`3 
 p@-
4 x`3 
 p@-
4 x`3 
3 h>
 p@-
4 x`3 
 p@-
4 x`3 
4 x`3 
4 x`3 
(p@-
4 x`3 
'	(0@-
h	(x
h	(x
h3 4(
4 d@
4 x`3 
(p@-
T	(hu
T	(hu
T	(hu
T	(hu
T	(hu
T	(hu
(p@-
& t3
& t3
'	((
T	(|C
T	(P5
Qgfff0@-
 p@-
(p@-
(0@-
Qgfff
H4 l
+' p@-
888888
3000
70401
#40#
#41#
#57#
#45#
0710
 0@-
 0@-
 p@-
& 0@-
 p@-
 p@-
 p@-
 p@-
 p@-
 p@-
 0@-
 p@-
 p@-
 p@-
 p@-
 _DelAllCallsLog: 0 - all calls log 
_DelAllCallsLog: 1 - incoming calls log
_DelAllCallsLog: 2 - outgoing calls log
_DelAllCallsLog: 3 - missing calls log
& l7
 p@-
& MMI table OK!
MMI table byte %4d is %4d
MMI table byte error in %4d has been corrected.
Reload MMI table block!
Success in Correcting MMI table block error!
 Flash Bad! Should Go to Power Off!
& User data should be recovered!
Backup data are bad too! Recover check design only.
Recover check design only.
User data OK!
 Fail in getting backup data!
Fail in recovering user data!
Success in recovering user data!
& 4L
 User data already bad, do NOT backup!
Fail in getting user data!
Fail in backuping user data!
Success in backuping user data
 0@-
& 0h
 Fail in cleaning backup area!
& 0h
 Fail in cleaning user data area!
& 0h
	((5
(p@-
	(<$
 p@-
 0@-
Ring 1
Ring 2
Ring 3
Ring 4
Ring 5
Ring 6
_EnableBackLight state is %d
& _EnableKeyLED state is %d
 _DelAllPBEntry: void - del all PB entry.
& 0h
 CCNA
MMIMQSend in SendKeyMsg is error
 p@-
 TFTP_Send_MMIMsg , msg bbuf is %d
>'  
Play Alert Tone.
UTStarcom
1949
F1000
SIP_0.1
(P"	(
& H$	(
(hW	(
3 v~
4 v~
--------
 P"	(
4 l<
 p@-
(0@-
& 0@-
& 0@-
& 0@-
& 0@-
 0@-
 0@-
4 x`3 
 0@-
3 0@-
 WFSETTING
set DHCP Type begin
set DHCP Type end
 get TFTP Work Mode begin
get TFTP Work Mode end
 set TFTP Work Mode begin
set TFTP Work Mode end
 get TFTP Server Domain begin
get TFTP Server Domain end
get TFTP Server Domain ERROR!!
 set TFTP Server Domain begin
set TFTP Server Domain end
 get TFTP Server IP begin
Get TFTP Server IP end
Get TFTP Server IP ERROR!!!
 set TFTP Server IP begin
set TFTP Server IP end
 get TFTP Server Port begin
get TFTP Server Port end
get TFTP Server Port ERROR!!!
 set TFTP Server Port begin
set TFTP Server Port end
 get TFTP Directory/File name begin
get TFTP Directory/File name end
get TFTP Directory/File name ERROR!!!
 set TFTP Directory/File name begin
set TFTP Directory/File name end
 get TFTP Encryption Key begin
get TFTP Encryption Key end
get TFTP Encryption Key ERROR!!!
 set TFTP Encryption Key begin
set TFTP Encryption Key end
 0@-
 get IPAddress begin
get IPAddress end
get IPAddress ERROR!!!
 set IPAddress begin
set IPAddress end
 get SubnetMask begin
get SubnetMask end
get SubnetMask ERROR!!!
 set SubnetMask begin
set SubnetMask end
 get Gateway IP begin
get Gateway IP end
get Gateway IP ERROR
 set Gateway IP begin
set Gateway IP end
 0@-
 get DNS Primary Server begin
 set DNS Primary Server begin
set DNS Primary Server end
 get DNS Secondary Server begin
get DNS Secondary Server end
get DNS Secondary Server ERROR!!!
 p@-
 Local First
DHCP First
Unknown
get DNS Priority begin
get DNS Priority end
 set DNS Priority begin
set DNS Priority end
 0@-
 0@-
& 0@-
 0@-
4 hT
4 LV
d3 `X
H4 l
H4 l
H4 l
d3 t
H4 l
3 LY
H4 l
H4 l
H4 l
H4 l
H4 l
H4 l
!	(u~
!	(u~
(p@-
4 x`3 
 0@-
 p@-
4 x`3 %02x:%02x:%02x:%02x:%02x:%02x
(WFSETTING
get SIP DNS SRV begin
get SIP DNS SRV end
 Use IP
Use DNS
Error!
set SIP DNS SRV begin
set SIP DNS SRV end
 get SIP Service Name begin
get SIP Service Name end
get SIP Service Name ERROR!!!
 set SIP Service Name begin
set SIP Service Name end
 get SIP Proxy Domain begin
get SIP Proxy Domain end
get SIP Proxy Domain ERROR!!!
 set SIP Proxy Domain begin
set SIP Proxy Domain end
 get SIP Proxy IP begin
get SIP Proxy IP end
get SIP Proxy IP ERROR!!!
 set SIP Proxy IP begin
set SIP Proxy IP end
 get SIP Proxy Port begin
get SIP Proxy Port end
get SIP Proxy Port ERROR!!!
 set SIP Proxy Port begin
set SIP Proxy Port end
 get SIP Outband Proxy begin
get SIP Outband Proxy end
 set SIP Outband Proxy begin
set SIP Outband Proxy end
 get SIP Register Server Domain begin
get SIP Register Server Domain end
get SIP Register Server Domain ERROR!!!
 set SIP Register Server Domain begin
set SIP Register Server Domain end
 get SIP Register Server IP begin
get SIP Register Server IP end
get SIP Register Server IP ERROR!!!
 set SIP Register Server IP begin
set SIP Register Server IP end
 get SIP Register Server Port begin
get SIP Register Server Port end
get SIP Register Server Port ERROR!!!
 set SIP Register Server Port begin
set SIP Register Server Port end
 get SIP User Name begin
get SIP User Name end
get SIP User Name ERROR!!!
 set SIP User Name begin
set SIP User Name end
 get SIP Authentication String begin
get SIP Authentication String end
get SIP Authentication String ERROR!!!
 set SIP Authentication String begin
set SIP Authentication String end
 get SIP Password begin
get SIP Password end
get SIP Password ERROR!!!
 set SIP Password begin
set SIP Password end
 get SIP Authentication Algorithm begin
get SIP Authentication Algorithm end
 set SIP Authentication Algorithm begin
set SIP Authentication Algorithm end
 get SIP Port begin
get SIP Port end
get SIP Port ERROR!!!
 set SIP Port begin
set SIP Port end
 0@-
 get RTP Port begin
get RTP Port end
get RTP Port ERROR!!!
 set RTP Port begin
set RTP Port end
 get RTP Pack Time begin
get RTP Pack Time end
 set RTP Pack Time begin
set RTP Pack Time end
 get RTP Jitter Buffer Compensation begin
get RTP Jitter Buffer Compensation end
get RTP Jitter Buffer Compensation ERROR!!!
 set RTP Jitter Buffer Compensation begin
set RTP Jitter Buffer Compensation end
 0@-
 get Voice Mail Access Number begin
get Voice Mail Access Number end
get Voice Mail Access Number ERROR!!!
 set Voice Mail Access Number begin
set Voice Mail Access Number end
 get Voice Mailbox Number begin
get Voice Mailbox Number end
get Voice Mailbox Number ERROR!!!
 set Voice Mailbox Number begin
set Voice Mailbox Number end
 get Voice Mailbox Password begin
get Voice Mailbox Password end
get Voice Mailbox Password ERROR!!!
 set Voice Mailbox Password begin
set Voice Mailbox Password end
 0@-
 get NAT Work Mode begin
get NAT Work Mode end
 set NAT Work Mode begin
set NAT Work Mode end
 get NAT IP begin
get NAT IP end
get NAT IP ERROR!!!
 set NAT IP begin
set NAT IP end
 get NAT Server Domain begin
get NAT Server Domain end
get NAT Server Domain ERROR!!!
 set NAT Server Domain begin
set NAT Server Domain end
 get NAT Server IP begin
get NAT Server IP end
get NAT Server IP ERROR!!!
 set NAT Server IP begin
set NAT Server IP end
 get NAT Server Port begin
get NAT Server Port end
get NAT Server Port ERROR!!!
 set NAT Server Port begin
set NAT Server Port end
 get NAT keep-alive Time begin
get NAT keep-alive Time end
get NAT keep-alive Time ERROR!!!
 set NAT keep-alive Time begin
set NAT keep-alive Time end
 get NAT keep-alive Pack Dest begin
get NAT keep-alive Pack Dest end
 NAT Server
SIP-Proxy
set NAT keep-alive Pack Dest begin
set NAT keep-alive Pack Dest end
 get NAT STUN Mode begin
get NAT STUN Mode end
 Disable
Enable
set NAT STUN Mode begin
set NAT STUN Mode end
 set STUN Server Name begin
set STUN Server Name end
 p@-
 0@-
 0@-
& 0@-
& 0@-
& 0@-
& 0@-
& 0@-
4 8(
 0@-
4 \.
4 l3
4 P5
4 47
4 ,;
3 pw
& rw
3  N
H4 l
3 pw
H4 l
3 pw
H4 l
3 pw
H4 l
3 pw
H4 l
3 pw
H4 l
3 pw
& 1x
H4 l
3 pw
& 6x
3 tN
H4 l
3 pw
& Vx
H4 l
G4 l
3 pw
& vx
d3 D
3 pO
H4 l
3 pw
d3 P
H4 l
3 pw
H4 l
H4 l
d3 X
3 |P
H4 l
3 P"	(
& Q"	(
d3 x
H4 l
3 P"	(
& h"	(
3 $Q
H4 l
3 P"	(
& r"	(
3 xQ
H4 l
H4 l
H4 l
& 36
H4 l
& B6
H4 l
& G6
H4 l
d3  R
& L6
H4 l
& ~6
H4 l
(050309
 p@-
& Lx
& Lx
(Q"	(
(h"	(
(r"	(
(p@-
4 x`3 p@-
4 x`3 
 0@-
 0@-
 0@-
 0@-
4 x`3 0@-
 0@-
 0@-
 0@-
 0@-
 p@-
4 x`3 p@-
4 x`3 wfsetting
About to get vendor name
Get vendor name failed
Get vendor name success. Value:
 About to get enterprise code
Get enterprise code failed
Get enterprise code success. Value:
 About to get product category
Get product category failed
Get product category success. Value:
 About to get model name
Get model name failed
Get model name success. Value:
iW	(
4 hW	(
+' p@-
4 hW	(
d3 l
+' p@-
4 hW	(
d3 l
4 hW	(l
4 hW	(
wfsetting
About to get CNG state
Get CNG state succeed. Value:
Get CNG state failed
 Set CNG state succeed
Set CNG state failed
 About to get PLC state
Get PLC state succeed. Value:
Get PLC state failed
 Set PLC state succeed
Set PLC state failed
 About to get VAD state
Get VAD state succeed. Value:
Get VAD state failed
 Set VAD state succeed
Set VAD state failed
 About to get noise suppression state
Get noise suppression state succeed. Value:
Get noise suppression state failed
 Set noise suppression state succeed
Set noise suppression state failed
 About to get Acoustics Echo Cancellation work mode state
Get Acoustics Echo Cancellation work mode state succeed. Value:
Get Acoustics Echo Cancellation work mode state failed
 Set Acoustics Echo Cancellation work mode state succeed
Set Acoustics Echo Cancellation work mode state failed
 About to get Acoustics Echo Cancellation tail time
Get Acoustics Echo Cancellation tail time succeed. Value:
Get Acoustics Echo Cancellation tail time failed
 About to set Acoustics Echo Cancellation tail time. Value:
Set Acoustics Echo Cancellation tail time succeed
Set Acoustics Echo Cancellation tail time failed
& 0g
 About to get g.711c codec priority
Get g.711c codec priority failed
Get g.711c codec priority succeed. Value:
About to get g.711mu codec priority
Get g.711mu codec priority failed
Get g.711mu codec priority succeed. Value:
About to get g.729 codec priority
Get g.729 codec priority failed
Get g.729 codec priority succeed. Value:
About to get g.729a codec priority
Get g.729a codec priority failed
Get g.729a codec priority succeed. Value:
About to get g.729b codec priority
Get g.729b codec priority failed
Get g.729b codec priority succeed. Value:
 GFHIJ
The codec index to set the highest priority is: 
About to set codecpriority, original highest priority codec is
About  get its original priority
Get its original priority failed.
Get its original priority succeed. Value:
It's already the highest priority, no change
About  to set it to the highest priority.
Set it to the highest priority failed.
Set it to the highest priority succeed.
Set the original one's priority with new one's original priority. Value:
Set  original one's priority failed.
Set  original one's priority succeed.
 About to get general jitter buffer max connection
Get general jitter buffer max connection succeed. Value:
Get general jitter buffer max connection failed
 About to set general jitter buffer max connection. Value:
Set general jitter buffer max connection succeed
Set general jitter buffer max connection failed
& 0g
 About to get general jitter buffer size
Get general jitter buffer size succeed. Value:
Get general jitter buffer size failed
 About to set general jitter buffer size. Value:
Set general jitter buffer size succeed
Set general jitter buffer size failed
& 0g
 H$	(
4 PW
d3 l
d3 <
4 H$	(l
4 H$	(l
4 x`3 
4 x`3 
 H$	(
(K$	(H$	(
& wfsetting
 Get Auth type failed
 Get Auth type succeed
  Set Auth type failed
 Set Auth type succeed
  Get WEP Auth method failed
 Get WEP Auth method succeed
  Set WEP Auth method failed
 Set WEP Auth method succeed
 Get Failed
Get successfully, value:
& (4
 Set SSID Failed
Set SSID successfully, value:
 Get WEP Key Failed
Get WEP key successfully, value:	
 WEP Key  to set:
Set WEP Key Failed
Set WEP key successfully
 About to Get WEP key bit mode Inf
 Get WEP key bit mode failed
 Get WEP key bit mode success
&  About to Set WEP key bit mode
 Set WEP key bit mode failed
 Set WEP key bit mode success
  Get WEP key index  failed
 Get WEP key index  succeed
&  Set WEP key index  failed
 Set WEP key index success
  Get PSK key failed
 Get PSK key succeed, value: 
  Set PSK key failed, Key: 
 Set PSK key succeed, key: 
   Get auto scan status failed
  Get auto scan status succeed
    Set auto scan status failed
   Set auto scan status succeed
& 0@-
& 050309
 About to search net
Net search succeed
Net search failed
@U	(T
@U	(T
(p@-
( E4 
 x`3 
& u~
+' l
d3 l
netser
Before pm_calltransfer_switch
After pm_calltransfer_switch
 Before pm_register_duration_set
After pm_register_duration_set
 Before pm_TftpUpdate
After pm_TftpUpdate
 Before pm_netservice_cancel
After pm_netservice_cancel
 set LOCT_Misc_PersonalInfo: 
 get LOCT_VonageSpec_CallTransfer: 
 set LOCT_VonageSpec_CallerIDBlock: 
 get LOCT_VonageSpec_CallerIDBlock: 
 set LOCT_VonageSpec_RDialonBusyuse: 
 get LOCT_VonageSpec_RDialonBusyuse: 
 set LOCT_VonageSpec_CallWaitingOnoff: 
 get LOCT_VonageSpec_CallWaitingOnoff: 
 set LOCT_VonageSpec_AnonymReject: 
 get LOCT_VonageSpec_AnonymReject: 
(IDLE
SetWLHoldoverDuration start!
SetWLHoldoverDuration end!
V	(0Y
(<<IDLE>>
Enter IDLE_STANDBYEXIT
@U	(
4 0@-
@U	(0
 0@-
 To TFTP from IDLE!
!	@X
!	@X
 0@-
(@U	(T
 0@-
 _IdelLeftSoftInit  start!
_IdelLeftSoftInit end!
3 (4
3 d%
4 @U	(l
& t3
 0@-
@U	(
(0@-
 0@-
 0@-
 @U	(
 p@-
(0@-
 _LabelStandbyPhotoInit start!
via 
_LabelStandbyPhotoInit end!
(@U	(
(p@-
(0@-
4 0@-
 p@-
 @U	(0
 0@-
 0@-
(0@-
 <IDLE>
 Enter Outgoing call from IDLE. 
 @U	(
  Enter Missed call from IDLE1. 
 Enter Missed call from IDLE2. 
 @U	(
  Enter Incoming call from IDLE. 
 @U	(
 0@-
 0@-
 0@-
 050309
 @U	( E4 
3 (2
4 d?
4 d?
4 d?
4 d?
4 d?
 0@-
4 d?
4 d?
4 @	
 0@-
 0@-
 @U	(T2
 RSSI:    
 Registered!
Registering!
Battery: 
 0@-
 0@-
 @U	(T
4 TW
 @U	(T
 p@-
 @U	(T
 @U	(
@Z4 (?
 xh3 
 4g3 
Watchdog reset!!!!!
IDLE :
Is going to start timer: _TM_ID_CHARGE_ANIMATION, 4 for charge, 5 for low battery: 
& t3
 0@-
 0@-
G4 l
3 p@-
3 p@-
3 p@-
4 t?
4 (?
 p@-
4 p@-
3 0@-
d3 T
 0@-
(p@-
 twatchdog_task
 <WATCHDOG>
 rssi task is dead now, then starting to delete it
 watchdog_main rssi taskDelete error!!!!!!!!!
 rssi task is deleted succesfully, then starting to create it again
trssi_task
 rssi task is recreated success
 pm task is dead now, then starting to delete it
 watchdog_main pm taskDelete error!!!!!!!!!
 pm task is deleted succesfully, then starting to create it again
tpm_task
 pm task is recreated success
 0@-
4 @U	(l
misc, sent MMIWUA_DOWNLOAD_SCRIPT_REQ! URL is: %s
& Hc
& [WEB AUTH]: in CrtMiscWebAuthScriptFilesDlg wua_get_scriptfile_info FAIL!!
[WEB AUTH]: wua_get_scriptfile_info Success!!
[WEB AUTH]: script count is: %d
[WEB AUTH]: default file is: %d
[WEB AUTH]: file1 is: %s
[WEB AUTH]: file2 is: %s
[WEB AUTH]: file3 is: %s
[WEB AUTH]: file4 is: %s
 misc, sent MMIWUA_GET_REQ!
& misc, sent MMIWUA_AUTH_STOP_REQ!
misc: download script failed!
misc: download script success!
[WEB AUTH]: Set default Script Number: %d
& 4(
, MISC: pfnCndWebAuthConnExit2Menu 1
MISC: pfnCndWebAuthConnExit2Menu 2
 username
password
 misc: connecting failed!
misc: already connected, connceting success!
 misc: parse msg is 1%s
misc: parse msg is 2
 MISC: webAuthBody.size is %d
MISC: Recieved web auth msg: %s
MISC: count: %d
MISC: Fieldname %d is: %s
MISC: free pStr
MISC: free webAuthBody.ptr
MISC: free pEvt->data
MISC: end
+' |
 MISC: pfnCndWebAuthConn2Menu 1
MISC: pfnCndWebAuthConn2Menu 2
 MISC: pfnCndWebAuthConn2Idle 1
MISC: pfnCndWebAuthConn2Idle 2
 MISC: pfnCondWebAuthInput2Menu 1
MISC: pfnCondWebAuthInput2Menu 2
 MISC: pfnCondWebAuthInputContiune 1
MISC: pfnCondWebAuthInputContiune 2
MISC: pfnCondWebAuthInputContiune 3
MISC: pfnCondWebAuthInputContiune 4
( E4 @U	(
 MISC: pfnCondWebAuthInput2Process 1
misc, sent MMIWUA_USER_INPUT_RSP, pData is: %s
MISC: pfnCondWebAuthInput2Process 2
 [WEB AUTH]: in pfnCndActiveScriptProcessTimeout wua_set_dft_script FAIL!!
(misc: get EVENT_WUA_GET_RSP, data is %d
 misc: get EVENT_WUA_SCRIPT_ACTIVE_RSP, data is %d
[WEB AUTH]: in pfnCndActiveScriptRsp, wua_set_dft_script FAIL!!
 p@-
4 @U	(l
4 p@-
4 @U	(l
(MISC
Set TFTP server error!
%	(T
%	(D
& t3
( E4 
 @U	(
3 Item
& t3
( E4 
 @U	(
3 [WEB AUTH]: Create Picklist
(NULL)
 x`3 
4 Tf
 p@-
3 NULL
Get local log count is 
3 misc: copy string to urledit %s
& Hc
H4 l
(MISC get server from field: 
H4 l
d3 Hc
d3 l
d3 *
d3 l
+' MISC: labeltxt.text is %s; length is %d
misc: Exit input dialog!
+' h
 misc: CrtMiscWebAuthProcessDlg 1 
Processing...
misc: CrtMiscWebAuthProcessDlg 2 
misc: CrtMiscWebAuthProcessDlg 3 
d3 l
 p@-
d3 l
+' Get TFTP server error!
d3 D
4 <.
4 ,!
4 <6
 netser
TFTP_Connecting_Entry
TFTP_MMI_RESYNC TFTP_Connecting_Entry
TFTP_MMI_RETRY TFTP_Connecting_Entry
4 `0
4 x3
 0@-
4 p@-
d3 `W
3 lableCallback
[] --TFTP -- The out put string: %s[]
[] -- TFTP --The string's lenth: %d[]
@U	(
G4 l
3 get LOCT_Misc_PersonalInfo: 
d3  
 Create_DlgTftpAskContinue_Remote TFTP_MMI_VERSION_OLDER_FIRMWARE
Create_DlgTftpAskContinue_Remote TFTP_MMI_FAIL_FILE_NOT_FOUND
Create_DlgTftpAskContinue_Remote TFTP_MMI_RESYNC
Create_DlgTftpAskContinue_Remote menu
d3 `
4 @U	(l
(netser
pm_nick_name_set: 
 0@-
(Have PM operating result
Operating timeout
PM operating result is ok
PM operating result is failure
 Cnd_TftpConnecting2AskContinue cnd 1
Cnd_TftpConnecting2AskContinue cnd 2
Cnd_TftpConnecting2AskContinue cnd 3
 Cnd_TftpError2Idle cnd
 Cnd_TftpConnecting cnd
 Cnd_Picklist2Menu cnd
(Cnd_tftp2Idle cnd
 Cnd_TftpConnectPCRestart cnd
 TFTP
TFTP restart in network service!
 0@-
 TFTP_MMI_FAIL_FILE_NOT_FOUND cnd
TFTP_MMI_VERSION_OLDER_FIRMWARE cnd
TFTP_MMI_RESYNC cnd
TFTP_MMI_RETRY cnd
Cnd_TftpAskContinue2PreDownloadRemote fatal error
menu cnd
 050309
& 46
& 46
	!	#	'	5	8	9	C	H	c	h	j	r	
ZUAN
ZONG
ZHUO
ZHUN
ZHUI
ZHUANG
ZHUAN
ZHUAI
ZHUA
ZHOU
ZHONG
ZHENG
ZHEN
ZHEI
ZHAO
ZHANG
ZHAN
ZHAI
ZENG
ZANG
YUAN
YONG
YING
YANG
XUAN
XIONG
XING
XIAO
XIANG
XIAN
WENG
WANG
TUAN
TONG
TING
TIAO
TIAN
TENG
TANG
SUAN
SONG
SHUO
SHUN
SHUI
SHUANG
SHUAN
SHUAI
SHUA
SHOU
SHENG
SHEN
SHEI
SHAO
SHANG
SHAN
SHAI
SENG
SANG
RUAN
RONG
RENG
RANG
QUAN
QIONG
QING
QIAO
QIANG
QIAN
PING
PIAO
PIAN
PENG
PANG
NUAN
NONG
NING
NIAO
NIANG
NIAN
NENG
NANG
MING
MIAO
MIAN
MENG
MANG
LUAN
LONG
LING
LIAO
LIANG
LIAN
LENG
LANG
KUANG
KUAN
KUAI
KONG
KENG
KANG
JUAN
JIONG
JING
JIAO
JIANG
JIAN
HUANG
HUAN
HUAI
HONG
HENG
HANG
GUANG
GUAN
GUAI
GONG
GENG
GANG
FENG
FANG
DUAN
DONG
DING
DIAO
DIAN
DENG
DANG
CUAN
CONG
CHUO
CHUN
CHUI
CHUANG
CHUAN
CHUAI
CHOU
CHONG
CHENG
CHEN
CHAO
CHANG
CHAN
CHAI
CENG
CANG
BING
BIAO
BIAN
BENG
BANG
4 to
4 pz
4 P~
4 0q
4 (y
 0@-
4 p@-
4 ---------
%d-%d%d-%d%d %d%d:%d%d
%d%d:%d%d
& 4U
d3 D
4 12121
d3 D
4 p@-
+' n
d3 D
d3 h
d3 |C
+' n
4 x`3 
4 x`3 
4 x`3 p@-
4 x`3 
(x`3 
d3 D
d3 D
3 X5
4 x`3 
d3 D
d3 D
d3 T
d3 D
H4 0
d3 D
d3 D
+' p@-
4 x`3 p@-
4 p@-
& ,2
4 p@-
d3 l
d3 D
d3 D
3  >
d3 D
d3 D
d3 D
3 <?
d3 pz
H4 l
3 t&
d3 l
3 4(
H4 l
+' 111222
d3 (
H4 l
d3 (
H4 l
+' p@-
3 p@-
d3 pz
3 %c 
d3 D
J4 (
+' p@-
4 x`3 
 calculator maloc size=%d,add=%x
& (Y
y5>	0
yU> 
3 X5
& x`3 
 0@-
3 X5
(p@-
(p@-
(p@-
(p@-
& calculator free add=%x
3 To
& `u
4 Get TFTP parameter
Set TFTP parameter
Toggle factory mode
Write SIP password
Write SIP username
Earphone insert
Earphone loop
Write Cal data
ate pc write para
ate pc read para
Clear user data
Read SW VER
Toggle ATE test mode
EEPROM init
RD/WR data 
Read data 
Paramtbl delivery
Paramtbl init
SRAM test
Flash test
Write PCDEBUG Flag
Vibrating test
Current test
Keypad test
Key tone test
Mic bias Vol test
Audio loop test
Speaker vol test
Charging test
Battery Vol test
LCD test
LED test
Not support
Toggle sleep mode
Write station number
Read station number
Write PS ID
Read PS ID
Write MAC
Read MAC
Ack result
Enter test mode
Check link
NULL cmd
Mac6
Mac5
Mac4
Mac3
Mac2
Mac1
PSID4
PSID3
PSID2
PSID1
0:diable
1:enable
1:All on 2:LCD on 3:Key on 4:All off
1:Disp all
2:Clear all
3:Auto
1:Volt low
2:Volt stop
1:Trick
2:Normal
1:Volume
2:Tone
1:Low 2:Mid
3:Hg 4:SHg
1:Talking
2:Standby
AddrL
AddrH
mode
data
1:Low 2:Mid 3:Hg 4:SHg
0:diable 1:enable
(get console com port name error!
g_ate_comfd = %d
close console error
tShell
tShell task can not be suspended
tLogTask
tLogTask task can not be suspended
 0@-
(read com port error
 write com port error
 DSP initiation failed!
command table check failed!
pc_ate
ERROR: ate_pc_task - Could not spawn Pc ATE Task !!!
PC ATE SUCCESS
 FIONREAD ERROR
%d bytes can read!
read comport error
read comport empty
total count: %d
time out now!
 Open comport error!
get cmd %d
cmd execute %d
ack result
 reading...
command too long!
chksum error
get cmd: 
%02x 
 command %d not find!
wrong parameter number!
addr of g_ate_cmd_table:%p
g_ate_mode:%d
func_ptr:%p
cmdid:%d
supportmode:%d
cmdinfo:%s
paranum:%d
proc:%p
execute command %d!
command %d not support!
 ATE test mode is disable!
Enter ATE
hand_ate
ERROR: ate_hand_task - Could not spawn Pc ATE Task !!!
HAND ATE SUCCESS
Hand ATE init failed, power off the phone!
(Func No?
Func 
command %d is not found
command %d not support hand mode
parameter number too long!
got hand command, id:%d, parameter: 
0x%x 
long press power key(down) detected!
(0@-
(Fail
Success
Para error
Not support
Chksum error
Unknown
 ATE receive msg error 
All On
LCD On
Keypad On
All OFF
Bad Param
 Contrast:
(Should>3.4
Should>3.2
 Trick Charge
Normal Charge
 Spk Volume:
Spk Tone:
 1: Low out put level
2: Middle out put level
3: High out put level
4: Super High out put level
AudLoop Error!
DSP audio loop error!
Set Volume Error!
DSP set volume error!
Volume = mode: %d
 OPEN Mic OK
 Pls In KEY:
KEY TONE TEST
LEFT ARROW
RIGHT ARROW
UP ARROW
DOWN ARROW
TALK
SOFTLEFT
SOFTRIGHT
Key %d has NOT been pushed!
 KEYPAD TEST:
 Talking...
Pls Measure
Standby...
 Vibrating...
Read checksum, code start address, code size failed!
chksum read:%#x
codeStartAddr:%#x
codeSize:%#x
SUM-
CHECKING...
ChksumCal:%#x
 SRAM test
MMI Init...
MMI OK!
MMI Fail!
 Pro Init...
Pro OK!
Pro Fail!
 InAddr:0~4095
Empty
 In(0~4095):
InData(0~255)
Re-Input!
Write Fail!
 ClrUsrData...
Result:
Clr Error!
Clr OK!
SW Version:
Software Version, %s .
 username
password
Clear user data failed!
Get mac address failed!
 Error: Multicast/Broadcast MAC address entered (must be unicast)
Error getting MAC address
newmac write success!
rebooting now!
STA NUM Read:
Earphone is not inserted
psw: %s
key: %s
hashdir: %s
SOWM
PMDN
CALG
PHSE
SWAP
into SoWriter Mode!
The system enter into PMM Mode!
The system enter into CALG Mode!
The system enter into PHSE Mode!
The system enter into SWAP Mode!
 tPST
ERROR: Dowmload_main - Could not spawn PST Task !!!
PST Task SUCCESS
ERROR: testPSTr state is not set by MMI !
Enter testPST Task
0x02 is received!
received byte is %d!
 _CallRecHead Open comport error!
in _CallRecHead Open COM Port: %d
Write %d bytes.
(p@-
(SendResponseInfo: This is Debug mode!
(0@-
(Get Commad ID is 0x%02x
 WF1000
Reponse PMM_PSType OK!
 Reponse PMM_Version OK!
 Reponse Proto Version OK!
 Reponse PMM_SupportMode OK!
(p@-
PMDM
PBDM
MDDM
PTDM
(PMM: open comport!
PMM_ModeProc() Open comport error!
in PMM_ModeProc() Open COM Port: %d
PMM: Watch link!
PMM: Enter Mode 
PhoneBook
PbTrans ends
PMM: Command mode exit!
PMM: close comport!
CALG
 F1000
sysReadHeader: ERROR reading size
 into calogTask
calogTask Open comport error!
in calogTask Open COM Port: %d
CalgTask: flashSectorAddr failed
flashBaseAdrs=%ld
CalgTask: ERROR reading
CalgTask: ERROR when get productID
CalgTask READTIME_CMD: ERROR bad size
CalgTask READ_IN_CALL_CMD: ERROR bad size
CalgTask READ_OUT_CALL_CMD: ERROR bad size
CalgTask READ_MISSED_CALL_CMD: ERROR bad size
CalgTask: Unknown command(0x%x)
CalgTask: exiting
 ERROR: testPSTr state is not set by MMI !
Enter CALG Task
tcalogTask
ERROR: taskSpawn(calog_Start) failed
 PHSE
 F1000
PhseReadHeader: ERROR reading size
PhseReadHeader: ERROR reading offset
 into phseTask
phseTask Open comport error!
in phseTask Open COM Port: %d
phseTask: flashSectorAddr failed
flashBaseAdrs=%ld
PhseTask: ERROR reading
PhseTask: ERROR when get productID
phseTask READ_CMD: flashAdrs(0x%x) out of range
phseTask READ_CMD: ERROR bad size
phseTask WRITE_CMD: flashAdrs(0x%x) out of range
phseTask WRITE_CMD: ERROR bad size
PhseTask WRITE_CMD: ERROR reading data
PhseTask WRITE_CMD: FlashWrite Failed
PhseTask: Unknown command(0x%x)
PhseTask: exiting
 ERROR: testPST state is not set by MMI !
Enter phone setting Task
tphseTask
ERROR: taskSpawn(phse_Start) failed
 SWAP
 F1000
SwapReadHeader: ERROR reading size
SwapReadHeader: ERROR reading offset
 into swapTask
swapTask Open comport error!
in swapTask Open COM Port: %d
swapTask: flashSectorAddr failed
SwapTask: ERROR reading
SwapTask: ERROR when get productID
swapTask READ_CMD: flashAdrs(0x%x) out of range
swapTask READ_CMD: ERROR bad size
SwapTask ERASE_CMD: Bad Sector
get the sector number of nvram  0x %x first
SwapTask ERASE_CMD: Erase Failed
get the sector number of nvram  0x %x second
get the sector number of nvram  0x %x third
get the sector number of nvram  0x %x forth
swapTask WRITE_CMD: flashAdrs(0x%x) out of range
swapTask WRITE_CMD: ERROR bad size
SwapTask WRITE_CMD: ERROR reading data
SwapTask WRITE_CMD: FlashWrite Failed
SwapTask: Unknown command(0x%x)
SwapTask: exiting
 ERROR: testPST state is not set by MMI !
Enter SWAP Task
tswapTask
ERROR: taskSpawn(swap_Start) failed
 Web-authenticatoin User Agent 1.0, Build on 2005-06-26, Copyright(c) 2005-2008 by UTStarcom, Inc.
<%s> msgQReceive Error!
wua_task
 <%s> wua_get_dft_script_name fail! 
wua_init
flash/script/
<%s> --> wua_parse_script fail!!
<%s> malloc fail (%dbytes)
(<%s> run
wua_free_ins
(<%s> invalid state=%d
wua_state_processing
<%s> reach end, state=%d, event_id=%d
<%s> event match, state=%d, event_id=%d
<%s> reach xxx, state=%d, event_id=%d
<%s> FSM_FAILURE, clr instance.
<%s> FSM_IGNORE, do nothing
<%s> reach STATE_IDLE, clr instance
<%s> Error, Not find event match! clr instance.
 200
<%s> 200: start to match keyword(%s)
wua_match_msgtype
<%s> not match
<%s> match
MMI_LOGIN_REQ
USER_INPUT_RSP
 GET
POST
USER_INPUT_REQ
MMI_RESULT_OK
MMI_RESULT_ERROR
<%s> invalid action is fsm_tbl
wua_run_action
 <%s> <- MMIWUA_DOWNLOAD_SCRIPT_REQ
wua_hndl_mmimsg
<%s> <- MMIWUA_LOGIN_REQ
<%s> <- MMIWUA_USER_INPUT_RSP
<%s> <- MMIWUA_AUTH_STOP_REQ
<%s> <- MMIWUA_ACTIVE_SCRIPT_REQ
<%s> <- Unknown Msg(%d)
 <%s> <- MSG_200
wua_hndl_wuamsg
<%s> <- MSG_XXX
<%s> <- Unknown Msg(%d), source=WUA
 <%s> strdup fail!
wua_hndl_downloadreq
(<%s> DOWNLAOD SCRIPT FIRST! or state(%d) error!
wua_hndl_authstart
 <%s> user_input=%s, size=%d
wua_hndl_uinput
(<%s> wua_get_dft_script_cont fail
wua_hndl_actscriptreq
<%s> It's not valid script file
<%s> wua_parse_script fail! 
<%s> wua_hndl_actscriptreq sucessfully
 META_REFRESH
<%s> final_url is different, url=%s
wua_hndl_get_req
<%s> other status_code(%d)
<%s> htc_get_file fail, ret=%d
 <%s> wua_compose_urlenc fail
wua_hndl_post_req
<%s> final_enc=%s
<%s> parse_url fail, ret=%d
<%s> htc_session_start fail, ret=%d
en-us
application/x-www-form-urlencoded
utstarcom wifi phone
Content-Length: %d
POST
<%s> htc_snd_request fail, ret=%d
 <%s> wua_snd_uinput_req fail
wua_hndl_uinput_req
 <%s> oapi_malloc(size=%d) fail
wua_snd_uinput_req
<%s> -> WUAMMI_USER_INPUT_REQ, str=%s
(%s%s%s
name="%s"
value
 $%s
 <%s> send %d to wua
wua_send_wuamsg
(<%s> send %d to mmi(rslt=%d)
wua_send_mmirsp
(URL=
<%s> htc_get_filelen fail, ret=%d
wua_get_rfrshloc
<%s> tmp file len <= 0, error!
<%s> calloc fail (%dbytes)
<%s> open file fail
<%s> fread fail, len=%d
<%s> Found META_REFRESH: %s
##<!@UTSTARCOM WIFI PHONE
<%s> wua_dnld_script fail! (ret=%d)
wua_handle_script
<%s> It's not valid script file
ram/script.tmp
flash/script.txt
 <%s> oapi_calloc fail! 
wua_dnld_script
<%s> open file error! 
<%s> get file len error! (ret=%d)
<%s> dnld script fail(ret=%d)
 <%s> lexical analyze fail!
wua_parse_script
RESPONSE:
BREAK
MMI_LOGIN_REQ
WITH
%s%s
 flash/script/
mkdir %s
wua_init_scriptfile fail
 opendir fail!
find %s
ignore it, %s
find default, i=%d
error reading dir %s, errno: %x
readdir finish!
(<%s> Length is too short!
wua_validate_script
 wrong index(%d)
 (0K
 <%s> wua_rename_script fail
wua_set_dft_script
(filename len is too long
d_1_
n_1_
file(%s) exist, remove it
<%s> fopen %s failed
wua_fopen
d_2_
n_2_
d_3_
n_3_
d_4_
n_4_
<wua_fopen> do as fopen %d
 <0K
 <0K
(<%s> wua_get_dft_script fail! 
wua_get_dft_script_cont
<%s> wua_fopen fail! 
<%s> wua_fread fail! 
(HTTP Client Stack 1.1, Build on 2005-08-25, Copyright(c) 2005-2008 by UTStarcom, Inc.
HTTP_MTX
<%s> oapi_mutex_create fail! ret=%d
htc_init
 http://
https://
 0@-
 <%s> malloc fail, size=%d
strdup
 <%s> local_htc_session_allocbuf fail, ret=%d
htc_session_start
<%s> strdup fail
<%s> htc_conn fail, ret=%d
 <%s> fatal error, session_id=%d is invalid
htc_session_stop
<%s> session is idle, fatal error
 htc_session_renew
<%d:%s> host=%s, port=%d
<%s> oapi_mutex_unlock fail!
local_htc_session_assign
<%s> Can't find a free session!
 0@-
(<%d:%s> Error! Outbuf is not free!
local_htc_session_allocbuf
<%d:%s> Error! Inbuf is not free!
<%s> Alloc memory fail, size=%d
 <%s> input parameter error!
htc_resolve
<%s> hostname=%s
<%s> hostname is ip_addr
<%s> malloc fail, size=513
<%s> resolvGetHostByName fail!
 <%s> fatal error, session_id=%d is invalid
htc_conn
<%s> session is idle, fatal error
<%s> host=%s, ip_addr=%s
<%s> local_http_dns_resolve fail
<%s> connect to %s:%d...
<%s> connect fail !
<%s> connect ok
 htc_disc
<%d:%s> shutdown socket
 htc_snd
<%d:%s> send Fail (len=%d)!
 htc_rcv
<%s> recv start...
<%s> recv fail or timeout
<%s> recv ok, %d bytes
 HTTP/1.1
HTTP/1.0
<%s> htc_session_start fail, ret=%d
htc_get_file
en-us
utstarcom wifi phone
Keep-Alive
 htc_put_file
<%s> fatal error, session_id=%d is invalid
htc_snd_request
<%s> session is idle, fatal error
<%d:%s> mthd=%s, path=%s, locfile=%s, need_sts=%d
<%d:%s> htc_snd_msg fail, ret=%d
<%d:%s> htc_rcv_rsp_hdr fail, ret=%d
<%d:%s> htc_get_status_code fail, ret=%d
<%d:%s> lcl_htc_hndl_200 fail, ret=%d
Location
<%d:%s> 302, but no Location
<%d:%s> htc_session_renew fail, ret=%d
<%d:%s> other status-code(%d)
 htc_snd_msg
%s %s %s
 htc_rcv_rsp_hdr
<%d:%s> rcv 1st package fail, ret=%d
<%d:%s> parse_status_line fail
<%s> lcl_htc_parse_rsp fatal error!
<%s> header is not complete, read %dth pacakge
<%s> header does not complete in 5 packages
<%d:%s> htc_rcv fail, ret=%d
 htc_rcv_rsp_bdy
<%s> last package exist, s->in_buf_len=%d
<%s> htc_rcv fail, ret=%d
 htc_schedule_standard
Host: %s
Host: %s:%d
 htc_schedule_payload
<%s> fatal error, strdup fail
<%s> fail, fields full!
 htc_schedule_field
Accept: %s
Accept-Charset: %s
Accept-Encoding: %s
Accept-Language: %s
Authorization: %s
Connection: %s
Content-Type: %s
Date: %s
Expect: %s
From: %s
Host: %s
If-Match: %s
If-Modified-Since: %s
If-None-Match: %s
If-Range: %s
If-Unmodified-Since: %s
Max-Forwards: %s
Proxy-Authorization: %s
Range: %s
Referer: %s
TE: %s
User-Agent: %s
 htc_unschedule_all
 htc_resend_last_req
<%s> out_buf is empty.
 htc_get_status_code
 htc_get_field
 htc_free_rsp_data
<%s> realloc fail
lcl_htc_parse_rsp
<%s> strdup fail(1)
<%s> strdup fail(2)
<%s> add_char fail
<%s> ok, offset=%d
<%s> fail
lcl_htc_parse_status_line
<%s> fopen fail
lcl_htc_hndl_200
Content-Length
<%s> no 'Content-Length' field
<%s> content-length: %d
******data of eloop******
user data : 0x%x
max_sock: %d, reader_count: %d
num: %02d,sock: 0x%x, eloop: 0x%x,user: 0x%x, handler: 0x%x
no time out node
num: %d, sec: %u,usec: %u,eloop: 0x%x, user: 0x%x, handler: %x
signal_count %d
no signals
sig: %d,user: 0x%x, handler: 0x%x, signaled: %d
signaled: %d,pending_terminate: %d, terminate: %d
(eloop: could not process SIGINT or SIGTERM in two seconds. Looks like there
is a bug that ends up in a busy loop that prevents clean shutdown.
Killing program forcefully.
 0@-
 0@-
 select
(gfff<eloop_terminate> statu is %d
<eloop_terminate>wait for wpa terminate,eloop status:%d
([wpa_drv_scan]Scan SSID
 PMK Name
 RSN: removed current PMKSA entry
 RSN: expired PMKSA cache entry for %02x:%02x:%02x:%02x:%02x:%02x
 0@-
 RSN: removed the oldest PMKSA cache entry (for %02x:%02x:%02x:%02x:%02x:%02x) to make room for new one
RSN: added PMKSA cache entry for %02x:%02x:%02x:%02x:%02x:%02x
 0@-
Index / AA / PMKID / expiration (in seconds)
%d %02x:%02x:%02x:%02x:%02x:%02x 
%02x
%s: ie len too short %u
wpa_parse_wpa_ie_wpa
dump_WPAIE:
%s: malformed ie or unknown version
group_cipher:
%s: ie length mismatch, %u too much
group-cipher ie:0x%x
%s: ie count botch (pairwise), count %u left %u
%s: ie too short (for key mgmt)
pairwise_cipher ie:0x%x
%s: ie count botch (key mgmt), count %u left %u
%s: ie too short (for capabilities)
%s: ie has %u trailing bytes
 wpa_parse_wpa_ie_rsn
%s: PMKID underflow (num_pmkid=%d left=%d)
%s: ie has %u trailing bytes - ignored
 p@-
Invalid group cipher (%d).
Invalid pairwise cipher (%d).
Invalid key management type (%d).
 p@-
Pairwise key expansion
WPA: PMK
WPA: PTK
 Could not read SSID from driver.
Could not read BSSID from driver.
 0@-
Failed to read BSSID for EAPOL-Key request
WPA: Sending EAPOL-Key Request (error=%d pairwise=%d ptk_set=%d len=%d)
WPA: TX EAPOL-Key Request
 WPA: setting dhcpWaitForWpa HIGH in wpa_supplicant_process_1_of_4()
WPA: RX message 1 of 4-Way Handshake from %02x:%02x:%02x:%02x:%02x:%02x (ver=%d)
WPA: No SSID info found (msg 1 of 4).
RSN: msg 1/4 key data
RSN: key data underflow (ie=%d len=%d)
RSN: PMKID from Authenticator
WPA: Failed to generate WPA IE (for msg 2 of 4).
WPA: WPA IE for msg 2/4
WPA:replay counter
WPA: Failed to get random data for SNonce
WPA: Renewed SNonce
RSN: found matching PMKID from PMKSA cache
RSN: no matching PMKID found
RSN: matched PMKID
RSN: PMK from PMKSA cache
WPA: PMK from EAPOL state machines
RSN: the new PMK matches with the PMKID
WPA: Failed to get master session key from EAPOL state machines
WPA: Key handshake aborted
RSN: Cancelled PMKSA caching attempt
RSN: no PMKSA entry found - trigger full EAP authenication
WPA: EAPOL-Key MIC
WPA: Sending EAPOL-Key 2/4
WPA: TX EAPOL-Key 2/4
 WPA: Key negotiation completed with %02x:%02x:%02x:%02x:%02x:%02x [PTK=%s GTK=%s]
WPA: setting dhcpWaitForWpa  LOW in wpa_supplicant_key_neg_complete()
WPA: setting dhcpWaitForWpaEap LOW in wpa_supplicant_key_neg_complete()
(WPA: Installing PTK to the driver.
WPA: Pairwise Cipher Suite: NONE - do not use pairwise keys
WPA: Unsupported pairwise cipher %d
WPA: RSC
WPA: Failed to set PTK to the driver.
 WPA: Unsupported CCMP Group Cipher key length %d (%d).
WPA: Unsupported TKIP Group Cipher key length %d (%d).
WPA: Unsupported WEP104 Group Cipher key length %d (%d).
WPA: Unsupported WEP40 Group Cipher key length %d (%d).
WPA: Unsupport Group Cipher %d
 WPA: Group Key
WPA: Installing GTK to the driver (keyidx=%d tx=%d).
WPA: Failed to set GTK to the driver (Group only).
WPA: Failed to set GTK to the driver.
 RSN: received GTK in pairwise handshake
RSN: Tx bit set for GTK IE, but pairwise keys are used - ignore Tx bit
 WPA: %s (src=%02x:%02x:%02x:%02x:%02x:%02x)
WPA: WPA IE in Beacon/ProbeResp
WPA: No WPA IE in Beacon/ProbeResp
WPA: WPA IE in 3/4 msg
WPA: RSN IE in Beacon/ProbeResp
WPA: No RSN IE in Beacon/ProbeResp
WPA: RSN IE in 3/4 msg
 WPA: RX message 3 of 4-Way Handshake from %02x:%02x:%02x:%02x:%02x:%02x (ver=%d)
WPA: IE KeyData
WPA: key data underflow (ie=%d len=%d)
WPA: GTK IE in unencrypted key data
IE in 3/4 msg does not match with IE in Beacon/ProbeResp
Possible downgrade attack detected - RSN was enabled and RSN IE was in msg 3/4, but not in Beacon/ProbeResp
WPA: ANonce from message 1 of 4-Way Handshake differs from 3 of 4-Way Handshake - drop packet (src=%02x:%02x:%02x:%02x:%02x:%02x)
WPA: Invalid CCMP key length %d (src=%02x:%02x:%02x:%02x:%02x:%02x)
WPA: Invalid TKIP key length %d (src=%02x:%02x:%02x:%02x:%02x:%02x)
WPA: Sending EAPOL-Key 4/4
WPA: TX EAPOL-Key 4/4
 WPA: RX message 1 of Group Key Handshake from %02x:%02x:%02x:%02x:%02x:%02x (ver=%d)
WPA: No GTK IE in Group Key message 1/2
WPA: Truncated EAPOL-Key packet: key_data_length=%d > extra_len=%d
RSN: received GTK in group key handshake
RSN: Too long GTK in GTK IE (len=%d)
WPA: Unsupported AES-WRAP len %d
WPA: AES unwrap failed - could not decrypt GTK
WPA: Tx bit set for GTK, but pairwise keys are used - ignore Tx bit
WPA: Sending EAPOL-Key 2/2
WPA: TX EAPOL-Key 2/2
WPA: Group rekeying completed with %02x:%02x:%02x:%02x:%02x:%02x [GTK=%s]
 WPA: Invalid EAPOL-Key MIC when using TPTK - ignoring TPTK
WPA: Invalid EAPOL-Key MIC - dropping packet
WPA: Could not verify EAPOL-Key MIC - dropping packet
 RSN: encrypted key data
WPA: PTK not available, cannot decrypt EAPOL-Key key data.
WPA: No memory for AES-UNWRAP buffer
WPA: AES unwrap failed - could not decrypt EAPOL-Key key data
WPA: decrypted EAPOL-Key key data
 WPA: EAPOL frame too short, len %u, expecting at least %u
IEEE 802.1X RX: version=%d type=%d length=%d
WPA: EAPOL frame (type %u) discarded, not a Key frame
WPA: Cancelling PMKSA caching attempt - attempt full EAP authentication
WPA: EAPOL frame payload size %u invalid (frame size %u)
  EAPOL-Key type=%d
WPA: EAPOL-Key type (%d) unknown, discarded
WPA: RX EAPOL-Key
WPA: ignoring %d bytes after the IEEE 802.1X data
WPA: Unsupported EAPOL-Key descriptor version %d.
WPA: CCMP is used, but EAPOL-Key descriptor version (%d) is not 2.
WPA: Backwards compatibility: allow invalid version for non-CCMP group keys
WPA: EAPOL-Key Replay Counter did not increase - dropping packet
WPA: No Ack bit in key_info
WPA: EAPOL-Key with Request bit - dropped
WPA: Invalid EAPOL-Key frame - key_data overflow (%d > %d)
WPA: Ignored EAPOL-Key (Pairwise) with non-zero key index
WPA: EAPOL-Key (Group) without Mic bit - dropped
 RX EAPOL from %02x:%02x:%02x:%02x:%02x:%02x
RX EAPOL
WPA: Countermeasures - dropped EAPOL packet
WPA: setting dhcpWaitForWpaEap HIGH in wpa_supplicant_rx_eapol()
WPA: IEEE802_1X_TYPE_EAPOL_START
WPA: IEEE802_1X_TYPE_EAPOL_LOGOFF
WPA: IEEE802_1X_TYPE_EAPOL_KEY
WPA: IEEE802_1X_TYPE_EAPOL_ENCAPSULATED_ASF_ALERT
(dot11RSNAConfigVersion=%d
dot11RSNAConfigPairwiseKeysSupported=5
dot11RSNAConfigGroupCipherSize=%d
dot11RSNAConfigPMKLifetime=%d
dot11RSNAConfigPMKReauthThreshold=%d
dot11RSNAConfigNumberOfPTKSAReplayCounters=1
dot11RSNAConfigSATimeout=%d
dot11RSNAAuthenticationSuiteSelected=%02x-%02x-%02x-%d
dot11RSNAPairwiseCipherSelected=%02x-%02x-%02x-%d
dot11RSNAGroupCipherSelected=%02x-%02x-%02x-%d
dot11RSNAPMKIDUsed=%s
dot11RSNAAuthenticationSuiteRequested=%02x-%02x-%02x-%d
dot11RSNAPairwiseCipherRequested=%02x-%02x-%02x-%d
dot11RSNAGroupCipherRequested=%02x-%02x-%02x-%d
dot11RSNAConfigNumberOfGTKSAReplayCounters=0
 RX pre-auth from %02x:%02x:%02x:%02x:%02x:%02x
RX pre-auth
RSN pre-auth frame received from unexpected source %02x:%02x:%02x:%02x:%02x:%02x - dropped
 RSN: pre-authentication with %02x:%02x:%02x:%02x:%02x:%02x %s
completed successfully
failed
RSN: PMK from pre-auth
RSN: failed to get master session key from pre-auth EAPOL state machines
 RSN: pre-authentication with %02x:%02x:%02x:%02x:%02x:%02x timed out
 RSN: starting pre-authentication with %02x:%02x:%02x:%02x:%02x:%02x
RSN: Failed to initialize L2 packet processing for pre-authentication
Failed to allocate EAPOL context.
RSN: Failed to initialize EAPOL state machines for pre-authentication
 0@-
 RSN: processing PMKSA candidate list
RSN: not in suitable state for new pre-authentication
RSN: PMKSA candidate %02x:%02x:%02x:%02x:%02x:%02x selected for pre-authentication
RSN: PMKSA candidate %02x:%02x:%02x:%02x:%02x:%02x does not need pre-authentication anymore
RSN: no more pending PMKSA candidates
 RSN: added PMKSA cache candidate %02x:%02x:%02x:%02x:%02x:%02x prio %d
[wpa_drv_scan]Scan SSID
 WPA: drop TX EAPOL in non-IEEE 802.1X mode (type=%d len=%d)
RSN: PMKSA caching - do not send EAPOL-Start
BSSID not set when trying to send an EAPOL frame
Using current BSSID %02x:%02x:%02x:%02x:%02x:%02x from the driver as the EAPOL destination
Using the source address of the last received EAPOL frame %02x:%02x:%02x:%02x:%02x:%02x as the EAPOL destination
TX EAPOL
 TX EAPOL (preauth)
 p@-
 WPA: Invalid mode %d (not IBSS/ad-hoc) for WPA-None
WPA: No PSK configured for WPA-None
WPA: Invalid group cipher %d for WPA-None
 WPA: EAPOL processing complete
WPA: setting dhcpWaitForWpaEap LOW in wpa_supplicant_notify_eapol_done()
(0@-
(Setting scan request: %d sec %d usec
 Cancelling scan request
 Authentication with %02x:%02x:%02x:%02x:%02x:%02x timed out.
 Setting authentication timeout: %d sec %d usec
 Cancelling authentication timeout
 WPA: setting dhcpWaitForWpaEap HIGH in wpa_supplicant_initiate_eapol()
(p@-
No network configuration found for the current AP
Network configuration found for the current AP
 0@-
No keys have been configured - skip key clearing
 WPA: TKIP countermeasures stopped
 0@-
RSN: PMKID from assoc IE %sfound from PMKSA cache
not 
 RSN: No data in PMKID candidate event
RSN: PMKID candidate event - bssid=%02x:%02x:%02x:%02x:%02x:%02x index=%d preauth=%d
RSN: Ignored PMKID candidate without preauth flag
Association event - clear replay counter
Associated to a new BSS: BSSID=%02x:%02x:%02x:%02x:%02x:%02x
Associated with %02x:%02x:%02x:%02x:%02x:%02x
Diconnect event - ignore in IBSS/WPA-None mode
Disconnect event - remove keys
Michael MIC failure detected
TKIP countermeasures started
Association info event
req_ies
resp_ies
Truncated IE in assoc_info
assoc_wpa_ie
Configured interface was added.
Failed to initialize the driver after interface was added.
Configured interface was removed.
Unknown event %d
 Signal %d received - terminating
 Failed to parse the configuration file '%s' - exiting
Reconfiguration completed
 Signal %d received - reconfiguring
 Already associated with a configured network - generating associated event
 [EricTest]  SSID[%d]:%s(scan:%s)
Starting AP scan (%s SSID)
specific
broadcast
Scan SSID
Failed to initiate AP scan.
WPA: Failed to parse WPA IE from association info
WPA: Using WPA IE from AssocReq to set cipher suites
WPA: Driver used disabled group cipher 0x%x (mask 0x%x) - reject
WPA: Driver used disabled pairwise cipher 0x%x (mask 0x%x) - reject
WPA: Driver used disabled key management 0x%x (mask 0x%x) - reject
 RSN: using IEEE 802.11i/D9.0
WPA: using IEEE 802.11i/D3.0
WPA: Set cipher suites based on configuration
WPA: Failed to parse WPA IE for the selected BSS.
WPA: Selected cipher suites: group %d pairwise %d key_mgmt %d
WPA: malloc failed
WPA: using GTK CCMP
WPA: using GTK TKIP
WPA: using GTK WEP104
WPA: using GTK WEP40
WPA: Failed to select group cipher.
WPA: using PTK CCMP
WPA: using PTK TKIP
WPA: using PTK NONE
WPA: Failed to select pairwise cipher.
WPA: using KEY_MGMT 802.1X
WPA: using KEY_MGMT WPA-PSK
WPA: using KEY_MGMT WPA-NONE
WPA: Failed to select authenticated key management type.
WPA: Failed to generate WPA IE.
WPA: Own WPA IE
WPA: ==PMK==
 Trying to associate with %02x:%02x:%02x:%02x:%02x:%02x (SSID='%s' freq=%d MHz)
Trying to associate with SSID '%s'
Automatic auth_alg selection: 0x%x
Overriding auth_alg selection: 0x%x
RSN: PMKID
WPA: Failed to set WPA key management and encryption suites
WPA: Failed to set WPA key management and encryption suites (no scan results)
 permanent identity from IMSI
 Selected network is configured to use SIM - initialize PCSC
Failed to initialize SIM (pcsc-lite)
Failed to get IMSI from SIM
IMSI
 Selecting BSS from priority group %d
%d: %02x:%02x:%02x:%02x:%02x:%02x ssid='%s' wpa_ie_len=%d rsn_ie_len=%d
   skip - no WPA/RSN IE
   skip - SSID mismatch
   skip - BSSID mismatch
   skip - could not parse WPA/RSN IE
   skip - proto mismatch
   skip - PTK cipher mismatch
pairwise cipher ie:0x%x (config 0x%x)
   skip - GTK cipher mismatch
group cipher ie:0x%x (config 0x%x)
   skip - key mgmt mismatch
   selected
   selected non-WPA AP %02x:%02x:%02x:%02x:%02x:%02x ssid='%s'
 Number of Scan results: %d
Failed to get number of scan results -  assume the maximum
No scan results - try scanning again
Failed to allocate for scan results - try scanning again
Scan results: %d
Failed to get scan results - try scanning again
Not enough room for all APs (%d < %d)
Already associated with the selected AP.
No suitable AP found.
 No driver interfaces build into wpa_supplicant.
Unsupported driver '%s'.
Waiting for interface..
Failed to get own L2 address
Own MAC address: %02x:%02x:%02x:%02x:%02x:%02x
Failed to enable WPA in the driver.
Initializing interface '%s' conf '%s' driver '%s'
default
Failed to get absolute path for configuration file '%s'.
Configuration file '%s' -> '%s'
Failed to read configuration file '%s'.
No networks (SSID) configured.
Interface name is required.
Too long interface name '%s'.
 Initializing interface (2) '%s'
Failed to allocate EAPOL context.
Failed to initialize EAPOL state machines.
Failed to initialize driver interface
Driver interface replaced interface name with '%s'
Failed to initialize control interface '%s'.
You may have another wpa_supplicant process already running or the file was
left by an unclean termination of wpa_supplicant in which case you will need
to manually remove this file before starting wpa_supplicant again.
 Failed to disable WPA in the driver.
delete wap task force, task id:%d, result: 0x%x
end of <deleteWpaTaskForce>
 end of eloop_run
end of wpa_supplicant_deauthenticate
end of wpa_supplicant_deinit
end of eloop_destroy
 tWpa
[wpa_drv_scan]Scan SSID
[WPADrivers]wpa_driver_hermes_scan_timeout() - Scan timeout - try to get results
 [WPADrivers]Processing PMKSA scan
[WPADrivers]Adding PMKID candidate on %02x:%02x:%02x:%02x:%02x:%02x
[WPADrivers]wpa_driver_hermes_pmksa_process() - setting PMKSA scan timeout 
 [WPADrivers]Initiating PMKSA scan on %s
 [WPADrivers]Called: wpa_driver_hermes_unsolicited_message 
[WPADrivers]wpa_driver_hermes_unsolicited_message() - scan complete
[WPADrivers]wpa_driver_hermes_unsolicited_message() - supplicant initiated scan, notifying
[WPADrivers]wpa_driver_hermes_unsolicited_message() - NON NON NON supplicant initiated scan complete 
[WPADrivers]wpa_driver_hermes_unsolicited_message() - got message of link-stat
[WPADrivers]wpa_driver_hermes_unsolicited_message() - got message of %d
[WPADrivers]wpa_driver_hermes_unsolicited_message() - assoc_wpa_ie_len=%d type=%d
[WPADrivers]wpa_driver_hermes_unsolicited_message() - RSN IE
[WPADrivers]num pmkid is %d, subtracting %d bytes from RSN IE
[WPADrivers]Assoc RSN IE len %d, valid len %d
[WPADrivers]wpa_driver_hermes_unsolicited_message() - reporting RSN IE
[WPADrivers]wpa_driver_hermes_unsolicited_message() - scan response=%d
[WPADrivers]wpa_driver_hermes_unsolicited_message() - Found matching RSN-IE scan result for new AP
**** Old RSN IE **** 
**** New RSN IE **** 
[WPADrivers]wpa_driver_hermes_unsolicited_message() -setting PMKSA scan timeout 
[WPADrivers]wpa_driver_hermes_unsolicited_message() - cancelling PMKSA scan timeout 
[WPADrivers]wpa_driver_hermes_unsolicited_message() - CFG_SECURITY_STAT
[WPADrivers]wpa_driver_hermes_unsolicited_message() - CFG_REASSOC_EVENT_PENDING
[WPADrivers]wpa_driver_hermes_unsolicited_message() - unhandled 0x%04x
[WPADrivers]Called: wpa_driver_hermes_set_wpa
[WPADrivers]%s: enabled=%d
wpa_driver_hermes_set_wpa
 [WPADrivers]%s: priv=%p alg=%d key_idx=%d set_tx=%d
wpa_driver_hermes_set_key
[WPADrivers]wpa_driver_hermes_set_key-WPA_ALG_WEP
[WPADrivers]wpa_driver_hermes_set_key-WPA_ALG_TKIP
[WPADrivers][UILPutInfo]tkipKey
[WPADrivers][UILPutInfo]txMICKey
[WPADrivers][UILPutInfo]rxMICKey
[WPADrivers][UILPutInfo]encryptionKey
[WPADrivers][UILPutInfo]txMicKey
[WPADrivers][UILPutInfo]rxMicKey
[WPADrivers]wpa_driver_hermes_set_key-WPA_ALG_CCMP
[WPADrivers]wpa_driver_hermes_set_key-WPA_ALG_NONE
[WPADrivers]CIPHER_WEP40/CIPHER_WEP104
[WPADrivers]CIPHER_TKIP
[WPADrivers]CIPHER_CCMP
[WPADrivers]CIPHER_NONE
 wvlan
[WPADrivers]Called: wpa_driver_hermes_init
[WPADrivers]Called: wpa_driver_hermes_set_countermeasures
 [WPADrivers]Called: wpa_driver_hermes_set_drop_unencrypted
 [WPADrivers]wpa_driver_hermes_scan() - cancelling PMKSA scan timeout 
[WPADrivers]wpa_driver_hermes_scan() - Supplicant initiating scan on %s
 [WPADrivers]Old scan results (%d) new scan results (%d)
[WPADrivers]free'ing drv->srt (0x%08x) %d bytes
[WPADrivers]Scan result (%d) %02x:%02x:%02x:%02x:%02x:%02x
[WPADrivers]**** Scan RSN IE **** 
SSID=%s
 [WPADrivers]Called: wpa_driver_hermes_deauthenticate
 [WPADrivers]Called: wpa_driver_hermes_disassociate
 [WPADrivers]Called: wpa_driver_hermes_associate
[WPADrivers]%s: priv=%p freq=%d pairwise_suite=%d group_suite=%d key_mgmt_suite=%d auth_alg=%d mode=%d
wpa_driver_hermes_associate() - error setting desired SSID(%d)
WPA: setting dhcpWaitForWpa HIGH in wpa_driver_hermes_associate()
wpa_driver_hermes_associate() - unknown pairwise suite(%d)
WPA: setting dhcpWaitForWpaEap HIGH in wpa_driver_hermes_associate()
 [WPADrivers]Called: wpa_driver_hermes_set_auth_alg
 [WPADrivers]wpa_driver_hermes_add_pmkid - BSSID 
[WPADrivers]wpa_driver_hermes_add_pmkid - PMKID 
[WPADrivers]Called: wpa_driver_hermes_get_num_scan_results
 Agere Systems Hermes 2.5.3 / Beagle driver
hermes
%s - hexdump(len=%d):
 %02x
<%02x>
  [REMOVED]
(%s - hexdump_ascii(len=%d): [REMOVED]
%s - hexdump_ascii(len=%d):
    
Line %d: failed to parse %s '%s'.
Line %d: too short %s (len=%d min_len=%d)
Line %d: too long %s (len=%d max_len=%d)
 %s=%d (0x%x)
Line %d: too small %s (value=%d min_value=%d)
Line %d: too large %s (value=%d max_value=%d)
 Line %d: Invalid BSSID '%s'.
BSSID
 Line %d: Invalid passphrase length %d (expected: 8..63) '%s'.
PSK (ASCII passphrase)
Line %d: Invalid PSK '%s'.
 WPA
WPA2
Line %d: invalid proto '%s'
Line %d: no proto values configured.
proto: 0x%x
 WPA-PSK
WPA-EAP
IEEE8021X
NONE
WPA-NONE
Line %d: invalid key_mgmt '%s'
Line %d: no key_mgmt values configured.
key_mgmt: 0x%x
 CCMP
TKIP
WEP104
WEP40
Line %d: invalid cipher '%s'.
Line %d: no cipher values configured.
 Line %d: not allowed pairwise cipher (0x%x).
pairwise: 0x%x
 Line %d: not allowed group cipher (0x%x).
group: 0x%x
 OPEN
SHARED
LEAP
Line %d: invalid auth_alg '%s'
Line %d: no auth_alg values configured.
auth_alg: 0x%x
 Line %d: unknown EAP method '%s'
You may need to add support for this EAP method during wpa_supplicant
build time configuration.
See README for more information.
eap methods
 Line %d: Invalid WEP key %d '%s'.
Line %d: Too long WEP key %d '%s'.
wep_key%d
mode
pac_file
eap_workaround
priority
wep_tx_keyidx
wep_key3
wep_key2
wep_key1
wep_key0
eapol_flags
pcsc
phase2
phase1
subject_match2
dh_file2
private_key2_passwd
private_key2
client_cert2
ca_cert2
subject_match
dh_file
private_key_passwd
private_key
client_cert
ca_cert
password
server_nai
eappsk
anonymous_identity
identity
auth_alg
group
pairwise
key_mgmt
proto
bssid
scan_ssid
ssid
Line: %d - start of a new network block
Line %d: Invalid SSID line '%s'.
Line %d: invalid quotation '%s'.
Line %d: unknown network field '%s'.
Line %d: network block was not terminated properly.
Line %d: both PSK and passphrase configured.
PSK (from passphrase)
Line %d: WPA-PSK accepted for key management, but no PSK configured.
Line %d: removed CCMP from group cipher list since it was not allowed for pairwise cipher
Reading configuration file '%s'
network={
Line %d: failed to parse network block.
Line %d: failed to add network block to priority list.
eapol_version=
Line %d: Invalid EAPOL version (%d): '%s'.
eapol_version=%d
ap_scan=
ap_scan=%d
fast_reauth=
fast_reauth=%d
Line %d: Invalid configuration line '%s'.
Priority group %d
   id=%d ssid='%s'
 p@-
WEP-40
WEP-104
UNKNOWN
 WPA2/IEEE 802.1X/EAP
WPA/IEEE 802.1X/EAP
WPA2-PSK
IEEE 802.1X (no WPA)
EAP: deinitialize previously used EAP method (%d, %s) at %s
 EAP: EAP entering state INITIALIZE
EAP: maintaining EAP method data for fast reauthentication
INITIALIZE
 EAP: EAP entering state DISABLED
 EAP: EAP entering state IDLE
 EAP: EAP entering state RECEIVED
 EAP: EAP entering state GET_METHOD
EAP: using previous method data for fast re-authentication
GET_METHOD
EAP: initialize selected EAP method (%d, %s)
EAP: Failed to initialize EAP method %d
 EAP: EAP entering state METHOD
EAP::METHOD - method not selected
EAP: method process -> ignore=%s methodState=%s decision=%s
TRUE
FALSE
 EAP: EAP entering state SEND_RESPONSE
 EAP: EAP entering state DISCARD
 EAP: EAP entering state IDENTITY
 EAP: EAP entering state NOTIFICATION
 EAP: EAP entering state RETRANSMIT
 EAP: EAP entering state SUCCESS
 EAP: EAP entering state FAILURE
 EAP: Workaround for unexpected identifier field in EAP Success: reqId=%d lastId=%d (these are supposed to be same)
 EAP: more than %d authentication rounds - abort
EAP: AS used the same Id again, but EAP packets were not identical
EAP: workaround - assume this is not a duplicate packet
(EAP: Building EAP-Nak (requested type %d not allowed)
EAP: allowed methods
 EAP: EAP-Request Identity data
 EAP: buildIdentity: configuration was not available
EAP: using method re-auth identity
EAP: using anonymous identity
EAP: using real identity
EAP: buildIdentity: identity configuration was not available
 EAP: EAP-Request Notification data
 EAP: Generating EAP-Response Notification
 EAP: Ignored truncated EAP-Packet (len=%d plen=%d)
EAP: Received EAP-Request method=%d id=%d
EAP: Received EAP-Response for LEAP method=%d id=%d
EAP: Ignored EAP-Response
EAP: Received EAP-Success
EAP: Received EAP-Failure
EAP: Ignored EAP-Packet with unknown code %d
EAP deinit
 p@-
DISABLED
IDLE
RECEIVED
METHOD
SEND_RESPONSE
DISCARD
IDENTITY
NOTIFICATION
RETRANSMIT
SUCCESS
FAILURE
UNKNOWN
 NONE
INIT
CONT
MAY_CONT
DONE
 FAIL
COND_SUCC
UNCOND_SUCC
 EAP state=%s
selectedMethod=%d (EAP-%s)
reqMethod=%d
methodState=%s
decision=%s
ClientTimeout=%d
 Identity
PASSWORD
Password
CTRL-REQ-%s-%d:%s needed for SSID %s
EAP-MD5: Password not configured
EAP-MD5: Invalid frame
EAP-MD5: Invalid challenge (challenge_len=%d len=%d
EAP-MD5: Challenge
EAP-MD5: generating Challenge Response
EAP-MD5: Response
 EAPOL: SUPP_PAE entering state LOGOFF
 EAPOL: SUPP_PAE entering state DISCONNECTED
 EAPOL: SUPP_PAE entering state CONNECTING
 EAPOL: SUPP_PAE entering state AUTHENTICATING
 EAPOL: SUPP_PAE entering state HELD
 EAPOL: SUPP_PAE entering state AUTHENTICATED
 EAPOL: SUPP_PAE entering state RESTART
 EAPOL: SUPP_PAE entering state S_FORCE_AUTH
 EAPOL: SUPP_PAE entering state S_FORCE_UNAUTH
 EAPOL: IEEE 802.1X for plaintext connection; no EAPOL-Key frames required
 EAPOL: KEY_RX entering state NO_KEY_RECEIVE
 EAPOL: KEY_RX entering state KEY_RECEIVE
EAPOL: SUPP_BE entering state REQUEST
 EAPOL: SUPP_BE entering state RESPONSE
 EAPOL: SUPP_BE entering state SUCCESS
 EAPOL: SUPP_BE entering state FAIL
 EAPOL: SUPP_BE entering state TIMEOUT
 EAPOL: SUPP_BE entering state IDLE
 EAPOL: SUPP_BE entering state INITIALIZE
 EAPOL: SUPP_BE entering state RECEIVE
 EAPOL: SUPP_BE REQUEST: both eapResp and eapNoResp set?!
 EAPOL: txLogoff
 EAPOL: txStart
 EAPOL: processKey
EAPOL: Received IEEE 802.1X EAPOL-Key even though this was not accepted - ignoring this packet
EAPOL: Too short EAPOL-Key frame
EAPOL: RX IEEE 802.1X ver=%d type=%d len=%d EAPOL-Key: type=%d key_length=%d key_index=0x%x
EAPOL: Could not get master key for decrypting EAPOL-Key keys
EAPOL: Could not get LEAP master key for decrypting EAPOL-Key keys
EAPOL: Could not get enough master key data for decrypting EAPOL-Key keys (res=%d)
EAPOL: EAPOL-Key replay counter did not increase - ignoring key
EAPOL: last replay counter
EAPOL: received replay counter
EAPOL: Invalid key signature in EAPOL-Key packet
EAPOL: EAPOL-Key key signature verified
EAPOL: Too long key data length %d
EAPOL: Decrypted(RC4) key
EAPOL: using part of EAP keying material data encryption key
EAPOL: Invalid key data length %d (key_length=%d)
EAPOL: Setting dynamic WEP key: %s keyidx %d len %d
unicast
broadcast
EAPOL: Failed to set WEP key to the  driver.
EAPOL: all required EAPOL-Key frames received
 EAPOL: getSuppRsp
 EAPOL: txSuppRsp
EAPOL: txSuppRsp - EAP response data not available
 0@-
 LOGOFF
DISCONNECTED
CONNECTING
AUTHENTICATING
HELD
AUTHENTICATED
RESTART
UNKNOWN
 REQUEST
RESPONSE
SUCCESS
FAIL
TIMEOUT
IDLE
INITIALIZE
RECEIVE
 Authorized
Unauthorized
 Auto
ForceUnauthorized
ForceAuthorized
Unknown
Supplicant PAE state=%s
suppPortStatus=%s
heldPeriod=%d
authPeriod=%d
startPeriod=%d
maxStart=%d
portControl=%s
Supplicant Backend state=%s
 dot1xSuppPaeState=%d
dot1xSuppHeldPeriod=%d
dot1xSuppAuthPeriod=%d
dot1xSuppStartPeriod=%d
dot1xSuppMaxStart=%d
dot1xSuppSuppControlledPortStatus=%s
dot1xSuppBackendPaeState=%d
dot1xSuppEapolFramesRx=%d
dot1xSuppEapolFramesTx=%d
dot1xSuppEapolStartFramesTx=%d
dot1xSuppEapolLogoffFramesTx=%d
dot1xSuppEapolRespFramesTx=%d
dot1xSuppEapolReqIdFramesRx=%d
dot1xSuppEapolReqFramesRx=%d
dot1xSuppInvalidEapolFramesRx=%d
dot1xSuppEapLengthErrorFramesRx=%d
dot1xSuppLastEapolFrameVersion=%d
dot1xSuppLastEapolFrameSource=%02x:%02x:%02x:%02x:%02x:%02x
 eapol_sm_rx_eapol: IEEE802_1x_TYPE_EAP_PACKET
EAPOL: Received EAP-Packet frame
eapol_sm_rx_eapol: IEEE802_1X_TYPE_EAPOL_KEY
EAPOL: Too short EAPOL-Key frame received
EAPOL: Ignoring WPA EAPOL-Key frame in EAPOL state machines
EAPOL: Ignored unknown EAPOL-Key type %d
EAPOL: Received EAPOL-Key frame
EAPOL: Received unknown EAPOL type %d
EAPOL: External notification - portEnabled=%d
 EAPOL: External notification - portValid=%d
 EAPOL: External notification - EAP success=%d
 EAPOL: External notification - EAP fail=%d
 0@-
RSN: Trying to use cached PMKSA
RSN: Do not try to use cached PMKSA
 RSN: Authenticator did not accept PMKID, doing full EAP authentication
EAPOL: External notification - portControl=%s
EAPOL: received control response (user input) notification - retrying pending EAP Request
ERROR - netTupleGet() failed
muxSend returned 0x%08x (%d)
 wvlan
l2_packet_init(): could not alloc extension for %s..
WPA Supplicant - EAP (802.1x)
WPA Supplicant - RSN preauth
muxBind - 0x%04x
l2_packet_init(): muxBind() failed for interface %s on packets of type 0x%04x with errno %d.
P00`
}++V
=j&&LZ66lA??~
\44h
S11b?
e##F^
i''N
t,,X.
M;;va
}{))R>
q//^
`  @
gK99r
U33f
D<<x
!H88p
c!!B0
G==z
f""D~**T
V22dN::t
l$$H
Y77n
o%%Jr..\$
B>>|
_55j
x((Pz
)w--Z
T00`P
++V}
&&Lj66lZ??~A
O44h\
s11bS
R##Fe
&''Ni
,,Xt
6-nn
;;vM
))R{
>//^q
,  @`
99rKJJ
33fU
<<xD
88pH
u!!Bc
==zGdd
2+ss
""Df**T~
;22dV::tN
$$Hl\\
C77nYmm
%%Jo..\r
>!KK
>>|B
55j_WW
"3ii
((Px
--Zw
0`P0
g+V}+
&Lj&6lZ6?~A?
4h\4
1bS1
#Fe#
'Ni'
,Xt,
R;vM;
)R{)
/^q/
 @` 
9rK9J
M3fU3
P<xD<
8pH8
!Bc!
~=zG=d
"Df"*T~*
2dV2:tN:
$Hl$\
7nY7m
x%Jo%.\r.
p>|B>
a5j_5W
U(Px(
-Zw-
`P00
ggV}++
Lj&&lZ66~A??
h\44Q
bS11*?
Fe##
Ni''
Xt,,4.
RRvM;;
R{))
^q//
@`  
rK99
MMfU33
PPxD<<%
pH88
Bc!! 0
DD.9
~~zG==
]]2+
Df""T~**;
dV22tN::
Hl$$
nY77
xxJo%%\r..8$
tt>!
pp|B>>q
aaj_55
UUPx((
Zw--
cccc||||wwww{{{{
kkkkoooo
0000
gggg++++
vvvv
}}}}
YYYYGGGG
rrrr
&&&&6666????
4444
qqqq
1111
####
''''
uuuu				
,,,,
nnnnZZZZ
RRRR;;;;
))))
////
SSSS
    
[[[[jjjj
9999JJJJLLLLXXXX
CCCCMMMM3333
EEEE
PPPP<<<<
QQQQ
@@@@
8888
!!!!
____
DDDD
~~~~====dddd]]]]
ssss````
OOOO
""""****
FFFF
^^^^
2222::::
IIII
$$$$\\\\
bbbb
yyyy
7777mmmm
NNNN
llllVVVV
eeeezzzz
xxxx%%%%....
tttt
KKKK
pppp>>>>
ffffHHHH
aaaa5555WWWW
iiii
UUUU((((
BBBBhhhhAAAA
----
TTTT
QSeA~
!tX)i
XhHp
NrZl
='9-6d
:.6$
aiKwZ
;fD4~
[v)C
cB@"
_jbF~T
11#?*0
,4$8_@
I<(A
t\lHBW
QPeA~S
0 Umv
-!tX
SbEwd
hHpX
Uf*(
+2Hp
rZlN
9-6'
\h!T[
.6$:g
KwZi
[4)C
F~Tb
#?*1
_[o=
>4$8,@
p\lHtW
A~Se
`3SbE
+HpXhE
pZlNr
-6'9
T6$:.
 wZiK
*"<C
[4~C
~TbF
	xYn
?*1#
fNt7
$8,4
lHt\
BWQP
~SeA
!tI)i
k>X'
`3QbE
pXhH
C@gw
lNrZ
6'9-
T[$:.6
ZiKw
;f[4~
_TbF~
	x&n
*1#?
h8,4$
2Ht\l
RRRR				jjjj
00006666
8888
@@@@
||||
9999
////
4444
CCCCDDDD
TTTT{{{{
2222
####====
LLLL
BBBB
NNNN
....
ffff((((
$$$$
vvvv[[[[
IIIImmmm
%%%%rrrr
dddd
hhhh
\\\\
]]]]eeee
llllppppHHHHPPPP
^^^^
FFFFWWWW
XXXX
EEEE
,,,,
????
kkkk::::
AAAAOOOOgggg
ssss
tttt""""
5555
7777
uuuu
nnnnGGGG
qqqq
))))
oooo
bbbb
VVVV>>>>KKKK
yyyy    
xxxx
ZZZZ
3333
1111
YYYY''''
____````QQQQ
JJJJ
----
zzzz
;;;;MMMM
****
<<<<
SSSS
aaaa
++++
~~~~
wwww
&&&&
iiii
ccccUUUU!!!!
}}}}
TLS: PKCS12 support disabled - cannot read p12/pfx files
:.0[
& 0k
& 0k
( TFTP Init_TFTPMsgQue Failed
(TFTP begain Writing TFTP log 
TFTP Start Configuration file upgrade: 
TFTP Start Firmware file upgrade: 
TFTP finish Writing TFTP log 
 There's no retry time in flash
Current time:%ld
Retry time:%ld,size:%ld
Current time less than retry time
Remainder time(.min):%d
 TFTP clean the retry timer
 W	(
 TftpShowLoctParam: 
config server:%s
config file name:%s
config file key:%s
firmware server:%s
firmware path:%s
firmware name:%s
config update protocol:%s
http
tftp
firmware update protocol:%s
config server port:%d
firmware server port:%d
  TFTP TFTP_init 
Tftp download file
Tftp Main
(TFTP TGetCurLoctParams error 
TFTP found there's firmware downloading error time:%d
TFTP resync timer arrival
TFTP_Main resync new time < old time 
TFTP first timer arrival
TFTP_Main 10 minutes new time - old time > 20 minutes
TFTP_Main 10 minutes new time < old time 
( W	(
 TFTPUpgradeTask exit 
(TFTPDownloadFileTask  msgQReceive error 
TFTPDownloadFileTask  start config upgrade 
TFTPDownloadFileTask  finish download the config file 
TFTPDownloadFileTask for download Firmware file,but MMI is not in IDLE state 
TFTPDownloadFileTask  firmware should be upgraded, so send firmware signal
TFTPDownloadFileTask  firmware need not be upgraded, so reboot 
TFTPDownloadFileTask for download firmware file,but MMI is not in IDLE state 
TFTPDownloadFileTask for download firmware file,but firmware's version is same with the parameter 
TFTPDownloadFileTask  start firmware upgrade 
TFTPDownloadFileTask  failed download the firmware file 
TFTPDownloadFileTask  phone's parameter changed, so reboot phone 
TFTPDownloadFileTask  msgQReceive undefined message:%d 
  W	(
 TFTP In auto config upgrade, so can't do manual upgrade
TFTP has been deinited, so can't do manual upgrade
TFTP upgrade start ...
TFTP upgrade
TFTPDownloadFile send a signal to start a find file process, file type:%d
TFTPDownloadFile  TFTP has been deinited 
MsgQTFTP_DOWNLOADFILE message queue is full 
I think TFTP download file task was dead now,restart it
tftpPeerSet %s: unknown host.
!!!!!!getaddrinfo %s
 TFTPResolv pHostName == 
 !!!!!test_resolv %s
TFTP TCreateLoctParams malloc error
(TActiveConfigParams TFTPConfigGet fail
TActiveConfigParams TFTPConfigSet fail, index:%d, value:%s
 Server name doesn't include the port info
 protocol_config_get error for LOCT_TFTP_ServerFQDN 
TFTP configuration server changed 
protocol_config_get error for LOCT_TFTP_ConfigurationPath 
TFTP configuration file path&name changed 
TFTP firmware file name isn't include the version info
 protocol_config_get error for LOCT_TFTP_FirmwareFileName 
TFTP local firmware file isn't include the version 
 TFTP there's no version in cofig file 
 protocol_config_get error for LOCT_TFTP_ConfigProtocol 
protocol_config_get error for LOCT_TFTP_EncryptKey 
protocol_config_get error for LOCT_TFTP_UpgradeProtocol 
protocol_config_get error for LOCT_TFTP_FirmwareServerFQDN 
protocol_config_get error for LOCT_TFTP_FirmwarePath 
 0@-
(ini
 %02X%02X%02X%02X%02X%02X
TGetCfgFileName:protocol_config_get error for PRV_Provisioning_EncryptKey 
.ini
.aes
TFTPTGetCfgFileName: %s 
TFTPResolv error : %s
TFTPResolv Success! ip:%s
TFTP malloc 64k error
TFTP process exit by user 
binary
TFTP transfer initiation failed.
TFTP after dxXfer ipAddr:%s	tftpPort:%d config file:%s
TFTP configuration file too big to receive on handset 
TFTP the all data bytes:%d
TFTP all port(69,21,2400) are be block at the current gateway
TFTP Current port maybe was blocked, I will try the next port 
TFTP File not found
TFTP Transfer file error
HTTP port block
HTTP file not found
HTTP Transfer file error
Fail unknow reason
TFTP File checksum error
<TFTP> encryption key: %s
TFTP malloc plainbuf error
TFTP decryption error %x %x %x %x 
TFTP Default reset fail!!!
TFTP Parse error %x %x %x %x 
TFTP restore current config location params which will be shown at user-agent
TRestoreConfigLoct TFTPConfigSet fail
TFTP before active config params
TFTP There's no parameters changed.
TFTP atfer active config params
TFTP upgrade task enter a loop,because it has downloaded 8 config files 
TFTPResolv error : %s  in download new config file
TFTP TFTPFirmwareUpgradeProc error
 @i	(
 TFTP after dxXfer ipAddr:%s tftpPort:%d config file:%s
TFTP Parse error: %s
TFTP firmware's version changed
 @i	(p
DX firmware upgrade start
DX Resolv error :%s
Provisioning process exit by user 
 flashUp: ERASE Addr ERROR: Sector #%3u, Abs Address %08X
flashUp4: ERASE_end: Sector #%3u, Abs Address %08X
flashup: ERROR erasing sector %d, base addr: %08X
 0@-
(paramParse: Can't find the :
paramParse: setgParam fail
(@@SHANGHAISAILONGFMCBUBUBU$$
TftpParamCheck: MIC doesn't match below:
 Param_MIC:%s
 Calc_MIC:%s
Model
TftpParamCheck: Model doesn't match
Version
TftpParamCheck: Version is same
TftpParamCheck: MIC or Model doesn't exist
 NENEFENHUANGJING
TftpCodeCheck: First try decompress whole file
TftpCodeCheck: PROGRAM Addr ERROR: Abs Address %08X
TftpCodeCheck: Image size info error (0x%08X)
TftpCodeCheck ERROR: Can not allocate enough memory for inflate
1.1.4
TftpCodeCheck ERROR: inflateInit error:%d
TftpCodeCheck: First try inflate error: err = %d.
TftpCodeCheck: Lastest block size:%d
TftpCodeCheck: Can't find the seperator
TftpCodeCheck: TftpParamCheck error
TftpCodeCheck: First try decompress whole file finished
 flashUp: PROGRAM Addr ERROR: Abs Address %08X
ERROR file type
flashUp: PROGRAM Sector ERROR: Sector #%3u, Abs Address %08X
DX transfer initiation failed.
After dxXfer ipAddr:%s Server port:%d Firmware file:%s
provisioning process exit by user 
TftFlashEraseSector:%d error
flashupProgramEx error
flashupProgramEx finish writting sector #%d
TftpCodeGet: Firmware file is too large
Flashing last buffer %d, length = %d,offset = %d
Got total bytes: %d
DX all port(69,21,2400) are be block at the current gateway
DX Current port maybe was blocked, I will try the next port 
DX firmware file error
Download unexpected errors, please capture this log for parsing, thanks.
Decompress Bin image download sucessfully
Firmware image download sucessfully
ERROR: The flash update failed
  W	(
TftpTxtParse  TDemoMenuSize <= 0
TftpTxtParse  TDemoMenuSize: %d
Reserved Parameter
TftpTxtParse  meet a Reserved Parameter 
TFTP In configuration file there are more than 300 items, the following will be discarded
(p@-
P00`
}++V
=j&&LZ66lA??~
\44h
S11b?
e##F^
i''N
t,,X.
M;;va
}{))R>
q//^
`  @
gK99r
U33f
D<<x
!H88p
c!!B0
G==z
f""D~**T
V22dN::t
l$$H
Y77n
o%%Jr..\$
B>>|
_55j
x((Pz
)w--Z
T00`P
++V}
&&Lj66lZ??~A
O44h\
s11bS
R##Fe
&''Ni
,,Xt
6-nn
;;vM
))R{
>//^q
,  @`
99rKJJ
33fU
<<xD
88pH
u!!Bc
==zGdd
2+ss
""Df**T~
;22dV::tN
$$Hl\\
C77nYmm
%%Jo..\r
>!KK
>>|B
55j_WW
"3ii
((Px
--Zw
0`P0
g+V}+
&Lj&6lZ6?~A?
4h\4
1bS1
#Fe#
'Ni'
,Xt,
R;vM;
)R{)
/^q/
 @` 
9rK9J
M3fU3
P<xD<
8pH8
!Bc!
~=zG=d
"Df"*T~*
2dV2:tN:
$Hl$\
7nY7m
x%Jo%.\r.
p>|B>
a5j_5W
U(Px(
-Zw-
`P00
ggV}++
Lj&&lZ66~A??
h\44Q
bS11*?
Fe##
Ni''
Xt,,4.
RRvM;;
R{))
^q//
@`  
rK99
MMfU33
PPxD<<%
pH88
Bc!! 0
DD.9
~~zG==
]]2+
Df""T~**;
dV22tN::
Hl$$
nY77
xxJo%%\r..8$
tt>!
pp|B>>q
aaj_55
UUPx((
Zw--
cccc||||wwww{{{{
kkkkoooo
0000
gggg++++
vvvv
}}}}
YYYYGGGG
rrrr
&&&&6666????
4444
qqqq
1111
####
''''
uuuu				
,,,,
nnnnZZZZ
RRRR;;;;
))))
////
SSSS
    
[[[[jjjj
9999JJJJLLLLXXXX
CCCCMMMM3333
EEEE
PPPP<<<<
QQQQ
@@@@
8888
!!!!
____
DDDD
~~~~====dddd]]]]
ssss````
OOOO
""""****
FFFF
^^^^
2222::::
IIII
$$$$\\\\
bbbb
yyyy
7777mmmm
NNNN
llllVVVV
eeeezzzz
xxxx%%%%....
tttt
KKKK
pppp>>>>
ffffHHHH
aaaa5555WWWW
iiii
UUUU((((
BBBBhhhhAAAA
----
TTTT
QSeA~
!tX)i
XhHp
NrZl
='9-6d
:.6$
aiKwZ
;fD4~
[v)C
cB@"
_jbF~T
11#?*0
,4$8_@
I<(A
t\lHBW
QPeA~S
0 Umv
-!tX
SbEwd
hHpX
Uf*(
+2Hp
rZlN
9-6'
\h!T[
.6$:g
KwZi
[4)C
F~Tb
#?*1
_[o=
>4$8,@
p\lHtW
A~Se
`3SbE
+HpXhE
pZlNr
-6'9
T6$:.
 wZiK
*"<C
[4~C
~TbF
	xYn
?*1#
fNt7
$8,4
lHt\
BWQP
~SeA
!tI)i
k>X'
`3QbE
pXhH
C@gw
lNrZ
6'9-
T[$:.6
ZiKw
;f[4~
_TbF~
	x&n
*1#?
h8,4$
2Ht\l
RRRR				jjjj
00006666
8888
@@@@
||||
9999
////
4444
CCCCDDDD
TTTT{{{{
2222
####====
LLLL
BBBB
NNNN
....
ffff((((
$$$$
vvvv[[[[
IIIImmmm
%%%%rrrr
dddd
hhhh
\\\\
]]]]eeee
llllppppHHHHPPPP
^^^^
FFFFWWWW
XXXX
EEEE
,,,,
????
kkkk::::
AAAAOOOOgggg
ssss
tttt""""
5555
7777
uuuu
nnnnGGGG
qqqq
))))
oooo
bbbb
VVVV>>>>KKKK
yyyy    
xxxx
ZZZZ
3333
1111
YYYY''''
____````QQQQ
JJJJ
----
zzzz
;;;;MMMM
****
<<<<
SSSS
aaaa
++++
~~~~
wwww
&&&&
iiii
ccccUUUU!!!!
}}}}
 Assertion failed: in && out && key, file E:/Ownlib/platformvob/src/protocol/provisioning/aes.c, line 1248
 Assertion failed: in && out && key, file E:/Ownlib/platformvob/src/protocol/provisioning/aes.c, line 1439
 Assertion failed: in && out && key && ivec, file E:/Ownlib/platformvob/src/protocol/provisioning/aes.c, line 1630
Assertion failed: (AES_ENCRYPT == enc)||(AES_DECRYPT == enc), file E:/Ownlib/platformvob/src/protocol/provisioning/aes.c, line 1631
tftpCopyEx step1
tftpCopyEx step2
 tftpInit pTftpDesc address: %d 
netascii
tftp pTftpDesc FREE 1
tftp pTftpDesc FREE 2
image
octet
binary
ascii
mode set to %s.
%s: unknown mode
valid modes: [
%s%s
tftp
tftpPeerSet %s: unknown host.
Connected to %s [%d]
 tftpGet: No target machine specified.
getting from %s:%s [%s]
tftpGet Step1
tftpGetEx ioctl  error   !!!
tftpGetEx amount == 0 will exit from clear loop
tftpSend FIONREAD amount:%d  TFTP message size: %ld
tftpGet: Error occurred while transferring the file.
tftpGet: Error occurred while writing the file.
 	Connected to %s [%d]
	Not connected
	Mode: %s  Verbose: %s  Tracing: %s
	Rexmt-interval: %d seconds, Max-timeout: %d seconds
 before close socket %d
tftpQuit free address: %d 
 tftpSend sendto num:%d
tftpSend sendto sizeMsg:%d
tftpSend sendto error no:0X%X
tftpSend  sendto error!!!
tftpSend select error !!!
Transfer Timed Out.
tftpSend timeWait:%d, reXmitTimer.tv_sec:%ld
tftpSend break error !!!
tftpSend ioctl read error !!!
tftpSend amount==0 continue1 !!!
tftpSend recvfrom error !!!
tftpSend recvfrom the data not from the prot we expect 
Expected port:%d, But Data from port:%d 
Error code %d: %s
tftpSend opcode!=opcode continue !!!
tftpSend enter another forever !!!
tftpSend ioctl  error9   !!!
tftpSend amount == 0 will exit from another forever
tftpSend recvfrom finished,received data num: %dr
tftpSend break out to send loop in order to resynch by reresending
tftpSend end internal loop
tftpSend end loop
No such user
File already exists
Unknown transfer ID
Illegal TFTP operation
Disk full or allocation exceeded
Access violation
File not found
Undefined error code
(127.0.0.1
%s [%s] %s:%d: 
DEBUG
E:/Ownlib/platformvob/src/protocol/provisioning/tftplib.c
%s: 
connectOverLoopback: connected over "%s"/port %d
dataXferInit semBCreate failed
dataXferInit tftpInit failed
tDataXferTask
dataXferInit taskSpawn failed
(dataXferInit failed
dataXferInit succeeded
dataXfer.dxParam != NULL, so there's a process in downloading file
(Enter dataXferTask 
dataXferTask waiting for semphore
dataXferTask got semphore
Leave dataXferTask 
(0@-
(Memory exhausted while demangling C++ symbol
("%s" is overloaded - Please select:
  %3d: %s
Enter <number> to select, anything else to stop: 
sizeof 
cond
compound
array
addr
->()
method_call
indirect
component
arshift
alshift
call
bit_not
bit_and
bit_xor
bit_ior
postdecrement
postincrement
truth_not
truth_orif
truth_andif
trunc_div
trunc_mod
negate
convert
mult
minus
plus
 delete []
 new []
delete
 delete
 new
GNAT style demangling
Java style demangling
GNU (g++) V3 ABI-style demangling
EDG style demangling
HP (aCC) style demangling
ARM style demangling
Lucid (lcc) style demangling
GNU (g++) style demangling
Automatic selection based on executable
 gfff
const
volatile
__restrict
const volatile
const __restrict
volatile __restrict
const volatile __restrict
operator 
operator
assign_
type
(0@-
_ada_
<%s>
global constructors keyed to 
global destructors keyed to 
import stub for 
 static
 template <
class
> class
false
true
 __tm__
__ps__
__pt__
_GLOBAL_
{anonymous}
 _imp__
__imp_
__std__
__sti__
  virtual table
0123456789Qt
__thunk_
virtual function thunk (delta:%d) for 
 type_info node
 type_info function
__vtbl__
 unsigned
signed
__complex
void
long long
long
short
bool
char
wchar_t
long double
double
float
int%u_t
 -2147483648
 0@-
__ct
__dt
 p@-
 !"#$%&'()*+,-./0123456789:;<=>?@abcdefghijklmnopqrstuvwxyz[\]^_`abcdefghijklmnopqrstuvwxyz{|}~
 !"#$%&'()*+,-./0123456789:;<=>?@ABCDEFGHIJKLMNOPQRSTUVWXYZ[\]^_`ABCDEFGHIJKLMNOPQRSTUVWXYZ{|}~
(p@-
(p@-
%c%lu
N_%lu_%lu
T_%lu_%lu
 p@-
true
false
virtual-function-
 cast
 [with 
 apl
new[]
delete[]
delete
sizeof(
__ALIGNOF__(
__uuidof(
 p@-
operator 
<unnamed>
__ps__
__pt__
__tm__
 [block 
 p@-
(const
volatile
 signed 
unsigned 
void
char
wchar_t
bool
short
long
long long
float
double
long double
__int8
__int16
__int32
__int64
 ...
(p@-
 p@-
__CPR
__vtbl__
virtual function table for 
 (ambiguous)
 in 
__CBI__
can-be-instantiated flag for 
__DNI__
do-not-instantiate flag for 
__TIR__
template-instantiation-request flag for 
__LSG__
initialization guard variable for 
__TID_
type identifier for 
__T_
typeinfo for 
__VFE__
surrogate in class 
 for 
__STV__
__STF__
(0@-
9exception
13bad_exception
 0@-
 bad_alloc
9bad_alloc
`$	(
 bad_alloc
 bad_alloc
 bad_alloc
 bad_alloc
 bad_alloc
 bad_alloc
 bad_alloc
 bad_alloc
 bad_alloc
 p@-
 0@-
 p@-
9type_info
8bad_cast
10bad_typeid
16__user_type_info
14__si_type_info
17__class_type_info
 0@-
 0@-
 0@-
 bad_alloc
 p@-
 0@-
 0@-
 0@-
 0@-
 p@-
19__pointer_type_info
16__attr_type_info
19__builtin_type_info
16__func_type_info
16__ptmf_type_info
16__ptmd_type_info
17__array_type_info
 "	(
 ,"	(`
T	(,5
(l$	(
 l$	(
(,"	(T5
T	(t
T	(D
T	(D$	(
-DT&
zhC@B.
v<y5G
=v<y5UU
?UUUU
Y=6+
?UUUUG
=1cb
!9A0_
IUUU
?cUUU
~}|{zyxwvvutsrqqponnmllkjjihhgffeddccbaa``__^^]]\\[[ZZYYXXWWVVUUUTTSSRRRQQPPPOOONNMMMLLLKKKJJJIIIHHHGGGGFFFEEEDDDDCCCCBBBBAAA
J@	|
@	sS
JN B
JN B
JN B
JN B
J@	|
@	sS
J@	|
@	sS
:  R
4#Bz
* 0b
1 0c
 p@-
(looutput no HDR
looutput: mbuf allocation failed
looutput: af=%d unexpected
 if_simloop: can't handle af=%d
pG2	P
@ #!
pG2	P
@2	@
@ c!
@ #!
@ c!
 0@-
(/dev/bpf
(p@-
(bpfLock error
(bpfDevLock error
bpfUnitLock error
%s%d
(0@-
Berkeley Packet Filter
(%s%d
_bpfProtoPromisc: failed to create a socket
@(#) $Header: bpf_filter.c,v 1.33 97/04/26 13:37:18 leres Exp $ (LBL)
%s%d
%s%d
/bpf/dhcpc-arp
/bpf/dhcpc-arp0
(255.255.255.255
(p@-
(IP address (%s) is already in use.
IP address (%s) doesn't match requested value.
 Releasing the current IP address (%s).
(setsockopt error %d (0x%x).
sendmsg error %d (0x%x).
"	(%s%d
"	(0@-
"	(if_rtdel: error %d
if_clone_create(): interface name too long
(p@-
"	(p@-
 p@-
(p@-
Interface admin status is down for %s%d
IPv4 not attached.
Admin status is down for IPv4 traffic on interface %s%d
 0@-
"	(0@-
 p@-
can't allocate dupsa for address family %d
 Can't free ifma->ifma_addr for address family %d
(0@-
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
if.c
link
Link layers
%s:%d sysctl_add_oid failed for parent=%s, var=%s
generic
Generic link-management
(admindebug interface:%s cmd:%d proto:%d status:%d
ifAdminstatus is %d
admin_inet_status is %d
admin_inet6_status is %d
admin inet status is %d
admin inet6 status is %d
(@h	(
 arp_rtrequest: bad gateway value
arp_rtrequest: malloc failed
(@h	(
(arpresolve: lookup failed for %s%s%s
 (resource shortage or network configuration error -- check netmask)
(arpintr: bad mbuf
arp: runt packet -- m_pullup failed
arp: unknown hardware address format (0x%2D)
arp: runt packet
in_arp: runt packet -- m_pullup failed
arp: link address is broadcast for IP address %s!
arp: link address is multicast for IP address %s!
arp: %s is using my IP address %s!
arp: %s is on %s%d but got reply from %s on %s%d
arp: %s moved from %s to 
%s on %s%d
arp: %s attempts to modify permanent entry for %s on %s%d
arp from %s: new addr len %d, was %d
arp from %s: addr len: new %d, i/f %d (ignored)
(arptfree
 host is not on local network
could not allocate llinfo
gateway route is not ours
arplookup %s failed: %s
 0@-
@h	(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
if_ether.c
ether
inet
inet group of ARP variables
ether_inet
prune_intvl
Sysctll failed
max_age
host_down_time
maxtries
useloopback
proxyall
log_arp_wrong_iface
log arp packets arriving on the wrong interface
# XS
(0@-
(p@-
(0@-
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
igmp.c
inet
igmp
IGMP
%s:%d sysctl_add_oid failed for parent=%s, var=%s
stats
S,igmpstat
Sysctll failed
# Hg
(0@-
(invalid argument to in_lifaddr_ioctl
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
in.c
subnets_are_local
Sysctll failed
cksum: out of data
(p@-
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
in_pcb.c
portrange
IP Ports
%s:%d sysctl_add_oid failed for parent=%s, var=%s
lowfirst
Sysctll failed
lowlast
first
last
hifirst
hilast
 internet
%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
in_proto.c
inet
Internet Family
%s:%d sysctl_add_oid failed for parent=%s, var=%s
icmp
ICMP
(icmp_error: bad length
icmp_error
icmp len
 icmp redirect from %d.%d.%d.%d: %d.%d.%d.%d => %d.%d.%d.%d
(X&	(t
(Limiting icmp unreach response
Limiting icmp ping response
Limiting icmp tstamp response
Limiting closed port RST response
Limiting open port RST response
 %s from %d to %d packets per second
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
ip_icmp.c
icmp
stats
S,icmpstat
Sysctll failed
maskrepl
drop_redirect
log_redirect
icmplim
icmplim_output
bmcastecho
icmpErrorLen
ip_init
	(X&	(|
$	(`
(ip_input: unrecognised MT_TAG tag %d
(X&	(l
(attempted source route from %s to %s
(p@-
(p@-
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
ip_input.c
forwarding
Enable IP forwarding between interfaces
Sysctll failed
redirect
Enable sending IP redirects
Maximum TTL on IP packets
sourceroute
Enable forwarding source routed IP packets
accept_sourceroute
Enable accepting source routed IP packets
maxfragpackets
Maximum number of IPv4 fragment reassembly queue entries
check_interface
Verify packet arrives on correct interface
stats
S,ipstat
IP statistics (struct ipstat, netinet/ip_var.h)
 ip_output: unrecognised MT_TAG tag %d
$	(`S
(delayed m_pullup, m->len: %d  off: %d  p: %d
(p@-
(ip_mloopback: bad address family %d
(0@-
rn_addmask: mask impossibly already in tree
Mask for route not entered
  Non-unique normal route, mask not entered
  rn_delete: inconsistent annotation
rn_delete: couldn't find our annotation
rn_delete: couldn't find us
rn_delete: Orphaned Mask %p at %p
	  x
  rn_init: radix functions require max_keylen be set
rn_init
rn_init 2
(X&	(`
	(`S
(p@-
$	(`S
(rip_attach
(rip_detach
`'  
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
raw_ip.c
inet
IP_RAW
%s:%d sysctl_add_oid failed for parent=%s, var=%s
maxdgram
Maximum outgoing raw IP datagram size
Sysctll failed
recvspace
Maximum incoming raw IP datagram size
pcblist
S,xinpcb
List of active raw IP sockets
+  t+  
+  8
,   ,  
,  H,  
(d,  X,  
,  0@-
(rtfree
rtfree 2
(ifafree
rtrequest delete
rtrequest: GATEWAY but no gateway
(D?  
(D?  
(0@-
(p@-
(0@-
(p@-
(0@-
(p@-
(route_output
0K  
PI  
(p@-
(%s%d
W  H
(route
%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
rtsock.c
routetable
%s:%d sysctl_add_oid failed for parent=%s, var=%s
\  8
[  $]  (]  
(,]  
(Connection attempt to TCP %s:%d from %s:%d
Connection attempt to TCP %s:%d from %s:%d flags:0x%x
tcp_input: TCPS_LISTEN
0p  
pt  |t  |t  |t  
t  |t  <
d~  
~  |
  `i
tcp_pulloutofband
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
tcp_input.c
inet
%s:%d sysctl_add_oid failed for parent=%s, var=%s
  stats
S,tcpstat
TCP statistics (struct tcpstat, netinet/tcp_var.h)
Sysctll failed
log_in_vain
Log all incoming TCP connections
blackhole
Do not send RST when dropping refused connections
delayed_ack
Delay ACK to try and piggyback it onto a data packet
(tcp_setpersist: retransmit pending
  %s:%d sysctl: parent node or its child link 			  NULL for parent=%s
tcp_output.c
path_mtu_discovery
Enable Path MTU Discovery
Sysctll failed
slowstart_flightsize
Slow start flight size
local_slowstart_flightsize
Slow start flight size for local networks
newreno
Enable NewReno Algorithms
  WARNING: TCB hash size not a power of 2
tcp_init
(gfff
  p@-
(p@-
(p@-
(p@-
 &	(@Q
(0&	(L
%p bw %ld rttbest %d srtt %d bwnd %ld
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
tcp_subr.c
mssdflt
Default TCP Maximum Segment Size
Sysctll failed
rfc1323
Enable rfc1323 (high performance TCP) extensions
rfc1644
Enable rfc1644 (TTCP) extensions
tcbhashsize
Size of TCP control-block hashtable
do_tcpdrain
Enable tcp_drain routine for extra help when low on mbufs
pcbcount
Number of active PCBs
icmp_may_rst
Certain ICMP unreachable messages may abort connections in SYN_SENT
isn_reseed_interval
Seconds between reseeding of ISN secret
inflight_enable
Enable automatic TCP inflight data limiting
inflight_debug
Debug TCP inflight calculations
inflight_min
Lower-bound for TCP inflight window
inflight_max
Upper-bound for TCP inflight window
pcblist
S,xtcpcb
List of active TCP connections
(0@-
(0@-
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
tcp_timer.c
keepinit
Sysctll failed
keepidle
keepintvl
delacktime
Time before a delayed ACK is sent
Maximum segment lifetime
rexmit_min
Minimum Retransmission Timeout
rexmit_slop
Retransmission Timer Slop
always_keepalive
Assume SO_KEEPALIVE on all TCP connections
  @e
  TIME_WAIT
FIN_WAIT_2
LAST_ACK
CLOSING
FIN_WAIT_1
CLOSE_WAIT
ESTABLISHED
SYN_RCVD
SYN_SENT
LISTEN
CLOSED
  (0
(0@-
  %s:%d sysctl: parent node or its child link 			  NULL for parent=%s
tcp_usrreq.c
sendspace
Maximum outgoing TCP datagram size
Sysctll failed
recvspace
Maximum incoming TCP datagram size
(Connection attempt to UDP %s:%d from %s:%d
(p@-
(0@-
%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
udp_usrreq.c
inet
%s:%d sysctl_add_oid failed for parent=%s, var=%s
checksum
Sysctll failed
log_in_vain
Log all incoming UDP packets
blackhole
Do not send port unreachables for refused connects
stats
S,udpstat
UDP statistics (struct udpstat, netinet/udp_var.h)
maxdgram
Maximum outgoing UDP datagram size
recvspace
Maximum incoming UDP datagram size
pcblist
S,xinpcb
List of active UDP sockets
! @s
! mbinit : _pNetDpool : no memory for mBlks/clBlks
mbinit : _pNetDpool : no memory for Clusters
mbinit: netPoolInit(_pNetDpool, ...) failed
mbinit : _pNetSysPool : no memory for mBlks/clBlks
mbinit : _pNetSysPool : no memory for Clusters
mbinit: netPoolInit(_pNetSysPool, ...) failed
(D	! 
	! x	! 
(0@-
%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
uipc_mbuf.c
max_linkhdr
Sysctll failed
max_protohdr
max_hdr
(0@-
(0@-
(0@-
panic: %s
(hashinit: bad elements
! phashinit: bad elements
phashinit: allocate hash table failed
! p@-
@h	(%x:%x:%x:%x:%x:%x
arp: invalid Ethernet address %s
d!! x!! 
(ipCtrsUpdate: m_pullup failed
ipShutdownRtn: Null pointer received for pCookie
ipShutdownRtn: detaching protocol unknown
Could not un-bind from the IP MUX!
'! d
arpShutdownRtn: pCookie is a NULL pointer
arpShutdownRtn: ARP protocol no longer attached to device
Could not un-bind from the ARP MUX!
 )! L)! 
ipError: pEnd is NULL, cannot proceed
+! <+! 
+! l+! 
l*! 
_ipAttach: type code %d not supported./n
ipAttach: Can't attach unknown device %s (unit %d).
ipAttach: Protocol is out of space. Increase IP_MAX_UNITS.
IPv4
ipAttach:  TCP/IP could not bind to the MUX device: mux[Tk]Bind! %s
_ipAttach: could not get MIB2 Table  for device %s %d
_ipAttach: Could not get memory for pDstAddr
_ipAttach: Could not get memory for pSrc or pDst
_ipAttach: Could not get memory for device name
ipAttach: if_attach returned error for  device %s
_ipAttach: ARP could not bind to the  MUX device: mux[Tk]Bind! %s
(,,! X,! 
%! ,'! 
+! (&! 
(P-! 
-! (9! 
.! P&! 
&! \*!  .! t
5! 0@-
6! @6! 
6! @6! @6! $6! 0
ipDetach: pEnd is NULL
ipDetach: Device is not attached
(D7! 
(\7! if_ioctl: pCookie is NULL, cannot proceed
if_ioctl: Invalid pIpCookie
if_ioctl: data pointer is NULL
9! (socket)
bsdSockLibInit: Could not register the functions with SOCK_BACKEND_INSTALL
(l>! p
(LK! 
F! @%% 
<! h
(bsdSocket: failed to create a socket. socreate returned error
=! h
(p@-
accept
t?! 
(p@-
(p@-
DHCP server (BOOTP proxy): 
%-18s
DHCP server: 
S! No timer values: BOOTP reply accepted.
time() error in dhcpcTimerShow() routine.
Timer T1 expired.
Timer T1: %ld seconds remaining.
Timer T2 expired.
Timer T2: %ld seconds remaining.
(DU! lU! 
U! No parameter values: BOOTP reply accepted.
DHCP server name: %s
Boot file name: %s
DHCP client name: %s
Merit dump file: %s
DNS domain name: %s
Client root path: %s
Options extension path: %s
NIS domain: %s
NetBIOS over TCP/IP scope: %s
Error message: %s
NIS+ domain: %s
IP forwarding enabled.
Non-local source route forwarding enabled.
All subnets are local is TRUE.
ICMP mask discovery enabled.
ICMP mask supplier is TRUE.
Router discovery enabled.
ARP trailers enabled.
RFC 1042 Ethernet encapsulation enabled.
RFC 894 Ethernet encapsulation enabled.
TCP keepalive garbage octet enabled.
Client time offset: %ld
Boot image size: %d
Maximum datagram size: %d
Default IP Time-to-live: %d
Path MTU timeout: %ld
Interface MTU: %d
ARP cache timeout: %ld
Default TCP Time-to-live: %d
TCP keepalive interval: %ld
NetBIOS node type: %d
Client lease origin: %ld
Client lease duration: %ld
Client renewal (T1) time value: %ld
Client rebinding (T2) time value: %ld
MTU plateau table:
empty.
Client IP address: 
Assigned IP address: 
Next server IP address: 
Relay agent IP address: 
Client subnet mask: 
Client swap server: 
Client broadcast address: 
Client router solicitation address: 
Client IP routers:
	%-18s
	none specified.
Client time servers:
Client IEN 116 name servers:
Client DNS name servers:
Client log servers:
Client cookie servers:
Client line printer servers:
Client impress servers:
Client resource location servers:
Client NIS servers:
Client NTP servers:
Client NetBIOS name servers:
Client NetBIOS datagram distribution servers:
Client X Window System font servers:
Available X Window Display Manager systems:
Available NIS+ servers:
Available mobile IP home agents:
Available SMTP servers:
Available POP3 servers:
Available NNTP servers:
Available World Wide Web servers:
Available Finger servers:
Available IRC servers:
Available StreetTalk servers:
Available StreetTalk Directory Assistance servers:
Client policy filters:
Destination        Subnet mask
-----------        -----------
%-18s 
Client static routes:
Destination        Router IP
-----------        ---------
Vendor-specific data:
none specified.
X! (X! @X! XX! pX! 
X! (Y! HY! hY! 
Z! <Z! XZ! pZ! 
[! 0[! H[! d[! 
\! $\! @\! $
\\! 
S! t\! 
]! 8]! T]! l]! 
^! 4^! d^! 
_! 4_! P_! t_! 
`! 4`! T`! \`! t`! 
( U	(`!	( 8
 U	(
! hP
`!	( 8
%s/%d
/bpf/dhcpc
! tDhcpcStateTask
tDhcpcReadTask
(`!	(
!  5
( U	(
(scsi
tffs
%s%d
Invalid target address "%s"
Invalid device "%s"
Error initializing DHCP boot lease.
Can't renew DHCP boot lease.
Can't get IP address for device.
Can't get network data from DHCP lease.
! @>
! %s
( U	(
(p@-
(p@-
(0@-
(0@-
(p@-
(`!	(
(p@-
(0@-
(`!	(
(Invalid address!
(p@-
(p@-
Q---> 
ftpCommandEnhanced: error during write to control socket - errno:0x%08x
QUIT
! ,>
! ftpXfer: host:%s user:%s passwd:%s acct:%s cmd:%s dir:%s
TYPE I
CWD %s
ftpXfer: Detected an error during command establishment errno:0x%08x
ftpXfer: error during command.  errno:0x%08x
ftpXfer: notice - mode succeeded.
ftpXfer: notice - PASV mode failed. Now trying older PORT connect method
ftpXfer:  ftpDataConnInit - error during trying of another port. errno:0x%08x
ftpXfer:  response 0x%08x - aborting transfer.
ftpXfer:  calling user-supplied applette to see if 0x%08x FTP_TRANSIENT is fatal for this command.
ftpXfer:  user-supplied applette says 0x%08x FTP_TRANSIENT  ** IS ** fatal for this command.
ftpXfer:  user-supplied applette says 0x%08x is  ** NOT ** fatal for this command.
ftpXfer: warning - reply was %d(decimal) - FTP_PRELIM - #%d attempt in %d ticks.
ftpXfer: error - reply was %d(decimal) - FTP_PRELIM - attempt limit (%d) exceeded.
ftpXfer: notice - cmdResult:%d dataSock:%d ctrlSock:%d  errno:0x%08x
ftpXfer: error - select()==ERROR. errno:0x%08x
ftpXfer: warning - control socket ready but data socket not ready
ftpXfer:  error - sending QUIT command to host. errno:0x%08x
ftpXfer: error - ftpDataConnGet()==ERROR. errno:0x%08x
Q%s [%s] %s:%d: 
ERROR
ftpLib.c
%s: 
ftpReplyGet: Timeout %lu sec. 
ftpReplyGet:  error - experienced eof - errno:0x%08x
! ftpHookup: error - failure to get socket. errno:0x%08x
ftpHookup: error - failure to bind socket. errno:0x%08x
ftpHookup: error - failure to connect socket. errno:0x%08x
! USER %s
PASS %s
ACCT %s
ftpLogin: error - failure to get complete login. errno:0x%08x
! ,>
! ftpDataConnInitPassiveMode:  getsockname() failure. errno:0x%08x
PASV
ftpDataConnInitPassiveMode: error - failure to get socket. errno:0x%08x
ftpDataConnInitPassiveMode:  getpeername() failure. errno:0x%08x
ftpDataConnInitPassiveMode: failure to connect. sock:%d sockMsb:%d sockLsb:%d errno:0x%08x
ftpDataConnInitPassiveMode: passive ftp connect established to host:%#x port:%d sock:%d
ftpDataConnInitPassiveMode: host failed to respond correctly to PASV command. errno:0x%08x
! @|
! ftpDataConnInit:  getsockname() failure. errno:0x%08x
ftpDataConnInit:  socket() failure. errno:0x%08x
ftpDataConnInit:  bind() failure. errno:0x%08x
ftpDataConnInit:  listen() failure. errno:0x%08x
PORT %d,%d,%d,%d,%d,%d
ftpDataConnInit:warning got FTP_PRELIM. 
ftpDataConnInit: error - reply was %d(decimal) - not FTP_COMPLETE or FTP_PRELIM.
ftpDataConnInit: error - 2nd try to get port number failed on socket(). errno:0x%08x
ftpDataConnInit: error -  bind failed on 2nd attempt  errno :0x%08x
ftpDataConnInit: error -  listen failed on 2nd attempt  errno :0x%08x
! 0@-
NLST
Can't open directory "%s"
! ,>
(227
ftpPasvReplyParse: error - '227' not part of PASV response
ftpPasvReplyParse: error - '(' not part of PASV response
%d,%d,%d,%d,%d,%d
! ,>
(0@-
(p@-
(p@-
(0@-
(p@-
(0@-
(@$  
delete 
%s%s
%s %s %s 
"	(@W
" 0@-
(@$  
(%d.%d.%d.%d
" 0@-
ipInstInit: Too many protocols
internet
$ 0@-
%  @$  0@-
  @$  
$" d
(D!"  
%s%d
(0@-
" 0 " 
" @ " 
" P " 
 " $ " 
" 8 " 
" H " 
&" 4
'" 0@-
(p@-
@h	(0@-
(0@-
(p@-
(p@-
start of muxLibInit
muxLibInit: Failed to create muxLock
muxLibInit: Failed to add the rebootHook
End of muxLibInit
E" L
(0a" 
F" 8F" Start of muxDevLoad
%d:%s
(@G" L
(XG" |N" 
m" muxDevStart: END_OBJ pointer is NULL
muxDevStart: Driver start routine returned error
J" 0@-
(Device %s unit %d not found.
(Device: %s Unit: %d  END_OBJ: %p
Description: %s
Output protocol {%s}: Recv %p
Protocol: %s	Type: 0x%04x	Recv %p	Shutdown %p
muxDevUnload: device unload failed!
muxTxRestart
[" muxError
END FLAGS changed by protocol ID 0x%x for: %s Unit %d
@a" 
Start of muxTkBindCommon
Found the END object
Can't bind to NPT style device with muxBind()
muxTkBind: EndBind failed
muxTkCommonBind: cannot allocate memory for protocol node
Protocol %d
(|g" 
h" \
(Dh" tt" 
{" h
(netCreate:  error calling netCreate2()  errno:0x%08x
(pv" netCreate2:  pNetFd == NULL errno:0x%08x
STOR %s
netCreate2:  error calling ftpXfer()  errno:0x%08x
netCreate2:  error calling pathCat()  errno:0x%08x
/bin/cat > %s
netCreate2:  error calling rcmd()  errno:0x%08x
(Xw" 
x" DELE %s
netDelete:  error calling ftpXfer()  errno:0x%08x
/bin/rm %s
netDelete:  error calling rcmd()  errno:0x%08x
netDelete:  error fioread()  errno:0x%08x
%s:%s errno:0x%08x
QUIT
netDelete:  error calling ftpCommand("QUIT")  errno:0x%08x
w" ,>
{" 8{" L{" T{" **** netOpen: name:%s mode:0x%x perm:0x%x Entered ***
netOpen:  error calling netFdCreate()  errno:0x%08x
**** netOpen: calling netFileExists ***
**** O_CREATE NOT USED!!! ***
netOpen: calling netCreate2 
**** netOpen: netCreate2 return error ***
netOpen: returning file descriptor pointer 0x%08x after creating file
netOpen: netFileExists - returned OK - file exists
netOpen: CREAT called, but file already exists
netOpen:  calling netGet() 
netOpen:  netGet() return !OK - errno:0x%08x
netOpen:  error calling netSeek()  errno:0x%08x
netOpen:  error calling netSockOpen()  errno:0x%08x
~" 0
" netClose: entered
netClose: error calling netPut to flush file errno=0x%08x
netClose: error calling netSockClose errno=0x%08x
read[hit=%d mis=%d] fseek[hit=%d mis=%d] bseek[hit=%d mis=%d]
" NLST
netLs:  error calling ftpXfer("NLST")  errno:0x%08x
NLST %s
netLs:  error calling pathCat("%s", "%s")  errno:0x%08x
/bin/ls -a %s
netLs:  error calling rcmd() errno:0x%08x
netLs:  error calling write()  errno:0x%08x
netLs:  error calling read()  errno:0x%08x
netLs:  error calling ftpReplyGet()  errno:0x%08x
netLs: %s:%s errno:0x%08x error calling fioread() 
netLs:  error calling ftpCommand()  errno:0x%08x
w" ,>
" L{" $
" netLsByName:  error calling ioFullFileNameGet()  errno:0x%08x
netLsByName:  error UNKNOWN_REQUEST errno:0x%08x
netFdCreate:  error callinf netFdCreate errno:0x%08x
" P&	(h
" netFileExists:  error S_ioLib_NO_FILENAME errno:0x%08x
netFileExists:  error calling ftpXfer(). errno:0x%08x
netFileExists:  error calling rcmd(). errno:0x%08x
netFileExists:  error calling read() on data socket for ls. errno:0x%08x
netFileExists:  full message:%s
netFileExists:  message:%s
netFileExists:  match error on ls 
netFileExists:  file does not exist
netFileExists:  error calling close() on dataSock. errno:0x%08x
netFileExists: error calling ftpReplyGet(). errno:0x%08x
netFileExists:  error calling read() on control socket. errno:0x%08x
netFileExists:  error calling ftpCommand("QUIT"). errno:0x%08x
netFileExists:  returning (%d)
w" D
" L{" P
" cat: read error: Is a directory
RETR %s
netGet:  error calling ftpXfer(). errno:0x%08x
netGet:  error calling pathCat(). errno:0x%08x
/bin/cat < %s
netGet:  error calling rcmd(). errno:0x%08x
netGet:  error calling ftpCommand("QUIT"). errno:0x%08x
netGet:  error calling netWrite(). errno:0x%08x
netGet:  error calling ftpReplyGet(). errno:0x%08x
netGet: %s:%s  . errno:0x%08x
w" ,>
" L{" 4
" netPut:  error calling ftpXfer()  errno:0x%08x
netPut:  error calling pathCat(). errno:0x%08x
netPut:  error calling rcmd(). errno:0x%08x
netPut: error calling ftpCommand("QUIT").  errno:0x%08x
netPut:  error calling write(). errno:0x%08x
netPut:  error calling netRead(). errno:0x%08x
netPut:  error calling close(). errno:0x%08x
netPut:  error calling ftpReplyGet(). errno:0x%08x
netPut: %s:%s  . errno:0x%08x
netPut:  error calling fioRead(). errno:0x%08x
netPut:  error calling ftpCommand(). errno:0x%08x
w" ,>
" L{" 
" : Permission denied
: No such file or directory
: Is a directory
netSockOpen:  error calling ftpXfer()  errno:0x%08x
w" ,>
w" cat: write error: Broken pipe
netSockClose: error closing fd:%d errno=0x%08x
netSockClose: error during ftpReplyGet ctrlSock:%d errno=0x%08x return value:%d
netSockClose: %s:%s   errno:0x%08x
netSockClose: error during fioread ctrlSock:%d errno=0x%08x return value:%d
netSockClose: error during ftpCommand (QUIT) ctrlSock:%d errno=0x%08x return value:%d
netSockClose: error closing ctrl sock fd:%d errno=0x%08x
" ,>
" L{" 
(not found
fileDoesNotExist:matches SunOs 1.x
 No such file
fileDoesNotExist:matches Solaris
fileDoesNotExist:NO MATCH - file must exist
" ,>
(%.*s.
 %-*.*s
" Active Internet connections (including servers)
%-8.8s %-5.5s %-6.6s %-6.6s  %-21.21s %-21.21s %s
Proto
Recv-Q
Send-Q
Local Address
Foreign Address
(state)
--------
-----
------
---------------------
-------
" %-8x 
%-5.5s %6ld %6ld 
" badaddr
nogif
notmember
toolong
rawout
badvers
noroute
badoptions
cantfrag
outfragments
fragmented
reassembled
nobuffers
localout
delivered
unknownprotocol
redirectsent
cantforward
fastforward
forward
fragtimeout
fragdropped
infragments
badlen
badhlen
toosmall
tooshort
badsum
total
%20s %10lu
" `S
(ping: unable to add task Delete hook
ping: unknown host %s
datalen value too large, maximum is %d
datalen value too small, minimum is 8
%s [%s] %s:%d: 
ERROR
pingLib.c
%s: 
Unable to allocate transmit buffer
Unable to allocate receive buffer
you need to increase socket buffer size
setsockopt(SO_SNDBUF)
setsockopt(SO_RCVBUF)
PING %s
 (%s)
 (%d=20+8+%d bytes)
ping: wrote %s %d chars, ret=%d
ping: ERROR
ping: timeout
" packet too short (%d bytes) from %s
%d bytes from %s (%s): 
%d bytes from %s: 
icmp_type=%d
x%2.2lx: x%8.8lx
icmp_code=%d
icmp_seq=%d. 
time=%d. ms
" ----%s PING Statistics----
%d packets transmitted, 
%d packets received, 
%d%% packet loss
round-trip (ms)  min/avg/max = %d/%d/%d
%s is alive
no answer from %s
(0@-
(User name or password too long
" %s
(sockLibInit: psockFdMap has not been initialized
" sockLibAdd: pSockFdMap has not been initialized
sockLibAdd: Could not allocate memory for SOCK_LIB_MAP from DS_MALLOC
sockLibAdd: Either sockLibInitRtn passed to us is NULL or the backend init routine returned an error
(p@-
(p@-
(0@-
  (b  
  0@-
(p@-
(0@-
(p@-
 0@-
 __________________
CLUSTER POOL TABLE
_______________________________________________________________________________
size      clusters  free      usage     minsize   maxsize   avgsize
-------------------------------------------------------------------------------
%-10d
%-10lu
# type        number
---------   ------
%-8s:    %3ld
%-8s:    %3d
TOTAL
number of mbufs: %ld
number of times failed to find space: %ld
number of times waited for space: %ld
number of times drained protocols for space: %ld
ZONEREF
ZONEINIT
UPDATEMA
UPDATEM
UPDATEDA
UPDATED
UPDATEA
CQUERYU
CQUERYM
IQUERY
QUERY
NOCHANGE
ZONEERR
NOTAUTH
NXRRSET
YXRRSET
YXDOMAIN
REFUSED
NOTIMP
NXDOMAIN
SERVFAIL
FORMERR
NOERROR
icmp
igmp
nvp-II
chaos
;; ->>HEADER<<- opcode: %s, status: %s, id: %d
; flags:
; Ques: %d
, Ans: %d
, Auth: %d
, Addit: %d
;; QUESTIONS:
, type = %s
, class = %s
;; ANSWERS:
;; AUTHORITY RECORDS:
;; ADDITIONAL RECORDS:
;; ...truncated
name = %s
(,&# 
(,&# 	%lu
	%s	; proto %d, port %d
	%.*s
			%lu	; serial
			%lu	; refresh (%s)
			%lu	; retry (%s)
			%lu	; expire (%s)
			%lu )	; minimum (%s)
	%d 
	%s %s ( 
	?%d?
;; packet size error (found %d, dlen was %d)
,# 4-# 
6# 4-# 
.# 4-# 4-# 4-# 
6#  5# 4-# 
2# 40# X0# 
2# 40# 
6# P4# 
)#  )# $)# p
(<)# D)# X)# p)# 
|8# 
x8# 
p8# 
l8# 
HESIOD
CHAOS
># p># 
h># X># 
T># @># 
<># 4># 
0># 
># 	
=# t=# 
p=# h=# 
d=# P=# 
H=# 4=# 
0=# $=# 
x<# h<# 
d<# X<# 
T<# 4<# 
0<# 
<#  
;# !
;# "
|;# l;# 
d;# @;# 
8;#  ;# d
:# e
:# f
:# #
l8# 
"any"
URN Naming Authority
NAPTR
group ID (nonstandard)
user ID (nonstandard)
user information (nonstandard)
UINFO
mail agent (deprecated)
MAILA
mailbox-related data (deprecated)
MAILB
zone transfer
AXFR
incremental zone transfer
IXFR
ATM address (unimplemented)
ATMA
server selection
NIMROD locator (unimplemented)
NIMLOC
endpoint identifier (unimplemented)
next valid name (unimplemented)
location
IPv6 address
AAAA
geographical position (withdrawn)
GPOS
mapping information
signature
NSAP_PTR
nsap address
NSAP
router
ISDN address
ISDN
X25 address
DCE or AFS server
AFSDB
responsible person
text
mail exchanger
mailbox information
MINFO
host information
HINFO
domain name pointer
well-known service (deprecated)
null
NULL
mail rename
mail group member
mailbox
start of authority
canonical name
CNAME
mail forwarder (deprecated)
mail destination (deprecated)
name server
address
# 0@-
$8# 0 secs
%d day%s
%d hour%s
%d min%s
%d sec%s
(\@# 
t@# p@# d@# x@# 
|C# 
C# tC# lC# 
%s.%s
%s [%s] %s:%d: 
DEBUG
res_send.c
%s: 
resSend()
ERROR
s out-of-bounds
old answer:
 server rejected query:
WARNING
server rejected query
got answer:
(8L#  L# 0L# DL# LL# XL# 
(\L# dL# tL# 
L# p@-
(DE# 
B# p@-
(p@-
(RTSOL
RTADV
RIP_V4
SYSCTL
DHCPD_V6
DHCP_V6
DHCPD_V4
DHCP_V4
FTPD
TFTPD
TFTP
TELNETD
PING_V6
PING_V4
RIPNG
(%s [%s] %s:%d: 
INFO
applUtilLib.c
%s: 
Changed category %s to LOG_DEBUG logging
Changed category %s to LOG_INFO logging
(,m# 
m# $m# <m# Dm# pm# tm# Logging Categories:
    %s (0x%.2x)
Logging Levels:
    DEBUG_LEVEL (0x%.2x), INFO_LEVEL (0x%.2x)
    WARNING_LEVEL (0x%.2x), ERROR_LEVEL(0x%.2x)
To change the logging level of a category use:
    changeLogLevel (categoryNumber, levelNumber)
p# 8p# lp# 
p# Active Logging Categories
    %s (0x%.2x) logging at DEBUG_LEVEL to %p
    %s (0x%.2x) logging at INFO_LEVEL to %p
    %s (0x%.2x) logging at WARNING_LEVEL to %p
    %s (0x%.2x) logging at ERROR_LEVEL to %p
s# 0s# 0s# 0s# 
s# 0s# 
q# @
r# @r# 
(0@-
netLibInit: couldn't allocate job nodes
tNetTask
# p@-
(netJobAdd: ring buffer overflow!
Invalid value for hints
System error returned in errno
ai_socktype not supported
servname not supported for ai_socktype
hostname nor servname provided, or not known
No address associated with hostname
Memory allocation failure
ai_family not supported
Non-recoverable failure in name resolution
Invalid value for ai_flags
Temporary failure in name resolution
Address family for hostname not supported
Success
Unknown error
# null
sink
name
routed
route
ripng
router
tftp
domain
nameserver
telnet
ftp-data
discard
tcpmux
No address associated with name
Unknown server error
Host name lookup failure
Unknown host
Resolver Error 0 (no error)
Resolver internal error
Unknown resolver error
getaddrinfo returned ERROR
(in-addr.arpa
0123456789
(<NULL>
# 0123456789ABCDEF
0123456789abcdef
(0@-
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
kern_sysctl.c
sysctl
debug
Sysctll failed
name
%s:%d sysctl_add_oid failed for parent=%s, var=%s
next
name2oid
oidfmt
kern
hostname
# 0@-
can't re-use a leaf (%s)!
sysctl_remove_oid: corrupt tree, entry: %s
# 0@-
can't remove non-dynamic nodes!
Warning: bad oid_refcnt=%u (%s)!
%d %s 
%c%c
 *Handler
 Node
 Int
 String
 Quad
 Opaque/struct
(0@-
(p@-
sysctl
Sysctl internal magic
kern
High kernel, proc, limits &c
Network
(@(#) Copyright (c) 1993
	The Regents of the University of California.  All rights reserved.
$FreeBSD: src/sbin/sysctl/sysctl.c,v 1.38 2001/10/30 20:15:32 tobez Exp $
%s [%s] %s:%d: 
ERROR
sysctl.c
%s: 
startGetOpt failed 
# %s
usage: sysctl [-beNnox] variable[=value] ...
       sysctl [-beNnox] -a
# AabeNnowxX
unknown oid '%s'
%d	%s
couldn't find format of oid '%s'
oid '%s' isn't a leaf node
oid '%s' is read only
oid '%s' is type %d, cannot set that
%s: value is not available
%s: specification is incomplete
%s: type is unknown to this program
WARNING
%s: errno=%x
 -> 
(p@-
sysctl fmt %d %lu %d
# sysctl name %d %lu %d
showvar: KHEAP_ALLOC failed for size=%lu
%s%s
%s%u
%s%d
%s%lu
%s%ld
Format:%s Length:%lu Dump:0x
%02x
# sysctl(getnext) %d %lu
'" 0
$ p@-
$ %s%d
$ p@-
'" 00
$ gtf_core.c
gtfBookkeeping
null handler
gtfTimerCreate
memory problem: Timer Free Queue exhausted
---     GTF General Timer Facility     ---
---  current ticks            : %10lu
---  timer unit %u
---- granularity [ticks]      : %10u
---- number fired timer       : %10lu
---- number outstanding timer : %10u
--- currAllocTimer:           : %10u
--- maxAllocTimer:            : %10u
$ Error
### Runtime Failure !!! File %s Function %s Line %d - %s
@(#) Copyright (c) 1983, 1989, 1991, 1993
	The Regents of the University of California.  All rights reserved.
$FreeBSD: src/sbin/route/route.c,v 1.40.2.4 2001/07/03 11:01:20 ume Exp $
xresolve
static
ssthresh
sendpipe
rttvar
reject
recvpipe
proxy
proto2
proto1
prefixlen
nostatic
netmask
monitor
mask
lockrest
lock
llinfo
link
inet6
inet
interface
iface
hopcount
host
genmask
gateway
flush
expire
delete
cloning
change
blackhole
atalk
bad keyword: %s
usage: route [-dnqtv] command [[modifiers] args]
no arguments
malloc
%d	%s
startGetOpt failed 
nqdtv
socket
&$ L2
'$ x($ x($ 
'$ x($ 
'$ x($ x($ <($ x($ x($ 
'$ x($ x($ x($ x($ x($ x($ x($ x($ x($ x($ x($ x($ x($ x($ 8($ 
(t#$ 
#$ route-sysctl-estimate
route-sysctl-get
Examining routing table from sysctl
Error writing to routing socket
got only %d for rlen
%-20.20s 
done
(<)$ 
#$ T)$ X
(h)$ d
)$ default
%u.%u.%u.%u
(%d)
(8-$ L-$ @
(@-$ T-$ %u
%u.%u
%u.%u.%u
af %d:
/$ 8-$ @
/$ @-$ T-$ 
2$ x2$ 
%s %s %s
: gateway %s
 (%s)
not in table
entry in use
routing table overflow
: %s
7$ H6$ 
7$ ,6$ 
6$ \5$ \5$ 
5$ $5$ 
5$ l5$ t5$ |5$ 
6$ t6$ d5$ 
6$ @5$ 
t3$ ,
(x3$ 
($"$ 
"$ |3$ 
(getifaddrs
internal error
bad address: %s
=$ x=$ 
=$ t
#$  
;$ 8-$ 0
;$ prefixlen not supported in this af
%s: bad value prefixlength
(h@$ 
(malloc failed
actual retrieval of interface table
<)$ 
got message of size %d on %s
(<C$ u
Error writing to routing socket
Error reading from routing socket
D$ (D$ 
(RTM_DELMADDR: multicast group membership removed from iface
RTM_NEWMADDR: new multicast group membership on iface
RTM_IFINFO: iface status change
RTM_DELADDR: address being removed from iface
RTM_NEWADDR: address being added to iface
RTM_RESOLVE: Route created by cloning
RTM_OLDDEL: caused by SIOCDELRT
RTM_OLDADD: caused by SIOCADDRT
RTM_LOCK: fix specified metrics
RTM_MISS: Lookup failed on this address
RTM_REDIRECT: Told to use different route
RTM_LOSING: Kernel Suspects Partitioning
RTM_GET: Report Metrics
RTM_CHANGE: Change Metrics or flags
RTM_DELETE: Delete Route
RTM_ADD: Add Route
routing message version %d not understood
%s: len %d, 
if# %d, flags:
metric %d, flags:
pid: %ld, seq %d, errno %d, flags:
L$ 8M$ 8M$ 
($L$ 
(4L$ (
(HL$    route to: %s
routing message version %d not understood
message length mismatch, in packet %d, returned %d
message indicates error %d
destination: %s
       mask: %s
    gateway: %s
  interface: %.*s
      flags: 
 recvpipe  sendpipe  ssthresh  rtt,msec    rttvar  hopcount      mtu     expire
%8ld%c 
%8ld%c
sockaddrs: 
O$  P$ 
P$  P$  P$  P$  P$  P$  P$  P$  P$  P$  P$  P$ 
N$ (N$ @
(<N$ PN$ dN$ xN$ (
N$ X
N$ X
locks: 
 inits: 
sockaddrs: 
3$ LS$ X
(\S$ %c
T$ 0@-
(%s: link %s; 
%s: inet %s; 
U$ (U$ 
dV$ pV$ `V$ |V$ 
@(#) Copyright (c) 1983, 1993
	The Regents of the University of California.  All rights reserved.
$FreeBSD: src/sbin/ifconfig/ifconfig.c,v 1.51.2.13 2001/08/20 18:38:41 brooks Exp $
$m$ 
$m$ 
$m$ 
$m$ 
$m$ 
|X$ 
xX$ 
Lq$ 
Hl$ 
broadcast
metric
netmask
remove
delete
-alias
alias
-debug
debug
-arp
down
(|Y$ 
Ly$ 
(tY$ 
Ly$ 
link
ether
inet
usage: ifconfig interface address_family [address [dest_address]]
                [parameters]
       ifconfig -a [-d] [-m] [-u] [address_family]
       ifconfig -l [-d] [-u] [address_family]
       ifconfig [-d] [-m] [-u]
Z$ ,Z$ <Z$ 
Z$ malloc
%d	%s
startGetOpt failed
inet6
adlmu
if   list-sysctl-estimate
actual retrieval of interface table
out of sync parsing NET_RT_IFLIST
expected %d, got %d
msglen = %d
buf:%p, next:%p, lim:%p
interface %s does not exist
x^$ 
^$ $
( h	(
(|[$ 
[$ tY$ 
X$ P
\$ ,\$ <\$ Ly$ p
(X\$ socket
'%s' requires argument
'%s' requires 2 arguments
interface %s cannot change %s addresses!
ioctl (SIOCDIFADDR)
ioctl (SIOCAIFADDR)
X$  ;
[$ hW$ 
(Hh$  d
(\h$ 
ioctl (SIOCGIFFLAGS)
Po$ `p$ 
o$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ <o$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ `p$ (o$ 
@p$ @p$ 
p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ ,p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ @p$ 
m$ P
(ioctl (set metric)
p$ ioctl (set mtu)
(<q$ ioctl (SIOCGIFMETRIC)
ioctl (SIOCGIFMTU)
%s: 
 flags
BROADCAST
DEBUG
LOOPBACK
POINTOPOINT
SMART
RUNNING
NOARP	PROMISC
ALLMULTI
OACTIVE
SIMPLEX
LINK0
LINK1
LINK2
MULTICAST
NOTRAILERS
INET_UP
INET6_UP
 metric %d
 mtu %d 
%s has no %s interface address!
X$  ;
q$  h	(
r$ p
(Ly$ 
r$ 	inet %s 
--> %s 
netmask 0x%lx 
broadcast %s
v$ p
(	ether 
	lladdr 
%02x%c
0y$ 8y$ Dy$ p
(%s: no such interface
%s: permission denied
r$ %u
%s: bad value
[$ %s=%o
%s=%x
}$ p
(deg : ether_getaddr not supported
[$ @(#) Copyright (c) 1983, 1993
	The Regents of the University of California.  All rights reserved.
$FreeBSD: src/sbin/ifconfig/ifconfig.c,v 1.51.2.13 2001/08/20 18:38:41 brooks Exp $
routing:
	%u bad routing redirect%s
	%u dynamically created route%s
	%u new gateway%s due to redirects
	%u destination%s found unreachable
	%u use%s of a wildcard route
$ ----------------------------------------------------------------------------
destination      gateway              flags  Refcnt  Use           Interface
ROUTE NET TABLE
ROUTE HOST TABLE
$ %-16s 
not AF_INET
%02x:%02x:%02x:%02x:%02x:%02x  
%-20s 
%-5lu  
%-5ld   
%-13ld 
%s%d
$ %-16s
%-10lx
%-21s
%-6lu
%-7ld
%-13ld
%s%d       
$ %-16s%-10s%-21s%-6s%-7s%-13s%-10s
Destination
Mask
Gateway
Flags
RefCnt
Interface
$ --------------------------------------------------------------------------
destination      gateway            flags  Refcnt  Use           Interface
LINK LEVEL ARP TABLE
hostname         inet address      aliases
--------         ------------      -------
%-16s %-18s
$ TUNNEL
FRAME_RELAY
ULTRA
SLIP
NSIP
ETHERNET_3MBIT
SOFTWARE_LOOPBACK
PROP_POINT_TO_POINT_SERIAL
PRIMARY_ISDN
BASIC_ISDN
SDLC
LAPB
FDDI
HYPERCHANNEL
PROTEON_80MBIT
PROTEON_10MBIT
STARLAN
ISO88026_MAN
ISO88025_TOKENRING
ISO88024_TOKENBUS
ISO88023_CSMACD
ETHERNET_CSMACD
RFC877_X25
DDN_X25
HDH1822
REGULAR_1822
OTHER
UNDEFINED
%s (unit number %d):
     Type: %s
inet
Destination Internet address
Broadcast address
     Netmask 0x%lx Subnetmask 0x%lx
     Metric is %lu
     Maximum Transfer Unit size is %lu
     %lu packets received; %lu packets sent
     %lu multicast packets received
     %lu multicast packets sent
     %lu input errors; %lu output errors
The driver does not support RFC2233!
     %.0f octets received
     %.0f octets sent
     %.0f unicast packets received
     %.0f unicast packets sent
     %.0f broadcast packets received
     %.0f multicast packets received
     %.0f broadcast packets sent
     %.0f multicast packets sent
     %lu octets received
     %lu octets sent
     %lu unicast packets received
     %lu unicast packets sent
     %lu broadcast packets received
     %lu broadcast packets sent
     %lu non-unicast packets received
     %lu non-unicast packets sent
     %lu incoming packets discarded
     %lu outgoing packets discarded
     %lu incoming errors
     %lu outgoing errors
     %lu unknown protos
     %ld collisions; %ld dropped
"%s" - No such interface
No network interface active.
"	(d
$ @W
$      %s: %s
$      Flags: (0x%x) 
DOWN 
LOOPBACK 
POINT-TO-POINT 
BROADCAST 
MULTICAST 
PROMISCUOUS 
TRAILERS 
ARP 
RUNNING 
FASTPATH_V4 
FASTPATH_V6 
NOFORWARD 
DEBUG 
$      Ethernet address is %02x:%02x:%02x:%02x:%02x:%02x
@ether_output: ifnet pointer is NULL, cannot proceed
ether_output: pDrvCtrl is NULL, cannot proceed
ether_output: interface is not UP or RUNNING
ether_output: no route to destination
%s%d: can't handle af%d
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
if_ethersubr.c
link
ether
Ethernet
%s:%d sysctl_add_oid failed for parent=%s, var=%s
(rtqkill route really not free
in_rtqkill: error %d
(VUUU
$ 0@-
$ in_ifadownkill: error %d
$ %s:%d sysctl: parent node or its child link 			  NULL for parent=%s
in_rmx.c
rtexpire
Default expiration time on dynamically learned routes
Sysctll failed
rtminexpire
Minimum time to attempt to hold onto dynamically learned routes
rtmaxcache
Upper limit on dynamically learned routes
(p@-
(domaininit: %ssw[%d] has no usrreqs!
$ d0
(0@-
$ 0@-
(gfff
(0@-
(WARNING: syncache hash size is not a power of 2.
syncache_init: unable to allocate hash table
$ p@-
(%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
tcp_syncache.c
syncookies
Use TCP SYN cookies if the syncache overflows
Sysctll failed
syncache
TCP SYN cache
%s:%d sysctl_add_oid failed for parent=%s, var=%s
bucketlimit
Per-bucket hash limit for syncache
cachelimit
Overall entry limit for syncache
count
Current number of entries in syncache
hashsize
Size of TCP syncache hashtable
rexmtlimit
Limit on SYN/ACK retransmissions
$ 0@-
(0@-
(sofree: not queued
$ soclose: NOFDREF
$ 0@-
soaccept: !NOFDREF
$ p@-
(ip6_sooptmcopyin
%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
uipc_socket.c
somaxconn
Maximum pending socket connection queue size
Sysctll failed
sbappendaddr
(sbappendcontrol
% semi-panic: sbcompress
% sbflush: locked
sbflush: cc %ld || mb %p || mbcnt %ld
	% sbdrop
%s:%d sysctl: parent node or its child link 			  NULL for parent=%s
uipc_socket2.c
maxsockbuf
Maximum socket buffer size
Sysctll failed
maxsockets
Maximum number of sockets avaliable
sockbuf_waste_factor
 p@-
(gfff@K
%  w
%  w
% p@-
(0@-
(p1% bf
,% %u.%u.%u.%u.in-addr.arpa
l/% 
(p@-
illegal option -- %c
option requires an argument -- %c
(<4% 
(@4% 
(X4%  
(udp
(p@-
%u.%u.%u.%u
(4N% 4I% 
(hP% 
(Hx% 
"& l
"& d
(dQ& 
L& 8K& 
B& $N& 
(PZ& 
(8}& 
(DU	(
(P&	(
' ,>
T	((
;' 4=' P;' 
T	(D
H' ,>
D' D
H' Pt
H' P5
(TI' 
(4F' 
(XF' $
(lF' H
Q' h
T	(DL
d' (
s' (\
(\g' 
dv' 
(hz' @z' x
(<}' 
>' p
' @;
((&	(Db
T	(\5
(l$	(D
( @$	(t
( 0\
( Ht
' ^	
83( 8
5( <
T	(D
?( ,>
>( DL
E( @E( 
	(U'
xT( 
(DU	(\
& |/
(@$	(:0
b( ,c( 
( ,Y
(P&	(=D
( M^
	(sa
) Error: Null framework object pointer!
Name                   : %s
Control Task Id        : 0x%x
Control Task Priority  : %d
Control Job Queue Size : %d Bytes
Data Task Id           : 0x%x
Data Task Priority     : %d
Data Job Queue Size    : %d Bytes
Number of Layers       : %d
Number of Components   : %d
Number of Parameters   : %d
Number of Interfaces   : %d
Number of Events       : %d
Number of Profiles     : %d
Number of Stacks       : %d
pfw.c
pfwCreate
Invalid argument: Null netPoolId
Invalid argument: Null partId
controlJobQueueSize is to small
dataJobQueueSize is to small
Invalid parameter: Framework name already exits
Unable to allocate memory
Unable to create memory manager 
Unable to add framework table
Unable to create the control task semaphore
Unable to allocate data job queue
Unable to create data task semaphore
%s_D_%d
Unable to spawn data task
Unable to allocate control job queue
%s_C_%d
Unable to spawn control task
	) (	) H	) 
) h	) 
	) gfff$
) p@-
pfwControlTask
Timer handler function pointer is null
) _pfwReceive
Null argument
) pfwReceive
Invalid argument: Null state object
Invalid argument: Null stack object
Unknown packet
The packetType function is NULL
Unknown plane
Null receive
) pfwSend
Null state
) pfwDataJobAdd
Invalid argument: Null framework object pointer
Data job queue does not exist
Invalid argument: Null fuction pointer
Invalid argument: size is out of range
) pfwControlJobAdd
) pfwNetPoolIdGet
Invalid argument: Null framework pointer
) Name              : %s
Framework         : %s
Stack Data Size   : %d
Profile Data Size : %d
) Error
File %s, Function %s, Line %d, Framework %s, Stack %d - %s
File %s, Function %s, Line %d, Framework %s - %s
File %s, Function %s, Line %d - %s
   ID      Object    Name
--------  --------  ------
%8d  %8x  %s
pfwComponent.c
pfwComponentAdd
Null layer
Null framework object
Null layer object
Component name already exits
Unable to allocate memory
semMCreate error
Component could not be added to the table
_add_static_
Unable to add framework parameter
_remove_
_add_dynamic_
%) <
) pfwComponentDelete
Reference count error
Reference count of the layer object is incorrect
,%)  ID       OBJECT   NAME 
-------- -------- --------------------------------
%8d %8x %s
%) pfwComponentShow
Invalid argument: Null component object pointer
Invalid component object pointer
Layer             : %s
Protocol          : %d
h&) 
) |&) 
() pfwEvent.c
pfwEventManagerCreate
Invalid argument: Null framework object pointer
pfwEventCreate
Unable to allocate tableObj
x() T() `() 
p6) T() x() `() pfwEventPublish
Unable to allocate memory
Unable to add event to eventTable
T() P6) x() 
*) pfwEventSubscribe
Invalid argument: Null plugin object pointer
Invalid argument: Null name pointer
Invalid argument: Null event handler function pointer
semTake error
pfwEventRegister
X+) T() D+) 
+) pfwEventUnsubscribe
Invalid argument: Null event object pointer
SemTake error
X+) T() 
-) pfwEventPluginObjUnsubscribe
X+) T() 
+) 0@-
pfwEventItemAdd
Invalid argument: Null state
t0) T() d0) 
t0) T() d0) Invalid argument: Null stack object
2) T() d0) 
t0) T() d0) 
P6)    ID      Object    Name
--------  --------  -------
%8d  %8x  %s
(5) D5) d5) Invalid argument: Null framework object pointer!
5) t5) 
pfwInterface.c
pfwInterfaceCreate
Invalid argument: Null framework object
Unable to allocate a table object
6) pfwInterfaceDelete
<B) 
7) pfwInterfaceRegister
Unable to allocate memory
Unable to add interface name to interfaceTable
B) $8) 
8) @8) pfwInterfaceBind
Invalid argument: Null interface object pointer
Invalid argument: Null plugin object pointer
Null framework object pointer
Invalid argument: Invalid interface id
X9) 
6) D9) 
9) $8) pfwInterfaceUnbind
Invalid interface id
9) D9) 
;) pfwInterfaceObjGetViaPluginObj
pfwInterfaceObjGetNext
D>) 
6) X9) pfwInterfaceObjAndPluginObjViaPfwObjGet
Invalid argument: Null framework object pointer
9) pfwInterfaceIdGet
B) pfwInterfaceReferenceAdd
Null plugin object pointer
@@) 
6) X9) \@) pfwInterfaceReferenceDelete
Cannot deacrease a zero reference count
6) X9) \@) ,A) 
   ID      Name
--------  ------
%8d  %s
PB) dB) xB) Invalid argument: Null framework object pointer!
B) pfwLayer.c
pfwLayerAdd
Null layer
Null framework object
Invalid plane id
Null stackAddStart function
Null profileDataConstruct function
Layer name already exists
pfwComponentAdd
Unable to allocate memory
semMCreate error
Layer could not be expanded
Layer could not be added
_add_static_
Unable to add framework parameter
_remove_
_add_dynamic_
xC) `C) lC) 
D) 8D) LD) 
M) hD) 
D) pfwLayerDelete
Reference count error
`C) hI) xI) 
L) pfwlayerShow
Invalid argument: Null layer object pointer
pfwLayerShow
Invalid layer object pointer
Plane             : 
FRAMING_PLANE
CONTROL_PLANE
DATA_PLANE
UNKNOWN
dJ) `C) TJ) 
L)    ID     Object   Name
-------- -------- ------
%8d %8x %s
LL) hL) 
(M) p@-
pfwMemory.c
pfwMemoryMalloc
Unable to allocate memory
N) pfwFree
Invalid argument: NUll pointer
Null chunk pointer
semTake failed
R) pfwMemoryManagerDelete
Invalid argument: Null framework object pointer
Null memory manager pointer
U) pfwMemoryManagerCreate
Invalid argument: Null memory partition id
pfwMemoryInit
M) ,V) DV) 
N) pV) Invalid argument: Null framework object pointer!
Z)  0
pfwProfile.c
_pfwParameterAdd
Unable to add _REMOVE_FROM_PROFILE param
Unable to add a framework parameter
Z)  [) pfwParameterAdd
Invalid argument: Null owner
Unable to allocate memory for a parameter
\) _pfwProfileDelete
Reference count error
]) pfwProfileDelete
Invalid argument: NULL profile object
Invalid profile object
semTake error
D_) 
Z) X_) 
pfwProfileTreeCopy
Unable to allocate memory
0c) 
c) pfwProfileCreate
0c) 
d) r
Profile Set could not open file %s
Could not read parameter name from file %s
Unknown Parameter name %s in file %s
Could not read value for parameter %s from file %s
Invalid NULL value for parameter %s
Invalid value %s for parameter %s
NULL
f) hf) 
f) <f) pfwNewComponentProfileItemAdd
Unable to create a new component profile Item
0i) 
i) pfwNewLayerProfileItemAdd
0c) 
Z) Dj) removeLayerProfileItem
Z) @k) 
]) removeComponentProfileItem
]) @k) pfwProfileSet
Invalid profile obj
Invalid parameter id
Unable to add new layer
Unable to add a new component profile item
Tn) 
Z) Dn) hn) 
n) 0c) 
n) _pfwStackParamOp
Invalid stack obj
Invalid parameter type
Layer obj not found
Component obj not found
@s) 
Z) ,s) hn) Ts) ls) 
pfwBaseProfileCreate: NULL framework 
Unable to allocate memory for pfw base profile: %d
File %s - Line %d - pfwBaseProfileCreate - Failed 
) Null framework object pointer!
)                 Parameters: 
                %6s %32s VALUE
  ID  
              NAME              
                %6s %32s -----
------
--------------------------------
HANDLER ERROR
	%6d %32s BAD PARAMETER TYPE
                %6d %32s %s
y) Dy) Ly) $y) py) 
z)  ID       Object   Name
-------- -------- ------
%8d %8x %s
{) 0@-
|) Null profile object pointer!
Profile : %s
    Plane : 
CONTROL
DATA
FRAMING
UNKNOWN
        Layer : %s 
(static)
(dynamic)
            Component : %s 
}) $}) 0}) <}) _pfwParameterItemShow
NUll parameter Object
   ID                 Name                             Owner
-------- -------------------------------- --------------------------------
%8d %32s %32s
Z)  
%s: EOF
%s: error
warning: word in file %s too long (%.20s...)
) pfwStack.c
pfwStackAdd
NULL profile
No memory for stack
Unable to copy profile information
Unable to create Layer stack Item
Unable to allocate component item
ERROR: No FRAMING plane plug-in object
Null stackAdd function pointer
pfwStackAdd: %s could not process add request for stack 0x%x
pfwStackItemDelete
Reference count error
) pfwStackItemCreate
Unable to allocate memory for stack Item
Unable to initialize stackData
(p@-
pfwStateGet
Invalid argument: Null stack object
Null protocol framework object
) pfwPluginObjStateRelease
Invalid argument: Null state
Null stack object
pfwStackAddComplete
Null state
Invalid Stack object
pfwStackAddComplete: %s couldn't process add request: stack 0x%x
) pfwStackAddError
Null state pointer is received
) pfwStackDelete
Invalid argument: NULL stack object
Invalid stack object
semTake error
Null stackDelete function pointer
pfwStackDelete:%s couldn't process delete request:stack 0X%X
) pfwStackDeleteComplete
pfwStackDeleteComplete: %s could not process delete request: stack 0x%x
) pfwStackDeleteError
) pfwStackDestroy
Invalid argument: Null stack object pointer
) File %s, Function pfwLayerStateGet, Framework %p, 
            Stack %p, Layer %s asking for its state given its own
) pppFirstComponentStateGet
) pfwNextComponentStateGet
 ID        Obj      Status
------  --------  ---------
%6d  %8x  
PFW_STACK_ADD_IN_PROGRESS: pending on %s
PFW_STACK_READY
PFW_STACK_DELETE_IN_PROGRESS: pending on %s
) Invalid argument: Null framework object pointer!
)         Layer : %s
            Component : %s
               Stack Data :
) Invalid argument: Null stack object pointer!
Invalid stack object
Stack : %d
    Plane : 
CONTROL
DATA
FRAMING PLANE
UNKNOWN
) pfwTable.c
pfwTableCreate
Invalid argument: Zero initial table size
Invalid argument: Initial size > max size
Unable to allocate memory
Mutex could not be created
Unable to expand table
) pfwTableDelete
Invalid argument: Null table obj
) pfwTableExpand
pfwTableTraverse
Null table object
Null function pointer
) pfwTableItemInsertBefore
Invalid argument: Null table object pointer
) pfwTableItemInsertAfter
) pfwTableShow
First full row      : %d
Last full row       : %d
Number of full rows : %d
First free row      : %d
Initial size        : %d
Current size        : %d
Maximum size        : %d
Mutex               : %x
) 0@-
) pfwTimer.c
pfwTimerManagerCreate
Invalid argument: Null framework object pointer
pfwTimerManagerInit
Unable to allocate a timer manager
Unable to allocate a timer unit manager
Watch dog timer could not be created
Timer mutex could not be created
) pfwTimerManagerDelete
) pfwTimerCreate
Invalid argument: Null state pointer
Unable to allocate memory
) pfwTimerDelete
Null timer object
) pfwTimerStart
Invalid timeout value
_pppTimerStart
Timeout function pointer is null
Null plugin obj state
Timer object has been started already
Invalid timer unit
) pfwTimerCancel
Null timer unit manager
) pfwTimerExpire
Null timer manager object pointer
) pfwTimeStampStart
Null framework object
Invalid time unit
Invalid argument: Null time stamp pointer
) pfwTimeStampExpired
) pfwTimerShow
Time Unit        : 
100_MILLISECOND
SECOND
MINUTE
UNKNOWN
----------------------------
Current Tick     : %u
Current Deadline : %u
) pppControlLayer.c
pppControlLayerInit
Unable to allocate memory
CONTROL_LAYER
Control layer could not be added to the stack
CONTROL_PROTOCOL_INTERFACE
AUTH_INFO_INTERFACE
AUTHEN_ATTRIBUTES_INTERFACE
PPP_CONTROL_LAYER_INTERFACE
MP_CONTROL_LAYER_INTERFACE
ppp_secretsDatabase
PPP_NETWORK_PHASE_UP
LCP_OPEN_EVENT
LCP_DOWN_EVENT
LCP_CLOSE_EVENT
PPP_AUTH_SUCCESSFUL_EVENT
PPP_AUTH_UNSUCCESSFUL_EVENT
PPP_LINK_RESET_EVENT
) PPP: Invalid OR Incomplete stackObj 0x%x
PPP: Invalid stackObj 0x%x
PPP: Could not find Control Layer plugin Obj
PPP: Control Layer pluginObj is not active in stackObj 0x%x
) p@-
) PPP_LINK_ID_INTERFACE
controlLayerComponentAddComplete
No CONTROL_PROTOCOL_INTERFACE published
Control Layer:No CONTROL_PROTOCOL_INTERFACE for protocol 0x%x
protocol: %x has bad phase %d
) sendIf
Control Layer sendIf routine is not supposed to be called
) MP_FRAMING_LAYER
) stackDelete
Null component
controlLayerStackDataConstruct
NO PPP_AUTH_SUCCESSFUL_EVENT
NO PPP_AUTH_UNSUCCESSFUL_EVENT
NO PPP_LINK_RESET_EVENT
) 0@-
) PPP_INTERFACE_UP_EVENT
PPP: no PPP_INTERFACE_UP_EVENT
PPP_INTERFACE_DOWN_EVENT
PPP: no PPP_INTERFACE_DOWN_EVENT
controlLayerStackAdd
) PPP: could not allocate memory for new protocol Item
componentStackAddDone
COMPONENT_ACCEPTABLE_PROTOCOLS_INTERFACE
PPP_LINK_STATUS_ENTRY_INTERFACE
Control Layer: Could not get linkStatus interface ID
No PPP_LINK_STATUS_ENTRY_INTERFACE!
LCP_EXTENDED_OPTIONS_INTERFACE
Control Layer:Could not get extendedOptions interface ID
No LCP_EXTENDED_OPTIONS_INTERFACE!
LCP_NEGOTIATED_AUTH_PROTOCOL_INTERFACE
Control Layer: Could not get Auth Protocol interface ID
No LCP_NEGOTIATED_AUTH_PROTOCOL_INTERFACE!
PPP_RADIUS
REMOTE_AUTHENTICATION_INTERFACE
No REMOTE_AUTHENTICATION_INTERFACE published
No REMOTE_AUTHENTICATION_INTERFACE!
REMOTE_ACCOUNTING_INTERFACE
No REMOTE_ACCOUNTING_INTERFACE published
No REMOTE_ACCOUNTING_INTERFACE!
noAuthenticationRequired
) PPP:could not find plugin obj for protocol #0x%lx
PPP:could not dynamically add protocol #0x%lx
PPP:No protocol item for dynamically added protocol #0x%lx
mpFraming_localUserName
) Null Framework Object
pppChallengeAuthVerify
* pppPasswordAuthVerify
PPP: no PPP_NETWORK_PHASE_UP
PPP Open: Expecting LCP found 0x%x
* `0
LOCAL
local
REMOTE
remote
EXTERNAL
* lcp_linkDiscriminator
lcp_endpointDiscriminator
lcp_ML_shortSeqNumberHdrFormat
lcp_ML_maxRcvdReconstructedUnit
lcp_passiveMode
lcp_maxUnAckedEchoRequests
lcp_echoRequestSendInterval
lcp_terminationReqInterval
lcp_maxTerminationRequests
lcp_configReqSendInterval
lcp_maxConfigFailure
lcp_maxConfigRequests
lcp_txIdentMessage
lcp_timeRemainingMessage
lcp_timeRemainingInterval
lcp_callbackMessage
lcp_callbackOperation
lcp_selfDescribingPadding
lcp_fcsAlternatives
lcp_ACFCompression
lcp_PFCompression
lcp_magicNumber
lcp_qualityProtocol
lcp_authProtocol
lcp_ACCM
lcp_MRU
PPP_LCP
CONTROL_LAYER
pppOEthernetInit: Couldn't add LCP component to pfw 0x%x
pppLcpComponent - Parameter %s could not be added
LMRU
LACCM
Magic Number
LPFC
LACFC
LSDP
LMDE
LMMRRU
LMSSNHF
LCP_UP_EVENT
PPP_SUB_LAYER_DEAD_EVENT
* $'* 
#* d
'* L(* 
)* |
* xb
* |b
* CONTROL_PROTOCOL_INTERFACE
PPP_LINK_STATUS_ENTRY_INTERFACE
PPP_LINK_CONFIG_ENTRY_INTERFACE
LCP_NEGOTIATED_AUTH_PROTOCOL_INTERFACE
LCP_EXTENDED_OPTIONS_INTERFACE
LCP_CONFIG_REQS_INTERFACE
LCP_PACKET_SEND_INTERFACE
PPP_LINK_STATUS_COUNTER_INCREMENT_INTERFACE
PPP_SECURITY_CONFIG_ENTRY_INTERFACE
LCP_PROXYLCP_INTERFACE
Error in binding LCP_PROXYLCP_INTERFACE
Error in registering LCP_PROXYLCP_INTERFACE
LCP_BUNDLE_OPTIONS_INTERFACE
Error in binding LCP_BUNDLE_OPTIONS_INTERFACE
Error in registering LCP_BUNDLE_OPTIONS_INTERFACE
PPP_LCP:WARNING! Failed to register Link Group MIB II interfaces
PPP_LCP:WARNING! Failed to register Security Config MIB II interfaces
* Local:Negotiation Required,Negotiable:1500
Remote:Negotiation Not Required,Negotiable
Remote:Negotiation Not Required,Negotiable:0
Local:
Remote:
* Remote
Local
LCP: MUST have a valid NetPoolId; See pfwCreate()
* d#* 
* |b
(0@-
PPP_CONTROL_LAYER_INTERFACE
PPP_NETWORK_PHASE_UP
PPP: no PPP_NETWORK_PHASE_UP event
(* ((* l>* 
>* 0@-
* Alternate
Range
{%s}
{Local:
{Remote:
Negotiation Required, 
Negotiation Not Required, 
Error in flag
Negotiable
Not Negotiable
{Local:Alternate:
{Remote:Alternate:
{Local:Range:
{Remote:Range:
,*  ,* $,* 8,* L,* \,* l,* p@-
5* p@-
5* p@-
5* p@-
5* p@-
5* p@-
5* p@-
5* TRUE
FALSE
B*  B* ,B* 8B* DB* PB* \B* 
A* hB* 
C* 4D* 8E* pE* |F* 
F* 0H* 
J* $J* 8J* hH* tB* `J* 
J* (K* HK* dK* 
PPP_LCP
Local:Negotiation Required,Negotiable:%d
Remote:Negotiation Not Required,Not Negotiable:%08x
Local:Negotiation Required,Negotiable:%08x
B* DE* 
Local:Negotiation Required,Negotiable:0
Local:Negotiation Required,Negotiable:%1d
B* <H* 
Local:Negotiation Required,Negotiable:
%04x
PPP: Out of Memory for data_buffer 
start periodic echo failed: state = %d stackObj = 0x%x
start Time remaining failed: state = %d
Q* xN, $R* 
PPP_O_ETHERNET
T* PPP_LCP
Local MRU: %ld, Remote MRU: %ld
LocalToPeer ACCM: %ld, PeerToLocal ACCM: %ld
LocalToRemote ProtocolComp.: %ld, RemoteToLocal ProtocolComp.: %ld
LocalToRemote ACComp.: %ld, RemoteToLocal ACComp.: %ld
LocalAuthProtocol .: %ld, RemoteAuthProtocol: %ld
W* ,X* pX* 
PPP: %s: Illegal transition; state %d, Event %d, stack 0x%x
mpStackConvert: NULL Framework
INTERFACE_LAYER
PPP_IPCP
MP_FRAMING_LAYER
Z* memberStackComponentRemove: NULL argument(s)
memberStackComponentRemove: Null framework object
memberStackComponentRemove: Could not delete                      %s component from Member Stack 0x%x
[* lcpstate.c
mpInterfaceLayerToStackAdd
NULL Framework reference
MP_INTERFACE_LAYER
MP:mpInterfaceLayerToStackAdd():Error in adding mpInterface 
				layer to the Member Stack 0x%x
H]* ,]* 
]* \]* ipcp_terminationReqInterval
ipcp_maxTerminationRequests
ipcp_configReqSendInterval
ipcp_secondaryDnsAddr
ipcp_primaryDnsAddr
ipcp_maxConfigRequests
ipcp_hcParams
ipcp_vjcParams
ipcp_ipAddr
pppIpcpInit - Unable to allocate memory
PPP_IPCP
CONTROL_LAYER
pppIpcpInit - IPCP could not be added to the framework
pppIpcpComponent: Parameter %s could not be added
IP Compression
VJC Compression
IP ADDRESS
PRIMARY DNS SERVER IP ADDRESS
SDNS
SECONDARY DNS SERVER IP ADDRESS
IPCP_UP_EVENT
IPCP_UP_EVENT publish failed 
IPCP_DOWN_EVENT
IPCP_DOWN_EVENT publish failed 
P_* |_* 
v* Hf* 
e* @f* 
t* \x* @x* 
_* Lc
`*  `* 4`* $`* 8`* D`* H`* h`* p`* 
_* D
|_* CONTROL_PROTOCOL_INTERFACE
PPP_IPCP_MIB_INTERFACE
PPP_IPCP: WARNING! Failed to register MIB II interface
 e* 
8, <e* Te* 
4`* 
D`* 
h`* 0@-
Remote
Local
RAS-AMM
Local:
Remote:
%s%s
Local:Negotiation Required, Not Negotiable:
Remote:Negotiation Required, Not Negotiable:
Alternate
Range
{%s}
,{%s}
{Local:
{Remote:
Negotiation Required, 
Negotiation Not Required, 
Error in flag
Negotiable
Not Negotiable
{Local:Alternate:
{Remote:Alternate:
{Local:Range:
{Remote:Range:
|_* 
i* Di* ti* 
j* (j* <j* Lj* \j* PPP_CONTROL_LAYER_INTERFACE
LCP_UP_EVENT
PPP_LINK_RESET_EVENT
`s* |s* 
s* 8
* 0@-
IPCP
|_* 
`* Tx* 
(IPCP_COMPONENT
D{* %s
%s%s%s
Negotiation Required, Not Negotiable:
{* Tx* #
Local:Negotiation Required,Not Negotiable:%s
Remote:Negotiation Required,Not Negotiable:%s
Remote:Alternate:%s@%d
D_* <~* 
i* @~* 
i* p~* 
~* Alternate:
RAS-AMM#%d
D_* 
i* ,
* p@-
|_* p@-
* p@-
send config Req: timerStart failed; state = %d
send Termination Req: timerStart failed; state = %d
* ncp_packet_received: code=%d
Number of bytes = %d len of last tx = %d
PPP:IPCP configuration ACK received with wrong length of 		packet for stack: 0x%x
* PPP:IPCP Configuration NAK Received with no NAK options in it 		for stack: 0x%x
NCP: received bad Configure Request
pppChapInit - Unable to allocate memory of size %d byte s
PPP_CHAP
CONTROL_LAYER
pppChapInit - CHAP could not be added to the framework
chap_localUserName
chap_maxRetries
chap_retryInterval
chap_challengeInterval
* CONTROL_PROTOCOL_INTERFACE
AUTH_INFO_INTERFACE
PPP_CONTROL_LAYER_INTERFACE
LCP_NEGOTIATED_AUTH_PROTOCOL_INTERFACE
* 0@-
vxTarget
* 0@-
* CHAP cannot handle event %d
* you are authenticated
* Authentication refused
* %ld
CHAP:Auth Info Interface:Invalid parameters
NULL Framework Reference
* 0@-
* CHAP:Auth Info Interface:Invalid Parameters
* pppPapInit - Unable to allocate memory of size %d byte s
PPP_PAP
CONTROL_LAYER
pppPapInit - PAP could not be added to the framework
pap_localUserName
pap_maxAuthRequestRetries
pap_authRequestInterval
* CONTROL_PROTOCOL_INTERFACE
pppPapComponent.c
interfaceBind
CONTROL_PROTOCOL_INTERFACE does not exist
AUTH_INFO_INTERFACE
PPP_CONTROL_LAYER_INTERFACE
LCP_NEGOTIATED_AUTH_PROTOCOL_INTERFACE
* 0@-
* PAP cannot handle event %d
send_pap_authentication_request
netTupleGet error
* you are authenticated
* send_pap_authentication_nak
you are not authenticated
* %ld
PAP:Auth Info Interface:Invalid parameters
NULL Framework Reference
* 0@-
* PAP:Auth Info Interface:Invalid Parameters
PPP_IPCP
Local:Negotiation Required,Not Negotiable:002D0F01
IPCP
* mpLcpInterfaces.c
lcpMpOptionsGet
NULL Framework reference
AUTH_INFO_INTERFACE
AUTH_INFO_INTERFACE is not available
* mpFraming_disableAuthOnBundle
TRUE
* p@-
(0@-
V	(p@-
* H1
V	(RAS_UTILS_ERROR: (RAS_getNumOfPools) --> %x
Total number of Address Pools in the System: %d
* RAS_UTILS_ERROR: (RAS_getMaxPoolId) --> %x
Maximum Address Pool ID in the System: %d
* RAS_UTILS_ERROR: (RAS_getAddrPoolSize) --> %x
Address Pool (#%d) contains --> %d IP addresses
* RAS_UTILS_ERROR: (RAS_getAddrPoolPrefix) --> %x
Address Pool (#%d) prefix length: %d
* RAS_UTILS_ERROR: (RAS_getAddrPoolRouterId) --> %x
Address Pool (#%d) Router-ID: %s
* RAS_UTILS_ERROR: (RAS_getAddrPoolFirstIp) --> %x
Address Pool (#%d) First IP addr: %s
* RAS_UTILS_ERROR: (RAS_getAddrPoolNumFreeAddrs) --> %x
Address Pool (#%d) Number of Free IP Addresses: %d
* YES
RAS_UTILS_ERROR: (RAS_getAddrPoolPMPmode) --> %x
Address Pool #%d support PMP: %s
* RAS_UTILS_ERROR: (RAS_getAddrPoolexptDrv) --> %x
Address Pool #%d Export Driver PMP: 0x%x
* RAS_UTILS_ERROR: (RAS_setAddrPoolexptDrv) --> %x
* RAS_UTILS_ERROR: (RAS_getAddrPoolNumDrvs) --> %x
Address Pool #%d contains %d drivers
V	(|
All addresses are available in this address pool.
can not allocate memory for retrieving IP addresses!
RAS_UTILS_ERROR: (RASIOCGETGETFREEADDRS) --> %x
		IP: %s
V	(%ld
* p@-
* p@-
* p@-
Back off start failed: state = %d
ipcp_this_layer_up: no compression option in rx list 
ipcp_this_layer_up: Copy VJC Option failed 
ipcp_this_layer_up: Copy HC Option failed 
PPP_IP_INTERFACE
pppIpStateMachineFunction.c
ipcp_this_layer_up
PPP_IP_INTERFACE get error
IPCP failed in shutdown HC interface: hcShutdown ()
PPP_IPV6CP
PPP_IP_DNS_INTERFACE
PPP_IP_DNS_INTERFACE get error
failed to get PPP_IP_DNS_INTERFACE:stack 0x%x
pfwInterfaceIdGet failed for PPP_IP_DNS_INTERFACE:stack 0x%x
+ p@-
IPCP tlu failed to get VJC componentObj
IPCP tlu failed to add VJC pluginObj
PPP_VJC_INTERFACE
PPP_VJC_INTERFACE get error
PPP_VJC_INTERFACE get failed
VJC Interface Id Get failed 
+ PPP_IPCP
%s: Invalid access to Header Compression 
%s failed to get HC component Obj 
HC component Addition failed for %s 
PPP_HC_INTERFACE
%s failed to get PPP_HC_INTERFACE interface id 
%s failed to get HC interface state pair 
%s failed in intializing HC interface: hcInitialize () 
+ 0@-
pppVsEndComponentCreate: NULL framework pointer
pppEndInit - Unable to allocate memory of size %d                  bytes
INTERFACE_LAYER
PPP_VS_END
pppVsEndComponentCreate: component could not be added to                  the framework
end_pollRxQueueSize
PPP_INTERFACE_UP_EVENT
PPP_INTERFACE_DOWN_EVENT
PPP_SUB_LAYER_TX_BLOCKED
PPP_SUB_LAYER_TX_UNBLOCKED
pppVsEndComponentCreate: could not create component
+ pppVsEndComponentDelete: NULL framework pointer
+ PPP_IP_INTERFACE
PPP_IP_ROUTES_INTERFACE
PPP_IP_DNS_INTERFACE
COMPONENT_ACCEPTABLE_PROTOCOLS_INTERFACE
PPP_LINK_ID_INTERFACE
PPP_IF_IFX_TABLE_INTERFACE
PPP_IF_STACK_TABLE_INTERFACE
(+ @)+ 
)+ D*+ $
"+ P
!+ h
+ |#+ 
PPP_VS_END: no PPP_INTERFACE_UP_EVENT
PPP_VS_END: no PPP_INTERFACE_DOWN_EVENT
"+ (
#+ h
+ ppp
+ Error: pppVsEndSend was called. Freeing packet
ppp END Driver.
(0@-
ppp%d
+ p@-
PPP_VS_END:PPP_SUB_LAYER_TX_BLOCKED when already blocked
p"+ PPP_VS_END:PPP_SUB_LAYER_TX_UNBLOCKED is already unblocked
+ PPP_LINK_STATUS_ENTRY_INTERFACE
+ `'+ -q add -interface -host %s %s
-q add %s %s netmask 0x%lx
t*+ -q delete %s netmask 0x%lx
*+ PPP_VS_END: Set Interface Mask ifName %s Mask %lx %s
FAILED
++ L++ 
pppOutput: invalid ifp pointer
,+ 0-+ 
pppVjcInit Unable to allocate memory
NETWORK_LAYER
pppVjcInit VJC component could not be added
8.+ 
.+ H.+ 
1+ $4+ 
0+ D1+ 
/+ L.+ 8
H.+ PPP_VJC_INTERFACE
COMPONENT_ACCEPTABLE_PROTOCOLS_INTERFACE
/+ 86+ 
/+ d6+ P6+ PPP_IF_IFX_TABLE_INTERFACE
0+ 0@-
pppInterfaceLayerInit Unable to allocate memory
INTERFACE_LAYER
pppInterfaceLayerInit Interface layer could not be added to the		 stack
9+ p:+ 
:+ (8+ 8
@+ 0@-
@+ pppInterfaceLayer.c
stackDelete
Interface Layer Null component
D:+ P:+ 0:+ 
LCP_PACKET_SEND_INTERFACE
interfaceLayerStackAdd
Null component
;+ 0:+ 
;+ NULL interface layer state
COMPONENT_ACCEPTABLE_PROTOCOLS_INTERFACE
componentStackAddDone
interface could not be found
interface could not find
PPP: could not allocate memory for new protocol Item
=+ 0:+ 8=+ T=+ 0@-
pppNetworkLayerInit Unable to allocate memory
NETWORK_LAYER
pppNetworkLayerInit Network layer could not be added to the                 stack
B+ $F+ DC+ 
A+ 8
G+ $J+ 0@-
K+ 0@-
PPP: Unknown Protocol 0x%x rejected
D+ LCP_PACKET_SEND_INTERFACE
pppNetworkLayer.c
networkLayerStackAdd
Null component
E+ NULL network layer state
COMPONENT_ACCEPTABLE_PROTOCOLS_INTERFACE
componentStackAddDone
interface could not be found
interface could not find
PPP: could not allocate memory for new protocol Item
F+ 8G+  G+ 
E+ XG+ tG+ 0@-
(0@-
LP+ 
P+ DR+ tP+ 
P+ DR+ 
pppAdapterLayer.c
pppAdapterLayerInit
Unable to allocate memory
ADAPTER_LAYER
Adapter layer could not be added to the stack
Y+ D[+ 
Y+ 8
pppFramingLayer.c
pppFramingLayerInit
Unable to allocate memory
FRAMING_LAYER
Framing layer could not be added to the stack
[+ t[+ L[+ `[+ 
[+ 8
sio_peerType
sio_maxSendQSize
sio_baudRate
sio_channelNum
SIO_ADAPTER
ADAPTER_LAYER
sioAdpterCreate: Could not add SIO ADAPTER component
sioAdptrCreate - Parameter %s could not be added
h]+ Dh+ 
o+ t]+ 
]+ 8d
]+ D
h]+ 
SIO: MUST have a valid NetPoolId; See pfwCreate()
COLLECT_PPP_ATTRIBUTES_EVENT
Sio Adapter: Channel Number %d in use by Stack ID %d
sioAdapter: Failed to install SIO_CALLBACK_GET_TX_CHAR 
sioAdapter: Failed to install SIO_CALLBACK_PUT_RCV_CHAR 
sioAdapter: Failed to set baud rate %d
sioAdapter: Failed to set Interrupt mode 
LCP_OPEN_EVENT
LCP_DOWN_EVENT
LCP_CLOSE_EVENT
LCP_UP_EVENT
PPP_SUB_LAYER_TX_BLOCKED
SIO_ADAPTER: Failed to get PPP_SUB_LAYER_TX_BLOCKED event
PPP_SUB_LAYER_TX_UNBLOCKED
SIO_ADAPTER: Failed to get PPP_SUB_LAYER_TX_UNBLOCKED event
PPP_LINK_STATUS_ENTRY_INTERFACE
PPP_IF_IFX_TABLE_INTERFACE
a+ tr+ 4b+ pb+ 
b+ 8z+ 
c+  c+ \c+ xc+ 
l+ tr+ CLIENT
y+ PPP_MODEM_INTERFACE
ADAPTER_COMPONENT_STATISTICS_INTERFACE
PHY_PORT_INTERFACE
Po+ do+ D
o+ p
+ modem: too many characters 
CLIENTSERVER
sioAdptr:Failed to get receive buffer for channel Id %d
sioAdptrReceiveOctet:Failed to get next receive mBlk for Stack Id %d
sioAdptrReceiveOctet: dropping tiny frame (%d bytes)
sioAdptrReceiveOctet: pfwDataJobAdd failed.
xq+ 
y+ Dr+ 0@-
i+ 0@-
0|+ 0@-
0|+ 0@-
0|+ NT_SERVER
WIN_SERVER
NT_CLIENT
WIN_CLIENT
REGULAR
MODEM
$}+ 0}+ <}+ H}+ T}+ \}+ p@-
modem flags=0x%x 
+ 0@-
pppAsyncFramingInit - Unable to allocate memory of size %d 		 bytes
ASYNC_FRAMING
FRAMING_LAYER
pppAsyncInit  Async Driver cannot be added to the framework
+ Async Framing:MUST have a valid NetPoolId;See pfwCreate()
+ COLLECT_PPP_ATTRIBUTES_EVENT
LCP_UP_EVENT
PPP_LINK_RESET_EVENT
PPP_LINK_STATUS_ENTRY_INTERFACE
PPP_LINK_STATUS_COUNTER_INCREMENT_INTERFACE
PPP_IF_IFX_TABLE_INTERFACE
+ 0@-
AsyncFraming:Failed to get encoded frame for Stack 0x%x
+ AsyncFraming:Failed to get another mBlk for 				encoded frame:Stack 0x%x
AsyncFraming:Failed to get another mBlk for encoded 			frame:Stack 0x%x
AsyncFraming:Failed to get decoded frame for StackObj 0x%x
PPP: flag after control escape.
PPP: Error: Flag in mid-frame.
PPP: Error: Consecutive control escape sequences found in packet on Async port
AsyncFraming:Failed to get another mBlk for decoded frame:Stack 0x%x
PPP: Error: frame ends with non-FLAG.
pppOE_vendorInfo
pppOE_acName
pppOE_svcName
pppOE_minDiscTimeout
pppOE_discRetries
pppOE_connectionMode
PPP_O_ETHERNET
FRAMING_LAYER
pppOEthernetInit: Couldn't add PPPOE component to pfw 0x%x
pppOEthernetInit - Parameter %s could not be added
PPPOE: Illegal mode:%x;Must be either HOST(0x%x) OR AC(0x%x)
pppOEthernetInit - could not allocate Service Name MAP
PPP_SUB_LAYER_DEAD_EVENT
+ ld
+ ADAPTER_COMPONENT_STATISTICS_INTERFACE
PHY_PORT_INTERFACE
FRAMING_COMPONENT_STACK_RESOLVE_INTERFACE
PPPOE: Could not Register FRAMING_STACK_RESOLVE_INTERFACE
+ PPPOE: Null profile object 
PPPOE: Null framework object 
PPPOE: Null plugin object 
0x%x
PPPOE: Stack add failed for service Name %s
WindNetPPPoEAC
PPPOE: Too many services; Max allowed = %d
+ %s
PPPOE: No such service: %s
+ PPPOE: AC SYSTEM ERROR: %s
PPPOE: must have a valid netPoolId; see pfwCreate()
COLLECT_PPP_ATTRIBUTES_EVENT
PPPOE:Configured in PPPOE_HOST_MODE: Bad Connection mode 0x%x
PPPOE:Configured in PPPOE_AC_MODE: Bad Connection mode 0x%x
ADAPTER_DESTINATION_AND_PROTOCOL_SET_INTERFACE
ADAPTER_INFO_GET_INTERFACE
LCP_OPEN_EVENT
LCP_UP_EVENT
LCP_DOWN_EVENT
PPP_IF_IFX_TABLE_INTERFACE
+ pd
(pppOE: Unexpected AC name %s
+ pd
(0@-
Stack ID = %d 
Stack state = %s 
SESSION
DISCOVERY
Session ID = %d = 0x%x 
Service Name = %s
AC Name = %s
HOST Ethenet Addr. = %s
AC Ethernet Addr. = %s
PADI Retries Remaining = %d
PADR Retries Remaining = %d
+ %d
+ p@-
pppOE: Failed to start timer for stack ID %d
PPPOE: Null plugin object in state 0x%x 
0123456789abcdef
+ pppOE_ver     = %d
pppOE_type    = %d
pppOE_code    = %d
pppOE_session = %d
pppOE_length  = %d
+ pppOE: Tag, Len, Val: %s, 
PPPOE_TAG_SVC_NAME
%d, 
PPPOE_TAG_AC_NAME
pppOE:Tag, Len, Val: %s, 
PPPOE_TAG_AC_COOKIE
0x%x
PPPOE_TAG_HOST_UNIQ
pppOE: Tag, Len, Val: %s,  
PPPOE_TAG_EOL
+ p@-
Session ID	 Stack ID
----------	 ---------
%8d	 %8d
+ Service Name 	 Stack ID
-------------	 -------------
%12s	 0x%x
PFWSTACK: Null Component Object 
PFWSTACK: Null Stack Object 
+ muxSvcType
muxL2SvcType
muxDevUnit
muxDevName
muAdapterCreate: Framework is NULL
muxAptrCreate: Could not malloc memory for MUX ADAPTER component
muxAptrCreate: Could not create semaphore for MUX ADAPTER component
MUX_ADAPTER
ADAPTER_LAYER
muxAdapterCreate: Could not add MUX ADAPTER component
muxAdapterCreate - Parameter %s could not be added
muxAdapterCreate: Could not malloc memory for bindInfo
ADAPTER_DESTINATION_AND_PROTOCOL_SET_INTERFACE
MUX ADAPTER: Failed to register %s 
ADAPTER_INFO_GET_INTERFACE
MUX_ADAPTER: No protocols to bind
COLLECT_PPP_ATTRIBUTES_EVENT
PPP_SUB_LAYER_TX_BLOCKED
MUX_ADAPTER: Failed to get PPP_SUB_LAYER_TX_BLOCKED event
PPP_SUB_LAYER_TX_UNBLOCKED
MUX_ADAPTER: Failed to get PPP_SUB_LAYER_TX_UNBLOCKED event
FRAMING_COMPONENT_STACK_RESOLVE_INTERFACE
muxAdptrStackAdd: No more Binds
MUX_ADPTR: Slot < 0
MUX_ADPTR: Protocol 0x%x already bound to Device %s,		Unit %d, on stackObj %p and did not supply		FRAMING_COMPONENT_STACK_RESOLVE_INTERFACE
-0x%lx
MUX_ADPTR: muxL2SvcType=0x%x cannot bind to NPT driver			%s%d
MUX_ADAPTER: Failed to bind protocol 0x%x
PPP_IF_IFX_TABLE_INTERFACE
%29s[%d] = 0x%x bound to Dev %s:Unit %u
muxSvc
+ MUX_ADAPTER: Failed to lock state for blocked stack %p
+ INFO: Device: %s Unit: %d Msg: %s
WARN: Device: %s Unit: %d Msg: %s
RESET: Device: %s Unit: %d Msg: %s
UP: Device: %s Unit: %d Msg: %s
DOWN: Device: %s Unit: %d Msg: %s
FLAGS CHANGED: Device: %s Unit: %d Msg: %s
MESSAGE FROM Device: %s Unit: %d Msg: %s
0x%x:
+ 0x%x
PHY_PORT_INTERFACE
(m2pppLibInit failed due to semaphore creation failure
m2pppLibInit was called but m2pppLibSem was not NULL
+ Failure to acquire #m2pppLibSem semaphore
malloc failure in m2pppInterfaceRegister; ifIndex = %u
semGive failed; #m2pppLibSem is likely invalid
+ a null stackObj is paired to input ifIndex = %u
+ ifIndex = %u; next node's key = %u, stackObj = NULL
+ ifIndex = %u; previous node's key = %u, stackObj = NULL
+ Tree memory deallocation failed
semDelete failed; m2pppLibSem is likely invalid
m2pppLinkGroupInit: Failed to create m2pppLinkGroupInterfacesTable 
PPP_LINK_STATUS_ENTRY_INTERFACE
m2LinkGroup: Could not get linkStatus interface ID
m2pppLinkGroup.c
m2pppLinkGroupInit
No PPP_LINK_STATUS_ENTRY_INTERFACE!
PPP_LINK_CONFIG_ENTRY_INTERFACE
m2LinkGroup: Could not get linkConfig interface ID
No PPP_LINK_CONFIG_ENTRY_INTERFACE!
+ 0@-
(p@-
m2pppIpcpGroupInit: Failed to create m2pppIpcpGroupInterfacesTable 
PPP_IPCP_MIB_INTERFACE
m2IpcpGroup: Could not get ipcpEntry MIB interface ID
m2pppIpcpGroup.c
m2pppIpcpGroupInit
No PPP_IPCP_MIB_INTERFACE!
, 0@-
(p@-
m2pppSecurityConfigInit: Failed to create m2pppSecurityConfigInterfacesTable 
PPP_SECURITY_CONFIG_ENTRY_INTERFACE
m2LinkGroup: Could not get Security Config interface ID
m2pppSecurityConfig.c
m2pppSecurityConfigInit
No PPP_SECURITY_CONFIG_ENTRY_INTERFACE !
, 0@-
m2pppSecuritySecretsLibInit failed; semMCreate failure
m2pppSecurityLibInit failed;  pppSecretsSem was not NULL
, Failure to acquire pppSecretsSem semaphore
semGive failed; pppSecretsSem is likely invalid
inconsistency: only secondary tree node will be deleted
1, t
, inconsistency: only primary tree node will be deleted
1, t
, malloc failure in m2pppSecretsEntrySet
inconsistency: only secondary node was inserted
1, t
1, t
, malloc failure in m2pppSecretsEntryAgentSet
inconsistency: secondary entry not visible
we will leave altering nothing
inconsistency: invisible primary node
SERIOUS INCONSISTENCY
recovery was not attempted
corresponding secondary node was removed
inconsistency; invisible improper primary node
recovery will not be attempted
inserted improper primary node is invisible
1, t
1, p
1, t
1, t
1, t
+, t
1, t
, Memory deallocation failed; data status indeterminate
semDelete failed; pppSecretsSem is likely invalid
(|1, 
((1, 
/, t
/, 0@-
secretsDataNodeNicePrint <nodep> input was NULL
%11u 
     PAP 
    CHAP 
unrecongnizable protocol
%28.28s
\2, 
2, The pppSecretsDatabase is empty
PAP identity/password and CHAP challenge/secret 
local to remote pairs:
 * An asterisk following a string indicates 
truncation after 28 characters
%11.11s%9.9s%29.29s%30.30s
link
protocol
identity
secret
----
--------
------
--- End of m2pppSecurityLocalSecretsShow printout
3, ,4, H4, x4, 
4, t
, remote to local pairs:
--- End of m2pppSecurityPeerSecretsShow printout
6, H4, x4, 
6, t
, PPP: %s: Illegal transition; state %d, Event %d, stack 0x%x
?, $D, 
send_lcp_packet: Unable to copy last transmit lcp packet
send config Req: timerStart failed; state = %d
send Termination Req: timerStart failed; state = %d
send Time Remaining: timerStart failed; state = %d
@, |
, <A, xN, tA, LCP: failed to copy last lcp request received packet
send Echo Request: timerStart failed; state = %d
(lcp_code_zero_received
P, p@-
LCP:Illegal code Received for stack: 0x%x
tQ, LCP: received bad Configure Request
LCP: failed to copy initial lcp request received packet
$S, LS, LCP:Config ACK received:bad length: expected %d: got %d:	    stack 0x%x
LCP:Config ACK:ID = %d doesn't echo config request:stack 0x%x
generate TO- event: timerStart failed; state = %d
, <Y, 
LCP:Bad Discard Request Received: stack 0x%x
@], LCP: ERROR Id Packet too large(%d): stack 0x%x
p^, 
PPP: Out of Memory for New Option 
\`, 
PPP_IPV6CP
Xb, 
PPP: Illegal Option Length 
dh, p@-
PPP: Copy Option Length too small
k, 0@-
<option: %d, 
length: %d
, data: 0x%04x
, data: 0x%08lx
, data: 0x
%02x
o, (o, 0o, 4o, LCP
PPP: Getting %s name from %s component failed
IPCP
PPP:Adding %s option to %s failed
Dp, Hp, xp, 
p, 0@-
p, PPP: Out of Memory for New Alternate Option 
PPP: Out of Memory for New Option 
tr, 
r, PPP: No matching primary option for Alternate Option 
s, 0@-
p, PPP: Out of Memory for Alternate Option 
PPP: Out of Memory for New Range Option 
u, PPP: Tried to delete option not present 
Dw, 
PPP: Out of Memory for Copy Option 
x, PPP: Illegal Option 
(z, p@-
PPP: Out of Memory for New Option 
PPP_IPV6CP
|{, 
{, option entry is NULL
<option: %d, 
length: %d
, data: 0x%04x
, data: 0x%08lx
, data: 0x
%02x
nak_option = %d>
Alternates: 
data: 0x%04x
data: 0x%08lx
data: 0x
Range values: 
Min: %d Max: %d Step = %d
Min: %ld Max: %ld Step: %ld
8~, P~, `~, l~, |~, 
%02x%02x%02x%02x%02x%02x
%02x%02x%02x%02x%02x
%02x%02x%02x%02x
%02x%02x%02x
%02x%02x
%02x
Remote
Local
, %d
Auto
%s%s
Alternate
Range
%s,%s,%s,%s,%s,%s
%s,%s,%s,%s,%s,%s,%s
Negotia
Magic Number
Unknown Configuration String %s
, Illegal Number of PPP Options %02x Entered %s!!!
, p@-
, p@-
(String
IPV6
pppConfg.c : Invalid class for the EID option
, LAP
%04x
RAS-AMM
%01x
, Illegal Number of PPP Options %02x Entered %s!!!
, Illegal List
Illegal Element to Add
, Illegal Element to Delete
, Illegal List Element
, Illegal Current List Element
, 0@-
Back off start failed: state = %d
(p@-
!	(dY
	(8v
T	(\5
T	(\5
T	(T5
(`/- 
,0- 
3- HL
(`4- 
($&	(
T	(D
"- |
 - 4 - 
 - L - d - < - D - T - x - 
(l$	(
T	(T5
( =- 
	(l'- 
l5- #'
D$	(
T	(D
T	(D
N=1 D=|
~componentDate
~componentName
wpaPSK4
wpaPSK3
wpaPSK2
wpaPSK1
wfMode4
wfMode3
wfMode2
wfMode1
wepkeylen4
wepkeylen3
wepkeylen2
wepkeylen1
wepkey42
wepkey41
wepkey32
wepkey31
wepkey22
wepkey21
wepkey12
wepkey11
wepAuth4
wepAuth3
wepAuth2
wepAuth1
version
userPwd
userNameIndex
tmnlSubMask
tmnlIPAddress
tmnlGWIPAddress
timeZoneOffset
tftpServerFQDN
tftpConfProtocol
stunUse
stunServerPort
stunServer
ssidConnectedTo
ssid4
ssid3
ssid2
ssid1
sipUserName
sipUseOutbandProxy
sipUseNullPacket
sipUseDNS
sipRegisterUsage
sipRegisterPort
sipRegisterName
sipRegisterIPAddress
sipProxyPort
sipProxyName
sipProxyIPAddress
sipPort
sipPassword
sipAuthString
serverIP
selected
rtpPort
rtpPacketSize
resetToDefault
regDuration
rebootcmd
productID
model
macAddress
localIPMask
localIPAddrs
index4
index3
index2
index1
gatewayIPAddr
g729a
g726
g711u
g711a
filename4_old
filename4_new
filename3_old
filename3_new
filename2_old
filename2_new
filename1_old
filename1_new
file_active
enterCode
dstFlag
drmfTxMode
dnsQueryType
dnsIPAddressSrc
dnsIPAddress2
dnsIPAddress1
displayName
dhcp_mode
delFile4
delFile3
delFile2
delFile1
currentStatus
checked
autoscanInter
autoscanFlag
adminPwd
SELECTED
ProvConfProtocol
CHECKED
publicWMB
webserver
R- L
R- l
(XS- 
M- ,
R- getDELETEfile1
getDELETEfile2
getDELETEfile3
getDELETEfile4
get RENAME file1
get RENAME file2
get RENAME file3
get RENAME file4
DV- l
W- XX- 
X- $Y- 
Z- X[- 
]- ,^- 
^- <_- 
a- Lb- 
d- 8e- 
f- lg- 
i- 0j- 
j- @k- 
k- tl- 0m- 
n- do- 
q- ,r- 
r- Hs- 
v- (w- 
w- 8x- 
x- Hy- 
y- Xz- 
z- h{- D|- 
~- h
pV- 
V- \
8W- x
- TW- hW- x
W- \
X- DX- 
X- x
X- x
Y- x
PY- hY- \
- xY- 
Z- \
- $Z- 8Z- XZ- 
Z- \
[- D[- 
[- \
H\- d\- \
- p\- 
]- (]- \
- 4]- H]- h]- 
]- x
^- x
X^- x
- t^- 
^- x
^- x
_- x
h_- 
_- \
,`- H`- \
- T`- h`- 
a- \
a- ,a- La- ta- 
a- \
b- 8b- 
xb- x
b- x
b- Pc- \
- \c- pc- 
S- d
S- h
S- l
S- p
T	( 
d- \
d- (d- Hd- xd- 
d- \
e- $e- 
de- te- \
(f- @f- \
- Pf- df- 
f- \
g- (g- Xg- 
g- \
Dh- th- \
- 0	
(i- @i- \
- Pi- di- 
i- x
j- x
\j- x
- xj- 
j- x
j- x
k- x
lk- x
k- x
l- \
l- 0l- Pl- `l- 
l- \
\m- tm- \
n- 0n- \
- <n- Pn- pn- 
n- \
o- ,o- Po- 
o- \
<p- Tp- \
- dp- xp- 
q- \
q- $q- Dq- 
S- t
("4	(
(64	(`
q- x
r- x
Xr- x
- tr- x
r- \
s- 4s- 
ts- x
s- x
t- \
-  t- 4t- Tt- xt- 
t- x
t- x
@u- x
- \u- pu- x
u- x
v- $v- \
- 4v- Hv- pv- 
v- x
v- x
Tw- x
- pw- 
w- x
w- x
x- x
dx- x
x- x
x- x
y- x
ty- x
y- x
y- x
z- ,z- x
z- x
z- x
{- x
- ({- <{- x
{- \
|- (|- 
p|- 
|- \
4}- x
- P}- d}- x
}- x
}- x
D~- x
- `~- t~- x
~- \
( T- 
WindManage Web Server Error Report:<HR>
- <HR>please mail problems to ???
- Out of memory, can not handle request
RPM configuration error
Access denied
IO error, transfer interrupted
File not found
URL parsing error
No RPM for this combination of URL and method
Internal httpd failure / program error
/user/webmain.html
administrator
admin
user
/admin/*
Everywhere
/adminprivate/*
/flash/script/*
/fs/*
/user/*
/userprivate/*
/admin/
admin/
/adminprivate/
adminprivate/
/flash/script/
flash/script/
/fs/
/user/
user/
/userprivate/
userprivate/
W/ ,
-  s/ 
f/ \
invalid component
 Quit
- wmbComponentResourceLoad: no backplane
wmbComponentResourceLoad: no component
wmbComponentResourceLoad: no entries
wmbComponentResourceLoad: no database
- wmbComponentTableLoad: no backplane
wmbComponentTableLoad: no component
wmbComponentTableLoad: no table entries
wmbComponentTableLoad: no database
- $0
listener
- no name
no backplane
no backplane name
wmbComponentSend: invalid component
wmbComponentSend: no data
- 3;
	(no memory
- component not found
- publicWMB
- wmbBackplaneRegistration: invalid backplane
 Quit
- wmbBackplaneCreate: no memory
tBackplane
temporary
- wmbBackplaneLookup: null pointer
wmbBackplaneLookup: no backplane
- 00
wmbDbEntryNew: invalid DB
wmbDbEntryNew: null entry pointer
wmbDbEntryNew: no memory
wmbDBConstruct: NULL db ptr
wmbDBConstruct: no memory
- wmbDBDestruct: invalid db
wmbDbEntryTempGet: no return pointer
wmbDbEntryTempGet: bad backplane
wmbDbEntryTempGet: no db
- null return pointer
no memory
- wmbDBAdd: failed
- invalid component
invalid backplane
- no backplane
no backplane db
SESSION
Entry: 
/%s/
(calculated)
Entry: %-18s Type: %-12s Value: %s
- 0@-
wmbDbTableNew: invalid DB
wmbDbTableNew: null table pointer
wmbDbTableNew: no memory
- wmbDBTableAdd: failed
- Table: 
Table: %4d IndexCnt: %-12s EntryCnt: %4d
- 0@-
- invalid command name
(null input
 Quit
wmbRequest: QUIT requested
not valid text message
wmbRequest: invalid request
wmbRequest: invalid type
wmbRequest: not handled
- wmbShareCreate: NULL pointer
wmbShareCreate: invalid type
Assertion failed: ! wmMemBlockBad(pBlock), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbLib.c, line 656
- wmbShareFree: invalid backplane
bad object
no memory
- 3;
wmbObjectOid: null ptr
invalid object
wmbObjectOid: bad entry
wmmOidLoad: bad entry
Assertion failed: NULL != ((WMB_OBJECT_T *) prior), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 868
- Assertion failed: NULL != ((WMB_OBJECT_T *) first), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 893
Assertion failed: NULL != ((WMB_OBJECT_T *) next), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 919
- Assertion failed: NULL != ((WMB_OBJECT_T *) added), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 977
Assertion failed: NULL != ((WMB_OBJECT_T *) added), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 978
Assertion failed: NULL != ((WMB_OBJECT_T *) matchOID), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 979
- wmbObjectAppend: no object
Assertion failed: NULL != ((WMB_OBJECT_T *) prior), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 1018
Assertion failed: NULL != ((WMB_OBJECT_T *) added), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 1019
Assertion failed: NULL != ((WMB_OBJECT_T *) prior), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 1033
Assertion failed: NULL != ((WMB_OBJECT_T *) added), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 1034
- wmbObjectInit: name buffer failed
wmbObjectInit: OID conversion failed
- variableGet: bad data
variableGet: NULL entry
- variableSet: bad data
variableSet: NULL entry
- wmbObjectVariable: not handled
wmbObjectResolver: invalid object
buffer overflow
invalid component
no database!
WindMark Not Found
Assertion failed: NULL != ((WMB_OBJECT_T *) obj), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 1701
Assertion failed: NULL != ((WMB_OBJECT_T *) obj), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 1703
Assertion failed: NULL != ((WMB_OBJECT_T *) obj), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 1704
Assertion failed: NULL != ((WMB_OBJECT_T *) obj), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 1706
Assertion failed: NULL != ((WMB_OBJECT_T *) obj), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbObjectLib.c, line 1707
wmbObjectResolver: OID conversion failed
not handled
wmbObjectGo: no handler
- no validation string
- enums are read only
wmbObjectDelete: invalid object
wmbObjectImport: no memory
. wmObjectExport
echo: bad object
echo: no string
. wmbObjectMake
. wmbObjectPermission: no db entry!
access denied
- 3;
wmbObjectCookieSet: overwriting cookie!
. wmbObjectBackup: can't make buffer
wmbObjectUndo: no db entry
wmbObjectUndo: no buffer
. wmbObjectRedo: overwriting cookie
. wmbObjectSavedGet: no buffer
wmbPortfolioStart: corrupt anchor
no memory
	(wmbTMNewPCB: no memory
(wmbPortfolioFromCIDGet: Portfolio not found
. wmbPortfolioFromFileNameGet
(wmbPortfolioGet: Not initialized
wmbPortfolioGet
wmbPortfolioHandler: Bad Command
wmbPortfolioHandler: Unknown ID
h!. 0@-
x#. wmbMakeXMLFromPCB
<?xml version="1.0" encoding="UTF-8"?>
<!DOCTYPE PORTFOLIO SYSTEM "">
PORTFOLIO
TYPE
FILE
FLAGS
. wmbMakeXMLFromRequest
REQUEST
BLADE
EXTENSION
. wmbTMNewPCB: no memory
,#. ,#. ,#. 
". ,#. 
". ,#. ,#. 
P!. 
. wmbPortfolioDocREQHandler
$. D$. 
p$. 
\#. 
wmbPortfolioGetRemote
WMB_PORTFOLIO_wmbPortfolioRequest
P%. h%. 
WMB_PORTFOLIO_wmbPortfolioDeregister
0'. WMB_PORTFOLIO_wmbPortfolioRegister
'. p@-
P%. 
	(0@-
	(wmbSessionCreate: entery 1 
no memory
wmbSessionCreate: entery 2 
wmbSessionCreate: entery 3 
 *. wmbSessionDestroy: invalid session
T+. 3
threads
stderr
debug
logfile
syslog
message
client
memory
uptime
name
(name: not handled
not writable!
wmbSystemHandler: not handled
/. D0. 
/. $/. 
	(0@-
	(wmbTMNewTCB: no memory
1. P
	(wmbTMTestTransactionProcess: Handler NULL
2. wmbTMObjectUnlock: bad TID
wmbTMObjectLock: bad TID
wmbTMObjectLock: Deadlock occurred
4. wmbTMObjectPermissionCheck: bad TID
\6. 
wmbTMAddObject: bad TID
wmbTMAddObject: bad session
wmbTMAddObject: bad backplane
h7. 
Assertion failed: NULL != ((WMB_OBJECT_T *) priorObj), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbTransactionCore.c, line 541
Assertion failed: NULL != ((WMB_OBJECT_T *) nextObj), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbTransactionCore.c, line 549
Assertion failed: NULL != ((WMB_OBJECT_T *) nextObj), file Z:/wfplt/src/protocol/webserver/pubsrc/backplane/wmbTransactionCore.c, line 551
h7. 
(9. 
9. D:. wmbTMProcessInput: bad Tcb
wmbTMProcessInput: bad state
wmbTMProcessInput: bad input
=. T
wmbTMBeginTransaction: bad Tcb
TransactionID: %l - Begin Transaction
wmbTMTestTransactionProcess: bad TID
TransactionID: %l - Test Transaction
A. (A. 
wmbTMTestTransaction: bad TID
C. PA. wmbTMCommitTransactionProcess: bad TID
TransactionID: %l - Commit Transaction
wmbTMCommitTransaction: bad TID
C. PE. 
C. wmbTMGetRequestProcess: bad TID
TransactionID: %l - Get Request
wmbTMGetRequest: bad TID
@G.  F. wmbTMAbortRequest: bad Tcb
TransactionID: %l - Abort Request
G. wmbTMRequestComplete: bad Tcb
TransactionID: %l - Request Complete
`H. @H. wmbTMTestAborted: bad Tcb
TransactionID: %l - Transaction Aborted during Test
wmbTMCommitAborted: bad Tcb
TransactionID: %l - Transaction Aborted during Commit
<J. XJ. 
wmbTMTransactionCompleteProcess: bad Tcb
K. TransactionID: %l - Transaction Complete
K. HL. 
TransactionID: %l - Transaction Error : %l
wmbTMError
XM. 
M. TransactionID: %l - Transaction Timeout
wmbTransactionCreate: entery 1, backplane:%d
wmbTransactionCreate: invalid backplane
wmbTransactionCreate: entery 2 
wmbTransactionCreate: entery 3 
no memory
wmbTransactionCreate: entery 4 
P. DP. hP. 
P. wmbTransactionBegin: bad tid
\R. 
S. wmbTransactionObjectAdd
`U. 0@-
`U. 3;
wmbTransactionLockDelete : Bad TID
TV. wmbTransactionLockAdd : Bad TID
HW. 
Input parameter is NULL!
Partition too small for admin data!
Y. 0Y. memPoolCleanup: NULL poolID
memPoolCleanup: pool corrupted!
Z. memPoolCheck: null poolID
memPoolCheck: descriptor table invalid!
memPoolCheck: end-of-pool overrun!
memPoolCheck: bad block type
[. D[. h[. memPoolCleanup: error during cleanup
\. memPoolAvail: no valid pool
\. memPoolAlloc: no valid pool
memPoolAlloc: wmosSemTake failed
memPoolAlloc: insufficient memory
Assertion failed: mcbTmp->ulBlockSize > 0, file Z:/wfplt/src/protocol/webserver/pubsrc/common/memPoolLib.c, line 557
Assertion failed: mcbBestFit->ulBlockSize >= ulBytes, file Z:/wfplt/src/protocol/webserver/pubsrc/common/memPoolLib.c, line 569
^.  ^. D^. h^. 
^. memPoolFree: no valid pool
memPoolFree: can't find memory
memPoolFree: invalid or already freed!
memPoolFree: block not found!
a. 4a. \a. 
no system access info
no access data
c.  
(0@-
lclBufMalloc: no pool memory
lclBufMalloc: no memory
wmBufferAssign: bad buffer
$j. 
lclResize: no new data!
m. wmBufferUpdate: bad buffer
wmBufferUpdate: null data pointer
<o. Xo. wmBufferAppend: invalid buffer
wmBufferAppend: no data
wmBufferAppend: no dest
xr. 
r. wmBufferCreate: no memory
wmBufferDelete: invalid buffer
root
full
$w. ,w. 3;
bad buffer
no ptr
hy. ty. 3;
access
ticks
time
void
absolute
list
enumerate
mac address
unsigned 64-bit int
unsigned long
unsigned short
unsigned char
unsigned integer
64-bit int
long
short
char
integer
ip address (version 6)
ip address
string
invalid
T|. t
(no return pointer
wmConvertStrSize()
~. d~. H~. 
~. t~. 
}. (unknown)
~. p@-
(p@-
wmConvertStrToInt: no data
wmConvertStrToInt: null ptr
wmConvertStrToInt: invalid data
. lclNumberToStrSize: null ptr
wmConvertNumberToStr()
(wmConvertStrToOid: no data
wmConvertStrToOid: null destination buffer
wmConvertStrToOid: NULL pBytesUsed not allowed
wmConvertStrToOid()
wmConvertStrToOid: buffer too small
. no string
true
false
no conversion!
wmConvertStrTo
null pointer
missing enumeration data
no enumerated value found
no enum found
. , 
. p@-
wmConvertOidToString: no data
wmConvertOidToString: invalid length
wmConvertOidToString: out of space
wmConvertOidToString()
. wmConvertMacAddrToStr: buffer too small
%2.2x:%2.2x:%2.2x:%2.2x:%2.2x:%2.2x
. %d.%d.%d.%d
lclConvertToStr()
. wmConvertToStr()
(p@-
(%3d days %02d:%02d:%02d
%02d:%02d:%02d
. buffer overrun
. TRUE
FALSE
buffer too small
. wmConvert: missing src data
wmConvert: null dest buffer
wmConvert: dest buffer too small
wmConvert()
wmConvert: buffer too small
wmConvert: buffer inadequate
wmConvert()
. L=0 U=255
L=0 U=65535
L=0 U=4294967295
L=-128 U=127
L=-32768 U=32767
L=-2147483648 U=2147483647
256.256.256.256
xx:xx:xx:xx:xx:xx
T=AL N=256
null pointers
. wmHashConstruct: invalid row count
no memory
. VUUU
. 0@-
wmHashEntryAdd: invalid table or entry
duplicate entry
(0@-
(wmMemoryInit: not enough memory
(Tasks open: %d
%4x:  
%02x 
(0@-
wmLogInit: name is null
wmLogInit: unable to open file
wmLogInit
. (no message)
(Thread (0x%x) : 
TID: %-5x 
. 0@-
no high bit found!
no memory
why no data?
wmMemBlockFree: bad block
wmMemBlockFree: NULL pointer
block header corrupted
corrupted tail
wmMemBlockFree: invalid data ptr
. 3;
(empty)
%s %s
no data
wmOidAppend: null arg(s)
wmOidTruncate: length too long
. p@-
wmOidStringGet: bad oid
wmOidStringGet: no data
. wmOidInvalid: bad OID
wmOidInvalid: bad data
Sun 
Mon 
Tue 
Wed 
Thu 
Fri 
Sat 
. Jan 
Feb 
Mar 
Apr 
May 
Jun 
Jul 
Aug 
Sep 
Oct 
Nov 
Dec 
(&amp;
&quot;
&apos;
&lt;
&gt;
. ?>
wmXmlParserProcessInstruction: no end bracket
<?xml
. --!>
wmXmlParserProcessComment: no end tag
. wmXmlParserProcessDoctype
<!DOCTYPE
SYSTEM
PUBLIC
(wmXmlParserProcessCharacters
wmlXmlAttributes
. wmXmlParserProcessElement
. <>&"'
wmXmlParserDocument: no data
wmXmlParserDocument: no preamble
<!--
wmnetUdpSocketCreate: failed
. failed to bind socket to local address
. invalid family entry
wmnetTcpServerOpen, listen-ing error
wmnetUdpRcvFrom: failed
. wmnetTcpAccept: accept failed
. unable to get address from socket
remote host unknown
connectToServer failed
. failed socket creation
failed socket bind
wmnetAddressResolve: invalid name
wmnetUdpIpSocketCreate is not implemented
. wmnetUdpIpBind is not implemented
. wmnetUdpIpRcvFrom is not implemented
. wmnetIpAddrResolve is not implemented
. wmnetClientIpAddrGet: NULL input
wmnetClientIpAddrGet: getpeername failed
wmnetClientIpAddrGet: unknown family
null pointer
Failed to create semaphr
Shared mem objs not included
unknown shared mem error
wmosThreadCreate: creation failed
Error =%d	[%s] errno:%d
/pipe/
Invalid pipe
. invalid pipe mode
failed to open pipe
. pipe write failed
. pipe read failed
. pipe close failed
wmosQueueCreate: queue creation failed
invalid file type
. 0@-
invalid filesystem
file not found
. httpFileGets not implemented for this filesystem
(getNextFs error
. <0
. 0@-
no mem pool
no mem
sem create error
	(registry not initialized
unable to register file
	(not found object to remove
	(0@-
www.wf10.com
WindWeb/4.00
http://
OWOWOWOWOWOWOWOW
/ N/A
HTTP Version not supported
Gateway Time-out
Service Unavailable
Bad Gateway
Internal Server Error
Unsupported Media Type
Request-URI Too Large
Request Entity Too Large
Precondition Failed
Length Required
Gone
Conflict
Request Time-out
Proxy Authentication Required
Not Acceptable
Method Not Allowed
Not Found
Forbidden
Payment Required
Unauthorized
Use Proxy
Not Modified
See Other
Moved Temporarily
Moved Permanently
Partial Content
Reset Content
No Content
Non-Authoritative Information
Accepted
Created
Switching Protocols
Not Implemented
Bad Request
Multiple Choices
Continue
VRML
x-world/x-vrml
video/x-msvideo
video/quicktime
video/mpeg
MPEG
AIFC
AIFF
audio/x-aiff
audio/mpeg
MPGA
audio/x-pn-realaudio-plugin
audio/x-pn-realaudio
audio/x-realaudio
audio/x-wav
audio/basic
image/x-xpixmap
image/x-xbitmap
image/x-portable-pixmap
image/x-portable-bitmap
image/jpeg
JPEG
image/gif
application/zip
application/x-gzip
application/x-compress
application/x-gtar
application/x-tar
application/x-tcl
application/postscript
application/octet-stream
CLASS
application/pdf
application/powerpoint
application/msword
text/tab-separated-values
text/x-sgml
SGML
text/html
HTML
JAVA
text/plain
Everywhere
/ httpInit: unable to initialize HTTP server.
httpInit: Upload RPM initialization failed.
httpInit: Upload RPM successfully initialized.
httpInit: System File Registry initialization failed.
httpInit: System File Registry successfully initialized.
httpInit: System File Manager initialization failed.
httpInit: System File Manager successfully initialized.
httpInit: File System RPM initialization failed.
httpInit: File System RPM successfully initialized.
httpInit: RPM dispatcher initialization failed.
httpInit: RPM dispatcher (system RPMs) initialization failed.
httpInit: RPM dispatcher successfully initialized.
httpInit: MIME type guessing RPM initialization failed.
httpInit: MIME type guessing RPM successfully initialized.
httpInit: HTTP server failed to register with WindManage Backplane.
httpInit: HTTP server connected successfully to WindManage Backplane.
httpInit: Post RPM initialization failed.
httpInit: Post RPM successfully initialized.
CONTENT-TYPE
ACCEPT-ENCODING
CONTENT-LENGTH
HOST
AUTHORIZATION
ACCESS-LANGUAGE
UTStarcom F1000/F1000G
httpInit: http Password Checking initialization failed.
httpInit: http Password Checking successfully initialized.
httpInit: http Access Control initialization failed.
httpInit: http Access Control successfully initialized.
/ h(/ 0
%/ @
'/ P
/ p+/ `
P2 h
/ l'/ 
/ Assertion failed: reqId != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpMem.c, line 127
no mem
1.1.4
unable to init inflate
 / $ / , / error cleanup after decompressing
!/ error decompressing from mem
bad crc on compressed file
!/ $ / , / 
 / ACCEPT_ENCODING
Content-Encoding
x-gzip
gzip
%/ Assertion failed: szLine != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpMimeAcceptLanguage.c, line 68
HTTP_ACCEPT
&/ `'/ Content-Length
CONTENT-LENGTH
'/ boundary
CONTENT_TYPE
Content-Type
<(/ H(/ X(/ T0
/ p@-
Assertion failed: szLine != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpMimeHost.c, line 51
HOST
*/ h+/ 
	(Assertion failed: reqId !=NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpMimeParse.c, line 135
Assertion failed: szLine != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpMimeParse.c, line 136
,/ p,/ 
	(00
4/ HTTP/1.1
HTTP/1.0
`5/ 
X5/ 
T5/ 
L5/ 
D5/ 
@5/ 
85/ 
05/ TRACE
DELETE
POST
HEAD
OPTIONS
UNKNOWN
Assertion failed: szName != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpRequestTranslation.c, line 149
5/ QUERY_STRING
7/ Assertion failed: szReqLine != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpRequestTranslation.c, line 255
SERVER_SOFTWARE
SERVER_NAME
SERVER_PROTOCOL
SERVER_PORT
REQUEST_METHOD
PATH_INFO
7/ \8/ 
/ `8/ 
(d8/ x
/ t8/ h
8/ N
8/ Assertion failed: reqId != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpRequestTranslation.c, line 374
Assertion failed: reqId->szAbsPath != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpRequestTranslation.c, line 375
Assertion failed: reqId->MimeHdrListId[HDR_IN] != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpRequestTranslation.c, line 376
Assertion failed: reqId->MimeHdrListId[HDR_OUT] != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpRequestTranslation.c, line 377
REMOTE_ADDR
END_OF_HEADERS
\;/ 
;/ X</ 
</ x=/ @
=/ , 
Assertion failed: NULL != szFailedWM, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpRequestUtil.c, line 311
	(Assertion failed: methodListId != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpRpmDispatch.c, line 155
A/ Assertion failed: methodListId != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpRpmDispatch.c, line 230
DC/ pC/ <C/ 0D/ 
D/ 8D/ 0D/ 
4/ HB/ Assertion failed: szString1 != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpStrCaseCmp.c, line 72
Assertion failed: szString2 != NULL, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpStrCaseCmp.c, line 73
Assertion failed: sStrLen > 0, file Z:/wfplt/src/protocol/webserver/pubsrc/http/httpStrCaseCmp.c, line 74
E/ p@-
	(p@-
(SELECTED
write attempt on a read only WindMark
invalid WindMark
I/ (I/ 
PI/ dI/ 
hI/ CHECKED
tK/ (I/ 
PI/ dI/ 
hI/ __js_
|M/ (I/ 
PI/ dI/ 
M/  
	(0@-
	(rb
Content-Type
	(DZ/ 
	(0@-
	(httpUserNameDecode(%s,szName,%d)
(]/ httpPwdDecode(%s,szName,%d
	(%s:%s
httpPwdConfAdd OK %s
httpPwdConfAdd Err %s
	(p@-
a/ 0@-
	(Basic realm="%s"
Basic 
USER NAME=%s
REMOTE_USER
xc/ 
Content-Type
application/x-www-form-urlencoded
Content-Length
httpRpmRcbPost: increase HTTP_MAX_REQ_PART_SIZE
httpRpmRcbPost: unable to allocate mem for entity
httpRpmRcbPost: unable evaluate posted data
f/ 0f/ df/ 
1111111111111111111
multipart/form-data
go into while(lContentLength>0)
common_file1
httpRpmUpload: backup file %d FAILURE
common_file2
common_file3
common_file4
firmware
File name = %s
fileIndex=%d
httpRpmUpload: wua_fopen(%d,%s,w+) open/create error
httpRpmUpload: wua_fopen(%d,%s,w+) OK
httpRpmUpload: file open/create error
 pCurrBuf=%s
httpRpmUpload: file open pCurrBuf=%s,iFile=%d
go into while ( (lFileSize > 0) && (lContentLength > 0) )
lFileSize:%d , lContentLength:%d
  if (flush)::::len=%d
 else if ( pFoundBoundary != NULL ) :::len=%d
 else if (!firsttime &&{ if ( pRestOfBoundary == pCurrBuf )} :::len=%d
 else if !firsttime &&{ else( pRestOfBoundary == pCurrBuf )} :::len=%d
 else  :::len=%d
go into  if (!firsttime)
go into if(firstdataline)!
Upload file %d validate FAILURE
pTempValidate=%s,len=%d
httpRpmUpload: close Upload file %d error
httpRpmUpload: recover file %d FAILURE
Upload file %d validate SUCCESS
httpRpmUpload: file write error
httpRpmUpload: file write SUCCESS
httpRpmUpload: file close error,iFile=%d
httpRpmUpload: file close SUCCESS,iFile=%d
outof while(Icontentlength>0)!!!
httpRpmUpload: buffer memory - deallocation failed
333333333333333333333333)!!!
44444444444444444444444444444444)!!!
555555555555555555555555555555)!!!
666666666666666666666666666)!!!
lContentLength=%d,iPostErrorMask=%d
iPostErrorMask != HTTP_OK iPostErrorMask=%d
return RPM_OK!!!!!!!!
httpPostReply!!!!!!!!
return RPM_DONE!!!!!!!!
|/ D|/ @
m/ D
/ Pm/  
	(Tm/ 
m/ dm/ 
m/ $n/ 
o/ (o/ Xo/ 
p/ 4p/ Xp/ tp/ 
n/ hq/ 
	(,m/ 
r/ 4r/ Xr/ |r/ 
r/ <q/ Ln/ 
m/ 0
s/ httpPostMultipartHeaderParse:LineRead=%s
httpPostMultipartHeaderParse: tagFlag=%d,tagValue=%s
/ httpPostMultipartHeaderParseAll:LineRead=%s
    if (( flag == 1) && (lRead > 10))
  if(HTTP_OK !=( httpPostContentDispositionParse_ForUpload(szTmp, tagFlag, tagValue)))
httpPostMultipartHeaderParseAll: tagFlag=%d,tagValue=%s
 if(HTTP_OK != ( httpPostCtrlNameParse(szTmp, sCtrlName)))
httpPostMultipartHeaderParseAll: sCtrlName=%s
if (lRead<0)
 if (fFoundCRLF)
if((memPoolFree( httpReqMemPartIdGet(reqId), szTmp )) == HTTP_ERROR)
else((memPoolFree( httpReqMemPartIdGet(reqId), szTmp )) == HTTP_ERROR)
/ filename=
 name=
/ <H2>Permission denied: Server cannot create/open file</H2> terminating...
<H2>Permission denied: Server cannot close file</H2> terminating...
<H2>Permission denied: Server cannot write to file</H2> terminating...
<H2>Error: Server cannot read from client</H2> terminating...
<H2>Error: Server cannot parse multipart header</H2> terminating...
<H2>Error: The files uploaded are not right script files!!!!!</H2> terminating...
	(text/html
Content-Type
/ unable to create WMB session
unable to create WMB session
unable to initialize WMB macro module
failed reading file
&nbsp;
Content-Type
application/x-www-form-urlencoded
multipart/form-data
httpRpmWmbPost: failed to process transaction
END_OF_HEADERS
CheckBoxManager
/ -------- %s --------
%s [%d bytes] = %s
%s [ERROR]
count:%d
file1:%s
file2:%s
file3:%s
file4:%s
/ deleteFile:%d OK
deleteFile:%d ERROR
/ @ 
3	(fileRename:%d OK
fileRename:%d ERROR
4	("4	(64	(LocalIPAddr:%s
GatewayIPAddr:%s
LocalIPMask:%s
/ admin
user
getUserName!:UserName=%s
userNameIndex=1
userNameIndex=0
getUserName Error!:UserName!=admin or user!
/ Registered
Connected
Connecting
Connect Failed
Not Registered
getCurrentStatus:%s
/ getSSIDConnectedTo:%s
/ macTemp malloc error! 
getMACAddress:%s
/ ResetToDefaultConfig
(getReboot!
/ `V
(Reboot!(web cmd)
gfff4
/ getServerIPConfig
wvlan0
(getDefaultScript = FAILURE
getDefaultScript SUCCESS = %d
/ setDefaultScript(%d) = FAILURE
setDefaultScript(%d) = SUCCESS
/ http
/ tftp
/ get %x: %d
LOCT_NET_DHCP: %d
LOCT_Misc_TimeZone: %d
/ LOCT_PSK1: %s
(getWFMode1Config
getWFMode1Config wifiWorkMode=%x,wfMode1=%d
/ setWFMode1Config
setWFMode1Config wifiWorkMode=%x,wfMode1=%d
/ getWFMode2Config
getWFMode2Config wifiWorkMode=%x,wfMode2=%d
U	(D
/ setWFMode2Config
setWFMode2Config wifiWorkMode=%x,wfMode2=%d
/ getWFMode3Config
getWFMode3Config wifiWorkMode=%x,wfMode3=%d
/ setWFMode3Config
setWFMode3Config wifiWorkMode=%x,wfMode3=%d
/ getWFMode4Config
getWFMode4Config wifiWorkMode=%x,wfMode4=%d
$	(L
/ setWFMode4Config
setWFMode4Config wifiWorkMode=%x,wfMode4=%d
/ getWEPAuth1Config
getWEPAuth1Config wifiWorkMode=%x,wepAuth1=%d
/ setWEPAuth1Config
setWEPAuth1Config wifiWorkMode=%x,wepAuth1=%d
/ getWEPAuth2Config
getWEPAuth2Config wifiWorkMode=%x,wepAuth1=%d
$	(H
/ setWEPAuth2Config
setWEPAuth2Config wifiWorkMode=%x,wepAuth1=%d
/ getWEPAuth3Config
getWEPAuth3Config wifiWorkMode=%x,wepAuth3=%d
(@W	(
/ setWEPAuth3Config
setWEPAuth3Config wifiWorkMode=%x,wepAuth3=%d
(@W	(
/ getWEPAuth4Config
getWEPAuth4Config wifiWorkMode=%x,wepAuth4=%d
V	(P
/ setWEPAuth4Config
setWEPAuth4Config wifiWorkMode=%x,wepAuth4=%d
/ getIndex1Config
(setIndex1Config
/ (W
(getWepkeylen1Config
(setWepkeylen1Config
(getIndex2Config
(setIndex2Config
(getWepkeylen2Config
(setWepkeylen2Config
(getIndex3Config
(setIndex3Config
/ 0H
(getWepkeylen3Config
(setWepkeylen3Config
(getIndex4Config
(setIndex4Config
(getWepkeylen4Config
(setWepkeylen4Config
/ hF
(OWOWOWOWOWOWOWOWOWOWOWOWOWOWOWOW
admin/admin_func.html
user/banner1.html
user/bbs.css
user/codec_dtmf.html
flash/script/com_postreply.html
user/contents.html
adminprivate/contents_admin.html
userprivate/contents_user.html
flash/script/firm_postreply.html
user/generic_infor.html
user/local_net_config.html
user/sip_rtp_config.html
user/stun_config.html
admin/tftp_config.html
fs/upload.html
user/user_settings.html
user/webmain.html
user/welcome.html
user/wireless_ap_config.html
user/arrow.gif
user/dotline.gif
user/head.gif
user/logo01.gif
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<!-- <META content=FrontPage.Editor.Document name=ProgId> 
<LINK href="/user/style.css" type=text/css rel=STYLESHEET>-->
<title>web management</title>
<style type="text/css">
<!--
body {
	background-color: #FFFFFF;
.style2 {	font-size: 16px;
	color: #000080;
	font-weight: bold;
</style>
<script>
function chkPwd() {
	if(document.admin_func.adminPwd.value.length==0) {
		alert('Administrator password could not be null.');
		return false;
	if(document.admin_func.adminPwd.value != document.admin_func.adminPwd2.value) {
                alert('The passwords you typed do not match.');
				admin_func.adminPwd2.value = "";
				return false;
    }
	return true;
</script>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312"></head>
<body>
<p align="center"><br><br><br><br>
  <span class="style2">Admin Functions</span><br>
</p>
<form name=reset_to_default action="admin_func.html" method="post" onSubmit="javascript:self.refresh()">
  <table width="500" height="49"  border="1" align="center">
    <tr>
      <td height="43" colspan="2"><div align="center"><strong>Reset To Default Parameters</strong>
          <input name="resetToDefault" type="hidden" id="resetToDefault" value="$%resetToDefault#$" maxlength="12">
      </div></td>
    </tr>
  </table>
  <p align="center">
    <input type="submit" name="toDefault" value="reset to default" align="center">
</p>  
</form>
<div align="center">
<form name=admin_func action="admin_func.html" method="post" onSubmit="return chkPwd();javascript:self.refresh()">
  <table width="500" height="85"  border="1" align="center">
    <tr>
      <td colspan="4"><div align="center"><strong>Administrator Password(Max Length:20):</strong> </div></td>
      <td width="31%"><div align="center">
        <input name="adminPwd" type="password" id="adminPwd" value="$%adminPwd#$" maxlength="20">
      </div></td>
    </tr>
    <tr>
      <td colspan="4"><div align="center"><strong>Re-enter Administrator Password To Confirm(Max Length:20):</strong></div></td>
      <td width="31%"> <div align="center">
        <input name="adminPwd2" type="password" id="adminPwd2" value="$%adminPwd#$" maxlength="20">
      </div></td>
    </tr>
  </table>
  <p align="center">
    <input type="submit" name="submit" value="submit" align="center">
</p>  
</form>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0 Transitional//EN">
<!-- saved from url=(0030)http://172.18.37.1/banner1.htm -->
<HTML><HEAD><TITLE>New Page 1</TITLE>
<META http-equiv=Content-Type content="text/html; charset=gb2312">
<META content="MSHTML 6.00.2800.1505" name=GENERATOR>
<META content=FrontPage.Editor.Document name=ProgId><style type="text/css">
<!--
BODY {
	FONT-SIZE: 12px; BACKGROUND: url(/images/ut/background.gif) #e0e0e0; MARGIN: 0px; COLOR: #000000; FONT-FAMILY: Arial, 
</style></HEAD>
<BODY>
<TABLE cellSpacing=0 cellPadding=0 width="100%" border=0>
  <TBODY>
  <TR>
    <TD width="100%"><div align="left"><IMG src="/user/head.gif" 
border=0></div></TD></TR></TBODY></TABLE></BODY></HTML>
BODY
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    FONT-SIZE: 12px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    PADDING-TOP: 0px;
    FONT-FAMILY: Verdana, Arial, Helvetica, sans-serif;
    BACKGROUND-COLOR: #eef3ff
    TEXT-DECORATION: none
A:visited
    COLOR: #0000ff
A:hover
    COLOR: #6600FF;
    TEXT-DECORATION: underline
#bbsleft
    BACKGROUND-COLOR: #6666CC}
#bbsfoot
    PADDING-LEFT: 10px;
    BACKGROUND-COLOR: #d6dff7
#newmail
    COLOR: #ff0000
#changeleft
#top
    HEIGHT: 5px
#title
    PADDING-RIGHT: 10px;
    BORDER-TOP: #ffffff 1px solid;
    PADDING-LEFT: 10px;
    FONT-WEIGHT: 600;
    FONT-SIZE: 14px;
    PADDING-BOTTOM: 10px;
    COLOR: #ffffff;
    PADDING-TOP: 10px;
    BORDER-BOTTOM: #ffffff 1px solid;
    TEXT-ALIGN: left
#user
    PADDING-LEFT: 25px;
    PADDING-BOTTOM: 10px;
    COLOR: #ffffff;
    LINE-HEIGHT: 150%;
    PADDING-TOP: 10px;
    TEXT-ALIGN: left
#user FORM
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    PADDING-TOP: 0px
#user .input
    BORDER-RIGHT: 1px inset;
    BORDER-TOP: 1px inset;
    FONT-SIZE: 12px;
    BORDER-LEFT: 1px inset;
    WIDTH: 70px;
    BORDER-BOTTOM: 1px inset;
    FONT-FAMILY: Verdana, Arial, Helvetica, sans-serif;
    BACKGROUND-COLOR: #fafafa
#user .button
    BORDER-RIGHT: #0066cc 1px solid;
    BORDER-TOP: #0066cc 1px solid;
    PADDING-BOTTOM: 3px;
    BORDER-LEFT: #0066cc 1px solid;
    PADDING-TOP: 3px;
    BORDER-BOTTOM: #0066cc 1px solid;
    HEIGHT: 22px;
    BACKGROUND-COLOR: #e0e0e0
#menu
    BORDER-RIGHT: #7897ed 1px solid;
    BORDER-LEFT: #7897ed 1px solid;
    BACKGROUND-COLOR: #d6dff7;
    TEXT-ALIGN: center
#menu UL
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    LINE-HEIGHT: normal;
    PADDING-TOP: 0px;
	LIST-STYLE-TYPE: none;
	text-align: left;
#menu LI
    PADDING-RIGHT: 0px;
    BORDER-TOP: #fff 1px solid;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
	PADDING-TOP: 0px;
	text-align: left;
#menu LI A
	WIDTH: 100%;
	COLOR: #000;
	LINE-HEIGHT: 30px;
	TEXT-DECORATION: none;
	text-align: left;
#menu LI A:hover
	COLOR: #6600FF;
	text-align: left;
	line-height: 30px;
#tool UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#talk UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#favorites UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#mail UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#menu UL LI.othersite
    PADDING-BOTTOM: 5px;
    MARGIN: 0px;
    PADDING-TOP: 10px
.bbssel
    BORDER-RIGHT: #cccccc 1px solid;
    BORDER-TOP: #999999 1px solid;
    FONT-SIZE: 12px;
    BORDER-LEFT: #999999 1px solid;
    BORDER-BOTTOM: #cccccc 1px solid
.bbsselb
    BORDER-RIGHT: #a2a2a2 1px solid;
    BORDER-TOP: #ffffff 1px solid;
    FONT-SIZE: 12px;
    BORDER-LEFT: #ffffff 1px solid;
    COLOR: #333333;
    BORDER-BOTTOM: #a2a2a2 1px solid;
    HEIGHT: 20px;
    BACKGROUND-COLOR: #eeeeee
FORM
    MARGIN-BOTTOM: 3px;
    PADDING-TOP: 3px
#header
    FONT-WEIGHT: 700;
    FONT-SIZE: 14px;
    PADDING-BOTTOM: 13px;
    PADDING-TOP: 18px;
    TEXT-ALIGN: center
#headerline
#headerline HR
    WIDTH: 98%;
    COLOR: #6600CC;
    HEIGHT: 2px
#downitem
#downitem H1
    FONT-WEIGHT: 700;
    FONT-SIZE: 12px;
    MARGIN: 10px;
    COLOR: #333366;
    TEXT-INDENT: 24px;
    PADDING-TOP: 18px
#downitem P
    FONT-SIZE: 12px;
    MARGIN: 10px;
    TEXT-INDENT: 24px;
    LINE-HEIGHT: 150%
#downitem A
    COLOR: #333366
#downitem A:hover
    COLOR: #6600CC;
    FONT-STYLE: italic;
    TEXT-DECORATION: underline
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId>
<title>web management</title>
<style type="text/css">
<!--
body {
	background-color: #FFFFFF;
.style2 {font-size: 16px;
	color: #000080;
	font-weight: bold;
.style3 {font-size: 12pt}
</style>
<script>
</script>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312"></head>
<body>
<p align="center"><br><br><br><br>
  <span class="style2">Codec and DTMF</span><br>
</p>
<div align="center">
<form  name="codec_dtmf" action="codec_dtmf.html" method="post" onSubmit="javascript:self.refresh()">
  <table width="562" height="285"  border="1" align="center">
    <tr>
      <td width="31%"><div align="center"><strong>G.711u:</strong></div></td>
      <td colspan="3"><div align="center">
        <select name="g711u" size="1" >
		  <option value=0 $%SELECTED(g711u,0)#$ >0</option>
          <option value=1 $%SELECTED(g711u,1)#$ >1</option>
          <option value=2 $%SELECTED(g711u,2)#$ >2</option>
		  <option value=3 $%SELECTED(g711u,3)#$ >3</option>
          <option value=4 $%SELECTED(g711u,4)#$ >4</option>
          <option value=5 $%SELECTED(g711u,5)#$ >5</option>
        </select>
        0-<span class="style3"><SPAN lang=EN-US 
style="FONT-FAMILY: 'Times New Roman'">D</SPAN></span><FONT face="Times New Roman" size=3><SPAN lang=EN-US 
style="FONT-SIZE: 12pt; FONT-FAMILY: 'Times New Roman'">isable</SPAN></FONT> 
 5-Highest Priority </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>G.711a: </strong></div></td>
      <td colspan="3" bgcolor="#FFFFFF"><div align="center">
        <select name="g711a" size="1" >
          <option value=0 $%SELECTED(g711a,0)#$ >0</option>
          <option value=1 $%SELECTED(g711a,1)#$ >1</option>
          <option value=2 $%SELECTED(g711a,2)#$ >2</option>
		  <option value=3 $%SELECTED(g711a,3)#$ >3</option>
          <option value=4 $%SELECTED(g711a,4)#$ >4</option>
          <option value=5 $%SELECTED(g711a,5)#$ >5</option>
        </select>
        0-<span class="style3"><SPAN lang=EN-US 
style="FONT-FAMILY: 'Times New Roman'">D</SPAN></span><FONT face="Times New Roman" size=3><SPAN lang=EN-US 
style="FONT-SIZE: 12pt; FONT-FAMILY: 'Times New Roman'">isable</SPAN></FONT> 
 5-Highest Priority</div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>G.729a:</strong></div></td>
      <td colspan="3"><div align="center">
        <select name="g729a" size="1" >
          <option value=0 $%SELECTED(g729a,0)#$ >0</option>
          <option value=1 $%SELECTED(g729a,1)#$ >1</option>
          <option value=2 $%SELECTED(g729a,2)#$ >2</option>
		  <option value=3 $%SELECTED(g729a,3)#$ >3</option>
          <option value=4 $%SELECTED(g729a,4)#$ >4</option>
          <option value=5 $%SELECTED(g729a,5)#$ >5</option>
        </select>
        0-<span class="style3"><SPAN lang=EN-US 
style="FONT-FAMILY: 'Times New Roman'">D</SPAN></span><FONT face="Times New Roman" size=3><SPAN lang=EN-US 
style="FONT-SIZE: 12pt; FONT-FAMILY: 'Times New Roman'">isable</SPAN></FONT> 
 5-Highest Priority</div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>G.726:</strong></div></td>
      <td colspan="3"><div align="center">
        <select name="g726" size="1" >
          <option value=0 $%SELECTED(g726,0)#$ >0</option>
          <option value=1 $%SELECTED(g726,1)#$ >1</option>
          <option value=2 $%SELECTED(g726,2)#$ >2</option>
		  <option value=3 $%SELECTED(g726,3)#$ >3</option>
          <option value=4 $%SELECTED(g726,4)#$ >4</option>
          <option value=5 $%SELECTED(g726,5)#$ >5</option>
        </select>
        0-<span class="style3"><SPAN lang=EN-US 
style="FONT-FAMILY: 'Times New Roman'">D</SPAN></span><FONT face="Times New Roman" size=3><SPAN lang=EN-US 
style="FONT-SIZE: 12pt; FONT-FAMILY: 'Times New Roman'">isable</SPAN></FONT> 
 5-Highest Priority</div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>DTMF Transfer Mode:</strong></div></td>
      <td width="23%"><div align="center">
          <input type="radio" name="drmfTxMode" value=0 $%CHECKED(drmfTxMode,0)#$>        
      RFC2833 </div></td>
      <td width="23%"><div align="center">
          <input type="radio" name="drmfTxMode" value=1 $%CHECKED(drmfTxMode,1)#$>
      In Band </div></td>
      <td width="23%"><div align="center">
          <input name="drmfTxMode" type="radio" value=2 $%CHECKED(drmfTxMode,2)#$>
      Not Supported</div></td>
    </tr>
  </table>
  <p align="center">
    <input type="submit"  value="submit" align="center">
</p>  
</form>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId><LINK 
href="/user/style.css" type=text/css rel=STYLESHEET>
<title>web management</title>
<style type="text/css">
<!--
body {
	background-color: #FFFFFF;
.wr_orange {margin-left:8px; color:#ff6600; font-weight:bold; font-size:14px;}
.style3 {font-size: 24px}
.style4 {color: #9900FF}
</style>
<script language="javascript">
<!--//
function countdown()
   location.href="http://$%serverIP#$/fs/upload.html";
setTimeout("countdown()",2000);
//--></script>
<meta http-equiv="Content-Type" content="text/html; charset=utf-8"></head>
<body>
<p align="center"><br><br><br><br><br>
</p>
<div align="center">
<div align="center">
  <p class="wr_orange style3">Script Files Upload Successfully!!! </p>
  <p class="wr_orange">&nbsp;</p>
  <p class="wr_orange style4">Please wait the system auto go back or </p>
  <p class="wr_orange style4">click: <a href="http://$%serverIP#$/fs/upload.html" target="details"><em>go back to upload page</em></a></p>
</div>
</body>
</html>
<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">
<html xmlns="http://www.w3.org/1999/xhtml" lang="gb2312">
<head>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312" />
<meta http-equiv="Content-Language" content="gb2312" />
<!--<link rel="stylesheet" rev="stylesheet" type="text/css" href="bbs.css" />-->
<link rel="icon" href="/favicon.ico" type="image/x-icon" />
<link rel="shortcut icon" href="/favicon.ico" type="image/x-icon" />
<script type="text/javascript">
<!--
function click_normal() {
	var normal = document.getElementById( "normal" );
    var advance = document.getElementById( "advance" );
	window.open("http://$%serverIP#$/user/welcome.html","details"); 
		if( "none" == normal.style.display ){
		 normal.style.display="";
		 advance.style.display="none";
		// tftp.style.display="none";
		} else {
		 normal.style.display="none";
		function click_advance() {
			var normal = document.getElementById( "normal" );
    var advance = document.getElementById( "advance" );
	window.open("http://$%serverIP#$/user/welcome.html","details"); 
		if( "none" == advance.style.display ){
		 advance.style.display="";
		 normal.style.display="none";
		// tftp.style.display="none";
		} else {
		 advance.style.display="none";
	function click_tftp() {
	window.open("http://$%serverIP#$/user/welcome.html","details"); 
		if( "none" == tftp.style.display ){
		 tftp.style.display="";
		 normal.style.display="none";
		 advance.style.display="none";
		} else {
		 tftp.style.display="none";
function init()
		var N=document.user_Name.userNameIndex.selectedIndex;
		document.user_Name.userNameIndex.value=document.user_Name.userNameIndex.options[N].value;
	if(document.user_Name.userNameIndex.value==0)
		window.location="http://$%serverIP#$/userprivate/contents_user.html";
				}
	else
		window.location="http://$%serverIP#$/adminprivate/contents_admin.html";
//-->
</script>
<style type="text/css">
<!--
BODY
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    FONT-SIZE: 12px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    PADDING-TOP: 0px;
    FONT-FAMILY: Verdana, Arial, Helvetica, sans-serif;
    BACKGROUND-COLOR: #eef3ff
    TEXT-DECORATION: none
A:visited
    COLOR: #0000ff
A:hover
    COLOR: #6600FF;
    TEXT-DECORATION: underline
#bbsleft
    BACKGROUND-COLOR: #6666CC}
#bbsfoot
    PADDING-LEFT: 10px;
    BACKGROUND-COLOR: #d6dff7
#newmail
    COLOR: #ff0000
#changeleft
#top
    HEIGHT: 5px
#title
    PADDING-RIGHT: 10px;
    BORDER-TOP: #ffffff 1px solid;
    PADDING-LEFT: 10px;
    FONT-WEIGHT: 600;
    FONT-SIZE: 14px;
    PADDING-BOTTOM: 10px;
    COLOR: #ffffff;
    PADDING-TOP: 10px;
    BORDER-BOTTOM: #ffffff 1px solid;
    TEXT-ALIGN: left
#user
    PADDING-LEFT: 25px;
    PADDING-BOTTOM: 10px;
    COLOR: #ffffff;
    LINE-HEIGHT: 150%;
    PADDING-TOP: 10px;
    TEXT-ALIGN: left
#user FORM
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    PADDING-TOP: 0px
#user .input
    BORDER-RIGHT: 1px inset;
    BORDER-TOP: 1px inset;
    FONT-SIZE: 12px;
    BORDER-LEFT: 1px inset;
    WIDTH: 70px;
    BORDER-BOTTOM: 1px inset;
    FONT-FAMILY: Verdana, Arial, Helvetica, sans-serif;
    BACKGROUND-COLOR: #fafafa
#user .button
    BORDER-RIGHT: #0066cc 1px solid;
    BORDER-TOP: #0066cc 1px solid;
    PADDING-BOTTOM: 3px;
    BORDER-LEFT: #0066cc 1px solid;
    PADDING-TOP: 3px;
    BORDER-BOTTOM: #0066cc 1px solid;
    HEIGHT: 22px;
    BACKGROUND-COLOR: #e0e0e0
#menu
    BORDER-RIGHT: #7897ed 1px solid;
    BORDER-LEFT: #7897ed 1px solid;
    BACKGROUND-COLOR: #d6dff7;
    TEXT-ALIGN: center
#menu UL
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    LINE-HEIGHT: normal;
    PADDING-TOP: 0px;
	LIST-STYLE-TYPE: none;
	text-align: left;
#menu LI
    PADDING-RIGHT: 0px;
    BORDER-TOP: #fff 1px solid;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
	PADDING-TOP: 0px;
	text-align: left;
#menu LI A
	WIDTH: 100%;
	COLOR: #000;
	LINE-HEIGHT: 30px;
	TEXT-DECORATION: none;
	text-align: left;
#menu LI A:hover
	COLOR: #6600FF;
	text-align: left;
	line-height: 30px;
#tool UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#talk UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#favorites UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#mail UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#menu UL LI.othersite
    PADDING-BOTTOM: 5px;
    MARGIN: 0px;
    PADDING-TOP: 10px
.bbssel
    BORDER-RIGHT: #cccccc 1px solid;
    BORDER-TOP: #999999 1px solid;
    FONT-SIZE: 12px;
    BORDER-LEFT: #999999 1px solid;
    BORDER-BOTTOM: #cccccc 1px solid
.bbsselb
    BORDER-RIGHT: #a2a2a2 1px solid;
    BORDER-TOP: #ffffff 1px solid;
    FONT-SIZE: 12px;
    BORDER-LEFT: #ffffff 1px solid;
    COLOR: #333333;
    BORDER-BOTTOM: #a2a2a2 1px solid;
    HEIGHT: 20px;
    BACKGROUND-COLOR: #eeeeee
FORM
    MARGIN-BOTTOM: 3px;
    PADDING-TOP: 3px
#header
    FONT-WEIGHT: 700;
    FONT-SIZE: 14px;
    PADDING-BOTTOM: 13px;
    PADDING-TOP: 18px;
    TEXT-ALIGN: center
#headerline
#headerline HR
    WIDTH: 98%;
    COLOR: #6600CC;
    HEIGHT: 2px
#downitem
#downitem H1
    FONT-WEIGHT: 700;
    FONT-SIZE: 12px;
    MARGIN: 10px;
    COLOR: #333366;
    TEXT-INDENT: 24px;
    PADDING-TOP: 18px
#downitem P
    FONT-SIZE: 12px;
    MARGIN: 10px;
    TEXT-INDENT: 24px;
    LINE-HEIGHT: 150%
#downitem A
    COLOR: #333366
#downitem A:hover
    COLOR: #6600CC;
    FONT-STYLE: italic;
    TEXT-DECORATION: underline
a:link {
	text-decoration: none;
a:visited {
	text-decoration: none;
a:hover {
	text-decoration: none;
a:active {
	text-decoration: none;
.style10 {font-size: 14px}
</style>
</head>
<body id="bbsleft" onload=init()>
<div align="left" id="menu">
  <ul>
    <li></li>
    <li><a href="javascript:click_normal();" title="normal" target="_self"><strong>USER MENU</strong></a>     
    </li>
    <li></li>
      <div  id="normal" style="display:none">
          <ul>
          <li>  <IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/local_net_config.html" target="details">Local Network Config</A></li>
		  <li></li>
              <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/wireless_ap_config.html" target="details"> Wireless AP Config</A></li>
		  <li></li>
              <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/generic_infor.html" target="details">Generic Information</A></li>
		  <li></li>
              <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/user_settings.html" target="details">User Settings</A></li>
		  <li></li>
		       <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/sip_rtp_config.html" target="details">SIP and RTP Config</A> </li>
		  <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/codec_dtmf.html" target="details">Codec and DTMF</A></li>
 		  <li></li>
         <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/stun_config.html" target="details">STUN Config</A></li>			
		  <li></li>
<!--		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/fs/upload.html" target="details">Script Upload</A></li>			
		  <li></li>
          </ul>
    </div>
    <li><a href="javascript:click_advance();" title="advance" target="_self" class="style1 style8"><strong>ADVANCED MENU</strong> </a></li>
    <li></li>
      <div id="advance" style="display:none">
        <ul>
<!--          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/sip_rtp_config.html" target="details">SIP and RTP Config</A> </li>
		  <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/codec_dtmf.html" target="details">Codec and DTMF</A></li>
 		  <li></li>
         <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/stun_config.html" target="details">STUN Config</A></li>			
		  <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/admin_func.html" target="details">Admin Funct</A></li>
		  <li></li>
		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/tftp_config.html" target="details">TFTP Config</A></li>
	      <li></li>
		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/fs/upload.html" target="details">File Upload</A></li>
	      <li></li>
        </ul>
      </div>
 <!-- 	  <li><a href="javascript:click_tftp();" title="tftp" target="_self" class="style2"><strong>TFTP MENU (admin only)</strong></a>
    <li> </li>     
      <div  id="tftp"  style="display:none">
        <ul>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/tftp/tftp_config.html" target="details">TFTP Config</A></li>
	      <li></li>
       
        </ul>
      </div>  -->
      <li>
  <form name=user_Name action="contents.html" method="post">
			  <div align="center"><span class="style13">Logged in as  
			  <select name="userNameIndex" size="1" class="style1"> 
                    <option value=0 $%SELECTED(userNameIndex,0)#$><strong>user</strong></option>
                    <option value=1 $%SELECTED(userNameIndex,1)#$ ><strong>admin</strong></option>
              </select>
			  </span></div>
			   </form>     
			   			   <form name=reboot_cmd action="contents_admin.html" method="post" onSubmit="javascript:self.refresh()">
         <div align="center">
           <p>
        <input name="rebootcmd" type="hidden" id="rebootcmd" value="$%rebootcmd#$">
        <input type="submit" name="reboot" value="REBOOT" align="center" class="bbsselb" >
           </p>
           <p>Note:Please REBOOT the handset after submitting configuration to make the changes effective.</p>
         </div>
	   </form>
    </li>
  </ul>
  <p>&nbsp;</p>
  <p>&nbsp;</p>
</div>
</body>
</html>
<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">
<html xmlns="http://www.w3.org/1999/xhtml" lang="gb2312">
<head>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312" />
<meta http-equiv="Content-Language" content="gb2312" />
<!--<link rel="stylesheet" rev="stylesheet" type="text/css" href="../user/bbs.css" />-->
<link rel="icon" href="/favicon.ico" type="image/x-icon" />
<link rel="shortcut icon" href="/favicon.ico" type="image/x-icon" />
<script type="text/javascript">
<!--
	function click_normal() {
		var normal = document.getElementById( "normal" );
    var advance = document.getElementById( "advance" );
	window.open("http://$%serverIP#$/user/welcome.html","details"); 
		if( "none" == normal.style.display ){
		 normal.style.display="";
		 advance.style.display="none";
//		 tftp.style.display="none";
		} else {
		 normal.style.display="none";
		function click_advance() {
			var normal = document.getElementById( "normal" );
    var advance = document.getElementById( "advance" );
	window.open("http://$%serverIP#$/user/welcome.html","details"); 
		if( "none" == advance.style.display ){
		 advance.style.display="";
		 normal.style.display="none";
		// tftp.style.display="none";
		} else {
		 advance.style.display="none";
	function click_tftp() {
	window.open("http://$%serverIP#$/user/welcome.html","details"); 
		if( "none" == tftp.style.display ){
		 tftp.style.display="";
		 normal.style.display="none";
		 advance.style.display="none";
		} else {
		 tftp.style.display="none";
function userName_set(num,F)
	F.userNameIndex.value=F.userNameIndex.options[num].value;
if(F.userNameIndex.value==0)
		{window.location="http://$%serverIP#$/userprivate/contents_user.html";}
function init()
	window.open("http://$%serverIP#$/user/welcome.html","details"); 
//-->
</script>
<style type="text/css">
<!--
BODY
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    FONT-SIZE: 12px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    PADDING-TOP: 0px;
    FONT-FAMILY: Verdana, Arial, Helvetica, sans-serif;
    BACKGROUND-COLOR: #eef3ff
    TEXT-DECORATION: none
A:visited
    COLOR: #0000ff
A:hover
    COLOR: #6600FF;
    TEXT-DECORATION: underline
#bbsleft
    BACKGROUND-COLOR: #6666CC}
#bbsfoot
    PADDING-LEFT: 10px;
    BACKGROUND-COLOR: #d6dff7
#newmail
    COLOR: #ff0000
#changeleft
#top
    HEIGHT: 5px
#title
    PADDING-RIGHT: 10px;
    BORDER-TOP: #ffffff 1px solid;
    PADDING-LEFT: 10px;
    FONT-WEIGHT: 600;
    FONT-SIZE: 14px;
    PADDING-BOTTOM: 10px;
    COLOR: #ffffff;
    PADDING-TOP: 10px;
    BORDER-BOTTOM: #ffffff 1px solid;
    TEXT-ALIGN: left
#user
    PADDING-LEFT: 25px;
    PADDING-BOTTOM: 10px;
    COLOR: #ffffff;
    LINE-HEIGHT: 150%;
    PADDING-TOP: 10px;
    TEXT-ALIGN: left
#user FORM
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    PADDING-TOP: 0px
#user .input
    BORDER-RIGHT: 1px inset;
    BORDER-TOP: 1px inset;
    FONT-SIZE: 12px;
    BORDER-LEFT: 1px inset;
    WIDTH: 70px;
    BORDER-BOTTOM: 1px inset;
    FONT-FAMILY: Verdana, Arial, Helvetica, sans-serif;
    BACKGROUND-COLOR: #fafafa
#user .button
    BORDER-RIGHT: #0066cc 1px solid;
    BORDER-TOP: #0066cc 1px solid;
    PADDING-BOTTOM: 3px;
    BORDER-LEFT: #0066cc 1px solid;
    PADDING-TOP: 3px;
    BORDER-BOTTOM: #0066cc 1px solid;
    HEIGHT: 22px;
    BACKGROUND-COLOR: #e0e0e0
#menu
    BORDER-RIGHT: #7897ed 1px solid;
    BORDER-LEFT: #7897ed 1px solid;
    BACKGROUND-COLOR: #d6dff7;
    TEXT-ALIGN: center
#menu UL
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    LINE-HEIGHT: normal;
    PADDING-TOP: 0px;
	LIST-STYLE-TYPE: none;
	text-align: left;
#menu LI
    PADDING-RIGHT: 0px;
    BORDER-TOP: #fff 1px solid;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
	PADDING-TOP: 0px;
	text-align: left;
#menu LI A
	WIDTH: 100%;
	COLOR: #000;
	LINE-HEIGHT: 30px;
	TEXT-DECORATION: none;
	text-align: left;
#menu LI A:hover
	COLOR: #6600FF;
	text-align: left;
	line-height: 30px;
#tool UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#talk UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#favorites UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#mail UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#menu UL LI.othersite
    PADDING-BOTTOM: 5px;
    MARGIN: 0px;
    PADDING-TOP: 10px
.bbssel
    BORDER-RIGHT: #cccccc 1px solid;
    BORDER-TOP: #999999 1px solid;
    FONT-SIZE: 12px;
    BORDER-LEFT: #999999 1px solid;
    BORDER-BOTTOM: #cccccc 1px solid
.bbsselb
    BORDER-RIGHT: #a2a2a2 1px solid;
    BORDER-TOP: #ffffff 1px solid;
    FONT-SIZE: 12px;
    BORDER-LEFT: #ffffff 1px solid;
    COLOR: #333333;
    BORDER-BOTTOM: #a2a2a2 1px solid;
    HEIGHT: 20px;
    BACKGROUND-COLOR: #eeeeee
FORM
    MARGIN-BOTTOM: 3px;
    PADDING-TOP: 3px
#header
    FONT-WEIGHT: 700;
    FONT-SIZE: 14px;
    PADDING-BOTTOM: 13px;
    PADDING-TOP: 18px;
    TEXT-ALIGN: center
#headerline
#headerline HR
    WIDTH: 98%;
    COLOR: #6600CC;
    HEIGHT: 2px
#downitem
#downitem H1
    FONT-WEIGHT: 700;
    FONT-SIZE: 12px;
    MARGIN: 10px;
    COLOR: #333366;
    TEXT-INDENT: 24px;
    PADDING-TOP: 18px
#downitem P
    FONT-SIZE: 12px;
    MARGIN: 10px;
    TEXT-INDENT: 24px;
    LINE-HEIGHT: 150%
#downitem A
    COLOR: #333366
#downitem A:hover
    COLOR: #6600CC;
    FONT-STYLE: italic;
    TEXT-DECORATION: underline
.style1 {
	font-size: 12px;
	font-weight: bold;
a:link {
	text-decoration: none;
a:visited {
	text-decoration: none;
a:hover {
	text-decoration: none;
a:active {
	text-decoration: none;
.style2 {font-size: 12px; font-weight: bold; color: #000000; }
.style8 {color: #666666}
.style14 {font-size: 12px}
</style>
</head>
<body id="bbsleft" onload=init()>
<div align="left" id="menu">
  <ul>
      <li></li>
    <li><a href="javascript:click_normal();" title="normal" target="_self" class="style2"><strong>USER MENU</strong></a>
    <li> </li>     
      <div  id="normal"  style="display:none">
        <ul>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/local_net_config.html" target="details">Local Network Config</A></li>
	      <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/wireless_ap_config.html" target="details">Wireless AP Config</A></li>
	      <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/generic_infor.html" target="details">Generic Information</A></li>
	      <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/user_settings.html" target="details">User Settings</A></li>
	      <li></li>
		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/sip_rtp_config.html" target="details">SIP and RTP Config</A> </li>
		  <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/codec_dtmf.html" target="details">Codec and DTMF</A></li>
 		  <li></li>
         <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/stun_config.html" target="details">STUN Config</A></li>			
		  <li></li>
<!--		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/fs/upload.html" target="details">Script Upload</A></li>			
		  <li></li>
        </ul>
      </div>
	 <li><a href="javascript:click_advance();" title="advance" target="_self" class="style1 style8">ADVANCED MENU </a></li>
      <li></li>
      <div id="advance" style="display:none">
        <ul>
 <!--         <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/sip_rtp_config.html" target="details">SIP and RTP Config</A> </li>
		  <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/codec_dtmf.html" target="details">Codec and DTMF</A></li>
   		  <li></li>
   		   <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/stun_config.html" target="details">STUN Configuration</A></li>	
          <li></li>
        -->
		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/admin_func.html" target="details">Admin Functions</A></li>
 		  <li></li>
		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/tftp_config.html" target="details">TFTP Config</A></li>
	      <li></li>
		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/fs/upload.html" target="details">File Upload</A></li>
	      <li></li>
       </ul>
      </div>
	 <!--    <li><a href="javascript:click_tftp();" title="tftp" target="_self" class="style2"><strong>TFTP MENU (admin only)</strong></a>
    <li> </li>     
     <div  id="tftp"  style="display:none">
        <ul>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/tftp/tftp_config.html" target="details">TFTP Config</A></li>
	      <li></li>
         <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/wireless_ap_config.html" target="details">Wireless AP Config</A></li>
	      <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/generic_infor.html" target="details">Generic Information</A></li>
	      <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/user_settings.html" target="details">User Settings</A></li>
	      <li></li>
        </ul>
      </div>  -->
      <li> 
              <form name=user_Name action="contents_admin.html" method="post">
			  <div align="center"><span class="style13">Logged in as  
			  <select name="userNameIndex" size="1" class="style1"   onChange=userName_set(this.form.userNameIndex.selectedIndex,this.form)>
                    <option value=0 $%SELECTED(userNameIndex,0)#$><strong>user</strong></option>
                    <option value=1 $%SELECTED(userNameIndex,1)#$ ><strong>admin</strong></option>
              </select>
			  </span></div>
	    </form>   
			   <form name=reboot_cmd action="contents_admin.html" method="post" onSubmit="javascript:self.refresh()">
         <div align="center">
           <p>
        <input name="rebootcmd" type="hidden" id="rebootcmd" value="$%rebootcmd#$">
        <input type="submit" name="reboot" value="REBOOT" align="center" class="bbsselb" >
           </p>
           <p>Note:Please REBOOT the handset after submitting configuration to make the changes effective.</p>
         </div>
	   </form>
     
    </li>
  </ul>
  <p>&nbsp;</p>
  <p>&nbsp;</p>
</div>
</body>
</html>
<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">
<html xmlns="http://www.w3.org/1999/xhtml" lang="gb2312">
<head>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312" />
<meta http-equiv="Content-Language" content="gb2312" />
<!--<link rel="stylesheet" rev="stylesheet" type="text/css" href="../user/bbs.css" />-->
<link rel="icon" href="/favicon.ico" type="image/x-icon" />
<link rel="shortcut icon" href="/favicon.ico" type="image/x-icon" />
<script type="text/javascript">
<!--
//var normal;
//var advance;
	function click_normal() {
	var normal = document.getElementById( "normal" );
    var advance = document.getElementById( "advance" );
	window.open("http://$%serverIP#$/user/welcome.html","details"); 
		if( "none" == normal.style.display ){
		 normal.style.display="";
		 advance.style.display="none";
		// tftp.style.display="none";
		} else {
		 normal.style.display="none";
		function click_advance() {
	window.open("http://$%serverIP#$/user/welcome.html","details"); 
	var normal = document.getElementById( "normal" );
    var advance = document.getElementById( "advance" );
//		if( "none" == advance.style.display ){
	//	 advance.style.display="";
		 normal.style.display="none";
//		} else {
		 advance.style.display="none";
//		}
		alert('Please log in as "admin".');
		/*
		function click_tftp() {
//	window.open("http://$%serverIP#$/user/welcome.html","details"); 
//		if( "none" == advance.style.display ){
	//	 advance.style.display="";
		 normal.style.display="none";
		 advance.style.display="none";
//		} else {
		 tftp.style.display="none";
//		}
		alert('Please log in as "admin".');
function userName_set(num,F)
	F.userNameIndex.value=F.userNameIndex.options[num].value;
if(F.userNameIndex.value==1)
window.location="http://$%serverIP#$/adminprivate/contents_admin.html";
function init()
	window.open("http://$%serverIP#$/user/welcome.html","details"); 
//-->
</script>
<style type="text/css">
<!--
BODY
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    FONT-SIZE: 12px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    PADDING-TOP: 0px;
    FONT-FAMILY: Verdana, Arial, Helvetica, sans-serif;
    BACKGROUND-COLOR: #eef3ff
    TEXT-DECORATION: none
A:visited
    COLOR: #0000ff
A:hover
    COLOR: #6600FF;
    TEXT-DECORATION: underline
#bbsleft
    BACKGROUND-COLOR: #6666CC}
#bbsfoot
    PADDING-LEFT: 10px;
    BACKGROUND-COLOR: #d6dff7
#newmail
    COLOR: #ff0000
#changeleft
#top
    HEIGHT: 5px
#title
    PADDING-RIGHT: 10px;
    BORDER-TOP: #ffffff 1px solid;
    PADDING-LEFT: 10px;
    FONT-WEIGHT: 600;
    FONT-SIZE: 14px;
    PADDING-BOTTOM: 10px;
    COLOR: #ffffff;
    PADDING-TOP: 10px;
    BORDER-BOTTOM: #ffffff 1px solid;
    TEXT-ALIGN: left
#user
    PADDING-LEFT: 25px;
    PADDING-BOTTOM: 10px;
    COLOR: #ffffff;
    LINE-HEIGHT: 150%;
    PADDING-TOP: 10px;
    TEXT-ALIGN: left
#user FORM
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    PADDING-TOP: 0px
#user .input
    BORDER-RIGHT: 1px inset;
    BORDER-TOP: 1px inset;
    FONT-SIZE: 12px;
    BORDER-LEFT: 1px inset;
    WIDTH: 70px;
    BORDER-BOTTOM: 1px inset;
    FONT-FAMILY: Verdana, Arial, Helvetica, sans-serif;
    BACKGROUND-COLOR: #fafafa
#user .button
    BORDER-RIGHT: #0066cc 1px solid;
    BORDER-TOP: #0066cc 1px solid;
    PADDING-BOTTOM: 3px;
    BORDER-LEFT: #0066cc 1px solid;
    PADDING-TOP: 3px;
    BORDER-BOTTOM: #0066cc 1px solid;
    HEIGHT: 22px;
    BACKGROUND-COLOR: #e0e0e0
#menu
    BORDER-RIGHT: #7897ed 1px solid;
    BORDER-LEFT: #7897ed 1px solid;
    BACKGROUND-COLOR: #d6dff7;
    TEXT-ALIGN: center
#menu UL
    PADDING-RIGHT: 0px;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
    LINE-HEIGHT: normal;
    PADDING-TOP: 0px;
	LIST-STYLE-TYPE: none;
	text-align: left;
#menu LI
    PADDING-RIGHT: 0px;
    BORDER-TOP: #fff 1px solid;
    PADDING-LEFT: 0px;
    PADDING-BOTTOM: 0px;
    MARGIN: 0px;
	PADDING-TOP: 0px;
	text-align: left;
#menu LI A
	WIDTH: 100%;
	COLOR: #000;
	LINE-HEIGHT: 30px;
	TEXT-DECORATION: none;
	text-align: left;
#menu LI A:hover
	COLOR: #6600FF;
	text-align: left;
	line-height: 30px;
#tool UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#talk UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#favorites UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#mail UL LI
    BORDER-TOP: #fff 1px solid;
    BORDER-BOTTOM: #fff 0px;
    BACKGROUND-COLOR: #eef3ff
#menu UL LI.othersite
    PADDING-BOTTOM: 5px;
    MARGIN: 0px;
    PADDING-TOP: 10px
.bbssel
    BORDER-RIGHT: #cccccc 1px solid;
    BORDER-TOP: #999999 1px solid;
    FONT-SIZE: 12px;
    BORDER-LEFT: #999999 1px solid;
    BORDER-BOTTOM: #cccccc 1px solid
.bbsselb
    BORDER-RIGHT: #a2a2a2 1px solid;
    BORDER-TOP: #ffffff 1px solid;
    FONT-SIZE: 12px;
    BORDER-LEFT: #ffffff 1px solid;
    COLOR: #333333;
    BORDER-BOTTOM: #a2a2a2 1px solid;
    HEIGHT: 20px;
    BACKGROUND-COLOR: #eeeeee
FORM
    MARGIN-BOTTOM: 3px;
    PADDING-TOP: 3px
#header
    FONT-WEIGHT: 700;
    FONT-SIZE: 14px;
    PADDING-BOTTOM: 13px;
    PADDING-TOP: 18px;
    TEXT-ALIGN: center
#headerline
#headerline HR
    WIDTH: 98%;
    COLOR: #6600CC;
    HEIGHT: 2px
#downitem
#downitem H1
    FONT-WEIGHT: 700;
    FONT-SIZE: 12px;
    MARGIN: 10px;
    COLOR: #333366;
    TEXT-INDENT: 24px;
    PADDING-TOP: 18px
#downitem P
    FONT-SIZE: 12px;
    MARGIN: 10px;
    TEXT-INDENT: 24px;
    LINE-HEIGHT: 150%
#downitem A
    COLOR: #333366
#downitem A:hover
    COLOR: #6600CC;
    FONT-STYLE: italic;
    TEXT-DECORATION: underline
.style1 {
	font-size: 12px;
	font-weight: bold;
a:link {
	text-decoration: none;
a:visited {
	text-decoration: none;
a:hover {
	text-decoration: none;
a:active {
	text-decoration: none;
.style8 {color: #666666}
.style10 {font-weight: bold}
.style13 {font-size: 12px}
</style>
</head>
<body id="bbsleft" onload=init()>
<div align="left" id="menu">
  <ul>
    <li></li>
    <li><span class="style10"><a href="javascript:click_normal();" title="normal" target="_self"><strong>USER MENU</strong></a></span></li>
    <li>      
      <div  id="normal"  style="display:none">
        <ul>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/local_net_config.html" target="details">Local Network Config</A></li>
          <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/wireless_ap_config.html" target="details">Wireless AP Config</A></li>
          <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/generic_infor.html" target="details">Generic Information</A></li>
          <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/user_settings.html" target="details">User Settings</A></li>
          <li></li>
		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/sip_rtp_config.html" target="details">SIP and RTP Config</A> </li>
		  <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/codec_dtmf.html" target="details">Codec and DTMF</A></li>
 		  <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/stun_config.html" target="details">STUN Config</A></li>			
		  <li></li>
<!--		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/fs/upload.html" target="details">Script Upload</A></li>			
		  <li></li>
        </ul>
      </div>
    </li>
    <li><a href="javascript:click_advance();" title="advance" target="_self" class="style1 style8">ADVANCED MENU</a></li>
      <li></li>
      <div id="advance" style="display:none">
        <ul>
    <!--      <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/sip_rtp_config.html" target="details">SIP and RTP Config</A> </li>
          <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/codec_dtmf.html" target="details">Codec and DTMF</A></li>
         <li></li>
         <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/stun_config.html" target="details">STUN Config</A></li>		
          <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/admin_func.html" target="details">Admin Functions</A></li>
          <li></li>
		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/admin/tftp_config.html" target="details">TFTP Config</A></li>
	      <li></li>
		  <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/fs/upload.html" target="details">File Upload</A></li>
	      <li></li>
        </ul>
      </div>	   
	<!--   <li><a href="javascript:click_tftp();" title="tftp" target="_self" class="style2"><strong>TFTP MENU (admin only)</strong></a>
    <li> </li>     
      <div  id="tftp"  style="display:none">
        <ul>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/tftp/tftp_config.html" target="details">TFTP Config</A></li>
	      <li></li>
         <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/wireless_ap_config.html" target="details">Wireless AP Config</A></li>
	      <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/generic_infor.html" target="details">Generic Information</A></li>
	      <li></li>
          <li><IMG height=12 src="/user/arrow.gif" width=12><A href="http://$%serverIP#$/user/user_settings.html" target="details">User Settings</A></li>
	      <li></li>
        </ul>
      </div>  -->
          <li>  
            
              <form name=user_Name action="contents_user.html" method="post">
			  <div align="center"><span class="style13">Logged in as  
			  <select name="userNameIndex" size="1" class="style1"   onChange=userName_set(this.form.userNameIndex.selectedIndex,this.form)>
                    <option value=0 $%SELECTED(userNameIndex,0)#$><strong>user</strong></option>
                    <option value=1 $%SELECTED(userNameIndex,1)#$ ><strong>admin</strong></option>
              </select>
			  </span></div>
			   </form>        
     <form name=reboot_cmd action="contents_admin.html" method="post" onSubmit="javascript:self.refresh()">
         <div align="center">
           <p>
        <input name="rebootcmd" type="hidden" id="rebootcmd" value="$%rebootcmd#$">
        <input type="submit" name="reboot" value="REBOOT" align="center" class="bbsselb" >
           </p>
           <p>Note:Please REBOOT the handset after submitting configuration to make the changes effective.</p>
         </div>
	   </form>         
        
    </li>
  </ul>
  <p>&nbsp;</p>
  <p>&nbsp;</p>
</div>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId><LINK 
href="/user/style.css" type=text/css rel=STYLESHEET>
<title>web management</title>
<style type="text/css">
<!--
body {
	background-color: #FFFFFF;
.wr_orange {margin-left:8px; color:#ff6600; font-weight:bold; font-size:14px;}
.style3 {margin-left: 8px; color: #ff6600; font-weight: bold; font-size: 24px; }
.style4 {color: #9900FF}
</style>
<script language="javascript">
<!--//
function countdown()
   location.href="http://$%serverIP#$/fs/upload.html";
setTimeout("countdown()",2000);
//--></script>
<meta http-equiv="Content-Type" content="text/html; charset=utf-8"></head>
<body>
<p><br><br><br><br>
</p>
<p><br>
</p>
<div align="center">
<div align="center"><span class="style3"> Firmware Upload<span class="wr_orange style3">Successfully!!!</span></span>
  <p class="wr_orange">&nbsp;</p>
  <p class="wr_orange"><span class="wr_orange style4">Please wait the system auto go back or</span></p>
  <p class="wr_orange"><span class="wr_orange style4"> click: </span><a href="http://$%serverIP#$/fs/upload.html" target="details"><em>go back to upload page</em></a></p>
</div>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId>
<title>web management</title>
<style type="text/css">
<!--
body {
	background-color: #FFFFFF;
.style2 {
	font-size: 16px;
	color: #000080;
	font-weight: bold;
</style>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312"></head>
<body>
<p align="center"><br><br><br><br>
  <span class="style2">Generic Information</span><br>
</p>
<div align="center">
<form action="generic_infor.html" method="post" onSubmit="javascript:self.refresh()">
  <table width="333" height="226"  border="1" align="center">
    <tr>
      <td width="50%" height="55"><div align="center"><strong>Enterprise Code: </strong></div></td>
      <td width="50%"><div align="center">
	<label>$%enterCode#$</label>
      </div></td>
    </tr>
    <tr>
      <td height="53"><div align="center"><strong>Product ID:</strong></div></td>
      <td><div align="center">
<label>$%productID#$</label>
      </div></td>
    </tr>
    <tr>
      <td height="54"><div align="center"><strong>Model Name:</strong></div></td>
      <td><div align="center">
<label>$%model#$</label>      </div></td>
    </tr>
    <tr>
      <td height="52"><div align="center"><strong>Firmware Version:</strong></div></td>
      <td><div align="center">
<label>$%version#$</label>
      </div></td>
    </tr>
  </table>
</form>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId>
<title>web management</title>
<style type="text/css">
<!--
body {
	background-color: #FFFFFF;
.style2 {
	font-size: 16px;
	font-weight: bold;
	color: #000080;
</style>
<SCRIPT LANGUAGE="JavaScript"> 
function dhcp_enable()
		document.local_net_config.tmnlIPAddress.disabled = true;
		document.local_net_config.tmnlSubMask.disabled = true;
		document.local_net_config.tmnlGWIPAddress.disabled = true;
function dhcp_disable()
		document.local_net_config.tmnlIPAddress.disabled = false;
		document.local_net_config.tmnlSubMask.disabled = false;
		document.local_net_config.tmnlGWIPAddress.disabled = false;
function dhcp_mode_set(num,F)
	F.dhcp_mode.value=F.dhcp_mode.options[num].value;
if(F.dhcp_mode.value==0)
	dhcp_disable();
	else
	dhcp_enable();
function init()
		var N=document.local_net_config.dhcp_mode.selectedIndex;
		document.local_net_config.dhcp_mode.value=document.local_net_config.dhcp_mode.options[N].value;
	//	document.local_net_config.dnsIPAddress1.disabled = true;
	//	document.local_net_config.dnsIPAddress2.disabled = true;
	//	document.local_net_config.dnsIPAddressSrc.disabled = true;
	if(document.local_net_config.dhcp_mode.value==0)
	dhcp_disable();
	else
	dhcp_enable();
function isip(s){ 
var check=function(v){try{return (v<=255 && v>=0)}catch(x){return false}}; 
var re=s.split(".") 
return (re.length==4)?(check(re[0]) && check(re[1]) && check(re[2]) && check(re[3])):false 
function is_subnet_mask(s){ 
var check=function(v){try{return (v<=255 && v>=0)}catch(x){return false}}; 
var re=s.split(".") 
return (re.length==4)?(check(re[0]) && check(re[1]) && check(re[2]) && check(re[3])):false 
function chk() {
	var tmnlip=document.local_net_config.tmnlIPAddress.value; 
	if(isip(tmnlip)==false) {
		alert('Terminal IP Address Error.');
		return false;
    var subnet_mask=document.local_net_config.tmnlSubMask.value; 
	if(is_subnet_mask(subnet_mask)==false) {
		alert('Terminal subnet mask Error.');
		return false;
	var gateway=document.local_net_config.tmnlGWIPAddress.value; 
	if(isip(gateway)==false) {
		alert('Terminal Gateway IP address Error.');
		return false;
	var dns1=document.local_net_config.dnsIPAddress1.value; 
	if(isip(dns1)==false) {
		alert('Primary DNS Server IP Address Error.');
		return false;
	var dns2=document.local_net_config.dnsIPAddress2.value; 
	if(isip(dns2)==false) {
		alert('Secondary DNS Server IP Address Error.');
		return false;
	return true;
</SCRIPT> 
<meta http-equiv="Content-Type" content="text/html; charset=gb2312"></head>
<body onLoad=init()>
<p align="center"><br><br>
</p>
<div align="center">
  <p class="style2">Status Table</p>
</div>
<table width="525" height="167"  border="1" align="center">
  <tr>
    <td width="240" height="28" nowrap><div align="center"><strong>IP Address: </strong></div></td>
    <td><div align="center"> $%localIPAddrs#$</div></td>
  </tr>
  <tr>
    <td width="240" height="28" nowrap><div align="center"><strong>Subnet Mask:</strong></div></td>
    <td><div align="center"> $%localIPMask#$</div></td>
  </tr>
  <tr>
    <td width="240" height="28" nowrap><div align="center"><strong>Gateway IP Address:</strong></div></td>
    <td><div align="center"> $%gatewayIPAddr#$</div></td>
  </tr>
  <tr>
    <td height="28" nowrap><div align="center"><strong>SSID Connected To:</strong></div></td>
    <td><div align="center">$%ssidConnectedTo#$</div></td>
  </tr>
  <tr>
    <td height="28" nowrap><div align="center"><strong>MAC Address:</strong></div></td>
    <td><div align="center"> $%macAddress#$</div></td>
  </tr>
  <tr>
    <td height="28" nowrap><div align="center"><strong>Current Status:</strong></div></td>
    <td><div align="center">$%currentStatus#$</div></td>
  </tr>
</table>
<p align="center"><span class="style2">Local Network Configuration</span></p>
<form name=local_net_config action="local_net_config.html" method="post" onSubmit="return chk();javascript:self.refresh()">
  <table width="525" height="204"  border="1" align="center">
    <tr>
      <td width="240" height="28" nowrap><div align="center"><strong>DHCP Work Mode:</strong></div></td>
      <td><div align="center">
          <label>
          <select name="dhcp_mode" size="1"   onChange=dhcp_mode_set(this.form.dhcp_mode.selectedIndex,this.form)>
            <option value=0 $%SELECTED(dhcp_mode,0)#$>Static IP for handset</option>
            <option value=1 $%SELECTED(dhcp_mode,1)#$ >DHCP</option>
          </select>
          </label>
      </div></td>
    </tr>
    <tr>
      <td width="240" height="26" nowrap><div align="center"><strong>Terminal IP Address: </strong></div></td>
      <td><div align="center">
          <input name="tmnlIPAddress" type="text" value="$%tmnlIPAddress#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td width="240" height="26" nowrap><div align="center"><strong>Terminal Subnet Mask:</strong></div></td>
      <td><div align="center">
          <input name="tmnlSubMask" type="text" value="$%tmnlSubMask#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td width="240" height="26" nowrap><div align="center"><strong>Terminal Gateway IP Address:</strong></div></td>
      <td><div align="center">
          <input name="tmnlGWIPAddress" type="text" value="$%tmnlGWIPAddress#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td width="240" height="26" nowrap><div align="center"><strong>Primary DNS Server IP Address:</strong></div></td>
      <td><div align="center">
          <input name="dnsIPAddress1" type="text" value="$%dnsIPAddress1#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td width="240" height="26" nowrap><div align="center"><strong>Secondary DNS Server IP Address:</strong></div></td>
      <td><div align="center">
          <input name="dnsIPAddress2" type="text" value="$%dnsIPAddress2#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td height="28" nowrap><div align="center"><strong>DNS Server IP Address Source:</strong></div></td>
      <td><div align="center">
          <label>
          <select name="dnsIPAddressSrc" size="1" >
            <option value=0 $%SELECTED(dnsIPAddressSrc,0)#$>Get DNS Server IP Address From DHCP Response</option>
            <option value=1 $%SELECTED(dnsIPAddressSrc,1)#$ >Get DNS Server IP Address From Local Setting</option>
          </select>
          </label>
      </div></td>
    </tr>
  </table>
  <p align="center">
    <input type="submit"  value="submit" align="center">
  </p>
</form>
<div align="center"></div>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId>
<title>web management</title>
<style type="text/css">
<!--
body {
	background-color: #FFFFFF;
.style2 {
	font-size: 16px;
	color: #000080;
	font-weight: bold;
</style>
<script>
function isip(s){ 
	var check=function(v){try{return (v<=255 && v>=0)}catch(x){return false}}; 
	var re=s.split(".") 
	return (re.length==4)?(check(re[0]) && check(re[1]) && check(re[2]) && check(re[3])):false 
function checkInteger(str){
	var rc=true;
	//try{
	    if (str+"" == "undefined" || str == null){
	            rc=false;
	    }
		else{
			for(i=0;i<str.length;i++){
				if(i==0 && str.charAt(i)=='-'){
					continue;
				}
	        	if(str.charAt(i)<'0' || str.charAt(i)>'9'){
	            	rc=false;
	            	break;
	            }
	        }
/*	}
	catch(ExcepitonObj0){
		rc=false
    return rc;
function checkIntegerMinValue(str,val)
    if(typeof(val) != "string")
        val = val + "";
    if(checkInteger(str) == true)
    {
        if(parseInt(str,10)>=parseInt(val,10))
            return true;
        else
            return false;
    }
    else
        return false;
function checkIntegerMaxValue(str,val)
    if(typeof(val) != "string")
        val = val + "";
    if(checkInteger(str) == true)
    {
        if(parseInt(str,10)<=parseInt(val,10))
            return true;
        else
            return false;
    }
    else
        return false;
function check() {
    var sip_p_ip=document.sip_rtp_config.sipProxyIPAddress.value;
	var sip_p_port=document.sip_rtp_config.sipProxyPort.value;
    var sip_r_ip=document.sip_rtp_config.sipRegisterIPAddress.value;
	var sip_r_port=document.sip_rtp_config.sipRegisterPort.value;
	var sip_t_port=document.sip_rtp_config.sipPort.value;
	var set_r_duration=document.sip_rtp_config.regDuration.value;
	var rtp_t_port=document.sip_rtp_config.rtpPort.value;
	var rtp_p_size=document.sip_rtp_config.rtpPacketSize.value;
	if(isip(sip_p_ip)==false) {
		alert('SIP proxy IP address Error.');
		return false;
    if(checkIntegerMaxValue(sip_p_port,65535)==false)
		document.sip_rtp_config.sipProxyPort.value='65535';
		alert('SIP proxy port must be integer and between 1024 and 65535.');
		return false;
	if(checkIntegerMinValue(sip_p_port,1024)==false)
		document.sip_rtp_config.sipProxyPort.value='1024';
		alert('SIP proxy port must be integer and between 1024 and 65535.');
		return false;
	if(isip(sip_r_ip)==false) {
		alert('SIP register IP address Error.');
		return false;
  if(checkIntegerMaxValue(sip_r_port,65535)==false)
		document.sip_rtp_config.sipRegisterPort.value='65535';
		alert('SIP register port must be integer and between 1024 and 65535.');
		return false;
	if(checkIntegerMinValue(sip_r_port,1024)==false)
		document.sip_rtp_config.sipRegisterPort.value='1024';
		alert('SIP register port must be integer and between 1024 and 65535.');
		return false;
	if(checkIntegerMaxValue(sip_t_port,65535)==false)
		document.sip_rtp_config.sipPort.value='65535';
		alert('SIP terminal port must be integer and between 1024 and 65535.');
		return false;
	if(checkIntegerMinValue(sip_t_port,1024)==false)
		document.sip_rtp_config.sipPort.value='1024';
		alert('SIP terminal port must be integer and between 1024 and 65535.');
		return false;
	if(checkIntegerMaxValue(set_r_duration,86400)==false)
		document.sip_rtp_config.regDuration.value='86400';
		alert('Set Registration duration must be integer and between 0 and 86400.');
		return false;
	if(checkIntegerMinValue(set_r_duration,0)==false)
		document.sip_rtp_config.regDuration.value='0';
		alert('Set Registration duration must be integer and between 0 and 86400.');
		return false;
	if(checkIntegerMaxValue(rtp_t_port,65535)==false)
		document.sip_rtp_config.rtpPort.value='65535';
		alert('Terminal audio RTP port must be integer and between 5000 and 65535.');
		return false;
	if(checkIntegerMinValue(rtp_t_port,5000)==false)
		document.sip_rtp_config.rtpPort.value='5000';
		alert('Terminal audio RTP port must be integer and between 5000 and 65535.');
		return false;
//	if((checkIntegerMaxValue(rtp_p_size,40)==false)||(checkIntegerMinValue(rtp_p_size,20)==false)){
//		alert('Terminal audio Packetize time must be integer and between 20 and 40.');
//		return false;
//	}
	return true;
</script>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312"></head>
<body  >
<p align="center"><br><br><br><br>
  <span class="style2">SIP and RTP Configuration</span><br>
</p>
<div align="center">
<form  name="sip_rtp_config" action="sip_rtp_config.html" method="post" onSubmit="return check();javascript:self.refresh()">
  <table width="671" height="575"  border="1" align="center">
    <tr>
      <td width="52%"><div align="center"><strong>SIP Terminal Use Outbound Proxy:</strong></div></td>
      <td width="19%">        <div align="center">
        <label>
          <input name="sipUseOutbandProxy" type="radio" value=0 $%CHECKED(sipUseOutbandProxy,0)#$ onClick=sipProxy_disable() >
        No</label>               
        <label>
        </label>
      </div></td>
      <td width="29%"><div align="center">
        <label>
          <input type="radio" name="sipUseOutbandProxy" value=1 $%CHECKED(sipUseOutbandProxy,1)#$ onClick=sipProxy_enable() >
          Yes</label>
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Terminal Use Register: </strong></div></td>
      <td><div align="center">
        <label>
          <input name="sipRegisterUsage" type="radio" value=0 $%CHECKED(sipRegisterUsage,0)#$ onClick=sipRegister_disable() >
  No</label>
      </div></td>
      <td><div align="center">
      <input type="radio" name="sipRegisterUsage" value=1 $%CHECKED(sipRegisterUsage,1)#$ onClick=sipRegister_enable() >
  Yes</div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Outbound Server Domain Name:</strong></div></td>
      <td colspan="2"><div align="center">
        <input name="sipProxyName" type="text" value="$%sipProxyName#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Outbound Server IP Address:</strong></div></td>
      <td colspan="2"><div align="center">
        <input name="sipProxyIPAddress" type="text" value="$%sipProxyIPAddress#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Outbound Server Port:</strong> </div></td>
      <td colspan="2"><div align="center">
        <input name="sipProxyPort" type="text" value="$%sipProxyPort#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Register Server Domain Name:</strong> </div></td>
      <td colspan="2"><div align="center">
        <input name="sipRegisterName" type="text" value="$%sipRegisterName#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Register Server IP Address:</strong> </div></td>
      <td colspan="2"><div align="center">
        <input name="sipRegisterIPAddress" type="text" value="$%sipRegisterIPAddress#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Register Server Port:</strong> </div></td>
      <td colspan="2"><div align="center">
        <input name="sipRegisterPort" type="text" value="$%sipRegisterPort#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Authentication String:</strong> </div></td>
      <td colspan="2"><div align="center">
        <input name="sipAuthString" type="text" value="$%sipAuthString#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP User Name:</strong> </div></td>
      <td colspan="2"><div align="center">
        <input name="sipUserName" type="text" value="$%sipUserName#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Password:</strong> </div></td>
      <td colspan="2"><div align="center">
        <input name="sipPassword" type="password" value="$%sipPassword#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Terminal Port:</strong> </div></td>
      <td colspan="2"><div align="center">
        <input name="sipPort" type="text" value="$%sipPort#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>SIP Terminal Use Null Packet:</strong> </div></td>
      <td><div align="center">
        <label>
        <input name="sipUseNullPacket" type="radio" value=0 $%CHECKED(sipUseNullPacket,0)#$>
No</label>
      </div></td>
      <td><div align="center">
      <input type="radio" name="sipUseNullPacket" value=1 $%CHECKED(sipUseNullPacket,1)#$>
  Yes</div></td>
    </tr>
    <tr>
      <td rowspan="4"><div align="center"><strong>SIP Terminal Use DNS:</strong> </div></td>
      <td colspan="2">
        <div align="left">
          <input name="sipUseDNS" type="radio" value=0 $%CHECKED(sipUseDNS,0)#$>
      Both SIP Proxy And Register Servers Use IP </div></td>
    </tr>
    <tr>
      <td colspan="2">
        <div align="left">
          <input type="radio" name="sipUseDNS" value=1 $%CHECKED(sipUseDNS,1)#$>
      Register Server Uses DNS And SIP Proxy Uses IP</div></td>
    </tr>
    <tr>
      <td colspan="2">
        <div align="left">
          <input type="radio" name="sipUseDNS" value=2 $%CHECKED(sipUseDNS,2)#$>
      Register Server Uses IP And SIP Proxy Server Uses DNS</div></td>
    </tr>
    <tr>
      <td colspan="2">
        <div align="left">
          <input type="radio" name="sipUseDNS" value=3 $%CHECKED(sipUseDNS,3)#$>
      Both Register And SIP Proxy Servers Use DNS</div></td>
    </tr>
    <tr>
      <td><div align="center"><strong><FONT color=black><SPAN lang=EN-US style="COLOR: black">DNS Query </SPAN></FONT><SPAN lang=EN-US style="COLOR: black">T</SPAN><FONT color=black><SPAN lang=EN-US style="COLOR: black">ype</SPAN></FONT>: </strong></div></td>
      <td><div align="center">
          <label>
          <input name="dnsQueryType" type="radio" value=0 $%CHECKED(dnsQueryType,0)#$>
      None SRV </label>
      </div></td>
      <td><div align="center">
          <input type="radio" name="dnsQueryType" value=1 $%CHECKED(dnsQueryType,1)#$>
      SRV</div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>Set Registration Duration:</strong> </div></td>
      <td colspan="2"><div align="center">
          <input name="regDuration" type="text" value="$%regDuration#$" maxlength="32">
      (sec)</div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>Terminal Audio RTP Port:</strong> </div></td>
      <td colspan="2"><div align="center">
          <input name="rtpPort" type="text" value="$%rtpPort#$" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td><div align="center"><strong>Terminal Audio Packetize Time:</strong> </div></td>
      <td colspan="2"><div align="center">
          <select name="rtpPacketSize" size="1" >
            <option value=20 $%SELECTED(rtpPacketSize,20)#$ >20</option>
            <option value=30 $%SELECTED(rtpPacketSize,30)#$ >30</option>
            <option value=40 $%SELECTED(rtpPacketSize,40)#$ >40</option>
          </select>
      (millisecond)</div></td>
    </tr>
  </table>
  <p align="center">
    <input type="submit"  value="submit" align="center">
  </p>  
</form>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId>
<title>web management</title>
<style type="text/css">
<!--
.style1 {
	font-size: 24px;
	font-weight: bold;
body {
	background-color: #FFFFFF;
.style2 {	font-size: 16px;
	color: #000080;
	font-weight: bold;
.style5 {font-size: 18px}
.style10 {font-size: 12px}
</style>
<script>
function stunUse_enable()
		document.stun_config.stunServerPort.disabled = false;
		document.stun_config.stunServer.disabled = false;
function stunUse_disable()
		document.stun_config.stunServerPort.disabled = true;
		document.stun_config.stunServer.disabled = true;
function stunUse_set(num,F)
	F.stunUse.value=F.stunUse.options[num].value;
	if(F.stunUse.value==0)
		stunUse_disable();
	else
		stunUse_enable();
function init()
		var N=document.stun_config.stunUse.selectedIndex;
		document.stun_config.stunUse.value=document.stun_config.stunUse.options[N].value;
	if(document.stun_config.stunUse.value==1)
		stunUse_enable();
	else
		stunUse_disable();
function checkInteger(str){
	var rc=true;
	//try{
	    if (str+"" == "undefined" || str == null){
	            rc=false;
	    }
		else{
			for(i=0;i<str.length;i++){
				if(i==0 && str.charAt(i)=='-'){
					continue;
				}
	        	if(str.charAt(i)<'0' || str.charAt(i)>'9'){
	            	rc=false;
	            	break;
	            }
	        }
/*	}
	catch(ExcepitonObj0){
		rc=false
    return rc;
function checkIntegerMinValue(str,val)
    if(typeof(val) != "string")
        val = val + "";
    if(checkInteger(str) == true)
    {
        if(parseInt(str,10)>=parseInt(val,10))
            return true;
        else
            return false;
    }
    else
        return false;
function checkIntegerMaxValue(str,val)
    if(typeof(val) != "string")
        val = val + "";
    if(checkInteger(str) == true)
    {
        if(parseInt(str,10)<=parseInt(val,10))
            return true;
        else
            return false;
    }
    else
        return false;
function check() {
    	
    var s=document.stun_config.stunServerPort.value;
    if((checkIntegerMaxValue(s,65535)==false)||(checkIntegerMinValue(s,1024)==false)){
		document.stun_config.stunServerPort.value ='65535';
		alert('Stun server port must be integer and between 1024 and 65535.');
		return false;
	return true;
</script>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312"></head>
<body  onload=init()>
<p align="center"><br><br><br><br>
  <span class="style2">STUN Configuration</span><br>
</p>
<div align="center">
<form  name="stun_config" action="stun_config.html" method="post" onSubmit="return check();javascript:self.refresh()">
  <table width="352" height="186"  border="1" align="center">
    <tr>
      <td width="43%" height="54"><div align="center"><strong>Use STUN:</strong></div></td>
      <td width="57%">        <div align="center">
        <label>          </label>
      </div>        <div align="center">
        <select name="stunUse" size="1"   onChange=stunUse_set(this.form.stunUse.selectedIndex,this.form)>
          <option value=0 $%SELECTED(stunUse,0)#$ >do not use STUN</option>
          <option value=1 $%SELECTED(stunUse,1)#$ >use STUN</option>
        </select>
        <label></label>
      </div>        </td>
    </tr>
    <tr>
      <td height="59" bgcolor="#FFFFFF"><div align="center"><strong>STUN Server Port: </strong></div></td>
      <td><div align="center">
        <input name="stunServerPort" type="text" VALUE="$%stunServerPort#$" maxlength="32">      
      </div></td>
    </tr>
    <tr>
      <td height="63"><div align="center"><strong>STUN Server Name:</strong></div></td>
      <td><div align="center">
        <input name="stunServer" type="text" value="$%stunServer#$" maxlength="32">      
      </div></td>
    </tr>
  </table>
  <p align="center">
    <input type="submit"  value="submit" align="center">
</p>  
</form>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId>
<title>web management</title>
<style type="text/css">
<!--
body {
	background-color: #FFFFFF;
.style2 {	font-size: 16px;
	color: #000080;
	font-weight: bold;
</style>
<script>
function init() {
	return true;
function check() {
	return true;
</script>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312"></head>
<body  onload=init()>
<p align="center"><br><br><br><br>
  <span class="style2">Provisioning Configuration</span><br>
</p>
<div align="center">
<form  name="tftp_config" action="tftp_config.html" method="post" onSubmit="return check();javascript:self.refresh()">
  <table width="506" height="130"  border="1" align="center">
    <tr>
      <td width="47%" height="59" bgcolor="#FFFFFF"><div align="center">
        <P class=MsoNormal style13 style12 style11><strong><FONT face=Arial size=1><SPAN lang=EN-US 
style="FONT-SIZE: 9pt; FONT-FAMILY: Arial">Provisioning Server FQDN:</SPAN></FONT></strong></P>
        </div></td>
      <td width="53%"><div align="center">
        <input name="tftpServerFQDN" type="text" VALUE="$%tftpServerFQDN#$" maxlength="32">      
      </div></td>
    </tr>
    <tr>
      <td height="63"><div align="center"><strong><FONT face=Arial size=1><SPAN lang=EN-US 
style="FONT-SIZE: 9pt; FONT-FAMILY: Arial">Provisioning Config Protocol:</SPAN></FONT></strong></div></td>
      <td><div align="center">
	  <!--
        <input name="tftpConfProtocol" type="text" value="$%tftpConfProtocol#$" maxlength="32">  
	  -->
	  <select name="ProvConfProtocol" size="1" >
              <option value=0 $%SELECTED(ProvConfProtocol,0)#$ >TFTP</option>
              <option value=1 $%SELECTED(ProvConfProtocol,1)#$ >HTTP</option>
      </select>    
      </div></td>
    </tr>
  </table>
  <p align="center">
    <input type="submit"  value="submit" align="center">
</p>  
</form>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0 Transitional//EN">
<html><head><title>web management</title>
<style>
div.content{ position:absolute; padding-top:30px; padding-bottom:30px;
	         top:90px; left:122px; width:475px;
	         font-family: verdana, arial, helvetica, sans-serif;}
div.top_box{ position:absolute; background-color: #0C2577;
			 layer-background-color: #0C2577;
			 top:0px; left:0px; width:755px; height:60px; }
.url       { color:blue; font: bold, 10pt, monospace; }
.fixed     { color:black; font-weight: bold; font-size: 10pt; font-family:monospace;}
.wr_orange { margin-left:8px; color:#ff6600; font-weight:bold; font-size:14px;}
.body_t    { margin-left:8px; color:#000000; font-size:12px;}
.bold      { font-weight:bold;}
.italic    { font-style:italic;}
</style>
<SCRIPT LANGUAGE="Javascript"> 
function chk_common_file() {
	var tempfile1=document.common_file.common_file1.value; 
	var tempfile2=document.common_file.common_file2.value; 
	var tempfile3=document.common_file.common_file3.value; 
	var tempfile4=document.common_file.common_file4.value; 
	var pattern = /[a-z]{1,1}:(\\[^\\\/:\*\?<>\|]+)*[^\\\/:\*\?<>\|]+.((txt)|(cfg))/i;
	if((tempfile1=="")&&(tempfile2=="")&&(tempfile3=="")&&(tempfile4==""))
		alert('The script files to be uploaded could not be null!');
		return false;
	else
		if((pattern.test(tempfile1)==false)&&(tempfile1!=""))
	 	{
			alert('The script file1 to be uploaded is invalid!');
			return false;
		else if((pattern.test(tempfile2)==false)&&(tempfile2!=""))
			alert('The script file2 to be uploaded is invalid!');
			return false;
		else if((pattern.test(tempfile3)==false)&&(tempfile3!=""))
	 	{
			alert('The script file3 to be uploaded is invalid!');
			return false;
		else if((pattern.test(tempfile4)==false)&&(tempfile4!=""))
	 	{
			alert('The script file4 to be uploaded is invalid!');
			return false;
		else
		{	
			return true;
function chk_firmware() {
	var tempfile=document.firmware.firmware.value; 
	var pattern = /[a-z]{1,1}:(\\[^\\\/:\*\?<>\|]+)*[^\\\/:\*\?<>\|]+.((sre)|(bin))/i;
	if(pattern.test(tempfile)==false)
		alert('The firmware to be uploaded is invalid!');
		return false;
	else
		return true;
function chk_File_del(obj) {
	var tempfile=obj.value; 
	var N=document.file_active.file_active.selectedIndex;
	document.file_active.file_active.value=document.file_active.file_active.options[N].value;
	if(tempfile=="")
		alert('There is no file to Delete!');
		return false;
	else
		if((1==document.file_active.file_active.value)&&(obj==document.File1_del.filename1_old))
	 	{
			alert('The default script file could not be Deleted!If you want to delete it,please active another script file first!');
			return false;
		else if((2==document.file_active.file_active.value)&&(obj==document.File2_del.filename2_old))
	 	{
			alert('The default script file could not be Deleted!If you want to delete it,please active another script file first!');
			return false;
		else if((3==document.file_active.file_active.value)&&(obj==document.File3_del.filename3_old))
	 	{
			alert('The default script file could not be Deleted!If you want to delete it,please active another script file first!');
			return false;
		else if((4==document.file_active.file_active.value)&&(obj==document.File4_del.filename4_old))
	 	{
			alert('The default script file could not be Deleted!If you want to delete it,please active another script file first!');
			return false;
		else
			return true;
function chk_File_act() {
	var N=document.file_active.file_active.selectedIndex;
	document.file_active.file_active.value=document.file_active.file_active.options[N].value;
		if((1==document.file_active.file_active.value)&&(""==document.File1_del.filename1_old.value))
	 	{
			alert('File 1 is not found,please active another script file!');
			return false;
		else if((2==document.file_active.file_active.value)&&(""==document.File2_del.filename2_old.value))
	 	{
			alert('File 2 is not found,please active another script file!');
			return false;
		else if((3==document.file_active.file_active.value)&&(""==document.File3_del.filename3_old.value))
	 	{
			alert('File 3 is not found,please active another script file!');
			return false;
		else if((4==document.file_active.file_active.value)&&(""==document.File4_del.filename4_old.value))
	 	{
			alert('File 4 is not found,please active another script file!');
			return false;
		else
			return true;
function chk_File_rename(obj_old,obj_new) {
	var tempfile_old=obj_old.value; 
	var tempfile_new=obj_new.value; 
	var pattern = /[^\\\/:\*\?<>\|\s]+.((txt)|(cfg))/;
 	if(tempfile_old=="")
		alert('There is no file to rename!');
		return false;
	else if(!pattern.test(tempfile_new))
		alert('The new filename is invalid!');
		return false;
	else
		return true;
</SCRIPT></head>
<body bgcolor="#ffffff" leftmargin="0" topmargin="0" marginwidth="0" marginheight="0">
<!-- begin content-->
<p>&nbsp;</p>
<div class="common">
<p align="center" class="wr_orange"> Common Files Upload: </p>
<table width="560" height="256" border="1" align="center" bordercolor="#CCCCCC">
  <tr>
    <td height="42" colspan="2">   <div align="center">&nbsp;</div></td>
    <td width="142"><div align="center"><strong>Filename/Delete Operation</strong></div></td>
    <td width="120"><div align="center"><strong>Rename Operation</strong></div></td>
    <td width="67"><div align="center"><strong>Activate Operation</strong></div></td>
    <td width="179"><div align="center"><strong>Upload Operation</strong></div></td>
  </tr>
  <tr>
    <td height="55" colspan="2"><div align="center"><strong>File1:</strong></div></td>
    <td height="50"><form name="File1_del" action="upload.html" method="post" onSubmit="return chk_File_del(document.File1_del.filename1_old);javascript:self.refresh()">
          <div align="center">
           
              <input name="filename1_old" type="text"  size="20" value="$%filename1_old#$" disabled>
                       
              <input name="delFile1" type="hidden" id="delFile1" value="$%delFile1#$" >         
              <input type="submit" value="Delete">
          </div>
    </form></td>
    <td height="50"><form name="File1_rename" action="upload.html" method="post" onSubmit="return chk_File_rename(document.File1_del.filename1_old,document.File1_rename.filename1_new);javascript:self.refresh()">
      <div align="center">
        <input name="filename1_new" type="text" value="$%filename1_new#$" size="20">
        <input type="submit" value="Rename">
      </div>
    </form></td>
    <td rowspan="4">
      <form name="file_active" action="upload.html" method="post" onSubmit="return chk_File_act();javascript:self.refresh()">
        <p align="center">      Set </p>
        <p align="center">File
          <select name="file_active" size="1" >        
              <option value=1 $%SELECTED(file_active,1)#$ >1</option>
              <option value=2 $%SELECTED(file_active,2)#$ >2</option>
		      <option value=3 $%SELECTED(file_active,3)#$ >3</option>
              <option value=4 $%SELECTED(file_active,4)#$ >4</option>
                </select>
        </p>
        <p align="center">          As Default</p>
        <p align="center"> Script </p>
        <p align="center">File </p>
        <p align="center">        <input type="submit" value="Activate">
    </p>
    </form></td>
  <td rowspan="4"> <FORM name="common_file" action="/flash/script/com_postreply.html"
method="post" enctype="multipart/form-data"  onSubmit="return chk_common_file()">
         <p align="center"><input name="common_file1" type="file" size="20" >
         </p>
         <p align="center">
            <input name="common_file2" type="file" id="common_file2" size="20">
         </p>
         <p align="center">
            <input name="common_file3" type="file" id="common_file3" size="20">
         </p>
         <p align="center">
            <input name="common_file4" type="file" id="common_file4" size="20">
         </p>
         <p align="center">              <input type="submit" value="Upload">
          </p>
      </FORM>
    </td>
  </tr>
  <tr>
    <td height="55" colspan="2"><div align="center"><strong>File2:</strong>
      </div></td>
    <td height="50"><form name="File2_del" action="upload.html" method="post"  onSubmit="return chk_File_del(document.File2_del.filename2_old);javascript:self.refresh()">
          <div align="center">
      
              <input name="filename2_old" type="text" value="$%filename2_old#$" size="20" disabled>
           
              <input name="delFile2" type="hidden" id="delFile2" value="$%delFile2#$" >
              <input type="submit" value="Delete">
          </div>
    </form></td><td height="50"><form name="File2_rename" action="upload.html" method="post"  onSubmit="return chk_File_rename(document.File2_del.filename2_old,document.File2_rename.filename2_new);javascript:self.refresh()">
      <div align="center">
        <input name="filename2_new" type="text" value="$%filename2_new#$" size="20">
        <input type="submit" value="Rename">
      </div>
    </FORM></td>
    </tr>
  <tr>
    <td height="55" colspan="2"><div align="center"><strong>File3:</strong>
      </div></td>
    <td height="50">        <form name="File3_del" action="upload.html" method="post" onSubmit="return chk_File_del(document.File3_del.filename3_old);javascript:self.refresh()">
          <div align="center">
              <input name="filename3_old" type="text" value="$%filename3_old#$" size="20" disabled>
           
              <input name="delFile3" type="hidden" id="delFile3" value="$%delFile3#$" >
              <input type="submit" value="Delete">
          </div>
    </form></td><td height="50"><form name="File3_rename" action="upload.html" method="post" onSubmit="return chk_File_rename(document.File3_del.filename3_old,document.File3_rename.filename3_new);javascript:self.refresh()">
        <div align="center">
          <input name="filename3_new" type="text" value="$%filename3_new#$" size="20">
          <input type="submit" value="Rename">
        </div>
    </form></td>
    </tr>
  <tr>
    <td height="55" colspan="2">
      <div align="center"><strong>File4:</strong></div></td>
    <td height="50">        <form name="File4_del" action="upload.html" method="post"  onSubmit="return chk_File_del(document.File4_del.filename4_old);javascript:self.refresh()">
          <div align="center">
              <input name="filename4_old" type="text" value="$%filename4_old#$" size="20" disabled>
            
              <input name="delFile4" type="hidden" id="delFile4" value="$%delFile4#$" >
              <input type="submit" value="Delete">
          </div>
    </form></td><td height="50"><form name="File4_rename" action="upload.html" method="post" onSubmit="return chk_File_rename(document.File4_del.filename4_old,document.File4_rename.filename4_new);javascript:self.refresh()">
        <div align="center">
          <input name="filename4_new" type="text" value="$%filename4_new#$" size="20">
          <input type="submit" value="Rename">
        </div>
    </form></td>
    </tr>
</table>
<!--
	<p>&nbsp;</p>
	<p align="center" class="wr_orange">Firmware Upload: </p>
	<table width="213" border="1" align="center">
      <tr>
        <td width="203">	<FORM name="firmware" action="/flash/script/firm_postreply.html"
      method="post" enctype="multipart/form-data" onSubmit="return chk_firmware()">
          <div align="center">
      <input type="file" name="firmware">
      <input type="submit" value="Upload">
          </div>
        </FORM>
</td>
      </tr>
    </table>
  -->
</div>
<br><br><br><br><br>
</div>
</body></html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId>
<title>web management</title>
<style type="text/css">
<!--
body {
	background-color: #FFFFFF;
.style2 {
	font-size: 16px;
	font-weight: bold;
	color: #000080;
.style5 {font-size: 18px}
.style10 {font-size: 12px}
</style>
<script>
function autoscan_enable()
		document.user_settings.autoscanInter.disabled = false;
function autoscan_disable()
		document.user_settings.autoscanInter.disabled = true;
function autoscanFlag_set(num,F)
	F.autoscanFlag.value=F.autoscanFlag.options[num].value;
	if(F.autoscanFlag.value==0)
		autoscan_disable();
	else
		autoscan_enable();
function init()
		var N=document.user_settings.autoscanFlag.selectedIndex;
		document.user_settings.autoscanFlag.value=document.user_settings.autoscanFlag.options[N].value;
	if(document.user_settings.autoscanFlag.value==0)
		autoscan_disable();
	if(document.user_settings.autoscanFlag.value==1)
		autoscan_enable();
function checkInteger(str){
	var rc=true;
	//try{
	    if (str+"" == "undefined" || str == null){
	            rc=false;
	    }
		else{
			for(i=0;i<str.length;i++){
				if(i==0 && str.charAt(i)=='-'){
					continue;
				}
	        	if(str.charAt(i)<'0' || str.charAt(i)>'9'){
	            	rc=false;
	            	break;
	            }
	        }
/*	}
	catch(ExcepitonObj0){
		rc=false
    return rc;
function checkIntegerMinValue(str,val)
    if(typeof(val) != "string")
        val = val + "";
    if(checkInteger(str) == true)
    {
        if(parseInt(str,10)>=parseInt(val,10))
            return true;
        else
            return false;
    }
    else
        return false;
function checkIntegerMaxValue(str,val)
    if(typeof(val) != "string")
        val = val + "";
    if(checkInteger(str) == true)
    {
        if(parseInt(str,10)<=parseInt(val,10))
            return true;
        else
            return false;
    }
    else
        return false;
function check() {
    	
    var s=document.user_settings.autoscanInter.value;
	var pwd=document.user_settings.userPwd.value;
	if(checkIntegerMaxValue(s,20)==false)
		document.user_settings.autoscanInter.value='20';
		alert('Auto scan interval must be integer and between 1 and 20.');
		return false;
	if(checkIntegerMinValue(s,1)==false)
		document.user_settings.autoscanInter.value='1';
		alert('Auto scan interval must be integer and between 1 and 20.');
		return false;
	if(document.user_settings.userPwd.value.length==0) {
		alert('Use password could not be null.');
		return false;
	if(checkInteger(pwd)==false) {
		alert('Use password could be only numbers.');
		return false;
	if(document.user_settings.userPwd.value != document.user_settings.userPwd2.value) {
                alert('The passwords you typed do not match.');
				user_settings.userPwd2.value = "";
				return false;
    }
	return true;
</script>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312"></head>
<body onload=init()>
<p align="center"><br><br><br><br>
  <span class="style2">User Settings</span><br>
</p>
<div align="center">
<form name=user_settings action="user_settings.html" method="post" onSubmit="return check();javascript:self.refresh()">
  <table width="561" height="281"  border="1" align="center">
    <tr>
      <td width="47%"><div align="center"><strong>Display Name:</strong></div></td>
      <td colspan="2"><div align="center">
        <input name="displayName" type="text" VALUE="$%displayName#$" maxlength="32">
      </div></td>
    </tr>
	<tr>
      <td width="47%" rowspan="2"><div align="center"><strong>Autoscan Flag: </strong></div></td>
      <td height="25" colspan="2"><div align="center">
        To Search And Connect For Open AP</div></td>
    </tr>
    <tr>
      <td height="23" colspan="2"><div align="center">
        <label>          </label><label>
        <select name="autoscanFlag" size="1"   onChange=autoscanFlag_set(this.form.autoscanFlag.selectedIndex,this.form)>
          <option value=0 $%SELECTED(autoscanFlag,0)#$ >Autoscan flag OFF</option>
          <option value=1 $%SELECTED(autoscanFlag,1)#$ >Autoscan flag ON</option>
        </select>
        </label>
        </div>        <div align="center"></div></td>
    </tr>
    <tr>
      <td width="47%"><div align="center"><strong>Auto Scan Interval:</strong></div></td>
      <td colspan="2"><div align="center">
        <input name="autoscanInter" type="text" value="$%autoscanInter#$" maxlength="32">
      (.min)</div></td>
    </tr>
    <tr>
      <td width="47%"><div align="center"><strong>Time Zone:</strong></div></td>
      <td colspan="2"><div align="center">
        <select name="timeZoneOffset" size="1" id="timeZoneOffset">
          <option value=-1200 $%SELECTED(timeZoneOffset,-1200)#$>GMT-12:00 Int'l Date Line</option>
          <!-- <option value=-1150 $%SELECTED(timeZoneOffset,-1150)#$>GMT-11:30 </option> -->
          <option value=-1100 $%SELECTED(timeZoneOffset,-1100)#$>GMT-11:00 Midway Island</option>
          <!-- <option value=-1050 $%SELECTED(timeZoneOffset,-1050)#$>GMT-10:30 </option> -->
          <option value=-1000 $%SELECTED(timeZoneOffset,-1000)#$>GMT-10:00 Hawaii</option>
          <!-- <option value=-950 $%SELECTED(timeZoneOffset,-950)#$>GMT-9:30</option> -->
          <option value=-900 $%SELECTED(timeZoneOffset,-900)#$>GMT-9:00 Alaska</option>
          <!-- <option value=-850 $%SELECTED(timeZoneOffset,-850)#$>GMT-8:30</option> -->
          <option value=-800 $%SELECTED(timeZoneOffset,-800)#$>GMT-8:00 US Pacific</option>
          <!-- <option value=-750 $%SELECTED(timeZoneOffset,-750)#$>GMT-7:30</option> -->
          <option value=-700 $%SELECTED(timeZoneOffset,-700)#$>GMT-7:00 US Mountain</option>
          <!-- <option value=-650 $%SELECTED(timeZoneOffset,-650)#$>GMT-6:30</option> -->
          <option value=-600 $%SELECTED(timeZoneOffset,-600)#$>GMT-6:00 US Central</option>
          <!-- <option value=-550 $%SELECTED(timeZoneOffset,-550)#$>GMT-5:30</option> -->
          <option value=-500 $%SELECTED(timeZoneOffset,-500)#$>GMT-5:00 US Eastern</option>
          <!-- <option value=-450 $%SELECTED(timeZoneOffset,-450)#$>GMT-4:30</option> -->
          <option value=-400 $%SELECTED(timeZoneOffset,-400)#$>GMT-4:00 Atlantic</option>
          <option value=-350 $%SELECTED(timeZoneOffset,-350)#$>GMT-3:30 Newfoundland</option>
          <option value=-300 $%SELECTED(timeZoneOffset,-300)#$>GMT-3:00 Buenos Aires</option>
          <!-- <option value=-250 $%SELECTED(timeZoneOffset,-250)#$>GMT-2:30</option> -->
          <option value=-200 $%SELECTED(timeZoneOffset,-200)#$>GMT-2:00 Mid-Atlantic</option>
          <!-- <option value=-150 $%SELECTED(timeZoneOffset,-150)#$>GMT-1:30</option> -->
          <option value=-100 $%SELECTED(timeZoneOffset,-100)#$>GMT-1:00 Azores</option>
          <!-- <option value=-50 $%SELECTED(timeZoneOffset,-50)#$>GMT-0:30</option> -->
          <option value=0 $%SELECTED(timeZoneOffset,0)#$>GMT 0:00 London</option>
          <!-- <option value=50 $%SELECTED(timeZoneOffset,50)#$>GMT+0:30</option> -->
          <option value=100 $%SELECTED(timeZoneOffset,100)#$>GMT+1:00 Central Europe</option>
          <!-- <option value=150 $%SELECTED(timeZoneOffset,150)#$>GMT+1:30</option> -->
          <option value=200 $%SELECTED(timeZoneOffset,200)#$>GMT+2:00 East Europe</option>
          <!-- <option value=250 $%SELECTED(timeZoneOffset,250)#$>GMT+2:30</option> -->
          <option value=300 $%SELECTED(timeZoneOffset,300)#$>GMT+3:00 Moscow</option>
          <!-- <option value=350 $%SELECTED(timeZoneOffset,350)#$>GMT+3:30</option> -->
          <option value=400 $%SELECTED(timeZoneOffset,400)#$>GMT+4:00 Abu Dhabi</option>
          <option value=450 $%SELECTED(timeZoneOffset,450)#$>GMT+4:30 Kabul</option>
          <option value=500 $%SELECTED(timeZoneOffset,500)#$>GMT+5:00 Islamabad</option>
          <option value=550 $%SELECTED(timeZoneOffset,550)#$>GMT+5:30 Delhi</option>
		  <option value=575 $%SELECTED(timeZoneOffset,575)#$>GMT+5:45 Katmandu</option>
          <option value=600 $%SELECTED(timeZoneOffset,600)#$>GMT+6:00 Novosibirsk</option>
          <option value=650 $%SELECTED(timeZoneOffset,650)#$>GMT+6:30 Rangoon</option>
          <option value=700 $%SELECTED(timeZoneOffset,700)#$>GMT+7:00 Bangkok</option>
          <!-- <option value=750 $%SELECTED(timeZoneOffset,750)#$>GMT+7:30</option> -->
          <option value=800 $%SELECTED(timeZoneOffset,800)#$>GMT+8:00 Beijing</option>
          <!-- <option value=850 $%SELECTED(timeZoneOffset,850)#$>GMT+8:30</option> -->
          <option value=900 $%SELECTED(timeZoneOffset,900)#$>GMT+9:00 Tokyo</option>
          <option value=950 $%SELECTED(timeZoneOffset,950)#$>GMT+9:30 Darwin</option>
          <option value=1000 $%SELECTED(timeZoneOffset,1000)#$>GMT+10:00 Sydney</option>
          <!-- <option value=1050 $%SELECTED(timeZoneOffset,1050)#$>GMT+10:30</option> -->
          <option value=1100 $%SELECTED(timeZoneOffset,1100)#$>GMT+11:00 Solomon Island</option>
          <!-- <option value=1150 $%SELECTED(timeZoneOffset,1150)#$>GMT+11:30</option> -->
          <option value=1200 $%SELECTED(timeZoneOffset,1200)#$>GMT+12:00 New Zealand</option>
          <!-- <option value=1250 $%SELECTED(timeZoneOffset,1250)#$>GMT+12:30</option> -->
          <option value=1300 $%SELECTED(timeZoneOffset,1300)#$>GMT+13:00 Nuku'alofa</option>
        </select>
      </div></td>
    </tr>
    <tr>
      <td width="47%" rowspan="2"><div align="center"><strong>DST Setting:</strong></div></td>
      <td colspan="2"><div align="center">Daylight Saving Time</div></td>
    </tr>
    <tr>
      <td width="23%"><div align="center">
        <label>
        <input name="dstFlag" type="radio" value=0  $%CHECKED(dstFlag,0)#$>
Disable</label>
</div></td>
      <td width="30%"><div align="center">
        <label>
        <input type="radio" name="dstFlag" value=1 $%CHECKED(dstFlag,1)#$>
Enable</label>
</div></td>
    </tr>
    <tr>
      <td width="47%"><div align="center"><strong>User Password:</strong></div></td>
      <td colspan="2"><div align="center">
        <input name="userPwd" type="password" id="upwd" value="$%userPwd#$" maxlength="6">
      (<FONT face=Arial size=1><SPAN lang=EN-US style="FONT-SIZE: 9pt; FONT-FAMILY: Arial">only numbers </SPAN></FONT>)</div></td>
    </tr>
    <tr>
      <td width="47%"><div align="center"><strong>Re-enter User Password To Confirm:</strong></div></td>
      <td colspan="2"><div align="center">
        <input name="userPwd2" type="password" id="adminPwd2" value="$%userPwd#$" maxlength="6">
      (<FONT face=Arial size=1><SPAN lang=EN-US style="FONT-SIZE: 9pt; FONT-FAMILY: Arial">only numbers </SPAN></FONT>)</div></td>
    </tr>
  </table>
  <p align="center">
    <input type="submit"  value="submit" align="center">
</p>  
</form>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0 Frameset//EN">
<html>
<head>
<title>UTStarcom Web Server Management</title>
<meta name="GENERATOR" content="Microsoft FrontPage 4.0">
<meta name="ProgId" content="FrontPage.Editor.Document">
</head>
<frameset framespacing="0" border="0" frameborder="0" rows="69,*">
  <frame name="banner" noresize  src="/user/banner1.html" scrolling="no" />
  <frameset cols="180,*">
    <frame  src="/user/contents.html" name="contents" scrolling="no" noresize/>
    <frame name="details" src="/user/welcome.html" scrolling="auto" />
  </frameset>
  <noframes>
  <body>
  <p>This page uses frames, but your browser doesn't support them.</p>
  </body>
  </noframes>
</frameset>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId>
<title>
</title>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312"></head>
<style type="text/css">
<!--
.style1 {
	font-size: 24px;
	font-weight: bold;
body {
	background-color: #FFFFFF;
</style>
<body>
<p>&nbsp;<br><br><br><br><br></p>
<div align="center">
<table>
<tr>
<td><img src="/user/logo01.gif" width="112" height="72"></td>
<td><div align="center"><span class="style1"> &nbsp; Welcome to WiFi Web Server Management </span></div></td>
  </tr>
</table>
</div>
</body>
</html>
<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN"
"http://www.w3.org/TR/html4/loose.dtd">
<html>
<head>
<META content=FrontPage.Editor.Document name=ProgId>
<title>web management</title>
<style type="text/css">
<!--
body {
	background-color: #FFFFFF;
.style4 {
	font-size: 16px;
	font-weight: bold;
	color: #000080;
.style5 {font-size: 18px}
.style10 {font-size: 12px}
</style>
<SCRIPT LANGUAGE="JavaScript"> 
function wfMode1_open()
		document.wireless_ap_config.wepAuth1.disabled = true;
		wep1_open();
		document.wireless_ap_config.wpaPSK1.disabled = true;
function wfMode1_WEP()
		var M1=document.wireless_ap_config.wepAuth1.selectedIndex;
		document.wireless_ap_config.wepAuth1.value=document.wireless_ap_config.wepAuth1.options[M1].value;
	document.wireless_ap_config.wepAuth1.disabled = false;
//		if(document.wireless_ap_config.wepAuth1.value == 0)
//			wep1_open();
//		else
			wep1_shared();
		document.wireless_ap_config.wpaPSK1.disabled = true;
function wfMode1_WAP()
		document.wireless_ap_config.wepAuth1.disabled = true;
		wep1_open();
		document.wireless_ap_config.wpaPSK1.disabled = false;
function wfMode2_open()
		document.wireless_ap_config.wepAuth2.disabled = true;
		wep2_open();
		document.wireless_ap_config.wpaPSK2.disabled = true;
function wfMode2_WEP()
		var M2=document.wireless_ap_config.wepAuth2.selectedIndex;
		document.wireless_ap_config.wepAuth2.value=document.wireless_ap_config.wepAuth2.options[M2].value;
		document.wireless_ap_config.wepAuth2.disabled = false;
	//	if(document.wireless_ap_config.wepAuth2.value == 0)
//			wep2_open();
//		else
			wep2_shared();
		document.wireless_ap_config.wpaPSK2.disabled = true;
function wfMode2_WAP()
		document.wireless_ap_config.wepAuth2.disabled = true;
		wep2_open();
		document.wireless_ap_config.wpaPSK2.disabled = false;
function wfMode3_open()
		document.wireless_ap_config.wepAuth3.disabled = true;
		wep3_open();
		document.wireless_ap_config.wpaPSK3.disabled = true;
function wfMode3_WEP()
		var M3=document.wireless_ap_config.wepAuth3.selectedIndex;
		document.wireless_ap_config.wepAuth3.value=document.wireless_ap_config.wepAuth3.options[M3].value;
		document.wireless_ap_config.wepAuth3.disabled = false;
//		if(document.wireless_ap_config.wepAuth3.value == 0)
//			wep3_open();
//		else
			wep3_shared();
		document.wireless_ap_config.wpaPSK3.disabled = true;
function wfMode3_WAP()
		document.wireless_ap_config.wepAuth3.disabled = true;
		wep3_open();
		document.wireless_ap_config.wpaPSK3.disabled = false;
function wfMode4_open()
		document.wireless_ap_config.wepAuth4.disabled = true;
		wep4_open();
		document.wireless_ap_config.wpaPSK4.disabled = true;
function wfMode4_WEP()
		var M4=document.wireless_ap_config.wepAuth4.selectedIndex;
		document.wireless_ap_config.wepAuth4.value=document.wireless_ap_config.wepAuth4.options[M4].value;
		document.wireless_ap_config.wepAuth4.disabled = false;
//		if(document.wireless_ap_config.wepAuth4.value == 0)
//			wep4_open();
//		else
			wep4_shared();
		document.wireless_ap_config.wpaPSK4.disabled = true;
function wfMode4_WAP()
		document.wireless_ap_config.wepAuth4.disabled = true;
		wep4_open();
		document.wireless_ap_config.wpaPSK4.disabled = false;
function wep1_open()
		document.wireless_ap_config.index1.disabled = true;
		document.wireless_ap_config.wepkeylen1.disabled = true;
		document.wireless_ap_config.wepkey12.disabled = true;
		document.wireless_ap_config.wepkey11.disabled = true;
function wep1_shared()
		var L1=document.wireless_ap_config.wepkeylen1.selectedIndex;
		document.wireless_ap_config.wepkeylen1.value=document.wireless_ap_config.wepkeylen1.options[L1].value;
		document.wireless_ap_config.index1.disabled = false;
		document.wireless_ap_config.wepkeylen1.disabled = false;
		if(document.wireless_ap_config.wepkeylen1.value == 2)
			weplen1_128();
		if(document.wireless_ap_config.wepkeylen1.value == 1)
			weplen1_64();
function wep2_open()
		document.wireless_ap_config.index2.disabled = true;
		document.wireless_ap_config.wepkeylen2.disabled = true;
		document.wireless_ap_config.wepkey22.disabled = true;
		document.wireless_ap_config.wepkey21.disabled = true;
function wep2_shared()
		var L2=document.wireless_ap_config.wepkeylen2.selectedIndex;
		document.wireless_ap_config.wepkeylen2.value=document.wireless_ap_config.wepkeylen2.options[L2].value;
		document.wireless_ap_config.index2.disabled = false;
		document.wireless_ap_config.wepkeylen2.disabled = false;
		if(document.wireless_ap_config.wepkeylen2.value == 2)
			weplen2_128();
		if(document.wireless_ap_config.wepkeylen2.value == 1)
			weplen2_64();
function wep3_open()
		document.wireless_ap_config.index3.disabled = true;
		document.wireless_ap_config.wepkeylen3.disabled = true;
		document.wireless_ap_config.wepkey32.disabled = true;
		document.wireless_ap_config.wepkey31.disabled = true;
function wep3_shared()
		var L3=document.wireless_ap_config.wepkeylen3.selectedIndex;
		document.wireless_ap_config.wepkeylen3.value=document.wireless_ap_config.wepkeylen3.options[L3].value;
		document.wireless_ap_config.index3.disabled = false;
		document.wireless_ap_config.wepkeylen3.disabled = false;
		if(document.wireless_ap_config.wepkeylen3.value == 2)
			weplen3_128();
		if(document.wireless_ap_config.wepkeylen3.value == 1)
			weplen3_64();
function wep4_open()
		document.wireless_ap_config.index4.disabled = true;
		document.wireless_ap_config.wepkeylen4.disabled = true;
		document.wireless_ap_config.wepkey42.disabled = true;
		document.wireless_ap_config.wepkey41.disabled = true;
function wep4_shared()
		var L4=document.wireless_ap_config.wepkeylen4.selectedIndex;
		document.wireless_ap_config.wepkeylen4.value=document.wireless_ap_config.wepkeylen4.options[L4].value;
		document.wireless_ap_config.index4.disabled = false;
		document.wireless_ap_config.wepkeylen4.disabled = false;
		if(document.wireless_ap_config.wepkeylen4.value == 2)
			weplen4_128();
		if(document.wireless_ap_config.wepkeylen4.value == 1)
			weplen4_64();
function weplen1_128()
		document.wireless_ap_config.wepkey12.disabled = false;
		document.wireless_ap_config.wepkey11.disabled = true;
function weplen1_64()
		document.wireless_ap_config.wepkey12.disabled = true;
		document.wireless_ap_config.wepkey11.disabled = false;
function weplen2_128()
		document.wireless_ap_config.wepkey22.disabled = false;
		document.wireless_ap_config.wepkey21.disabled = true;
function weplen2_64()
		document.wireless_ap_config.wepkey22.disabled = true;
		document.wireless_ap_config.wepkey21.disabled = false;
function weplen3_128()
		document.wireless_ap_config.wepkey32.disabled = false;
		document.wireless_ap_config.wepkey31.disabled = true;
function weplen3_64()
		document.wireless_ap_config.wepkey32.disabled = true;
		document.wireless_ap_config.wepkey31.disabled = false;
function weplen4_128()
		document.wireless_ap_config.wepkey42.disabled = false;
		document.wireless_ap_config.wepkey41.disabled = true;
function weplen4_64()
		document.wireless_ap_config.wepkey42.disabled = true;
		document.wireless_ap_config.wepkey41.disabled = false;
function  wepauth1_set(num,F)
	F.wepAuth1.value=F.wepAuth1.options[num].value;
	if(F.wepAuth1.value==0)
		wep1_open();
	if(F.wepAuth1.value==1)
		wep1_shared();
function  wepauth2_set(num,F)
	F.wepAuth2.value=F.wepAuth2.options[num].value;
	if(F.wepAuth2.value==0)
		wep2_open();
	if(F.wepAuth2.value==1)
		wep2_shared();
function  wepauth3_set(num,F)
	F.wepAuth3.value=F.wepAuth3.options[num].value;
	if(F.wepAuth3.value==0)
		wep3_open();
	if(F.wepAuth3.value==1)
		wep3_shared();
function  wepauth4_set(num,F)
	F.wepAuth4.value=F.wepAuth4.options[num].value;
	if(F.wepAuth4.value==0)
		wep4_open();
	if(F.wepAuth4.value==1)
		wep4_shared();
function  wfMode1_set(num,F)
	F.wfMode1.value=F.wfMode1.options[num].value;
	if(F.wfMode1.value==0)
		wfMode1_open();
	if(F.wfMode1.value==1)
		wfMode1_WEP();
	if(F.wfMode1.value==2)
		wfMode1_WAP();
function  wfMode2_set(num,F)
	F.wfMode2.value=F.wfMode2.options[num].value;
	if(F.wfMode2.value==0)
		wfMode2_open();
	if(F.wfMode2.value==1)
		wfMode2_WEP();
	if(F.wfMode2.value==2)
		wfMode2_WAP();
function  wfMode3_set(num,F)
	F.wfMode3.value=F.wfMode3.options[num].value;
	if(F.wfMode3.value==0)
		wfMode3_open();
	if(F.wfMode3.value==1)
		wfMode3_WEP();
	if(F.wfMode3.value==2)
		wfMode3_WAP();
function  wfMode4_set(num,F)
	F.wfMode4.value=F.wfMode4.options[num].value;
	if(F.wfMode4.value==0)
		wfMode4_open();
	if(F.wfMode4.value==1)
		wfMode4_WEP();
	if(F.wfMode4.value==2)
		wfMode4_WAP();
function  wepkeylen1_set(num,F)
	F.wepkeylen1.value=F.wepkeylen1.options[num].value;
	if(F.wepkeylen1.value==1)
		weplen1_64();
	if(F.wepkeylen1.value==2)
		weplen1_128();
function  wepkeylen2_set(num,F)
	F.wepkeylen2.value=F.wepkeylen2.options[num].value;
	if(F.wepkeylen2.value==1)
		weplen2_64();
	if(F.wepkeylen2.value==2)
		weplen2_128();
function  wepkeylen3_set(num,F)
	F.wepkeylen3.value=F.wepkeylen3.options[num].value;
	if(F.wepkeylen3.value==1)
		weplen3_64();
	if(F.wepkeylen3.value==2)
		weplen3_128();
function  wepkeylen4_set(num,F)
	F.wepkeylen4.value=F.wepkeylen4.options[num].value;
	if(F.wepkeylen4.value==1)
		weplen4_64();
	if(F.wepkeylen4.value==2)
		weplen4_128();
function init()
		var N1=document.wireless_ap_config.wfMode1.selectedIndex;
		var N2=document.wireless_ap_config.wfMode2.selectedIndex;
		var N3=document.wireless_ap_config.wfMode3.selectedIndex;
		var N4=document.wireless_ap_config.wfMode4.selectedIndex;
		var M1=document.wireless_ap_config.wepAuth1.selectedIndex;
		var M2=document.wireless_ap_config.wepAuth2.selectedIndex;
		var M3=document.wireless_ap_config.wepAuth3.selectedIndex;
		var M4=document.wireless_ap_config.wepAuth4.selectedIndex;
		document.wireless_ap_config.wfMode1.value=document.wireless_ap_config.wfMode1.options[N1].value;
		document.wireless_ap_config.wfMode2.value=document.wireless_ap_config.wfMode2.options[N2].value;
		document.wireless_ap_config.wfMode3.value=document.wireless_ap_config.wfMode3.options[N3].value;
		document.wireless_ap_config.wfMode4.value=document.wireless_ap_config.wfMode4.options[N4].value;
		document.wireless_ap_config.wepAuth1.value=document.wireless_ap_config.wepAuth1.options[M1].value;
		document.wireless_ap_config.wepAuth2.value=document.wireless_ap_config.wepAuth2.options[M2].value;
		document.wireless_ap_config.wepAuth3.value=document.wireless_ap_config.wepAuth3.options[M3].value;
		document.wireless_ap_config.wepAuth4.value=document.wireless_ap_config.wepAuth4.options[M4].value;
	if(document.wireless_ap_config.wfMode1.value==1)
		wfMode1_WEP();
	else if(document.wireless_ap_config.wfMode1.value==2)
		{wfMode1_WAP();}
	else
		wfMode1_open();
	if(document.wireless_ap_config.wfMode2.value==1)
		wfMode2_WEP();
	else if(document.wireless_ap_config.wfMode2.value==2)
		{wfMode2_WAP();}
	else
		wfMode2_open();
	if(document.wireless_ap_config.wfMode3.value==1)
		wfMode3_WEP();
	else if(document.wireless_ap_config.wfMode3.value==2)
		{wfMode3_WAP();}
	else
		wfMode3_open();
	if(document.wireless_ap_config.wfMode4.value==1)
		wfMode4_WEP();
	else if(document.wireless_ap_config.wfMode4.value==2)
		{wfMode4_WAP();}
	else
		wfMode4_open();
	return true;
function CheckHex(str)
   	var rc=true;
   	//try{
	    if (str+"" == "undefined" || str == null){
	            rc=false;
	    }
		else {
	        for(i=0;i<str.length;i++)
	        {
	                if(str.charAt(i)<'0'||(str.charAt(i)>'9' && str.charAt(i)<'A')||(str.charAt(i)>'F' && str.charAt(i)<'a')||str.charAt(i)>'f'){
	                        rc= false;
	                        break;
	                }
	        }
	    }
	catch(ExceptionObj0){
		rc=false;
        return rc;
function check()
	var regExp1 = /^0x/;
	var regExp2 = /^0X/;
	var str11=document.wireless_ap_config.wepkey11.value; 
	var str12=document.wireless_ap_config.wepkey12.value; 
	var str21=document.wireless_ap_config.wepkey21.value; 
	var str22=document.wireless_ap_config.wepkey22.value; 
	var str31=document.wireless_ap_config.wepkey31.value; 
	var str32=document.wireless_ap_config.wepkey32.value; 
	var str41=document.wireless_ap_config.wepkey41.value; 
	var str42=document.wireless_ap_config.wepkey42.value; 
	var strwpa1=document.wireless_ap_config.wpaPSK1.value; 
	var strwpa2=document.wireless_ap_config.wpaPSK2.value; 
	var strwpa3=document.wireless_ap_config.wpaPSK3.value; 
	var strwpa4=document.wireless_ap_config.wpaPSK4.value; 
	//str11
	var N1=document.wireless_ap_config.wfMode1.selectedIndex;
	var N2=document.wireless_ap_config.wfMode2.selectedIndex;
	var N3=document.wireless_ap_config.wfMode3.selectedIndex;
	var N4=document.wireless_ap_config.wfMode4.selectedIndex;
	var M1=document.wireless_ap_config.wepAuth1.selectedIndex;
	var M2=document.wireless_ap_config.wepAuth2.selectedIndex;
	var M3=document.wireless_ap_config.wepAuth3.selectedIndex;
	var M4=document.wireless_ap_config.wepAuth4.selectedIndex;
	var L1=document.wireless_ap_config.wepkeylen1.selectedIndex;
	var L2=document.wireless_ap_config.wepkeylen2.selectedIndex;
	var L3=document.wireless_ap_config.wepkeylen3.selectedIndex;
	var L4=document.wireless_ap_config.wepkeylen4.selectedIndex;
	document.wireless_ap_config.wfMode1.value=document.wireless_ap_config.wfMode1.options[N1].value;
	document.wireless_ap_config.wfMode2.value=document.wireless_ap_config.wfMode2.options[N2].value;
	document.wireless_ap_config.wfMode3.value=document.wireless_ap_config.wfMode3.options[N3].value;
	document.wireless_ap_config.wfMode4.value=document.wireless_ap_config.wfMode4.options[N4].value;
		document.wireless_ap_config.wepAuth1.value=document.wireless_ap_config.wepAuth1.options[M1].value;
		document.wireless_ap_config.wepAuth2.value=document.wireless_ap_config.wepAuth2.options[M2].value;
		document.wireless_ap_config.wepAuth3.value=document.wireless_ap_config.wepAuth3.options[M3].value;
		document.wireless_ap_config.wepAuth4.value=document.wireless_ap_config.wepAuth4.options[M4].value;
	document.wireless_ap_config.wepkeylen1.value=document.wireless_ap_config.wepkeylen1.options[L1].value;
	document.wireless_ap_config.wepkeylen2.value=document.wireless_ap_config.wepkeylen2.options[L2].value;
	document.wireless_ap_config.wepkeylen3.value=document.wireless_ap_config.wepkeylen3.options[L3].value;
	document.wireless_ap_config.wepkeylen4.value=document.wireless_ap_config.wepkeylen4.options[L4].value;
	switch(str11.length)
		case 0:
			if((document.wireless_ap_config.wepkeylen1.value==1)&&(document.wireless_ap_config.wfMode1.value==1))
			{
				alert('SSID1:The WEPkey could not be null!');
				return false;
			}
			else
				break;
		case 5:
			break;
		case 10:
			if(CheckHex(str11))
				break;
			else
			{
				alert('SSID1:64 bit should be 5 ASCII or 10 HEX');
				return false;
			}
		/*
		case 12:
			if ((str11.search(regExp1) == -1)&&(str11.search(regExp2) == -1))
			{
				alert('SSID1:64 bit should be 5 ASCII or 10 HEX');
				return false;
			}
			else
			{
				if(CheckHex(str11.substring(2,12)))
					break;
				else
				{
					alert('SSID1:64 bit should be 5 ASCII or 10 HEX');
					return false;
				}
			}
		*/
		default:
			alert('SSID1:64 bit should be 5 ASCII or 10 HEX');
			return false;
	//str12
	switch(str12.length)
		case 0:
			if((document.wireless_ap_config.wepkeylen1.value==2)&&(document.wireless_ap_config.wfMode1.value==1))
			{
				alert('SSID1:The WEPkey could not be null!');
				return false;
			}
			else
				break;
		case 13:
			break;
		case 26:
			if(CheckHex(str12))
				break;
			else
			{
				alert('SSID1:128 bit should be 13 ASCII or 26 HEX');
				return false;
			}
		/*
		case 28:
			if ((str12.search(regExp1) == -1)&&(str12.search(regExp2) == -1))
			{
				alert('SSID1:128 bit should be 13 ASCII or 26 HEX');
				return false;
			}
			else
			{
				if(CheckHex(str12.substring(2,28)))
					break;
				else
				{	
					alert('SSID1:128 bit should be 13 ASCII or 26 HEX');
					return false;
				}
			}
		*/
		default:
			alert('SSID1:128 bit should be 13 ASCII or 26 HEX');
			return false;
	//str21
	switch(str21.length)
		case 0:
			if((document.wireless_ap_config.wepkeylen2.value==1)&&(document.wireless_ap_config.wfMode2.value==1))
			{
				alert('SSID2:The WEPkey could not be null!');
				return false;
			}
			else
				break;
		case 5:
			break;
		case 10:
			if(CheckHex(str21))
				break;
			else
			{
				alert('SSID2:64 bit should be 5 ASCII or 10 HEX');
				return false;
			}
		/*
		case 12:
			if ((str21.search(regExp1) == -1)&&(str21.search(regExp2) == -1))
			{
				alert('SSID2:64 bit should be 5 ASCII or 10 HEX');
				return false;
			}
			else
			{
				if(CheckHex(str21.substring(2,12)))
					break;
				else
				{
					alert('SSID2:64 bit should be 5 ASCII or 10 HEX');
					return false;
				}
			}
		*/
		default:
			alert('SSID2:64 bit should be 5 ASCII or 10 HEX');
			return false;
			//str22
	switch(str22.length)
		case 0:
			if((document.wireless_ap_config.wepkeylen2.value==2)&&(document.wireless_ap_config.wfMode2.value==1))
			{
				alert('SSID2:The WEPkey could not be null!');
				return false;
			}
			else
				break;
		case 13:
			break;
		case 26:
			if(CheckHex(str22))
				break;
			else
			{
				alert('SSID2:128 bit should be 13 ASCII or 26 HEX');
				return false;
			}
		/*
		case 28:
			if ((str22.search(regExp1) == -1)&&(str22.search(regExp2) == -1))
			{
				alert('SSID2:128 bit should be 13 ASCII or 26 HEX');
				return false;
			}
			else
			{
				if(CheckHex(str22.substring(2,28)))
					break;
				else
				{	
					alert('SSID2:128 bit should be 13 ASCII or 26 HEX');
					return false;
				}
			}
		*/
		default:
			alert('SSID2:128 bit should be 13 ASCII or 26 HEX');
			return false;
	//str31
	switch(str31.length)
		case 0:
			if((document.wireless_ap_config.wepkeylen3.value==1)&&(document.wireless_ap_config.wfMode3.value==1))
			{
				alert('SSID3:The WEPkey could not be null!');
				return false;
			}
			else
				break;
		case 5:
			break;
		case 10:
			if(CheckHex(str31))
				break;
			else
			{
				alert('SSID3:64 bit should be 5 ASCII or 10 HEX');
				return false;
			}
		/*
		case 12:
			if ((str31.search(regExp1) == -1)&&(str31.search(regExp2) == -1))
			{
				alert('SSID3:64 bit should be 5 ASCII or 10 HEX');
				return false;
			}
			else
			{
				if(CheckHex(str31.substring(2,12)))
					break;
				else
				{
					alert('SSID3:64 bit should be 5 ASCII or 10 HEX');
					return false;
				}
			}
		*/
		default:
			alert('SSID3:64 bit should be 5 ASCII or 10 HEX');
			return false;
	//str32
	switch(str32.length)
		case 0:
			if((document.wireless_ap_config.wepkeylen3.value==2)&&(document.wireless_ap_config.wfMode3.value==1))
			{
				alert('SSID3:The WEPkey could not be null!');
				return false;
			}
			else
				break;
		case 13:
			break;
		case 26:
			if(CheckHex(str32))
				break;
			else
			{
				alert('SSID3:128 bit should be 13 ASCII or 26 HEX');
				return false;
			}
		/*
		case 28:
			if ((str32.search(regExp1) == -1)&&(str32.search(regExp2) == -1))
			{
				alert('SSID3:128 bit should be 13 ASCII or 26 HEX');
				return false;
			}
			else
			{
				if(CheckHex(str32.substring(2,28)))
					break;
				else
				{	
					alert('SSID3:128 bit should be 13 ASCII or 26 HEX');
					return false;
				}
			}
		*/
		default:
			alert('SSID3:128 bit should be 13 ASCII or 26 HEX');
			return false;
	//str41
	switch(str41.length)
		case 0:
			if((document.wireless_ap_config.wepkeylen4.value==1)&&(document.wireless_ap_config.wfMode4.value==1))
			{
				alert('SSID4:The WEPkey could not be null!');
				return false;
			}
			else
				break;
		case 5:
			break;
		case 10:
			if(CheckHex(str41))
				break;
			else
			{
				alert('SSID4:64 bit should be 5 ASCII or 10 HEX');
				return false;
			}
		/*
		case 12:
			if ((str41.search(regExp1) == -1)&&(str41.search(regExp2) == -1))
			{
				alert('SSID4:64 bit should be 5 ASCII or 10 HEX');
				return false;
			}
			else
			{
				if(CheckHex(str41.substring(2,12)))
					break;
				else
				{
					alert('SSID4:64 bit should be 5 ASCII or 10 HEX');
					return false;
				}
			}
		*/
		default:
			alert('SSID4:64 bit should be 5 ASCII or 10 HEX');
			return false;
	//str42
	switch(str42.length)
		case 0:
			if((document.wireless_ap_config.wepkeylen4.value==2)&&(document.wireless_ap_config.wfMode4.value==1))
			{
				alert('SSID4:The WEPkey could not be null!');
				return false;
			}
			else
				break;
		case 13:
			break;
		case 26:
			if(CheckHex(str42))
				break;
			else
			{
				alert('SSID4:128 bit should be 13 ASCII or 26 HEX');
				return false;
			}
		/*
		case 28:
			if ((str42.search(regExp1) == -1)&&(str42.search(regExp2) == -1))
			{
				alert('SSID4:128 bit should be 13 ASCII or 26 HEX');
				return false;
			}
			else
			{
				if(CheckHex(str42.substring(2,28)))
					break;
				else
				{	
					alert('SSID4:128 bit should be 13 ASCII or 26 HEX');
					return false;
				}
			}
		*/
		default:
			alert('SSID4:128 bit should be 13 ASCII or 26 HEX');
			return false;
	if(strwpa1.length==0)
		if(document.wireless_ap_config.wfMode1.value==2)
			alert('SSID1:WPA-PSK could not be null!');
			return false;
	if(strwpa2.length==0)
		if(document.wireless_ap_config.wfMode2.value==2)
			alert('SSID2:WPA-PSK could not be null!');
			return false;
	if(strwpa3.length==0)
		if(document.wireless_ap_config.wfMode3.value==2)
			alert('SSID3:WPA-PSK could not be null!');
			return false;
	if(strwpa4.length==0)
		if(document.wireless_ap_config.wfMode4.value==2)
			alert('SSID4:WPA-PSK could not be null!');
			return false;
	return true;
</SCRIPT>
<meta http-equiv="Content-Type" content="text/html; charset=gb2312">
</head>
<body onLoad=init()>
<p align="center"><br><br><br><br>
  <span class="style4">Wireless Access Point Configuration</span><br>
</p>
<div align="center">
<form name="wireless_ap_config" action="wireless_ap_config.html" method="post" onSubmit="return check();javascript:self.refresh()" onReset="return init();javascript:self.refresh();">
  <table width="636" height="602"  border="1" align="center" bordercolor="#999999">
    <tr bordercolor="#999999">
      <td width="45">&nbsp;</td>
      <td width="151"><div align="center"><strong>WiFi Work Mode:</strong></div></td>
      <td width="113"><div align="center"><strong>Param Type:</strong></div></td>
      <td height="25" colspan="2"><div align="center"><strong>Params</strong>:</div></td>
    </tr>
    <tr bordercolor="#999999">
      <td rowspan="5"><div align="center"><strong>SSID1:</strong></div></td>
      <td>
      <div align="left">      </div>        <div align="center"><strong>SSID:</strong></div></td>
      <td height="25" colspan="3" nowrap>        <div align="center">
          <input name="ssid1" type="text" VALUE="$%ssid1#$" size="32" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td rowspan="4" bordercolor="#999999">
        <div align="center">
            <p>WiFi Work Mode:
              <select name="wfMode1" size="1"  onChange=wfMode1_set(this.form.wfMode1.selectedIndex,this.form)>
                  <option value=0 $%SELECTED(wfMode1,0)#$ >OPEN</option>
                  <option value=1 $%SELECTED(wfMode1,1)#$ >WEP</option>
                  <option value=2 $%SELECTED(wfMode1,2)#$ >WPA</option>
              </select>
          </p>
      </div>
         </td>
      <td rowspan="3" bordercolor="#999999"><div align="center">WEP Auth:      </div>
        <div align="center">
            <select name="wepAuth1" size="1" >
              <!--onChange=wepAuth1_set(this.form.wepAuth1.selectedIndex,this.form) -->
              <option value=0 $%SELECTED(wepAuth1,0)#$ >Open key</option>
              <option value=1 $%SELECTED(wepAuth1,1)#$ >Shared key</option>
            </select>
      </div>       </td>
      <td width="81" rowspan="3" bordercolor="#999999"><div align="center">Key Index
          <select name="index1" size="1" >
            <option value=1 $%SELECTED(index1,1)#$>1</option>
            <option value=2 $%SELECTED(index1,2)#$>2</option>
            <option value=3 $%SELECTED(index1,3)#$>3</option>
            <option value=4 $%SELECTED(index1,4)#$>4</option>
          </select>
      </div></td>
      <td width="212" height="28" bordercolor="#999999"><div align="center">          
	    <select name="wepkeylen1" size="1" onChange=wepkeylen1_set(this.form.wepkeylen1.selectedIndex,this.form) >
            <option value=1 $%SELECTED(wepkeylen1,1)#$ >64bit(5 ASCII or 10 HEX)</option>
            <option value=2 $%SELECTED(wepkeylen1,2)#$ >128bit(13 ASCII or 26 HEX)</option>
          </select>
      </div>       </td>
    </tr>
    <tr>
      <td height="26" bordercolor="#999999"><div align="center">64bit:
          <input name="wepkey11" type="text" value="$%wepkey11#$" size="20" maxlength="10">
      </div></td>
    </tr>
    <tr>
      <td height="25" bordercolor="#999999"><div align="center">128bit: 
          <input name="wepkey12" type="text" value="$%wepkey12#$" size="20" maxlength="26">
      </div></td>
    </tr>
    <tr>
      <td height="25" nowrap bordercolor="#999999">        <div align="center">
          <strong>WPA-PSK:</strong>
      </div></td>
      <td height="25" colspan="2" nowrap bordercolor="#999999"><div align="center">
        <input name="wpaPSK1" type="text" VALUE="$%wpaPSK1#$" size="32" maxlength="63">
      </div></td>
    </tr>
    <tr bordercolor="#999999">
      <td rowspan="5"><div align="center"><strong>SSID2:</strong></div></td>
      <td bordercolor="#999999">
      <div align="left">      </div>        <div align="center"><strong>SSID:</strong></div></td>
      <td height="25" colspan="3" nowrap bordercolor="#999999">        <div align="center">
          <input name="ssid2" type="text" value="$%ssid2#$" size="32" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td rowspan="4" bordercolor="#999999">
        <div align="center">WiFi Work Mode:
<select name="wfMode2" size="1"  onChange=wfMode2_set(this.form.wfMode2.selectedIndex,this.form)>
                  <option value=0 $%SELECTED(wfMode2,0)#$ >OPEN</option>
                  <option value=1 $%SELECTED(wfMode2,1)#$ >WEP</option>
                  <option value=2 $%SELECTED(wfMode2,2)#$ >WPA</option>
          </select>
      </div>
             </td>
      <td rowspan="3"><div align="center">WEP Auth: </div>        <div align="center">
          <select name="wepAuth2" size="1" >
            <!--onChange=wepAuth2_set(this.form.wepAuth2.selectedIndex,this.form) -->
              <option value=0 $%SELECTED(wepAuth2,0)#$ >Open key</option>
              <option value=1 $%SELECTED(wepAuth2,1)#$ >Shared key</option>
          </select>
        </div></td>
      <td width="81" rowspan="3" bordercolor="#999999"><div align="center">Key Index
              <select name="index2" size="1" >
            <option value=1 $%SELECTED(index2,1)#$>1</option>
            <option value=2 $%SELECTED(index2,2)#$>2</option>
            <option value=3 $%SELECTED(index2,3)#$>3</option>
            <option value=4 $%SELECTED(index2,4)#$>4</option>
              </select>
      </div></td>
      <td height="25" bordercolor="#999999">        <div align="center">
        <select name="wepkeylen2" size="1" onChange= wepkeylen2_set(this.form.wepkeylen2.selectedIndex,this.form) >
            <option value=1 $%SELECTED(wepkeylen2,1)#$ >64bit(5 ASCII or 10 HEX)</option>
            <option value=2 $%SELECTED(wepkeylen2,2)#$ >128bit(13 ASCII or 26 HEX)</option>
        </select>
      </div>        </td>
    </tr>
    <tr>
      <td height="25" bordercolor="#999999"> <div align="center">64bit:
          <input name="wepkey21" type="text" value="$%wepkey21#$" size="20" maxlength="10">
      </div></td>
    </tr>
    <tr>
      <td height="25" bordercolor="#999999"><div align="center">128bit:
          <input name="wepkey22" type="text" value="$%wepkey22#$" size="20" maxlength="26">
      </div></td>
    </tr>
    <tr>
      <td height="25" nowrap bordercolor="#999999">        <div align="center"><strong>WPA-PSK:</strong>
      </div></td>
      <td height="25" colspan="2" nowrap bordercolor="#999999"><div align="center">
        <input name="wpaPSK2" type="text" VALUE="$%wpaPSK2#$" size="32" maxlength="63">
      </div></td>
    </tr>
    <tr bordercolor="#999999">
      <td rowspan="5"><div align="center"><strong>SSID3:</strong></div></td>
      <td>
           <div align="center"><strong>SSID:</strong></div></td>
      <td height="25" colspan="3" nowrap>        <div align="center">
          <input name="ssid3" type="text" value="$%ssid3#$" size="32" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td rowspan="4" bordercolor="#999999">
        <div align="center">WiFi Work Mode:
<select name="wfMode3" size="1"  onChange=wfMode3_set(this.form.wfMode3.selectedIndex,this.form)>
                  <option value=0 $%SELECTED(wfMode3,0)#$ >OPEN</option>
                  <option value=1 $%SELECTED(wfMode3,1)#$ >WEP</option>
                  <option value=2 $%SELECTED(wfMode3,2)#$ >WPA</option>
          </select>
      </div></td>
      <td rowspan="3"><div align="center">WEP Auth: </div>        <div align="center">
          <select name="wepAuth3" size="1" >
            <!--onChange=wepAuth3_set(this.form.wepAuth3.selectedIndex,this.form) -->
              <option value=0 $%SELECTED(wepAuth3,0)#$ >Open key</option>
              <option value=1 $%SELECTED(wepAuth3,1)#$ >Shared key</option>
          </select>
        </div></td>
      <td width="81" rowspan="3" bordercolor="#999999"><div align="center">Key Index
              <select name="index3" size="1" >
            <option value=1 $%SELECTED(index3,1)#$>1</option>
            <option value=2 $%SELECTED(index3,2)#$>2</option>
            <option value=3 $%SELECTED(index3,3)#$>3</option>
            <option value=4 $%SELECTED(index3,4)#$>4</option>
              </select>
      </div></td>
      <td height="25" bordercolor="#999999">
          <div align="center">
        <label>
        <select name="wepkeylen3" size="1" onChange= wepkeylen3_set(this.form.wepkeylen3.selectedIndex,this.form)-->
            <option value=1 $%SELECTED(wepkeylen3,1)#$ >64bit(5 ASCII or 10 HEX)</option>
            <option value=2 $%SELECTED(wepkeylen3,2)#$ >128bit(13 ASCII or 26 HEX)</option>
        </select>
</label>
      </div>        </td>
    </tr>
    <tr>
      <td height="25" bordercolor="#999999"><div align="center">64bit:
          <input name="wepkey31" type="text" value="$%wepkey31#$" size="20" maxlength="10">
      </div></td>
    </tr>
    <tr>
      <td height="25" bordercolor="#999999"><div align="center">
          <label>128bit:</label>
          <input name="wepkey32" type="text" value="$%wepkey32#$" size="20" maxlength="26">      
      </div></td>
    </tr>
    <tr>
      <td>
          <div align="center"><strong>WPA-PSK:</strong></div></td>
      <td height="25" colspan="2" nowrap bordercolor="#999999"><div align="center">
        <input name="wpaPSK3" type="text" VALUE="$%wpaPSK3#$" size="32" maxlength="63">
      </div></td>
    </tr>
    <tr bordercolor="#999999">
      <td rowspan="5"><div align="center"><strong>SSID4:</strong></div></td>
      <td bordercolor="#999999">
            <div align="center"><strong>SSID:</strong></div></td>
      <td height="25" colspan="3" nowrap bordercolor="#999999">        <div align="center">
          <input name="ssid4" type="text" value="$%ssid4#$" size="32" maxlength="32">
      </div></td>
    </tr>
    <tr>
      <td rowspan="4" bordercolor="#999999">
        <div align="center">WiFi Work Mode:
<select name="wfMode4" size="1"  onChange=wfMode4_set(this.form.wfMode4.selectedIndex,this.form)>
                  <option value=0 $%SELECTED(wfMode4,0)#$ >OPEN</option>
                  <option value=1 $%SELECTED(wfMode4,1)#$ >WEP</option>
                  <option value=2 $%SELECTED(wfMode4,2)#$ >WPA</option>
          </select>
      </div>
              </td>
      <td rowspan="3"><div align="center">WEP Auth: </div>        <div align="center">
          <select name="wepAuth4" size="1" >
            <!--onChange=wepAuth4_set(this.form.wepAuth4.selectedIndex,this.form) -->
              <option value=0 $%SELECTED(wepAuth4,0)#$ >Open key</option>
              <option value=1 $%SELECTED(wepAuth4,1)#$ >Shared key</option>
          </select>
        </div></td>
      <td width="81" rowspan="3" bordercolor="#999999"><div align="center">Key Index
              <select name="index4" size="1" >
            <option value=1 $%SELECTED(index4,1)#$>1</option>
            <option value=2 $%SELECTED(index4,2)#$>2</option>
            <option value=3 $%SELECTED(index4,3)#$>3</option>
            <option value=4 $%SELECTED(index4,4)#$>4</option>
              </select>
      </div></td>
      <td height="25" bordercolor="#999999">        <div align="center">
        <select name="wepkeylen4" size="1" onChange=wepkeylen4_set(this.form.wepkeylen4.selectedIndex,this.form) >
            <option value=1 $%SELECTED(wepkeylen4,1)#$ >64bit(5 ASCII or 10 HEX)</option>
            <option value=2 $%SELECTED(wepkeylen4,2)#$ >128bit(13 ASCII or 26 HEX)</option>
        </select>
          </div>        
      </td>
    </tr>
    <tr>
      <td height="25" bordercolor="#999999"><div align="center">64bit:
          <input name="wepkey41" type="text"value="$%wepkey41#$" size="20" maxlength="10">
      </div></td>
    </tr>
    <tr>
      <td height="29" bordercolor="#999999"> <div align="center">128bit:
          <input name="wepkey42" type="text" value="$%wepkey42#$" size="20" maxlength="26">
      </div></td>
    </tr>
    <tr>
      <td height="26" nowrap bordercolor="#999999">        <div align="center">
          <strong>WPA-PSK:</strong>
      </div></td>
      <td height="26" colspan="2" nowrap bordercolor="#999999"><div align="center">
        <input name="wpaPSK4" type="text" VALUE="$%wpaPSK4#$" size="32" maxlength="63">
      </div></td>
    </tr>
  </table>
  <p>&nbsp;</p>
  <p align="center">
    <input type="submit"  value="submit" align="center">
    
</p>  
</form>
</body>
</html>
GIF89a
:P)d
GIF89a
GIF89a
NgX>OE
l [6M
c8^F<aJ
f1|L1{Ln
xxxwwwvvvrrrpppooocccXXXWWWIIIFFF@@@:::
vM|uq
HV$2
Z}5Q
+[;T
pMO&
}L-+
)qB)oXb\
PJ$td
>.3)#L
F(	Sy
b?CK
j&_pC
1pmO
#B)(o
k=McSTj+mA
*Eir1
s6_,D
XSw->
LlK4
XgoX
QhZS
[z>v
)w==s4
y~f}
wq]G
k68o
:szYP
|RHo
3f(,D
;vS2
vW$7
(pXt3
 q"&
`IV{
7JY/
Z[T?ni?
[z#]
GIF89ap
P B,}
&5ze 0	
0:1?
>?*'
	@R!
5d|` 
V5F|+
(81S
j&L7
^a,p
3r3B
'(&P
o_<pN
1na2B
!	4@
JP<>
L@-F8
>A4"
=-(n
X@1/
2"\@
@)T]^q
,`>H
0@hTP`
WindMark(%s) set attempt failed. errno: %08x
unable to store error message for %s
1 WindMark(%s) read attempt failed. errno: %08x
Location
<HTML><BODY>
redirected to %s
click <a href="%s">here </a>
if your browser doesn't redirect you automatically
</BODY></HTML>
1 text/html
<CENTER><H1>Post received</H1></CENTER>
<HR><H3>The following WMB access errors were encountered:</H3>
<B>%s</B> <FONT COLOR="red">%s</FONT><BR>
</HTML></BODY>
<HR><H2>Post failed!</H2>
The transmitted file was not stored on the server
1 p@-
(p@-
(0@-
no backplane db
object not found
wmbtLock: Bad Object Pointer
1 wmbUnlock: Bad Object Pointer
wmbObjectLock: No Entry Pointer
1 wmbTableLevelLock: Table not found
1 wmbComponentLevelLock: Component not found
2 wmbWindMarkLevelUnlock: No Entry Pointer
wmbWindMarkLevelUnlock: no lock head
2 wmbTableLevelUnlock: Table not found
2 wmbComponentLevelUnlock: Component not found
wmbComponentLevelUnlock: no lock
wmmOidLoad: bad entry
wmbTableColumnCreate: no memory
wmbTableParse: bad OID entry
no memory
wmbTableRowNext: bad table
wmbTableRowNext: no index
wmbTableRowNext: bad handler
wmbTableRowNext: handler failed
no difference
2 wmbTableCreate: bad session
wmbTableCreate: no multiple tables
wmbTableCreate: no memory
wmbTableCreate: no index obj
no table available
wmbTableDestroy: invalid table
wmbTableTitles: bad table
%%%ds 
2 wmbTableRowPrint: bad table
2 wmbTablePrint: bad table
2 0@-
MUD requires a non-NULL error handler
MUD requires a non-NULL connection handler
MUD requires maxActiveCons > 0
unable to allocate memory for MUD
pipe_mud%d
unable to allocate memory for MUD managed memory pool
unable to create MUD managed memory pool
unable to create MUD connection array
unable to allocate memory for MUD internal structures
unable to allocate mem for MUD managed memory pool
MUD semaphore creation failed
mudCreate: Problems creating the main socket
mud%d_%d
Could not open MUD named pipe
(2 h
2 Attempt to register an invalid initialization handler or MUD
h$2 attempted to start an invalid mud
$2 unable to spawn stop task
92 @%2 unable to delete MUD managed memory pool
%2 p@-
unable to open pipe
Assertion failed: activeCon, file Z:/wfplt/src/protocol/webserver/pubsrc/common/mudLib.c, line 630
Assertion failed: mud->connHandler, file Z:/wfplt/src/protocol/webserver/pubsrc/common/mudLib.c, line 631
(2 unable to take the lead semaphore
mudWaitOnData: Error on mask
wmosSocketGroupWait returned unrecognized error
unable to determine which socket unblocked the thread
*2 0*2 
*2 P*2 
error handler returned illegal value
x-2 error on socket while probing for data
.2 Assertion failed: ioCurrentConId->sockHandle, file Z:/wfplt/src/protocol/webserver/pubsrc/common/mudLib.c, line 976
t/2 could not turn off blocking on socket
could not accept new connection
could not turn on blocking on socket
t12 
12 mud attempt to close a connection twice
could not take connection array semaphore
could not close socket
22  32 L32 0@-
 32 0@-
 32 busy
idle
free
????
p%d:%s sk:%d --
52 p@-
t12 
12 null connection or environment
invalid attempt to free temporary memory
invalid attempt to free permanent memory
72 j
unable to send mud signal
92 ?
unable to read mud signal
 n;^
Qkkbal
i]Wb
9a&g
MGiI
wn>Jj
#.zf
+o*7
:2 1.1.4
%c%c%c%c%c%c%c%c%c%c
<fd:%d>
B2 p@-
(p@-
(0@-
O2 Authorization
P2 WWW-Authenticate
P2 AUTH_TYPE
P2 P
U2 INFO(): %s
HU2 INFO(): 
xU2 
U2 0@-
unable to write to socket
 V2 %x
V2  V2 
V2 unable to peek at socket
DW2 
httpPrintf failed
X2 Bad HTTP_REQ
unable to get client socket address
%u.%u.%u.%u
%x:%x:%x:%x:%x:%x:%x:%x
unknown IP address type
dY2 tY2 
Y2 function deprecated
[2 c
[2 c
[2 c
[2 *
(Content-Encoding
|^2 
|^2 
|^2 Content-Length
^2 %ld
$_2 
^2 Content-Type
_2 HTTP/1.1 %d %s
Transfer-Encoding
chunked
l`2 
- text/html
<P></P><HR><H2>Transfer interrupted!</H2>
<H1>Server Error: %d %s</H1>
Operating System Error Nr:%d: %s 
<P><HR><H2>%s</H2><P>
<P><HR><H1>%s</H1><P>
`2 T
a2 4a2 Ta2 xa2 
a2 x
- Server: %s
Content-Length
Connection: 
Keep-Alive
Keep-Alive:
Persist:
close
Set-Cookie: %s=%s
%s: %s
c2 x
c2 $c2 4c2 Xc2 `c2 tc2 
c2 0@-
endTable
createTable
endRow
REPEAT
(invalid parameters
could not alloc REPEAT stack
could not alloc IF stack
f2 called httpMacroInit() yet?
h2 (
unable to locate macro parameters
BEGIN
ELSE
parseVar: out of mem -- increase request part size
Pl2 Xl2 \l2 dl2 
h2 hl2 ll2 pl2 tl2 xl2 |l2 
l2  
y2 4y2 
x2 X0
z2 (z2 
y2 \
run out of internal buffer.  increase kCreateTableIncColsLength
wmbTableCreate returned error %0x
wmbTableCreate() failed
z2 dl2 
z2 wmbTableDestroy  failed (errno=%0x)
2 no memory
wmbLockRelease: Lock status is not granted
wmbLockAddNew: no memory
wmbLockAddNew: Intent mode incompatible
2 wmbLockRemove: Lock not found
2  deflate 1.1.4 Copyright 1995-2002 Jean-loup Gailly 
1.1.4
2 0@-
								
(0@-
2 p@-
2 0@-
	(`Y
	(`Y
	(`Y
(p@-
(0@-
(0@-
: %s
E_NO_SYS_RESOURCE
E_ACCESS_DENIED
E_SYS_CALL_FAIL
E_INVALID_PARAM
E_SKT_ALREADY_EXIST
E_TRY_ANOTHER_SRC_PORT
E_NO_ONE_LISTENS
E_NOT_CONN
E_INTERNAL
E_NET_UNREACHABLE
E_CONN_ALREADY_EXIST
E_DUPLICATE_ATTEMPT
E_SKT_CLOSED
ERR: UNKNOWN ERR
(0@-
(0@-
(0@-
(Assertion failed: cookie != 0, file C:/IPPhone/hcl/CAPI/VxWorks-CAPI/src/osapi_timer.c, line 147
Assertion failed: TimerFreeListHead->TimerStat == TIMER_IDLE, file C:/IPPhone/hcl/CAPI/VxWorks-CAPI/src/osapi_timer.c, line 148
Assertion failed: TimerFreeListHead->Period == 0, file C:/IPPhone/hcl/CAPI/VxWorks-CAPI/src/osapi_timer.c, line 149
Assertion failed: 0, file C:/IPPhone/hcl/CAPI/VxWorks-CAPI/src/osapi_timer.c, line 280
(0@-
ERROR:Failed to create socket !
WARNING:<new_and_bind_socket>bind socket!%d
WARNING: <new_and_bind_socket>port cannot be reused.%d
3 the address of STUN server is too longer!!
(stun_parse_server_name return error!
stun_parse_client_name return error!
%d.%d.%d.%d
3 begin query_stun_lifetime_api.
 the lifte time is too short.
end of query_stun_lifetime_api() gStunConfig.liveTime = %d
(get_mappedPort(),there isn't the orignal port! origPort=%d
WARNING: <keep_address_mapping>bind failed %d
ERROR:<keep_address_mapping> sendto failed.
hmac-not-implemented
bind error! port:%d
3 stun_parse_hostname() host =%s 
stun_parse_hostname()  error
port:%d
 addr:%d.%d.%d.%d
3 stun_parse_server_name input error
3 stun_parse_client_name input error
stun_parse_client_name input port 0, use random port
client :
port:%d
 addr:%d.%d.%d.%d
 testNum input error
send message error!
\(3 `(3 |(3 
(3 \(3 \(3 
(3 \(3 
l'3 
QReceived a message that was too large!
33 $43 l43 
43 D53 
53 863 
73 073 
Some problem opening port/interface to send on!
select return error
get message error!
StunTypeConeNat
StunTypeRestrictedNat
StunTypePortRestrictedNat
StunTypeSymNat
StunTypeOpen
StunTypeSymFirewall
StunTypeBlocked
StunTypeUnknown
@3 \A3 \A3 \A3 \A3 \A3 \A3 $@3 $A3 
$83 X83 p83 
93 stun_parse_server_name return error!
stun_parse_client_name return error!
0C3 XC3 stun_query_by_IPAddr() the type of nat is:%d
tD3 StunTypeFailure
F3 h
93 <E3 
Q NAT lifetime test %d
lifetime send test I
lifetime send test II
lifetime test I received
lifetime test II received
G3 X83 
G3 p83 
G3 set low : %d
set upper : %d
At the beginning, upper : %d   low : %d
-----upper : %d low : %d
0C3 XC3 $83 
L3 ,L3 XL3  life time: %d
 P3 ATELog: 
lP3 ERROR: ioctl for FIOGETNAME is not supported
COM port name: %s
Q3 ATETask 
ERROR: AteTaskInit - Could not spawn ATETask !!!
SUCCESS
(PY3 
Q3 T
Q3 ERROR deleting ATETask, error = %d
R3 ERROR opening common port %s
ATE Comm port fd: %d
Can not close console
((S3 
S3 @S3 consoleFd = %d
T3 ERROR writing to comm port
SUCCESS writing %d bytes to comm port !!!!!!!
ATE write %d bytes to comm port
T3  U3 ERROR reading from comm port
(tShell
tShell TID: 0x%x
tShell task can not be suspended
tShell task successfully suspended
tLogTask
tLogTask task can not be suspended
V3 L
W3 P
((W3 ERROR resuming shell task
ERROR resuming tLogTask task
X3 P
((X3 ERROR: Can not get name of comm port
Commfd = %d
ERROR reading from SIO!!!
ERROR: Communication protocol not supported
AteTask exiting
X3 X
Y3 <Y3 Line:
(utils:tftp event=%d
utils:   msg type is: %d
utils:   msg data is: %d
a3  b3 
c3 <b3 Lb3 Xb3 
c3 |b3 
b3 g0
@U	(T0
(@U	(
@U	(`
(@U	(
	(0@-
	(06
	(06
,.:;?!*#"'~/%&@$()<>
abcABC#
defDEF#
ghiGHI#
jklJKL#
mnoMNO#
pqrsPQRS#
tuvTUV#
wxyzWXYZ#
abcABC
defDEF
ghiGHI
jklJKL#
mnoMNO
pqrsPQRS#
tuvTUV
wxyzWXYZ#
abcABC
defDEF
ghiGHI
jklJKL#
mnoMNO
pqrsPQRS#
tuvTUV
wxyzWXYZ#
abcABC
defDEF
ghiGHI
jklJKL#
mnoMNO
pqrsPQRS#
tuvTUV
wxyzWXYZ#
abcABC
defDEF
ghiGHI#
jklJKL#
mnoMNO
	pqrsPQRS
tuvTUV
wxyzWXYZ#
abcABC
defDEF
ghiGHI
jklJKL#
mnoMNO
pqrsPQRS#
tuvTUV
wxyzWXYZ#
abcABC
defDEF
ghiGHI
jklJKL#
mnoMNO
pqrsPQRS#
tuvTUV
wxyzWXYZ#
($w3 
 5 p@-
Qp@-
(v3 (v3 (v3 (v3 (v3 (v3 (v3 
v3 0u3 
T	(CCE
CCE malloc 5k memory fail!!!!!!!!!!!!!!!!!!!!
( {3 px3 
ty3 
z3 (y3 Ly3 
t}3 t}3 t}3 t}3 t}3 t}3 t}3 
}3 T}3 d}3 
(0@-
3 u 
gfff0@-
(0@-
m3 gfff
3 X7
	(@\
3 u`
3 `0
(0@-
3 `0
(0@-
!n3 
o3 jp3 
@U	(`
(p@-
@U	(`
ENTITY
Return to IDLE_STANDBY error!
abc2
def3
ghi4
jkl5
mno6
pqrs7
tuv8
wxyz9
jkl5
pqrs7
wxyz9
jkl5
pqrs7
wxyz9
jkl5
pqrs7
wxyz9
u4 P
Q4 `K4 
3 dH4 
(p@-
(H"	(
(@U	( R
(p@-
(0@-
P4 8Q4 XQ4 
$T4 $T4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 hY4 pU4 hY4 
S4 hY4 
W4 hY4 hY4 hY4 hY4 hY4 <S4 <S4 <S4 <S4 <S4 <S4 <S4 <S4 <S4 <S4 
(H"	(
(p@-
[4 :
]4 p@-
_4 @
d4 ,d4 Hd4 E0
Pk4 
k4 Hk4 
k4  k4 (k4 0k4 8k4 @k4 
pw4 
x4 Dx4 
Pz4 `z4 Pz4 Xz4 Pz4 Xz4 Pz4 Pz4 Xz4 Pz4 Xz4 Pz4 
{4 X|4 1
{4 D|4 X|4 0
|4 X|4 D|4 X|4 
x~4 P
4 x~4 
~4 x~4 
~4 x~4 x~4 
~4 x~4 
~4 x~4 
(p@-
4 0@-
4 0@-
<MENU>
 Before call GetDhcpType from menu. 
4 0@-
(@U	(0@-
@U	(`
@U	(`
(p@-
@U	(`
(p@-
(@U	(
@U	(
4 0@-
4 E@
4 0@-
4 @U	(l
4 @U	(l
4 p@-
4 06
4 p@-
@U	(
d3 `
4 ,B
4 XB
3 Xo
 !"#
%&'()*+,-./0123456789:;<=>?
ABCDEFGHIJKLMNOPQRSTUVWXYZ
abcdefghijklmnopqrstuvwxyz
`AAAA[
EEIIIID]OOOO\x
UUU^Y
aaa{
iiio}
ooo|
uu~ypy
:I5 
<K5 
LK5 <J5 A
	<	X	
	<	Y	
	<	Z	
	<	[	!	<	\	"	<	]	+	<	^	/	<	_	(	<	)	0	<	1	3	<	4	
XO5 
*!0[
*!0[
XO5 
pK5 8L5 
TK5 
TK5 
TK5 
TK5 
e5 ,f5 `f5 
j5 Hj5 |j5 
gfff
5 01
5 01
h>6 
B6 @?6 d?6 
?6 0@6 T@6 
B6 x@6 
B6 ,A6 
B6 PA6 
B6 tA6 
B6 \B6 
C6  D6 
D6 XE6 
P6 $F6 xF6 
P6 PG6 
P6 <I6 
P6 8J6 
J6 4K6 
K6 LL6 
L6 HM6 
P6  N6 tN6 
P6 pO6 
P6 <P6 `P6 
$Q6 XQ6 
X6  U6 
X6 4X6 PT6 hX6 
X6 $V6 
X6 XV6 
X6 TU6 
X6 (W6 
V6 !
c6 Hc6 
e6 pZ6 |c6 
d6 Hd6 |d6 
d6 Le6 
Y6 tZ6 
e6 <[6 
e6 <Z6 
\6 h\6 0]6 
e6 T`6 
e6 `^6 
e6 ,^6 
e6 (_6 
_6 Hb6 
e6 `^6 
f6 Lf6 
h6 Ti6  i6 
i6 Ph6 
j6 Pj6 
k6 Tk6 
j6  k6 
,m6 
l6 `m6 
l6 \n6 \n6 \n6 \n6 \n6 \n6 0n6 
o6 Lp6 
p6 |o6 
p6 Ho6 
q6 Lq6 
r6 Pr6 
u6  u6 (u6 0u6 8u6 @u6 Hu6 Pu6 Xu6 `u6 hu6 pu6 xu6 
w6  w6 (w6 0w6 8w6 @w6 Hw6 Pw6 Xw6 `w6 hw6 pw6 xw6 
x6 Hx6 Hx6 Hx6 Hx6 Hx6 Hx6 Hx6  x6 (x6 0x6 8x6 @x6 X
pz6 
z6 ,0
{6 ${6 t{6 ${6 t{6 
6  0
6 80
VUUUP	7 
P!7 
47 $47 847 	
77 $77 477 D77 T77 d77 t77 
 ;  
Host
H7 the url result allocation wrong!
http
$I7 
(HI7 /
$I7 
(HI7 
I7 GET
Host: 
GET 
User-Agent: UTStarcom F1000 V
 HTTP/1.1
Accept: */*
Accept-Encoding: deflate
TE: deflate
Connection: TE
Proxy-Connection: Keep-Alive
Connection: TE,Keep-Alive
POST
K7  K7 PK7 
(lK7 
globalNet->server:%s
getFileState: %d 
N7 ip address or url is null!
http method should be GET or POST!
DataSock invalid!
malloc for globalNet error!
J7 lK7  O7 DO7 
(XO7 
M7 go into HTGetHostByName!hostname:%s
go into gethostbyname!
gethostbyname wrong!
(go into HTParseInet!hostname:%s
inet_addr
gethostbyname's status:%d
go into HTDoConnect!
socket make failed!
socket :%d,errno:%d
address:%s
connection failed! errno:%d
 connect result status :%d
 HTDoConnect. WOULD BLOCK
($S7 <S7 HS7 hS7 
S7 go into HTDoClose
go into the HTTPEvent, and the eventtype is %d
go to the http state of HTTP_BEGIN
go into HTTP_CONNECTED!
go into HTEvent_WRITE!
go into HTEvent_READ!
`V7 
X7 `V7 
V7 LW7 hW7 
xU7 
(HTTP
[7 Content-Length
remain:%d
[7  
[7 remain:%d,size:%d
(X\7 
go into HTReader_read!
begin reading!
end reading!
do not read any data,reading failed.
finished reading data
read data successfully.
before push data down the stream.
($^7 4^7 D^7 
(l^7 
(__ctors
_ctors
__dtors
_dtors
`7 `
cplusCtors: can't find module "%s"
0b7 ,>
(hb7 cplusDtors: can't find module "%s"
Lb7 ,>
{7 P
e7 4f7 <f7 Df7 Lf7 Tf7 \f7 df7 lf7 tf7 |f7 
h7 $h7 ,h7 Lh7 Lh7 Lh7 4h7 Lh7 Lh7 Lh7 <h7 Lh7 Lh7 Lh7 Dh7 X
s7 pt7 pt7 pt7 @y7 @y7 $y7 $y7 
x7  {7  {7 
zlib_zcfree
zlib_zcalloc
zlib_z_inflateSyncPoint
zlib_z_inflateSync
zlib_z_inflateSetDictionary
zlib_z_inflateReset
zlib_z_inflateInit_
zlib_z_inflateInit2_
zlib_z_inflateEnd
zlib_z_inflate
zlib_z_get_crc_table
zlib_z_errmsg
zlib_z_deflateSetDictionary
zlib_z_deflateReset
zlib_z_deflateParams
zlib_z_deflateInit_
zlib_z_deflateInit2_
zlib_z_deflateEnd
zlib_z_deflateCopy
zlib_z_deflate
zlib_z_crc32
zlib_z_adler32
zlib_zError
zlib_inflate_set_dictionary
zlib_inflate_mask
zlib_inflate_flush
zlib_inflate_fast
zlib_inflate_codes_new
zlib_inflate_codes
zlib_inflate_blocks_sync_point
zlib_inflate_blocks_reset
zlib_inflate_blocks_new
zlib_inflate_blocks_free
zlib_inflate_blocks
zlib_gzwrite
zlib_gztell
zlib_gzsetparams
zlib_gzseek
zlib_gzrewind
zlib_gzread
zlib_gzputs
zlib_gzputc
zlib_gzprintf
zlib_gzopen
zlib_gzgets
zlib_gzgetc
zlib_gzflush
zlib_gzerror
zlib_gzdopen
zlib_gzclose
zlib_deflate_copyright
zlibVersion
zi8para4Chn
zi8ZYinitialSpelling
zi8ZYfinalSpelling
zi8PYinitialSpelling
zi8PYfinalSpelling
zi8CangjieCodes
zeroin_addr
yyval
yytmp
yystate
yystart
yypv
yyps
yyparse
yynerrs
yylval
yyerrflag
yydebug
yychar
yy_yyv
yy_yys
yEndPixel
yDrawPixel
yCursorPixel
xrealloc
xmalloc
xdelete
xcopy
xattrib
xEndPixel
xDrawPixel
xCursorPixel
www_authenticate_setstale
www_authenticate_setrealm
www_authenticate_setqop_options
www_authenticate_setopaque
www_authenticate_setnonce
www_authenticate_setdomain
www_authenticate_setauth_type
www_authenticate_setalgorithm
www_authenticate_parse
www_authenticate_init
www_authenticate_getstale
www_authenticate_getrealm
www_authenticate_getqop_options
www_authenticate_getopaque
www_authenticate_getnonce
www_authenticate_getdomain
www_authenticate_getauth_type
www_authenticate_getalgorithm
www_authenticate_free
www_authenticate_clone
www_authenticate_2char
wvlanUnlock
wvlanUnload
wvlanStopDriver
wvlanStop
wvlanStart
wvlanSendPort
wvlanSend
wvlanPutLtv
wvlanPollSendPort
wvlanPollSend
wvlanPollReceivePort
wvlanPollReceive
wvlanPcmciaRequestISR
wvlanPcmciaReleaseISR
wvlanMCastAddrGet
wvlanMCastAddrDel
wvlanMCastAddrAdd
wvlanLock
wvlanLoad
wvlanKeyCheck
wvlanIoctl
wvlanIntEnable
wvlanIntDisable
wvlanInit
wvlanISR
wvlanGo
wvlanGetPenguinVersion
wvlanGetHermesVersion
wvlanEndianTranslateMailbox
wvlanEnable
wvlanDisable
wvlanApplyLight
wvlanApply
wvObjIsEnabled
wvInstIsOn
wvEvtClass
wua_ver
wua_validate_script
wua_task
wua_syntax_script
wua_state_processing
wua_snd_uinput_req
wua_set_dft_script
wua_send_wuamsg
wua_send_mmirsp
wua_search_keyword
wua_script_init
wua_run_action
wua_replace_string
wua_rename_script
wua_rename
wua_remove
wua_recover
wua_parse_script
wua_omit_commentsline
wua_match_msgtype
wua_list_free
wua_list_add
wua_lex_script
wua_ins
wua_init_scriptfile
wua_init_ins
wua_init_fsm_tables
wua_init
wua_hndl_xxx
wua_hndl_wuamsg
wua_hndl_uinput_req
wua_hndl_uinput
wua_hndl_post_req
wua_hndl_mmimsg
wua_hndl_get_req
wua_hndl_downloadreq
wua_hndl_authstart
wua_hndl_actscriptreq
wua_handle_script
wua_get_state_ptr
wua_get_scriptfile_info
wua_get_rfrshloc
wua_get_keyword_value
wua_get_dft_script_name
wua_get_dft_script_cont
wua_get_dft_script
wua_fwrite
wua_fsm_update
wua_fsm_fill
wua_free_ins
wua_fread
wua_fopen
wua_fclose
wua_dnld_script
wua_compose_urlenc
wua_backup
wtd_set_task_bit
wtd_no_task_bit
wtd_clr_task_bit
wtd_clr_alltask_bits
writev
write_sip_username
write_sip_password
write_psc
write
wpa_supplicant_scan
wpa_supplicant_rx_eapol
wpa_supplicant_req_scan
wpa_supplicant_req_auth_timeout
wpa_supplicant_reload_configuration
wpa_supplicant_notify_eapol_done
wpa_supplicant_key_request
wpa_supplicant_get_ssid
wpa_supplicant_event
wpa_supplicant_drivers
wpa_supplicant_disassociate
wpa_supplicant_deauthenticate
wpa_supplicant_cancel_scan
wpa_supplicant_cancel_auth_timeout
wpa_status
wpa_ssid_txt
wpa_printf
wpa_parse_wpa_ie
wpa_msg
wpa_key_mgmt_txt
wpa_hexdump_key
wpa_hexdump_ascii_key
wpa_hexdump_ascii
wpa_hexdump
wpa_get_mib
wpa_gen_wpa_ie
wpa_eapol_send_preauth
wpa_eapol_send
wpa_driver_hermes_wpa2_eap
wpa_driver_hermes_unsolicited_message
wpa_driver_hermes_set_wpa
wpa_driver_hermes_set_key
wpa_driver_hermes_set_drop_unencrypted
wpa_driver_hermes_set_countermeasures
wpa_driver_hermes_set_auth_alg
wpa_driver_hermes_scan_timeout
wpa_driver_hermes_scan
wpa_driver_hermes_remove_pmkid
wpa_driver_hermes_pmksa_scan
wpa_driver_hermes_pmksa_process
wpa_driver_hermes_ops
wpa_driver_hermes_init
wpa_driver_hermes_get_ssid
wpa_driver_hermes_get_scan_results
wpa_driver_hermes_get_num_scan_results
wpa_driver_hermes_get_capa
wpa_driver_hermes_get_bssid
wpa_driver_hermes_flush_pmkid
wpa_driver_hermes_disassociate
wpa_driver_hermes_deinit
wpa_driver_hermes_deauthenticate
wpa_driver_hermes_associate
wpa_driver_hermes_add_pmkid
wpa_debug_timestamp
wpa_debug_show_keys
wpa_debug_level
wpa_config_read
wpa_config_free
wpa_config_allowed_eap_method
wpa_cipher_txt
wpaSupplicant
wpaSupInit
wpaPSK4
wpaPSK3
wpaPSK2
wpaPSK1
wpaGetVersion
wpaConfigFile
worldtime_addSucMsgbox
worldtime_addErrMsgbox
workQWriteIx
workQReadIx
workQPanic
workQIsEmpty
workQInit
workQDoWork
workQAdd2
workQAdd1
workQAdd0
wordBuffer2
wordBuffer
wmosYield
wmosTimeSleep
wmosTimeGet
wmosThreadSuspend
wmosThreadResume
wmosThreadKill
wmosThreadDataSet
wmosThreadDataInit
wmosThreadDataGet
wmosThreadDataExit
wmosThreadCreateError
wmosThreadCreate
wmosSemTake
wmosSemGive
wmosSemFlush
wmosSemDestroy
wmosSemCreate
wmosSemBinaryTake
wmosSemBinaryCreate
wmosQueueSend
wmosQueueReceive
wmosQueueDelete
wmosQueueCreate
wmosNamedPipeWrite
wmosNamedPipeRead
wmosNamedPipeOpen
wmosNamedPipeCreate
wmosNamedPipeClose
wmosMalloc
wmosInit
wmosFree
wmosFini
wmosError
wmosClock
wmosCalloc
wmnetUdpSocketCreate
wmnetUdpSendTo
wmnetUdpRcvFrom
wmnetUdpIpSocketCreate
wmnetUdpIpRcvFrom
wmnetUdpIpBind
wmnetUdpBind
wmnetTcpWrite
wmnetTcpServerOpen
wmnetTcpRead
wmnetTcpPeek
wmnetTcpConnect
wmnetTcpAccept
wmnetStdoutToSocket
wmnetStdoutRestore
wmnetSocketWantsAction
wmnetSocketVprintf
wmnetSocketPrintf
wmnetSocketGroupWait
wmnetSocketGroupClear
wmnetSocketGroupAddTo
wmnetSocketGroupAddPipe
wmnetSocketClose
wmnetSocketBlocking
wmnetPipeWantsAction
wmnetIpAddrResolve
wmnetInitialize
wmnetClientIpAddrGet
wmnetClientAddrGet
wmnetAddressResolve
wmbValidate
wmbUnlock
wmbTransactionTest
wmbTransactionStop
wmbTransactionStart
wmbTransactionSharedGet
wmbTransactionSessionTidAppend
wmbTransactionReplyGet
wmbTransactionProcess
wmbTransactionObjectRemove
wmbTransactionObjectAdd
wmbTransactionLockDelete
wmbTransactionLockAdd
wmbTransactionIsBestEffort
wmbTransactionEnd
wmbTransactionCreate
wmbTransactionComplete
wmbTransactionCommit
wmbTransactionBegin
wmbTransactionBad
wmbTransactionBackplaneGet
wmbTransactionAbort
wmbTableWriteUnlock
wmbTableWriteLock
wmbTableTitles
wmbTableSkipAhead
wmbTableRowPrint
wmbTableRowNext
wmbTableRoot
wmbTableReadUnlock
wmbTableReadLock
wmbTablePrint
wmbTableMember
wmbTableInstanceSfxGet
wmbTableInstanceGet
wmbTableInnermostGet
wmbTableGet
wmbTableFlagsGet
wmbTableFilter
wmbTableEndRow
wmbTableDestroy
wmbTableCreate
wmbTableColumnLength
wmbTableColumnDestroy
wmbTMTimerEvent
wmbTMRemoveObject
wmbTMProcessInput
wmbTMNewTCB
wmbTMAddObject
wmbSystemLoad
wmbSystemHandler
wmbSystem
wmbStop
wmbStart
wmbShareFree
wmbShareCreate
wmbSessionValidate
wmbSessionTidSet
wmbSessionStop
wmbSessionStart
wmbSessionPrintf
wmbSessionDestroy
wmbSessionCwdGet
wmbSessionCreate
wmbSessionBackplaneGet
wmbSessionAddressGet
wmbSessionAccessSet
wmbResourceRegister
wmbRequest
wmbPortfolioStop
wmbPortfolioStart
wmbPortfolioRequestRemote
wmbPortfolioRegisterRemote
wmbPortfolioRegister
wmbPortfolioRegDeregRemote
wmbPortfolioNew
wmbPortfolioHandler
wmbPortfolioGetRemote
wmbPortfolioGet
wmbPortfolioFromFileNameGetRemote
wmbPortfolioFromFileNameGet
wmbPortfolioFromCIDGetRemote
wmbPortfolioFromCIDGet
wmbPortfolioDocREQHandler
wmbPortfolioDocPCBHandler
wmbPortfolioDeregisterRemote
wmbPortfolioDeregister
wmbObjectVariable
wmbObjectValuesReset
wmbObjectValueGet
wmbObjectValueCreate
wmbObjectValueBufferSet
wmbObjectValueBufferGet
wmbObjectValidationString
wmbObjectUnlock
wmbObjectUndo
wmbObjectTypeNativeSet
wmbObjectTypeNativeGet
wmbObjectTypeLocalSet
wmbObjectTypeLocalGet
wmbObjectTableGet
wmbObjectStoredGet
wmbObjectStore
wmbObjectStatusSet
wmbObjectStatusGet
wmbObjectSet
wmbObjectSavedSet
wmbObjectSavedGet
wmbObjectSavedFree
wmbObjectResolver
wmbObjectRedo
wmbObjectPermission
wmbObjectOidLoad
wmbObjectOid
wmbObjectNativeSizeGet
wmbObjectNameSet
wmbObjectNamePtrSet
wmbObjectNamePtrGet
wmbObjectNameGet
wmbObjectNameBufferSet
wmbObjectNameBufferGet
wmbObjectNameBaseGet
wmbObjectMake
wmbObjectLock
wmbObjectLocalGet
wmbObjectLoad
wmbObjectLevelGet
wmbObjectInstanceSuffixGet
wmbObjectInstanceSet
wmbObjectInstancePtrGet
wmbObjectInit
wmbObjectImport
wmbObjectHandlerLocked
wmbObjectHandlerGet
wmbObjectGroupListSet
wmbObjectGroupClear
wmbObjectGroup
wmbObjectGoGetNext
wmbObjectGo
wmbObjectGet
wmbObjectExport
wmbObjectExecLookup
wmbObjectExec
wmbObjectEnum
wmbObjectEntryGet
wmbObjectEcho
wmbObjectDelete
wmbObjectCreate
wmbObjectCopy
wmbObjectCookieSet
wmbObjectCookieGet
wmbObjectComponentGet
wmbObjectAsciiOid
wmbObjectAppend
wmbMakeXMLFromRequest
wmbMakeXMLFromPCB
wmbMakeRequestfromXML
wmbMakePCBfromXML
wmbLockRemove
wmbLockMgrInit
wmbLockHeadNew
wmbLockHeadFree
wmbLockFromTIDFind
wmbLockDeadlockFind
wmbLockAdd
wmbLock
wmbIpcDone
wmbExec
wmbEntryWriteUnlock
wmbEntryWriteLock
wmbEntryReadUnlock
wmbEntryReadLock
wmbDbEntryTempGet
wmbDataType
wmbDataTrustedSet
wmbDataTrustedNvmSet
wmbDataTrustedGetNext
wmbDataTrustedGet
wmbDataStringSet
wmbDataStringGet
wmbDataNativeSet
wmbDataNativeGet
wmbDataExists
wmbDBTablesShow
wmbDBTableNxNameGet
wmbDBTableNxCountGet
wmbDBTableName
wmbDBTableGet
wmbDBTableCreate
wmbDBTableAdd
wmbDBRemove
wmbDBEntryName
wmbDBEntryGet
wmbDBEntryCreate
wmbDBEntriesShow
wmbDBDestruct
wmbDBConstruct
wmbDBAdd
wmbComponentTableLoad
wmbComponentStop
wmbComponentStateSet
wmbComponentStart
wmbComponentShow
wmbComponentSend
wmbComponentResourceLoad
wmbComponentRemote
wmbComponentRegister
wmbComponentPoolSet
wmbComponentMemGet
wmbComponentLookup
wmbComponentLockHeadSet
wmbComponentLocal
wmbComponentListener
wmbComponentDeregister
wmbComponentBackplaneGet
wmbCmd
wmbCidByName
wmbBackplaneStop
wmbBackplaneStart
wmbBackplaneRegistration
wmbBackplaneRegister
wmbBackplanePooledGet
wmbBackplaneNameSet
wmbBackplaneMaster
wmbBackplaneLookup
wmbBackplaneGet
wmbBackplaneDBGet
wmbBackplaneCreate
wmbBackplaneComponentGet
wmbBackplaneComponentDestroy
wmbBackplaneComponentCreate
wmbBackplaneClose
wmbAllUnlock
wmbAction
wm_filesys
wmXmlParserTransformStringToXML
wmXmlParserStop
wmXmlParserStart
wmXmlParserGetAttributeCount
wmXmlParserGetAttribute
wmXmlParserDocument
wmXmlParserDatumDelete
wmXmlParserDatumAdd
wmThreadStart
wmStop
wmStart
wmOidValid
wmOidTruncate
wmOidSuffix
wmOidStringSet
wmOidStringGet
wmOidScalerSet
wmOidScaler
wmOidPrint
wmOidMax
wmOidLen
wmOidFromString
wmOidEqual
wmOidCmp
wmOidAppend
wmMin
wmMemoryUsed
wmMemoryGet
wmMemoryFailEnable
wmMemoryDebugStdout
wmMemoryDebugGet
wmMemoryDebug
wmMemBlockOkay
wmMemBlockFree
wmMemBlockEntryGet
wmMemBlockEntryCreate
wmMemBlockDestroy
wmMemBlockCreate
wmMax
wmMalloc
wmLogWrite
wmLogThreadsGet
wmLogThreads
wmLogSyslogSend
wmLogSyslog
wmLogStderrGet
wmLogStderr
wmLogReset
wmLogPrintf
wmLogOpen
wmLogClose
wmHashPrime
wmHashKeyGenerate
wmHashEntryFind
wmHashEntryAdd
wmHashDestruct
wmHashConstruct
wmFree
wmError
wmErrNo
wmDumpHex
wmConvertValidate
wmConvertValid
wmConvertTypeToInfo
wmConvertToStr
wmConvertSuffix
wmConvertStrTypeTo
wmConvertStrToOid
wmConvertStrToOctets
wmConvertStrToNumber
wmConvertStrToMacAddr
wmConvertStrToList
wmConvertStrToIP
wmConvertStrToEnum
wmConvertStrTo
wmConvertStrSize
wmConvertStrNumCmp
wmConvertStr
wmConvertSizeOf
wmConvertSecsToStr
wmConvertReverseString
wmConvertOidToString
wmConvertOidToStr
wmConvertOctetsToStr
wmConvertNumberToStr
wmConvertMacAddrToStr
wmConvertLongToStr
wmConvertListToStr
wmConvertIsNumber
wmConvertIntToString
wmConvertIntToStr
wmConvertIPToStr
wmConvertHex2Dec
wmConvertGetEnumCount
wmConvertGetDTProtoType
wmConvertEnumStr
wmConvertEnumFromStr
wmConvertEnum
wmConvertDec2Hex
wmConvertDataTypeName
wmConvertDataTypeByName
wmConvertBoolToStr
wmConvert
wmCalloc
wmBufferUsedSet
wmBufferUpdate
wmBufferTypeSet
wmBufferSuffix
wmBufferStringSize
wmBufferShared
wmBufferReset
wmBufferLocalSet
wmBufferInit
wmBufferExport
wmBufferDuplicate
wmBufferDelete
wmBufferDataGet
wmBufferCreate
wmBufferCopy
wmBufferAssign
wmBufferAppend
wmAccessWriteAllowed
wmAccessToStr
wmAccessReadOkay
wmAccessReadAllowed
wmAccessLevelGet
wmAccessInfoSet
wmAccessInfoGet
wmAccessGroupsGet
wmAccessFromString
wlmexit_tomenu
wlcGetBaseIOAddress
wlcEnable
wlcCardInserted
wlcCardInsertHandler
wlcCardDetect
wlan_reboot_timer
wlan_reboot_time
windWdStart
windWdCancel
windUndelay
windTickAnnounce
windSuspend
windSpawn
windSemDelete
windResume
windReadyQRemove
windReadyQPut
windPrioritySet
windPriNormalSet
windPendQTerminate
windPendQRemove
windPendQPut
windPendQGet
windPendQFlush
windIntStackSet
windExit
windDelete
windDelay
wifiWorkMode
whoami
what__C9exception
what__C9bad_alloc
wfMode4_backup
wfMode4
wfMode3_backup
wfMode3
wfMode2_backup
wfMode2
wfMode1_backup
wfMode1
wfDisConnectSem
wepkeylen4_backup
wepkeylen4
wepkeylen3_backup
wepkeylen3
wepkeylen2_backup
wepkeylen2
wepkeylen1_backup
wepkeylen1
wepkeyConv
wepkey42
wepkey41
wepkey32
wepkey31
wepkey22
wepkey21
wepkey12
wepkey11
wepAuth4_backup
wepAuth4
wepAuth3_backup
wepAuth3
wepAuth2_backup
wepAuth2
wepAuth1_backup
wepAuth1
welcome
wel_to_oper
webserver_Web_Start
webserverComponent
webphonecore_uninit
webphonecore_set_enable_video
webphonecore_set_enable_local_video
webphonecore_is_video_enabled
webphonecore_is_local_video_enabled
webphonecore_init
webphonecore_get_connection_type
webphone_init_sip_timers
webphone_dialog_params_new
webphone_dialog_params_destroy
webphone_core_update_contact_info
webphone_core_unhold
webphone_core_terminate_dialog
webphone_core_set_sip_port
webphone_core_set_registrar_usage
webphone_core_set_registrar_passwd
webphone_core_set_registrar_addr
webphone_core_set_proxy_addr
webphone_core_set_primary_contact
webphone_core_set_alias
webphone_core_send_dtmf
webphone_core_refer
webphone_core_option
webphone_core_message
webphone_core_invite_3way
webphone_core_invite
webphone_core_hold
webphone_core_get_sip_port
webphone_core_get_registrar_passwd
webphone_core_get_registrar_addr
webphone_core_get_primary_contact
webphone_core_get_addr_of_rec
webphone_core_conf
webphone_core_accept_dialog
wdbDbgTrap
wdbDbgTraceModeSet
wdbDbgTraceModeClear
wdbDbgGetNpc
wdbDbgBpRemoveAll
wdbDbgBpRemove
wdbDbgBpListInit
wdbDbgBpGet
wdbDbgBpFind
wdbDbgArchInit
wdTick
wdTerminate
wdStart
wdLibInit
wdInstClassId
wdInit
wdDestroy
wdDelete
wdCreate
wdClassId
wdCancel
wctomb
wcstombs
watchdog_main
watchdog_init
wart_connected
wakeup_charge_sleep
wakeupDSP
wakeup
wait_wpa_counter
wait_offer
wait_for_timer_events
wait_for_events
wait_conn
wFID
wFD86
wFD14
wFD10
wFD0D
wFD0C
wFD0B
wFD09
vxWorksVersion
vxTicks
vxTaskEntry
vxTas
vxSvcIntStackEnd
vxSvcIntStackBase
vxMemProbeSup
vxMemProbe
vxMemArchProbe
vxIrqIntStackEnd
vxIrqIntStackBase
vxIntStackEnd
vxIntStackBase
vxEventPendQ
vxAbsTicks
vsyslog
vsprintf
vsnprintf
vprintf
voicemail_parseresp
vmMpuStateSet
vmMpuPageSizeGet
vmMpuLibInit
vmMpuGlobalMapInit
vmLibInfo
vindex31
vindex3
vindex21
vindex2
vindex11
vindex1
video_config_uninit
video_config_init
video_codec_list
vibrator_motor_ctrl
vibrator_ctrl
vibratorUnmute
vibratorMute
vibratorInit
vibratorFreqAndDutyRatioAndMotorVoltageSet
vibratorEnable
vibratorDrvStop
vibratorDrvStart
vibratorDrvInit
vibratorDrvDeInit
vibratorDisable
via_setversion
via_setprotocol
via_setport
via_sethost
via_setcomment
via_parse
via_match
via_init
via_getversion
via_getprotocol
via_getport
via_gethost
via_getcomment
via_free
via_clone
via_branch_new_random
via_2char
vfprintf
vfdprintf
version
verrsys
verrmsg
verify
vdbgmsg
valuelimitblock
valloc
vallid_rtp_session
validate_rtp_event
utime
ut_printf
ut_Init_printf
ut_Destroy_printf
uswab
usrToolsInit
usrStandaloneInit
usrShowInit
usrShellInit
usrSerialInit
usrSecurity
usrRoot
usrRemoteAccess
usrNetworkInit
usrNetworkAddrInit
usrNetworkAddrCheck
usrNetmaskGet
usrNetUtilsInit
usrNetUdpv4Init
usrNetTcpv4Init
usrNetSocketInit
usrNetRtSockInit
usrNetRouteCmdInit
usrNetRemoteInit
usrNetRemoteCreate
usrNetRawv4Init
usrNetProtoInit
usrNetPoolConfig
usrNetMib2Init
usrNetLoopbackStart
usrNetIpv4Init
usrNetIpProtoInit
usrNetIpAttachCommon
usrNetInit
usrNetIgmpInit
usrNetIfconfigInit
usrNetIcmpv4Init
usrNetHostSetup
usrNetGtfTimerStart
usrNetGtfInit
usrNetEther
usrNetEndLibInit
usrNetDevStart
usrNetDevNameGet
usrNetDaemonInit
usrNetBsdSocket
usrNetBpfDrvInit
usrNetBootConfig
usrNetBoot
usrNetArpLibInit
usrNetAppInit
usrMmuInit
usrKernelInit
usrKernelExtraInit
usrKernelCoreInit
usrIosExtraInit
usrIosCoreInit
usrInit
usrFtpInit
usrEntry
usrDosFsInit
usrDhcpcStart
usrDhcpcLeaseTest
usrDhcpcLeaseSave
usrDhcpcLeaseGet
usrDhcpcLeaseClean
usrClock
usrCacheEnable
usrBreakpointSet
usrBootLineParse
usrBootLineInit
usrBootLineCrack
usrBasicPPPProfileInit
usrBasicPPPFrameworkInit
usrAppInit
userland_sysctl
userinfo_def
userPwd
userNameIndex
userName
used_port_pa
use_parameter
useDSPTimer
url_unescape
url_setusername
url_setscheme
url_setport
url_setpassword
url_sethost
url_parse_params
url_parse_headers
url_parse
url_param_set
url_param_init
url_param_getbyname
url_param_freelist
url_param_free
url_param_clone
url_param_add
url_init
url_getusername
url_getscheme
url_getport
url_getpassword
url_gethost
url_free
url_escape_userinfo
url_escape_uri_param
url_escape_password
url_escape_nonascii_and_nondef
url_escape_header_param
url_clone1
url_2char_canonical
url_2char1
urlEdit
uri_param_def
update_remsrc_info
updateWifiConfig
updatePDA
updateHeaderSize
upcast__C16__user_type_infoRC9type_infoPvPPv
upDateLcd
unregister_video_codec
unregister_audio_codec
unpack_ip__FPcl
unlink
ungetc
unexpected__Fv
uncaught_exception__Fv
ultostr__FPcUi
uiomove
udpv4SysctlInit
udpstat
udp_usrreqs
udp_shutdown
udp_sendspace
udp_send
udp_recvspace
udp_notify
udp_node
udp_input
udp_init
udp_ctlinput
udp_cksum
udpInstInit
udbinfo
ua_transaction_set_outgoing_register_tr
ua_transaction_set_outgoing_refer_tr
ua_transaction_set_outgoing_ping_tr
ua_transaction_set_outgoing_option_tr
ua_transaction_set_outgoing_notify_tr
ua_transaction_set_outgoing_message_tr
ua_transaction_set_outgoing_invite_tr
ua_transaction_set_outgoing_cancel_tr
ua_transaction_set_outgoing_bye_tr
ua_transaction_set_incoming_refer_tr
ua_transaction_set_incoming_option_tr
ua_transaction_set_incoming_notify_tr
ua_transaction_set_incoming_message_tr
ua_transaction_set_incoming_invite_tr
ua_transaction_set_incoming_info_tr
ua_transaction_set_incoming_cancel_tr
ua_transaction_set_incoming_bye_tr
ua_transaction_set_destination
ua_transaction_new
ua_transaction_get_destination
ua_transaction_free
ua_transaction_execute
ua_list
u_logfullflag
u_log_w_offset
u_log_fifo_write__FP15locallog_info_s
u_log
uNum
uDelay
tyWrite
tyRead
tyMonitorTrapSet
tyIoctl
tyITx
tyIRd
tyEofChar
tyEOFSet
tyDevRemove
tyDevInit
tyDeleteLineSet
tyDeleteLineChar
tyBackspaceSet
tyBackspaceChar
tyAbortSet
tyAbortFuncSet
tvToTicks
ttyDrv
ttyDevCreate
truespeech
trgEvtClass
trgCnt
trcStack
trcDefaultArgs
transaction_set_your_instance
transaction_set_topvia
transaction_set_to
transaction_set_state
transaction_set_out_socket
transaction_set_orig_request
transaction_set_last_response
transaction_set_in_socket
transaction_set_from
transaction_set_cseq
transaction_set_config
transaction_set_call_id
transaction_set_ack
transaction_matching_response_to_xict_17_1_3
transaction_matching_request_to_xist_17_2_3
transaction_init
transaction_get_your_instance
transaction_get_destination
transaction_free2
transaction_free
transaction_execute
transaction_add_event
tracing_table
trace_initialize
trace_enable_level
trace_disable_level
toupper
tools_CalendarEntry
tools_CalcEntry
tone_playing
tone_enabled
tolower
token_set
to_tag_new_random
to_tag_match
to_parse
to_init
to_free
to_clone
to_2char
tmpnam
tmpfile
tmp_fsm
tmp_file
tmpGJBSize
tmpGJBMaxConnection
tmpAECTailTime
tmnlSubMask
tmnlIPAddress
tmnlGWIPAddress
tls_prf
tls_init
tls_global_private_key
tls_global_client_cert
tls_global_ca_cert
tls_get_errors
tls_get_cipher
tls_deinit
tls_connection_shutdown
tls_connection_set_verify
tls_connection_set_master_key
tls_connection_set_anon_dh
tls_connection_server_handshake
tls_connection_resumed
tls_connection_private_key
tls_connection_init
tls_connection_handshake
tls_connection_get_keys
tls_connection_established
tls_connection_encrypt
tls_connection_enable_workaround
tls_connection_dh
tls_connection_deinit
tls_connection_decrypt
tls_connection_client_cert
tls_connection_ca_cert
tkRcvRtnCall
timexShow
timexPre
timexPost
timexN
timexInit
timexHelp
timexFunc
timexClear
timex
timer_show
timer_settime
timer_handle_p
timer_gettime
timer_getoverrun
timer_delete
timer_create
timer_connect
timer_cancel
timerLibLog
timecvt
time_disp_sel
time_disp_needdata
timeZoneOffset
timeFormat24HourSelect
timeFormat12HourSelect
time
tickSet
tickQHead
tickGet
tickAnnounce
tick64Set
tick64Get
theCalen
tftp_thread
tftpVerbose
tftpTrace
tftpTimeout
tftpTaskStackSize
tftpTaskPriority
tftpTaskOptions
tftpServerFQDN
tftpReXmit
tftpQuitEx
tftpPeerSetEx
tftpModeSetEx
tftpInitEx
tftpInfoShowEx
tftpGetEx
tftpCopyEx
tftpConfProtocol
test_stopmelody
test_stopVib
test_startVib
test_resolv
test_lifetime
test_led
test_gmt1
test_gmt
test_getaddr
test_autoscan
test_SIP_reset
test_Play
test_DrawRowLine
testSetSSIDWepKey
testSem2
testSem1
testRead
testPST
testNetInfo
testFlashWriteTime
terminate_rtp
terminate__Fv
telephone_event
tele_event_pt
tcpv4SysctlInit
tcpstates
tcpstat
tcp_xmit_bandwidth_limit
tcp_usrreqs
tcp_timer_rexmt
tcp_timer_persist
tcp_timer_keep
tcp_timer_delack
tcp_timer_2msl
tcp_syn_backoff
tcp_slowtimo
tcp_setpersist
tcp_sendspace
tcp_rtlookup
tcp_rexmit_slop
tcp_rexmit_min
tcp_respond
tcp_recvspace
tcp_quench
tcp_output
tcp_outflags
tcp_node
tcp_newtcpcb
tcp_new_isn
tcp_mtudisc
tcp_mssopt
tcp_mssdflt
tcp_mss
tcp_msl
tcp_maxpersistidle
tcp_maxidle
tcp_maketemplate
tcp_keepintvl
tcp_keepinit
tcp_keepidle
tcp_input
tcp_init
tcp_gettaocache
tcp_fillheaders
tcp_drop_syn_sent
tcp_drop
tcp_drain
tcp_do_rfc1644
tcp_do_rfc1323
tcp_do_newreno
tcp_delacktime
tcp_delack_enabled
tcp_ctloutput
tcp_ctlinput
tcp_close
tcp_ccgen
tcp_canceltimers
tcp_backoff
tcpUsrReqSysctlInit
tcpTraceRtn
tcpTimerSysctlInit
tcpSyncacheSysctlInit
tcpSubrSysctlInit
tcpReportRtn
tcpOutputSysctlInit
tcpOutRsts
tcpLogWrite__FPUci
tcpLogSockFd
tcpLogRead__FPUci
tcpLogPut__FPc
tcpLogProcessor__Fv
tcpLogMsgQId
tcpLogHexDump__FPUci
tcpLogEnabled__Fv
tcpLogAcceptFd
tcpInstInit
tcbinfo
task_2
task_1
taskVarSet
taskVarInit
taskVarInfo
taskVarGet
taskVarDelete
taskVarAdd
taskUnsafe
taskUnlock
taskUndelay
taskTerminate
taskTcb
taskSwitchTable
taskSwitchHookDelete
taskSwitchHookAdd
taskSwapTable
taskSwapReference
taskSwapHookDetach
taskSwapHookDelete
taskSwapHookAttach
taskSwapHookAdd
taskSuspend
taskStatusString
taskStackAllot
taskSpawn
taskShowInit
taskShow
taskSafe
taskRtnValueSet
taskResume
taskRestart
taskRegsShow
taskRegsSet
taskRegsInit
taskRegsGet
taskRegsFmt
taskRegName
taskPrioritySet
taskPriorityGet
taskPriRangeCheck
taskOptionsString
taskOptionsSet
taskOptionsGet
taskNameToId
taskName
taskLock
taskLibInit
taskIsSuspended
taskIsReady
taskInstClassId
taskInit
taskInfoGet
taskIdVerify
taskIdSelf
taskIdListSort
taskIdListGet
taskIdFigure
taskIdDefault
taskIdCurrent
taskHookInit
taskDestroy
taskDeleteTable
taskDeleteHookDelete
taskDeleteHookAdd
taskDeleteForce
taskDelete
taskDelay
taskData
taskCreateTable
taskCreateHookDelete
taskCreateHookAdd
taskCreat
taskClassId
taskBpHookSet
taskBpHook
taskArgsSet
taskArgsGet
taskActivate
tanh
tOldTimeForToIdle
tOldTimeCheckAlarm
tOldTime
tLogTaskId
t8307SioIntTx
t8307SioIntRx
t8307SioIntMs
t8307SioInt
t8307SioDevInit
t8307IntLvlVecChk
t8307IntLvlVecAck
t8307IntLvlEnable
t8307IntLvlDisable
t8307IntLvlChg
t8307IntDevInit
szRtpName
system_pause
system
syslogtask
syslog_send
syslog_recv
syslog_init
syslog_enable
syslog_disable
syslogSem
syslog
sysctlnametomib
sysctlbyname
sysctl_unregister_oid
sysctl_sysctl_debug_dump_node
sysctl_remove_oid
sysctl_register_oid
sysctl_node
sysctl_handle_string
sysctl_handle_opaque
sysctl_handle_long
sysctl_handle_int
sysctl_find_oid
sysctl_ctx_init
sysctl_ctx_free
sysctl_ctx_entry_find
sysctl_ctx_entry_del
sysctl_ctx_entry_add
sysctl_add_oid
sysctl__children
sysctlLibInit
sysctlInit
sysctlCtxList
sysctl
sysWriteNack
sysWriteAck
sysWrite
sysToMonitor
sysTimeSync
sysSymTbl
sysStartType
sysStartImage
sysStart
sysSioChans
sysShutdown
sysSerialReset
sysSerialHwInit2
sysSerialHwInit
sysSerialChanGet
sysSectorErase
sysRtcSet
sysRtcInt
sysRtcGet
sysRestoreConsole
sysReadExact
sysReadCmdHeader
sysRead
sysPwmSet
sysProcNumSet
sysProcNumGet
sysProcNum
sysPhysMemTop
sysPhysMemDescNumEnt
sysPhysMemDesc
sysPauseSet
sysPauseSem
sysPause
sysNvRamSet
sysNvRamGet
sysModel
sysMmuLibInit
sysMemTop
sysMblkClBlkDesc
sysMailboxEnable
sysMailboxConnect
sysLocalToBusAdrs
sysLedsReadWrite
sysIntStackSplit
sysIntLvlVecChkRtn
sysIntLvlVecAckRtn
sysIntLvlEnableRtn
sysIntLvlDisableRtn
sysIntLvlChgRtn
sysInit
sysHwInit2
sysHwInit0
sysHwInit
sysGetCPUVer
sysFlashWriteEx
sysFlashWriteEnable
sysFlashWriteDisable
sysFlashWrite
sysFlashTaskCleanup
sysFlashTask
sysFlashSet
sysFlashGet
sysFlashDetect
sysFlags
sysFTInit
sysExcMsg
sysDebugPrint
sysCpu
sysCplusEnable
sysClkRateSet
sysClkRateGet
sysClkInit
sysClkFreqSet
sysClkEnable
sysClkDisable
sysClkConnect
sysClDescTblNumEnt
sysClDescTbl
sysCanEnterSleep
sysCacheLibInit
sysBusToLocalAdrs
sysBusTas
sysBusIntGen
sysBusIntAck
sysBus
sysBspRev
sysBootParams
sysBootLine
sysBootHost
sysBootFile
sysAuxClkRateSet
sysAuxClkRateGet
sysAuxClkEnable
sysAuxClkDisable
sysAuxClkConnect
sysAdaEnable
syncache_unreach
syncache_node
syncache_lookup
syncache_init
syncache_expand
syncache_chkrst
syncache_badack
syncache_add
syncSymRemoveRtn
syncSymAddRtn
syncLoadRtn
symValueGet
symTypeGet
symTblTerminate
symTblRemove
symTblInit
symTblDestroy
symTblDelete
symTblCreate
symTblClassId
symTblAdd
symSAdd
symRemove
symNameGet
symName
symLibInit
symInit
symGroupDefault
symFree
symFindSymbol
symFindByValueAndType
symFindByValue
symFindByNameAndType
symFindByName
symFindByCName
symEach
symByValueFind
symByValueAndTypeFind
symByCNameFind
symAlloc
symAdd
swap_getProductID
swap_Start
swapWriteNack
swapWriteAck
swapTask
swapReadCmdHeader
swab
susleep
supportWPA
supportLangNum
supmedia
substrcmp
subs_state_setelement
subs_state_parse
subs_state_init
subs_state_getelement
subs_state_get_status
subs_state_get_expires
subs_state_free
subs_state_clone
subs_state_2char
sub_send_rssi_batt
sub_rgst_ok
sub_call_transfer_res
stun_test
stun_random
stun_query_by_hostName
stun_query_by_IPAddr
stun_parse_server_name
stun_parse_message
stun_parse_hostname
stun_parse_client_name
stun_nat_type
stun_encode_message
stun_debug
stun_build_req_simple
stunUse
stunServerPort
stunServer
strxfrm
strtoul
strtol
strtok_r
strtok
strtod
strstr
strspn
strrchr
strpbrk
strncpy
strncmp
strncat
strlen
stringSWAP
stringPHSE
stringCALG
stricmp
strftime
strerror_r
strerror
strdup
strcspn
strcpy
strcoll
strcmp
strchr
strcat_simple_header
strcat_headers_one_per_line
strcat_headers_all_on_one_line
strcat
strcasecmp1
str_num
strSWAP
strSOWM
strPMDN
strPHSE
strCALG
str2num
store_video_config
store_registrar_config
store_ppp_options_in_packet
store_local_hostname
store_local_SIP_port
store_local_RTP_port
stopRinger__15CdspRootManager
stopRinger__11CdspManager
stopGetOpt
stopButtonClick__15CdspRootManager
stopButtonClick__11CdspManager
stopApplLogger
stolowercase
sthread_setpriority
sthread_join
sthread_exit
sthread_create
stdioInit
stdioFpDestroy
stdioFpCreate
stdioFp
status
station_infoidentity
station_infocompat
station_code
station_4_data
station_3_data
station_2_data
station_1_data
station
statfs
state_machine_table
statSymTbl
stat
startline_parseresp
startRinger__15CdspRootManagerUs
startRinger__11CdspManagerUs
startGetOpt
startButtonClick__15CdspRootManageri
startButtonClick__11CdspManageri
stTotalStat
stIntervalStat
sstrncpy
ssidConnectedTo
ssid4
ssid3
ssid2
ssid1
ssiInit
ssem_wait
ssem_trywait
ssem_post
ssem_init
ssem_destroy
sscanf
ss_fltsz_local
ss_fltsz
srvSendTask__Fv
srvQuery
srandom
srand
sqrt
spyTotalTicks
spyTaskStackSize
spyTaskPriority
spyTaskOptions
spyTaskId
spyTask
spyStopCommon
spyStop
spyReportCommon
spyReport
spyLibInit
spyKernelTicks
spyKernelIncTicks
spyInterruptTicks
spyInterruptIncTicks
spyIncTicks
spyIdleTicks
spyIdleIncTicks
spyHelp
spyCommon
spyComTask
spyClkStopCommon
spyClkStop
spyClkStartCommon
spyClkStart
spudph
sprintf
splx
splnet2
splnet
splimp
splTid
splSemInit
splSemId
speex_wb
speex_nb
speex_info
spTaskStackSize
spTaskPriority
spTaskOptions
sowakeupHook
sowakeup
soundUnmute
soundPrescalerInit
soundPowerSaver
soundPowerRestore
soundMute
soundMixModeDrvInit
soundMixModeDrvDeInit
soundInit
soundFreqAndDutyRatioSet
soundEnable
soundDisable
sound32UDiv16Const16
sotoxsocket
soshutdown
sosetopt
sosend
sorflush
soreserve
soreceive
sopoll
sooptcopyout
sooptcopyin
soopt_mcopyout
soopt_mcopyin
soopt_getm
soo_unselect
soo_select
soo_ioctl
sonewconn3
sonewconn
solisten
soisdisconnecting
soisdisconnected
soisconnecting
soisconnected
sohasoutofband
sogetopt
softResetDSP__15CdspRootManager
softResetDSP__11CdspManager
sofree
sodropablereq
sodisconnect
sodealloc
socreate
soconnect2
soconnect
soclose
socketSysctlInit
socket
sock_nb2read
sockSysctlInit
sockLibInit
sockLibAdd
socantsendmore
socantrcvmore
sobind
soalloc
soaccept
soabort
so_gencnt
sntpcTimeGet
sntpcPort
sntpcInit
sntp_sync
sntp_client
snprintf
sndTaskMsgQID
smutex_unlock
smutex_lock
smutex_init
smutex_destroy
smObjTcbFreeRtn
smObjTcbFreeFailRtn
smObjTaskDeleteFailRtn
smObjPoolMinusOne
smMemPartShowRtn
smMemPartReallocRtn
smMemPartOptionsSetRtn
smMemPartFreeRtn
smMemPartFindMaxRtn
smMemPartAllocRtn
smMemPartAddToPoolRtn
sllTerminate
sllRemove
sllPutAtTail
sllPutAtHead
sllPrevious
sllInit
sllGet
sllEach
sllDelete
sllCreate
sllCount
sleep
sl_uncompress_tcp
sl_compress_tcp
sl_compress_init
sipxtab
sipmsg2locallog
sipd_thread
sipconfig
sip_username
sip_ua_init
sip_registar_ip
sip_prxoy_ip
sip_pm_callback
sip_password
sip_msg_print
sip_config_uninit
sip_config_init
sipUserName
sipUseOutbandProxy
sipUseNullPacket
sipUseDNS
sipRegisterUsage
sipRegisterPort
sipRegisterName
sipRegisterIPAddress
sipProxyPort
sipProxyName
sipProxyIPAddress
sipPort
sipPassword
sipAuthString
sioAdapterDelete
sioAdapterCreate
sintab
sinh
sigwaitinfo
sigwait
sigvec
sigtimedwait
sigsuspend
sigsetmask
sigsetjmp
sigreturn
sigqueueInit
sigqueue
sigprocmask
sigpending
signature
signal
sigismember
sigfillset
sigemptyset
sigdelset
sigblock
sigaddset
sigaction
sigPendKill
sigPendInit
sigPendDestroy
sigInit
sigEvtRtn
shutdown
shutMg
show_eloop
showWPAinfo
showUTTimer
showPhoneParam
showMGCPDetails
showLoggerInfo
showCoreParam
showConnList
showConnDetails
showCP15Regs
showActiveLogging
show
shellTaskStackSize
shellTaskPriority
shellTaskOptions
shellTaskName
shellTaskId
shellScriptAbort
shellRestart
shellPromptSet
shellOrigStdSet
shellLogoutInstall
shellLogout
shellLoginInstall
shellLogin
shellLock
shellIsRemoteConnectedSet
shellIsRemoteConnectedGet
shellInit
shellHistory
shellHistSize
shell
sha1_vector
sha1_transform
sha1_t_prf
sha1_prf
sha1_mac
sgetcopy_unquoted_string
sgetcopy
sfpFloatSetup
sfpFloatNormalize
sfpDoubleSetup
sfpDoubleNormalize2
sfpDoubleNormalize
setvbuf
settingsecretmenu_exit
settingmenu_exit
setting_wel_set
setting_time_set
setting_time_format
setting_secret_sel
setting_saver_time
setting_saver_set
setting_saver_pick
setting_saver_onoff
setting_resume_default
setting_password_prj
setting_password_change
setting_ownnumno
setting_ownnumEntry
setting_long_lock
setting_langrage_sel
setting_ipphone_sel
setting_idle_set
setting_date_shw
setting_date_adj
setting_contr_set
setting_backl_set
setting_answer_mod
setting_alarm_switch
setting_alarm_set
setting_alarm_lazy
setting_alarm_circle
setting_TestEntry
setsockopt
setmask
setlogmask
setlocale
setlinebuf
setjmp
setipdst
setifnetmask
setifmtu
setifmetric
setifflags
setifdstaddr
setifbroadaddr
setifaddr
sethostname
setbuffer
setbuf
setaddr
set_video_offer
set_unexpected__FPFv_v
set_uname
set_terminate__FPFv_v
set_suspend
set_stun_params_api
set_stun_params
set_sip_params
set_sip_config
set_session_remote
set_rtp_samplesize
set_rtp_samples_count
set_rtcp_fds
set_route
set_rfc2833_pltype_value
set_relinfo
set_random_gen_seed
set_ppp_state
set_phno
set_option_values_from_nak
set_option_values_for_nak
set_non_blocking
set_next_token
set_new_handler__FPFv_v
set_mute_on_state
set_mute_off_state
set_missing_required_options_in_nak
set_location
set_hex
set_g726_pltype_value
set_email_addr
set_eloop_terminated
set_eloop_stop
set_eloop_running
set_declinfo
set_cplus_marker_for_demangling
set_audio_offer
set__8CdspPort
set__15CdspRootManager
setWepkeylen4Config
setWepkeylen3Config
setWepkeylen2Config
setWepkeylen1Config
setWepkey
setWFMode4Config
setWFMode3Config
setWFMode2Config
setWFMode1Config
setWEPAuth4Config
setWEPAuth3Config
setWEPAuth2Config
setWEPAuth1Config
setVolume__15CdspRootManagerUsUs
setVolume__11CdspManagerUsUs
setUserPassword
setReboot
setProvConfProtocol
setIndex4Config
setIndex3Config
setIndex2Config
setIndex1Config
setHandsetMixerGain__11CdspDecoderUs
setHalfDuplexParams__15CdspRootManagerPs
setHalfDuplexParams__11CdspManagerPs
setGains__15CdspRootManagerUlPUs
setGains__11CdspManagerUlPUs
setGainStep__15CdspRootManager7GainMapUs
setGainStep__11CdspManager7GainMapUs
setGainMap__15CdspRootManager7GainMapUsUs
setGainMap__11CdspManager7GainMapUsUs
setEncoderGain__15CdspRootManagerUsUs
setEncoderGain__11CdspManagerUsUs
setEncoderConfGain__15CdspRootManagerUsUs
setEncoderConfGain__11CdspManagerUsUs
setDefaultScript
setDefaultParam
setDecoderHandsetGain__15CdspRootManagerUsUs
setDecoderHandsetGain__11CdspManagerUsUs
setDecoderAudioDestination__15CdspRootManagerUsUs
setDecoderAudioDestination__11CdspManagerUsUs
setDateTime
setCurTFTPPort
setConfig
setCodecType__15CdspRootEncoderUsUc
setCodecType__15CdspRootDecoderUsUc
setCodecType__11CdspEncoderUsUc
setCodecType__11CdspDecoderUsUc
setAudioSource__15CdspRootManagerUs
setAudioSource__11CdspManagerUs
setAudioOutput__15CdspRootManagerUs
setAudioOutput__11CdspManagerUs
setAudioDestination__15CdspRootManagerUs
setAudioDestination__11CdspManagerUs
services
server_port
serverIP_backup
serverIP
server
sendto
sendmsg
send_unicast
send_udp_msg
send_rtpteleph_events_pack
send_rtp_pack
send_rtcp_sesscmd
send_rtcp_pack
send_pack
send_ncp_termination_request
send_ncp_termination_ack
send_ncp_packet
send_ncp_configuration_request
send_ncp_configuration_reject
send_ncp_configuration_nak
send_ncp_configuration_ack
send_ncp_code_reject
send_message
send_lcp_time_remaining_packet
send_lcp_protocol_reject
send_lcp_id_packet
send_lcp_discard_request
send_dtmf
send
semTerminate
semTakeTbl
semTake
semSmShowRtn
semSmInfoRtn
semShowInit
semShow
semQPut
semQInit
semQGet
semQFlushDefer
semQFlush
semOTake
semMTake
semMPendQPut
semMLibInit
semMInit
semMGiveKernWork
semMGiveKern
semMGiveForce
semMGive
semMCreate
semMCoreInit
semLibInit
semInvalid
semIntRestrict
semInstClassId
semInstClass
semInfo
semGiveTbl
semGiveDeferTbl
semGiveDefer
semGive
semFlushTbl
semFlushDeferTbl
semFlushDefer
semFlush
semEvStop
semEvStart
semEvRsrcSend
semEvLibInit
semEvIsFreeTbl
semDestroy
semDelete
semClear
semClassId
semClass
semCTake
semCLibInit
semCInit
semCGiveDefer
semCGive
semCCreate
semCCoreInit
semBTake
semBLibInit
semBInit
semBGiveDefer
semBGive
semBCreate
semBCoreInit
seltemp
selecting
selectInit
select
selWakeupType
selWakeupListTerm
selWakeupListLen
selWakeupListInit
selWakeupAll
selWakeup
selTaskDeleteHookAdd
selNodeDelete
selNodeAdd
selHandler
secretsDataNodeNicePrint
secret_needdata
secCounter
sdp_z_adjustments_set
sdp_z_adjustments_get
sdp_v_version_set
sdp_v_version_get
sdp_u_uri_set
sdp_u_uri_get
sdp_time_descr_init
sdp_time_descr_free
sdp_t_time_descr_add
sdp_t_stop_time_get
sdp_t_start_time_get
sdp_s_name_set
sdp_s_name_get
sdp_r_repeat_get
sdp_r_repeat_add
sdp_payload_uninit
sdp_payload_init
sdp_parse_z
sdp_parse_v
sdp_parse_u
sdp_parse_t
sdp_parse_s
sdp_parse_r
sdp_parse_p
sdp_parse_o
sdp_parse_m
sdp_parse_k
sdp_parse_i
sdp_parse_e
sdp_parse_c
sdp_parse_b
sdp_parse_a
sdp_parse
sdp_p_phone_get
sdp_p_phone_add
sdp_o_username_get
sdp_o_sess_version_get
sdp_o_sess_id_get
sdp_o_origin_set
sdp_o_nettype_get
sdp_o_addrtype_get
sdp_o_addr_get
sdp_negotiation
sdp_media_init
sdp_media_free
sdp_m_proto_get
sdp_m_port_get
sdp_m_payload_get
sdp_m_payload_add
sdp_m_number_of_port_get
sdp_m_media_get
sdp_m_media_add
sdp_key_init
sdp_key_free
sdp_k_keytype_get
sdp_k_keydata_get
sdp_k_key_set
sdp_init
sdp_i_info_set
sdp_i_info_get
sdp_handler_uninit
sdp_handler_set_write_offer_fcn
sdp_handler_set_read_answer_fcn
sdp_handler_set_accept_offer_fcn
sdp_handler_read_remote_answer
sdp_handler_new
sdp_handler_init
sdp_handler_guess_config
sdp_handler_generate_offer
sdp_handler_generate_answer_according_localprofile
sdp_handler_generate_answer
sdp_handler_destroy
sdp_handler_class_init
sdp_handler_add_video_payload
sdp_handler_add_payload
sdp_handler_add_audio_payload
sdp_free
sdp_endof_media
sdp_e_email_get
sdp_e_email_add
sdp_context_uninit
sdp_context_notify_inc_resp
sdp_context_notify_inc_req
sdp_context_new
sdp_context_init
sdp_context_gen_out_resp
sdp_context_gen_out_req
sdp_context_destroy
sdp_context_class_init
sdp_connection_init
sdp_connection_get
sdp_connection_free
sdp_clone
sdp_c_nettype_get
sdp_c_connection_add
sdp_c_addrtype_get
sdp_c_addr_set
sdp_c_addr_multicast_ttl_get
sdp_c_addr_multicast_int_get
sdp_c_addr_get
sdp_bandwidth_init
sdp_bandwidth_get
sdp_bandwidth_free
sdp_b_bwtype_get
sdp_b_bandwidth_get_with_pt
sdp_b_bandwidth_get
sdp_b_bandwidth_add
sdp_attribute_init
sdp_attribute_get
sdp_attribute_free
sdp_append_time_descr
sdp_append_string
sdp_append_media
sdp_append_key
sdp_append_connection
sdp_append_bandwidth
sdp_append_attribute
sdp_a_attribute_add
sdp_a_attr_value_get_without_pt
sdp_a_attr_value_get_with_pt
sdp_a_att_value_get
sdp_a_att_field_get
sdp_2char
script_tag
script_is_ready
script_init_flag
script_info
script_heading
script_backup
screen_saver_needdata
sclrspace
sched_yield
sched_setscheduler
sched_setparam
sched_rr_get_interval
sched_getscheduler
sched_getparam
sched_get_priority_min
sched_get_priority_max
scanf
scanField
scanCharSet
scalloc
scalbn
sbwakeup
sbwait
sbuf
sbtoxsockbuf
sbselqueue
sbseldequeue
sbreserve
sbrelease
sbinsertoob
sbflush
sbdroprecord
sbdrop
sbcreatecontrol
sbcompress
sbappendrecord
sbappendcontrol
sbappendaddr
sbappend
sb_max
sb_lock
savewelcome
savetime
saverexit_tomenu
saver_to_oper
saver_time_sel
saver_time_needdata
saver_time_data
saver_time
saver_picklist_needdata
saver_pick_judge
saver_pick_3
saver_pick_2
saver_pick_1
saver_pick_0
saver_onoff_needdata
saver_onoff_flag
saver_onoff
saveipphone
saveippassword
saveipaccount
saveidletxt
saveidle
savedate
savecallfdnum
savealarmtime
save_constrast
saveRTPSession
saveNamePsw
satoi
sMailPwNum
sMailBoxNum
sAcessNum
runtimeVersion
runtimeName
rttrash_get
rtstat
rtsockSysctlInit
rtrequest1
rtrequest
rtredirect
rtp_srandom
rtp_sleep
rtp_random
rtp_profile_new
rtp_profile_move_payload
rtp_profile_get_payload_number_from_rtpmap
rtp_profile_get_payload_number_from_mime
rtp_profile_get_payload_from_rtpmap
rtp_profile_get_payload_from_mime
rtp_profile_find_payload_number
rtp_profile_find_payload
rtp_profile_destroy
rtp_profile_clone_full
rtp_port_use_unlock
rtp_port_use_lock
rtp_payload_init
rtp_handle_p
rtp_data_lock
rtp_config_uninit
rtp_config_init
rtp_close_sock
rtpStatTaskId
rtpPort
rtpPacketSize
rtn2solar
rtioctl
rtinit
rtfree
rtcpfds_a
rtcp_tqid
rtcp_tid
rtcp_proc_pack_event
rtcp_msgqid
rtcp_init
rtcp_handle_p
rtcp_data_lock
rtc_set_test
rtcInt
rtalloc_ign
rtalloc1
rtalloc
rt_xaddrs
rt_tables
rt_setgate
rt_newmaddrmsg
rt_newaddrmsg
rt_missmsg
rt_ifmsg
rt_ifannouncemsg
rt_getifa
rsn_preauth_scan_results
rsn_preauth_init
rsn_preauth_deinit
rsm_msg_match
rsm_msg_dismatch
rresvportCommon
rresvport
routetable_node
routestatShow
routedomain
routecInit
routec
route_parse
route_init2
route_init
route_free
route_cb
route_2char
routeShowInit
routeShow
routeCmdInit
roundRobinSlice
roundRobinOn
rootTaskId
rootMemNBytes
rngPutAhead
rngNBytes
rngMoveAhead
rngIsFull
rngIsEmpty
rngFreeBytes
rngFlush
rngDelete
rngCreate
rngBufPut
rngBufGet
rn_walktree
rn_refines
rn_match
rn_lookup
rn_inithead
rn_init
rn_delete
rn_addroute
rn_addmask
rmdir
ripcbinfo
ripcb
rip_usrreqs
rip_sendspace
rip_recvspace
rip_output
rip_input
rip_init
rip_ctloutput
rip_ctlinput
ringer_ctrl
ringerUnmute
ringerMute
ringerInit
ringerFreqAndDutyRatioSet
ringerEnable
ringerDrvStop
ringerDrvStartSevraltone
ringerDrvStartOnetonerep5
ringerDrvStartOnetone
ringerDrvStartMuchtone
ringerDrvStart
ringerDrvInit
ringerDrvDeInit
ringerDownload__15CdspRootManagerUsUsUsPUs
ringerDownload__11CdspManagerUsUsUsPUs
ringerDisable
rindex
rijndaelKeySetupEnc
rijndaelKeySetupDec
rijndaelEncrypt
rijndaelDecrypt
ridreq
rewinddir
rewind
returnTag
retry_lcp_termination_request
retry_lcp_configure_request
retry_ipcp_termination_request
retry_ipcp_configure_request
retrieve_if
retrans_wait_offer
retrans_requesting
retrans_renewing
retrans_reboot_verify
retrans_rebinding
resume_pwd_right
restore_video_config
restore_registrar_config
restore_local_hostname
restore_local_SIP_port
restore_local_RTP_port
restartTaskStackSize
restartTaskPriority
restartTaskOptions
restartTaskName
restartMg
respond_to_request_without_FSM
respond_to_request
resolvtest
resolver_thread
resolveInfo
resolvSend
resolvQueryN
resolvQuery
resolvParamsSet
resolvParamsGet
resolvMkQuery
resolvInit
resolvGetHostByName
resolvGetHostByAddr
resolvDomain
resolvDNExpand
resolvDNComp
resolv
reset_period
reset_if
reset_counter
reset_conf_gain
reset__8CdspPort
reset__15CdspRootManager
resetToDefault
resetEncoder__15CdspRootManagerUs
resetDecoder__15CdspRootManagerUs
resetDSP__15CdspRootManager
resetDSP__11CdspManager
reserve_port
reschedule
res_querydomainN
res_querydomain
res_queriesmatch
res_nameinquery
res_isourserver
res_hnok
res_dnok
resSearchN
resSearch
requesting
replaces_parse
replaces_init
replaces_free
replaces_clone
replaces_2char
replace_data_field_in_option
repeatRun
repeat
renewing
rename
remove_rtcp_fds
remove_configuration_option
removeAlternateValues
remove
remoteTftpState
rem_write_msgq
rem_write_fd
rem_read_msgq
rem_read_fd
remStdErrSetupTimeout
remLibInit
remLastResvPort
remCurIdSet
remCurIdGet
release_port
release
rel2abs_path
reject
registration_ctxt_set_registrar
registration_ctxt_set_password
registration_ctxt_set_address_of_record
registration_ctxt_new
registration_ctxt_free
registration_ctxt_destroy
registrar_config_uninit
registrar_config_init
register_video_codec
register_talktime
register_name
register_labelid
register_groupid
register_fieldtelnum
register_editnum
register_calltimeon
register_calltimedate
register_audio_codec
reg_totaltime_time
reg_totaltime_label
reg_searchuserinfo
reg_searchcalllog
reg_savepwd
reg_savename
reg_gettalkingtime
reg_getgroupnameid
reg_getcallname
reg_getcallid
reg_getalltime
reg_get_timedatatext
reg_get_calltimeontext
reg_faillure_cnt
reg_dialog_log
reg_dialog_addquestionbox
reg_dialog_addcmdmsgbox
reg_comp_calltime
regNumberStore
regDuration
referred_by_parse
referred_by_init
referred_by_free
referred_by_clone
referred_by_2char
refer_to_parse
refer_to_init
refer_to_free
refer_to_clone
refer_to_2char
redirOutFd
redirInFd
recvmsg
recvfrom
recv_counter
recv
record_route_parse
record_route_init
record_route_free
record_route_2char
receive_udp_msg
rebootcmd
reboot_verify
rebootHookAdd
reboot
rebinding
realloc
readyQHead
readyQBMap
ready
readv
readdir
read_video_answer
read_random_unlimited
read_random
read_psc
read_local_log
read_audio_answer
read
rd_fds
rcvTaskMsgQID
rcvEtherAddrAdd
rcmd
rc_filearray
rc4_skip
rawcb_list
raw_usrreqs
raw_node
raw_input
raw_init
raw_disconnect
raw_detach
raw_ctlinput
raw_attach
rasNumAddrPool
rasAddrPools
rasAddrPoolId
range_option_value_match
random_poll
random32
random16
random
rand_initialize
rand
ram_fs_write_to_flash
ram_fs_read_from_flash
ram_fs_ram_init
ram_fs_invalidate_flash
ram_fs_init
ram_fs_flash_init
ram_fs_flash_flag
ram_fs_flag_str
ramDrv
ramDevCreate
raise
quoted_string_set
quote_find
query_stun_lifetime_api
query_stun_for_sipua_api
qsort
qksort
qkNumsort
qTerminate
qResort
qRemove
qPut
qPriListTerminate
qPriListResort
qPriListRemove
qPriListPutFromTail
qPriListPut
qPriListKey
qPriListInit
qPriListInfo
qPriListGetExpired
qPriListGet
qPriListFromTailClassId
qPriListEach
qPriListDelete
qPriListCreate
qPriListClassId
qPriListCalibrate
qPriListAdvance
qPriBMapResort
qPriBMapRemove
qPriBMapPut
qPriBMapListDelete
qPriBMapListCreate
qPriBMapKey
qPriBMapInit
qPriBMapInfo
qPriBMapGet
qPriBMapEach
qPriBMapDelete
qPriBMapCreate
qPriBMapClassId
qKey
qJobTerminate
qJobPut
qJobInit
qJobInfo
qJobGet
qJobEach
qJobDelete
qJobCreate
qJobClassId
qInit
qInfo
qGetExpired
qGet
qFirst
qFifoRemove
qFifoPut
qFifoInit
qFifoInfo
qFifoGet
qFifoEach
qFifoDelete
qFifoCreate
qFifoClassId
qEach
qDelete
qCreate
qCalibrate
qAdvance
pwmPrescalerInit
pwmPowerSaver
pwmPowerRestore
pwd_protect_sel
pwd_protect_needdata
pwd_dismatch
putw
puts
putenv
putchar
putc
putBuffer__16CdspRootDataPortPvUlUs
putBuffer__15CdspRootDecoderPvUsUsUc
putBuffer__11CdspDecoderPvUsUsUc
push_dhcp_fsm_counter
punc_char
puGlobal
pthread_testcancel
pthread_sigmask
pthread_setspecific
pthread_setschedparam
pthread_setcanceltype
pthread_setcancelstate
pthread_self
pthread_once
pthread_mutexattr_setprotocol
pthread_mutexattr_setprioceiling
pthread_mutexattr_init
pthread_mutexattr_getprotocol
pthread_mutexattr_getprioceiling
pthread_mutexattr_destroy
pthread_mutex_unlock
pthread_mutex_trylock
pthread_mutex_setprioceiling
pthread_mutex_lock
pthread_mutex_init
pthread_mutex_getprioceiling
pthread_mutex_destroy
pthread_kill
pthread_key_delete
pthread_key_create
pthread_join
pthread_getspecific
pthread_getschedparam
pthread_exit
pthread_equal
pthread_detach
pthread_create
pthread_condattr_init
pthread_condattr_destroy
pthread_cond_wait
pthread_cond_timedwait
pthread_cond_signal
pthread_cond_init
pthread_cond_destroy
pthread_cond_broadcast
pthread_cleanup_push
pthread_cleanup_pop
pthread_cancel
pthread_attr_setstacksize
pthread_attr_setstackaddr
pthread_attr_setscope
pthread_attr_setschedpolicy
pthread_attr_setschedparam
pthread_attr_setname
pthread_attr_setinheritsched
pthread_attr_setdetachstate
pthread_attr_init
pthread_attr_getstacksize
pthread_attr_getstackaddr
pthread_attr_getscope
pthread_attr_getschedpolicy
pthread_attr_getschedparam
pthread_attr_getname
pthread_attr_getinheritsched
pthread_attr_getdetachstate
pthread_attr_destroy
pthreadLibInit
pstempty
pst_dummy
psrShow
psc_open
psc_close
pscWrite
pscSetVibratorMotor
pscSetVibrator
pscSetRinger
pscSetLedBrightness
pscSetBatteryCurrent
pscSetBattery
pscSetBacklightDelay
pscSetBacklight
pscSetAccSupply
pscRead
pscInit
pscGetVibratorMotor
pscGetVersion
pscGetMainPwrSwitch
pscGetLidSwitch
pscGetLedBrightness
pscGetBatteryInfo
pscGetBattery
pscGetBacklightDelay
pscGetAccSupply
pscGetADC
pru_sense_null
pru_rcvoob_notsupp
pru_rcvd_notsupp
pru_listen_notsupp
pru_control_notsupp
pru_connect_notsupp
pru_connect2_notsupp
pru_accept_notsupp
prt_pwd_match
proxyBroadcastHook
provConfProtocol
protocol_param_reset
protocol_config_set
protocol_config_get
productID
processRequest__FPPUsT0P15CdspRootManager
processRTTMsg__Fv
proc_time_out
proc_rtcpfd_close
proc_rtcpfd
proc_rtcp
proc_rcvd_rtcp
pro_delay2
pro_delay
pro_adderrorbox
pro_addcommandmsgbox
privateImeConfig
printf
printb
print_sem
print_ip
print_err
print_char
printLogo
printExc
printErrno
printErr
print64Row
print64Mult
print64Fine
print64
prefixLibInit
pppoe_user_password
pppoe_user_name
pppoe_service_name
pppoeOpen
pppoeInit
pppoeCreateProfile
pppoeClose
ppp_negotiation_error
ppp_configure_request_option_processor
ppp_configure_nak_option_processor
pppVsEndLoad
pppVsEndComponentDelete
pppVsEndComponentCreate
pppVjcComponentDelete
pppVjcComponentCreate
pppSysProfileCreate
pppSysProfile
pppSysFramework
pppResolveRtn
pppResolveFuncsUnregister
pppResolveFuncsRegister
pppPapComponentDelete
pppPapComponentCreate
pppOutput
pppOeSysProfileCreate
pppOeSysProfile
pppOe1SysProfile
pppOe1Stack
pppOEthernetDelete
pppOEthernetCreate
pppOESessionListShow
pppOEServiceNameDelete
pppOEServiceNameAdd
pppOEServiceListShow
pppOEPrintPacket
pppOEPrintPADPayload
pppOEPrintHeader
pppNetworkLayerDelete
pppNetworkLayerCreate
pppMultiResolveRtn
pppLinkIdGet
pppIpcpComponentDelete
pppIpcpComponentCreate
pppInterfaceLayerDelete
pppInterfaceLayerCreate
pppFramingLayerDelete
pppFramingLayerCreate
pppControlLayerDelete
pppControlLayerCreate
pppConnectionOpen
pppConnectionClose
pppChapComponentDelete
pppChapComponentCreate
pppBasicLinkProfile
pppAsyncFramingComponentDelete
pppAsyncFramingComponentCreate
pppAddressSet
pppAdapterLayerDelete
pppAdapterLayerCreate
ppGlobalEnviron
posixPriorityNumbering
portrange_node
port_range_low
port_range_high
pmksa_candidate_free
pmksa_candidate_add
pmksa_cache_list
pmksa_cache_get
pmksa_cache_free
pm_wifi_rssi_cb
pm_unhold
pm_to_idle
pm_stack_reset
pm_sip_event_cb
pm_send_sms
pm_send_12
pm_searchnet
pm_register_duration_set
pm_protocol_config_set
pm_protocol_config_get
pm_power_off
pm_nick_name_set
pm_netservice_cancel
pm_main
pm_init
pm_hold
pm_hangup
pm_callwaiting_switch
pm_calltransfer_switch
pm_callforward_switch
pm_callerblock_switch
pm_call_transfer_resume
pm_call_transfer
pm_call_park
pm_call_out
pm_battery_event_cb
pm_answer
pm_anonymous_reject_switch
pm_TftpUpdate
pm_3_way_call
pm2IfTable
pllInit
playTone__15CdspRootManagerUsUsUsUsUs
playTone__11CdspManagerUsUsUsUsUs
pl2_buff
pktMblkClBlkDesc
pktClDescTblNumEnt
pktClDescTbl
pipeMsgQOptions
pipeDrv
pipeDevDelete
pipeDevCreate
pinyincpy
pinyin_tbl
pinyinStr
pingLibInit
ping
pickup_opt
picklist_secret_needdata
picklist_idle_needdata
pic_exit
phse_getProductID
phse_Start
phseWriteNack
phseWriteAck
phseTask
phseReadCmdHeader
phonesetting_exit
phone_pwd
phashinit
pfw_start_address
pfw_section0
pfw_count
pfwTimerTickShow
pfwTimerStart
pfwTimerManagerDelete
pfwTimerManagerCreate
pfwTimerExpire
pfwTimerDelete
pfwTimerCreate
pfwTimerCancel
pfwTimeStampStart
pfwTimeStampExpired
pfwTableTraverse
pfwTableShow
pfwTableItemInsertBefore
pfwTableItemInsertAfter
pfwTableItemGet
pfwTableItemDelete
pfwTableItemCountGet
pfwTableItemAdd
pfwTableDelete
pfwTableCreate
pfwTable
pfwStackTableDelete
pfwStackTableCreate
pfwStackStatusGet
pfwStackShow
pfwStackPluginObjDelete
pfwStackPluginObjAdd
pfwStackParamSet
pfwStackParamGet
pfwStackObjPfwGet
pfwStackObjGet
pfwStackListShow
pfwStackIdGet
pfwStackDestroy
pfwStackDelete
pfwStackAdd
pfwShow
pfwSend
pfwReceive
pfwProfileTreeCopy
pfwProfileTableDelete
pfwProfileTableCreate
pfwProfileShow
pfwProfileSet
pfwProfilePfwObjGet
pfwProfileObjGet
pfwProfileListShow
pfwProfileDelete
pfwProfileCreate
pfwPrintError
pfwPluginObjStateRelease
pfwPluginObjStateLock
pfwPluginObjStateGet
pfwPluginObjStateExclusiveGet
pfwPluginObjShow
pfwPluginObjGet
pfwParameterTableDelete
pfwParameterTableCreate
pfwParameterListShow
pfwParameterIdGet
pfwParameterAdd
pfwObjGet
pfwNextComponentStateGet
pfwNewLayerProfileItemAdd
pfwNewComponentProfileItemAdd
pfwNetPoolIdGet
pfwMemoryShow
pfwMemoryManagerDelete
pfwMemoryManagerCreate
pfwMalloc
pfwListShow
pfwLayerTableDelete
pfwLayerTableCreate
pfwLayerStateGet
pfwLayerShow
pfwLayerObjGet
pfwLayerListShow
pfwLayerDelete
pfwLayerAdd
pfwInterfaceUnbind
pfwInterfaceRegister
pfwInterfaceReferenceDelete
pfwInterfaceReferenceAdd
pfwInterfaceObjGetViaPluginObj
pfwInterfaceObjGetViaPfwObj
pfwInterfaceObjGetNext
pfwInterfaceObjAndStateGetViaStackObj
pfwInterfaceManagerDelete
pfwInterfaceManagerCreate
pfwInterfaceListShow
pfwInterfaceIdGet
pfwInterfaceBind
pfwInit
pfwIdGet
pfwFree
pfwFirstComponentStateGet
pfwEventUnsubscribe
pfwEventSubscribe
pfwEventStackSubscribe
pfwEventRaise
pfwEventPublish
pfwEventPluginObjUnsubscribe
pfwEventObjGet
pfwEventManagerDelete
pfwEventManagerCreate
pfwEventListShow
pfwEventItemListDelete
pfwEventItemDelete
pfwEventItemAdd
pfwDelete
pfwDataJobAdd
pfwCreate
pfwControlJobAdd
pfwComponentTableDelete
pfwComponentTableCreate
pfwComponentShow
pfwComponentObjGetByProtocol
pfwComponentObjGetByName
pfwComponentListShow
pfwComponentDelete
pfwComponentAdd
pfwBaseProfileCreate
pfn_setting_needdata
pfn_reg_svnmcallbk
pfn_pro_volume_ok
pfn_pro_main_whisper
pfn_pro_main_warning
pfn_pro_main_volume
pfn_pro_main_start
pfn_pro_main_ringtone
pfn_pro_main_ringmode
pfn_pro_main_keytone
pfn_pro_main_infotone
pfn_picfield_Puncdraw
pfn_entry_volume
pfn_entry_tone
pfn_Save_Draw
pfn_Pro_start_mainmenu
pfn_ProSpeedMenuClose
pfn_ProMenuClose
pfn_Needdata_WorkModePicklist
pfn_Needdata_TimeFormatPicklist
pfn_Needdata_ScriptFilesPicklist
pfnTran_ToolMenuClose
pfnTran_RegMenuClose
pfnCond_VoiceProcess
pfnCond_VendorVersion
pfnCond_VendorProductCategory
pfnCond_VendorName
pfnCond_VendorModeName
pfnCond_VendorInf
pfnCond_VendorEnterpriseCode
pfnCond_VMBoxPwEdit
pfnCond_VMBoxNumEdit
pfnCond_VMAccessNumEdit
pfnCond_VAD
pfnCond_TFTPWorkModePicklist
pfnCond_TFTPPortEdit
pfnCond_TFTPIPEdit
pfnCond_TFTPEncrKeyEdit
pfnCond_TFTPDomainEdit
pfnCond_TFTPDirFileEdit
pfnCond_StunServerPortEdit
pfnCond_StunServerNameEdit
pfnCond_StunOnOffPicklist
pfnCond_SoWrite
pfnCond_SIPUserNameEdit
pfnCond_SIPServiceNameEdit
pfnCond_SIPRegSerPortEdit
pfnCond_SIPRegSerIPEdit
pfnCond_SIPRegSerDomainEdit
pfnCond_SIPProxyPortEdit
pfnCond_SIPProxyIPEdit
pfnCond_SIPProxyDomainEdit
pfnCond_SIPPortEdit
pfnCond_SIPPasswordProtect
pfnCond_SIPPasswordEdit
pfnCond_SIPOBProxyPicklist
pfnCond_SIPDNSSRVPicklist
pfnCond_SIPAuthStrEdit
pfnCond_SIPAuthAlgEdit
pfnCond_RTPPortEdit
pfnCond_RTPPackTimePicklist
pfnCond_RTPJitbufCompEdit
pfnCond_PLC
pfnCond_NoiseSuppression
pfnCond_NATWorkModePicklist
pfnCond_NATSerPortEdit
pfnCond_NATSerIPEdit
pfnCond_NATSerDomainEdit
pfnCond_NATKATimeEdit
pfnCond_NATKAPackDestPicklist
pfnCond_NATIPEdit
pfnCond_Menu2WfconfigPickList
pfnCond_Menu2WfconfigOperating
pfnCond_IPSubnetMaskEdit
pfnCond_IPGatewayIPEdit
pfnCond_IPDHCPInfo
pfnCond_IPAddrEdit
pfnCond_GeneralJitterBuffer
pfnCond_GJBMaxConnection
pfnCond_GJBBufferSize
pfnCond_Exit_TftpServer
pfnCond_Exit_Auth
pfnCond_Exit
pfnCond_DNSSecIPEdit
pfnCond_DNSPriorityPicklist
pfnCond_DNSPriIPEdit
pfnCond_DHCPPicklist
pfnCond_ConfirmDlg_Stay
pfnCond_ConfirmDlg
pfnCond_Confirm
pfnCond_CodecPriority
pfnCond_CNG
pfnCond_AcousticsEchoCancellation
pfnCond_AECWorkMode
pfnCond_AECTailTime
pfnCondWebAuthInputContiune
pfnCondWebAuthInput2Process
pfnCondWebAuthInput2Menu
pfnCndWebAuthScriptFileSelect
pfnCndWebAuthProcessTimeout
pfnCndWebAuthProcessRsp
pfnCndWebAuthProcessPCRsp
pfnCndWebAuthProcess2Menu
pfnCndWebAuthProcess2Idle
pfnCndWebAuthDownScriptTimeout
pfnCndWebAuthDownScriptRsp
pfnCndWebAuthDownScriptExit2Menu
pfnCndWebAuthDownScript2Menu
pfnCndWebAuthConnTimeout
pfnCndWebAuthConnSuccess
pfnCndWebAuthConnRsp
pfnCndWebAuthConnExit2Menu
pfnCndWebAuthConn2Menu
pfnCndWebAuthConn2Input
pfnCndWebAuthConn2Idle
pfnCndTftpServerProcess
pfnCndTftpServerOK
pfnCndTftpServerEmpty
pfnCndMisc2WebAuthUrl
pfnCndMisc2WebAuthScriptFiles
pfnCndMisc2WebAuthDownScript
pfnCndMisc2WebAuthConn
pfnCndActiveScriptRsp
pfnCndActiveScriptProcessTimeout
pffindtype
pffindproto
pfctlinput2
pfctlinput
perror
periodic_lcp_echo_request
periodic_ipcp_configure_or_termination_request
periodRun
period
pdnsDebugFunc
pcmu8000
pcma8000
pcm8000
pcCard
pbkdf2_sha1
pbidx_init_e
pbidx_init
pbidx2srchidx
pb_search_idx
pb_listview_createEx
pb_list_create
pbGbToPinyin
payload_type_new
payload_type_get_rtpmap
payload_type_destroy
payload_type_clone
payload_is_supported
pause
path_mtu_discovery
pathSplit
pathParse
pathLastNamePtr
pathLastName
pathCondense
pathCat
pathBuild
password_def
parser_isknownheader
parser_init
parser_callmethod
parse_rtp_pack
parse_ppp_options_from_reject_configure
parse_ppp_options_from_packet
parse_ppp_options_from_nak_configure
parse_ppp_options_from_configure_request
parse_option_value
parse_audio_codec_list
paramSet__15CdspRootManager
paramReset__15CdspRootManager
papRemoteUserNameGet
papLocalUserNameSet
papLocalUserNameGet
panicSuspend
panic
packetLossConcealment__15CdspRootDecoderUsUc
packetLossConcealment__11CdspDecoderUsUc
p_rr
p_fqname
p_cdnname
p_cdname
pWvNetEventMap
pWFSettingMenu
pToolsMenu
pTgtName
pTaskLastFpTcb
pTaskLastDspTcb
pSysctlCtxList
pSysMenu
pSuppPrj
pSockFdMap
pSmsMenu
pShortMenu
pSettingSecretMenu
pSettingMenu
pRootMemStart
pRightArrowMenu
pRegisterMenu
pProfileMenu
pPortEditField
pPbMenu
pOwnNumField
pOpeMenu
pNetServiceMenu
pMiscMenu
pMibRtn
pMemoMenu
pM2TrapRtnArg
pM2TrapRtn
pM2IfRootPtr
pM2IfRoot
pLocalInputLabel
pLocalInputField
pJobPool
pIfTypes
pIPEditField
pGamesMenu
pFppTaskIdPrevious
pFSpKey_lBtn
pDomainEditField
pDhcpcBootCookie
pDevName
pDTushort
pDTulong
pDTuint4
pDTuint2
pDTuchar
pDTstring
pDTshort
pDTmacaddr
pDTlong
pDTipaddress
pDTint4
pDTint2
pDTchar
pBpfDevTbl
pAddrString
own_number_edited
ownNumEdit
osipua_init
osipua_fix_via_header
osipua_exit
osipua_execute
osipua_distribute_event
osip_ua_signal_connect
osip_ua_set_registrar
osip_ua_set_proxy
osip_ua_set_presence_mode
osip_ua_set_presence_delay
osip_ua_set_presence_contact_url
osip_ua_set_outbound_proxy
osip_ua_set_max_dialogs
osip_ua_set_ip4addr
osip_ua_set_contact
osip_ua_remove_alias
osip_ua_new
osip_ua_init
osip_ua_get_dialog
osip_ua_find_handler
osip_ua_find
osip_ua_destroy
osip_ua_clean_alias
osip_ua_call_leg_exists
osip_ua_add_body_handler
osip_ua_add_alias
osip_transaction_find
osip_trace
osip_timers_nist_execute
osip_timers_nict_execute
osip_timers_ist_execute
osip_timers_init
osip_timers_ict_execute
osip_stop_retransmissions_from_dialog
osip_stop_200ok_retransmissions
osip_start_ack_retransmissions
osip_start_200ok_retransmissions
osip_setcb_send_message
osip_setcb_nist_unknown_received
osip_setcb_nist_transport_error
osip_setcb_nist_subscribe_received
osip_setcb_nist_request_received2
osip_setcb_nist_register_received
osip_setcb_nist_refer_received
osip_setcb_nist_options_received
osip_setcb_nist_notify_received
osip_setcb_nist_message_received
osip_setcb_nist_kill_transaction
osip_setcb_nist_info_received
osip_setcb_nist_cancel_received
osip_setcb_nist_bye_received
osip_setcb_nist_6xx_sent
osip_setcb_nist_5xx_sent
osip_setcb_nist_4xx_sent
osip_setcb_nist_3xx_sent
osip_setcb_nist_3456xx_sent2
osip_setcb_nist_2xx_sent2
osip_setcb_nist_2xx_sent
osip_setcb_nist_1xx_sent
osip_setcb_nict_unknown_sent
osip_setcb_nict_transport_error
osip_setcb_nict_subscribe_sent
osip_setcb_nict_request_sent2
osip_setcb_nict_register_sent
osip_setcb_nict_refer_sent
osip_setcb_nict_options_sent
osip_setcb_nict_notify_sent
osip_setcb_nict_message_sent
osip_setcb_nict_kill_transaction
osip_setcb_nict_info_sent
osip_setcb_nict_cancel_sent
osip_setcb_nict_bye_sent
osip_setcb_nict_6xx_received
osip_setcb_nict_5xx_received
osip_setcb_nict_4xx_received
osip_setcb_nict_3xx_received
osip_setcb_nict_3456xx_received2
osip_setcb_nict_2xx_received2
osip_setcb_nict_2xx_received
osip_setcb_nict_1xx_received
osip_setcb_ist_transport_error
osip_setcb_ist_kill_transaction
osip_setcb_ist_invite_received2
osip_setcb_ist_invite_received
osip_setcb_ist_ack_received2
osip_setcb_ist_ack_received
osip_setcb_ist_6xx_sent
osip_setcb_ist_5xx_sent
osip_setcb_ist_4xx_sent
osip_setcb_ist_3xx_sent
osip_setcb_ist_3456xx_sent2
osip_setcb_ist_2xx_sent2
osip_setcb_ist_2xx_sent
osip_setcb_ist_1xx_sent
osip_setcb_ict_transport_error
osip_setcb_ict_kill_transaction
osip_setcb_ict_invite_sent2
osip_setcb_ict_invite_sent
osip_setcb_ict_ack_sent2
osip_setcb_ict_ack_sent
osip_setcb_ict_6xx_received
osip_setcb_ict_5xx_received
osip_setcb_ict_4xx_received
osip_setcb_ict_3xx_received
osip_setcb_ict_3456xx_received2
osip_setcb_ict_2xx_received2
osip_setcb_ict_2xx_received
osip_setcb_ict_1xx_received
osip_set_application_context
osip_send_response
osip_retransmissions_execute
osip_reset
osip_reregistration_execute
osip_remove_nist
osip_remove_nict
osip_remove_ist
osip_remove_ict
osip_parse
osip_nist_unlock
osip_nist_lock
osip_nist_execute
osip_nict_unlock
osip_nict_lock
osip_nict_execute
osip_new_outgoing_sipmessage
osip_new_incoming_sipmessage
osip_new_event
osip_manager_stop_udp_daemon
osip_manager_stop_resolver
osip_manager_start_udp_daemon
osip_manager_start_resolver
osip_manager_set_send_port
osip_manager_remove_udpport_all
osip_manager_remove_udpport
osip_manager_new
osip_manager_destroy
osip_manager_add_udpport
osip_ist_unlock
osip_ist_lock
osip_ist_execute
osip_init
osip_ict_unlock
osip_ict_lock
osip_ict_execute
osip_global_initialized
osip_global_init
osip_global_free
osip_get_application_context
osip_generate_response_out_of_dialog
osip_free
osip_find_transaction_and_add_event
osip_find_transaction
osip_event_init
osip_dialog_unregister
osip_dialog_send_response
osip_dialog_send_request
osip_dialog_respond
osip_dialog_replaces_find
osip_dialog_release
osip_dialog_reject_invite
osip_dialog_register_with_authentication
osip_dialog_register
osip_dialog_refer_with_authentication
osip_dialog_refer
osip_dialog_ping
osip_dialog_option
osip_dialog_notify
osip_dialog_new_from_incoming_trn
osip_dialog_new
osip_dialog_message
osip_dialog_invite_with_authentication
osip_dialog_invite_3way
osip_dialog_invite
osip_dialog_init2
osip_dialog_init
osip_dialog_hold
osip_dialog_get_body_context
osip_dialog_generate_response_default
osip_dialog_generate_request_within_dialog
osip_dialog_find_simple
osip_dialog_find
osip_dialog_exists
osip_dialog_destroy
osip_dialog_bye_with_authentication
osip_dialog_bye
osip_dialog_alloc
osip_dialog_add_message_body_to_request
osip_dialog_add_body_to_request
osip_dialog_add_body_context
osip_dialog_ack
osip_dialog_accept_invite
osip_create_transaction
osip_create_proxy_authorization_header_indialog
osip_create_proxy_authorization_header
osip_create_authorization_header
osip_add_nist
osip_add_nict
osip_add_ist
osip_add_ict
osip_ack_retransmission
osapi_thrid
osapi_mutex_unlock
osapi_mutex_lock
osapi_mutex_init
osapi_mutex_destroy
osapi_exit_thr
osapi_create_thr
ori_getBuf
optreset
optopt
option_value_match
option_list_print
option_entry_print
optind
opterr
optarg
openlog
opendir
open_udp_unconn
open_udp_conn
open_rtp_session
open_port
open
onxoff_pwd_needdata
onoff_animate_set
onoff_animate_needdata
on_replaces_invite
on_other_invite
on_first_invite
onCharger
omac1_aes_128
oisp_dialog_set_sdp_c
oidsInList
oidfmt_node
offset127
offset0xD5
offset0
objShow
objFree
objCoreTerminate
objCoreInit
objAllocExtra
objAlloc
nvttostr
num_count
numBpfDevs
null_state
nstp_task_id
notify_sip_sem
nothrow
notealias
noprint__Fe
nolog__Fe
no_check
noOfCategories
nmbufs
nmbclusters
nist_unload_fsm
nist_timeout_j_event
nist_snd_23456xx
nist_snd_1xx
nist_register_received
nist_refer_received
nist_rcv_request
nist_options_received
nist_notify_received
nist_need_timer_j_event
nist_message_received
nist_load_fsm
nist_kill_transaction
nist_init
nist_info_received
nist_get_fsm
nist_fsm
nist_free
nist_cancel_received
nist_bye_received
nict_unload_fsm
nict_timeout_k_event
nict_timeout_f_event
nict_timeout_e_event
nict_snd_request
nict_set_destination
nict_rcv_23456xx
nict_rcv_1xx
nict_need_timer_k_event
nict_need_timer_f_event
nict_need_timer_e_event
nict_load_fsm
nict_kill_transaction
nict_init
nict_get_fsm
nict_fsm
nict_free
nict_6xx_received
nict_5xx_received
nict_4xx_received
nict_3xx_received
nict_2xx_received
nict_1xx_received
next_separator
next_port
next_node
nextIndex
newaddr
new_random_number
new_and_bind_socket
netmask
nethash
net_node
net_config_uninit
net_config_init
net_add_domain
netTypeInit
netTypeDelete
netTypeAdd
netTupleGet
netTaskStackSize
netTaskSemId
netTaskPriority
netTaskOptions
netTaskId
netTask
netStackSysPoolShow
netStackDataPoolShow
netShowInit
netPoolShow
netPoolKheapInit
netPoolInit
netPoolDelete
netMessageHandler
netMblkToBufCopy
netMblkOffsetToBufCopy
netMblkGet
netMblkFromBufCopy
netMblkFree
netMblkDup
netMblkClJoin
netMblkClGet
netMblkClFree
netMblkClChainFree
netMblkChainDup
netLsByName
netLibInit
netJobNum
netJobAlloc
netJobAdd
netInfo
netHelp
netGtfTickInformation
netGtfTickFunc
netFlashUp
netErrnoSet
netDrvFileDoesNotExistInstall
netDrvFileDoesNotExist
netDrvDebugLevelSet
netDrv
netDiscoverResponseTask
netDevCreate2
netDevCreate
netDevBootFlag
netCoreInstInit
netClusterGet
netClPoolIdGet
netClFree
netClBlkJoin
netClBlkGet
netClBlkFree
netBufLibInit
netAttachFlag
ncp_packet_received
ncpLinkReset
nanosleep
namelessPrefix
name_node
name__C9type_info
name6Init
name
nPartitionCount
nOperator
nCursorFlag
mykey
muxUnbind
muxTxRestart
muxTkSend
muxTkReceive
muxTkPollSend
muxTkPollReceive
muxTkPktsReceive
muxTkLibInit
muxTkDrvCheck
muxTkDebug
muxTkCookieGet
muxTkBindCommon
muxTkBind
muxShow
muxSend
muxReceive
muxPollSend
muxPollReceive
muxPacketDataGet
muxPacketAddrGet
muxMCastAddrGet
muxMCastAddrDel
muxMCastAddrAdd
muxLock
muxLinkHeaderCreate
muxLibInit
muxIterateByName
muxIoctl
muxIfTypeGet
muxIfFuncGet
muxIfFuncDel
muxIfFuncAdd
muxError
muxEndProtoRegister
muxEndProtoFree
muxDevUnload
muxDevStopAll
muxDevStop
muxDevStart
muxDevLoad
muxDevExists
muxDebug
muxBind
muxAddressForm
muxAddrResFuncGet
muxAddrResFuncDel
muxAddrResFuncAdd
muxAdapterDelete
muxAdapterCreate
mutexOptionsVmMpuLib
mutexOptionsUnixLib
mutexOptionsTyLib
mutexOptionsSymLib
mutexOptionsSelectLib
mutexOptionsNetDrv
mutexOptionsMemLib
mutexOptionsLogLib
mutexOptionsIosLib
mutexOptionsHostLib
muted
muteOn__15CdspRootManager
muteOn__11CdspManager
muteOff__15CdspRootManager
muteOff__11CdspManager
mudTempMemIdGet
mudTempMemFree
mudTempMemFlush
mudTempMemAlloc
mudStop
mudStart
mudSocketGet
mudShowCons
mudPermMemIdGet
mudPermMemFree
mudPermMemFlush
mudPermMemAlloc
mudErrorGet
mudEnvSet
mudEnvGet
mudDestroy
mudCreate
mudAddConnInitHandler
msgprint_buffer
msgbox_test
msg_startline_init
msg_startline_free
msg_setwww_authenticate
msg_setvia
msg_setversion
msg_seturi
msg_settopheader
msg_setto
msg_setstatuscode
msg_setroute
msg_setreplaces
msg_setrecord_route
msg_setreasonphrase
msg_setproxy_authorization
msg_setproxy_authenticate
msg_setmime_version
msg_setmethod
msg_setheader
msg_setfrom
msg_seterror_info
msg_setcseq
msg_setcontent_type
msg_setcontent_length
msg_setcontent_encoding
msg_setcontact
msg_setcall_info
msg_setcall_id
msg_setbody_mime
msg_setbody
msg_setauthorization
msg_setallow
msg_setalert_info
msg_setaccept_language
msg_setaccept_encoding
msg_setaccept
msg_set_subs_state
msg_set_referto
msg_set_referred_by
msg_set_header
msg_set_event
msg_set_allow_events
msg_parse
msg_init
msg_headers_parse
msg_header_getbyname
msg_handle_multiple_values
msg_getwww_authenticate
msg_getvia
msg_getversion
msg_geturi
msg_getto
msg_getstatuscode
msg_getroute
msg_getreplaces
msg_getrecord_route
msg_getreasonphrase
msg_getreason
msg_getproxy_authorization
msg_getproxy_authenticate
msg_getmime_version
msg_getmethod
msg_getheader
msg_getfrom
msg_geterror_info
msg_getcseq
msg_getcontent_type
msg_getcontent_length
msg_getcontent_encoding
msg_getcontact
msg_getcall_info
msg_getcall_id
msg_getbody_by_mime
msg_getbody
msg_getauthorization
msg_getallow
msg_getalert_info
msg_getaccept_language
msg_getaccept_encoding
msg_getaccept
msg_get_subs_state
msg_get_referred_by
msg_get_refer_to
msg_get_event
msg_get_allow_events
msg_free
msg_force_update
msg_fix_last_via_header
msg_clone
msg_body_parse
msg_appendtopvia
msg_2char
msgQTerminate
msgQSmShowRtn
msgQSmSendRtn
msgQSmReceiveRtn
msgQSmNumMsgsRtn
msgQSmInfoGetRtn
msgQShowInit
msgQShow
msgQSend
msgQReceive
msgQNumMsgs
msgQLibInit
msgQInstClassId
msgQInit
msgQInfoGet
msgQEvStop
msgQEvStart
msgQEvLibInit
msgQDistShowRtn
msgQDistSendRtn
msgQDistReceiveRtn
msgQDistNumMsgsRtn
msgQDistInfoGetRtn
msgQDelete
msgQCreate
msgQClassId
msgBuf
msf_enable
msf_disconnect
msf_disable
msf_connect
mrt_ioctl
mpStackConvert
moduleTerminate
moduleShow
moduleSegNext
moduleSegGet
moduleSegFirst
moduleSegEach
moduleSegAdd
moduleNameGet
moduleLibInit
moduleInit
moduleInfoGet
moduleIdListGet
moduleIdFigure
moduleFlagsGet
moduleFindByNameAndPath
moduleFindByName
moduleFindByGroup
moduleEach
moduleDelete
moduleCreateHookDelete
moduleCreateHookAdd
moduleCreate
moduleClassId
moduleCheck
modf
model
mmuStateTransArraySize
mmuStateTransArray
mmuSoftCrGet
mmuReadId
mmuPhysAddrShift
mmuPageBlockSize
mmuModifySoftCr
mmuModifyHardCr
mmuModifyCr
mmuLibFuncs
mmuHardCrGet
mmuCrGet
mmuArm946eWbcrSet
mmuArm946eWbcrGet
mmuArm946ePrrSet
mmuArm946ePrrGet
mmuArm946ePrSet
mmuArm946ePrGet
mmuArm946eLibInstall
mmuArm946eCcrSet
mmuArm946eCcrGet
mmuArm946eAEnable
mmuArm946eADisable
mmd_check_comp
mmbfree
mktime
mkdir
microtime
micBiasSwitch__15CdspRootManagerUs
micBiasSwitch__11CdspManagerUs
mibIfAlloc
mib2Init
mib2ErrorAdd
mg_trigger_ata_event
mg_add_read_msgq
mfi_sup
metric
merge_param
menuIdNetSrv
memset
memmove
memcpy
memcmp
memchr
memalign
memSysPartId
memShowInit
memShow
memPoolUsed
memPoolNew
memPoolFree
memPoolDelete
memPoolCleanup
memPoolCheck
memPoolAvail
memPoolAlloc
memPartShow
memPartSemInitRtn
memPartRealloc
memPartOptionsSet
memPartOptionsDefault
memPartLibInit
memPartInstClassId
memPartInit
memPartInfoGet
memPartFree
memPartFindMax
memPartCreate
memPartClassId
memPartBlockIsValid
memPartBlockErrorRtn
memPartAllocErrorRtn
memPartAlloc
memPartAlignedAlloc
memPartAddToPool
memOptionsSet
memLibInit
memInit
memGzSeek
memGzRead
memGzOpen
memGzClose
memFindMax
memDefaultAlignment
memAddToPool
melodyTone__15CdspRootManagerUsUsUsUsUs
melodyTone__11CdspManagerUsUsUsUsUs
melodyToneDownload__15CdspRootManagerUsUsPUsUsUsUsUs
melodyToneDownload__11CdspManagerUsUsPUsUsUsUsUs
melodyCadenceOn
md5_mac
mbufSysctlInit
mbufShow
mbtypes
mbtowc
mbstowcs
mblen
mbinit
maxsockets
max_protohdr
max_linkhdr
max_hdr
max_fd
max_datalen
maxPinYinStr
maxFiles
maxDrivers
mathSoftInit
manufacId
malloc1
malloc
make_request
make_release
make_message
make_discover
make_decline
make_cancel
main_config
magic_init
macAddress
m_split
m_realloc
m_pullup
m_prepend
m_pDIdxTblHead
m_mballoc_wid
m_malloc
m_gethdr
m_getclr
m_get
m_freem
m_free
m_devget
m_definitmemory
m_copypacket
m_copym
m_copydata
m_copyback
m_clalloc_wid
m_cat
m_calloc
m_adj
mRouteShow
mRegs
mCastRouteFwdHook
m2pppSecuritySecretsLibInit
m2pppSecuritySecretsLibClear
m2pppSecurityPeerSecretsShow
m2pppSecurityLocalSecretsShow
m2pppSecurityConfigUnregister
m2pppSecurityConfigRegister
m2pppSecurityConfigEntrySetWrap
m2pppSecurityConfigEntrySet
m2pppSecurityConfigEntryLookup
m2pppSecretsSecretGet
m2pppSecretsEntrySet
m2pppSecretsEntryDelete
m2pppSecretsEntryAgentSet
m2pppSecretsEntryAgentLookup
m2pppSecretsEntryAgentDelete
m2pppSecretsDataEntryPtrAgentLookup
m2pppPreviousSecretsDataEntryPtrAgentLookup
m2pppPreviousInterfaceStackObjGet
m2pppNextSecretsEntryAgentLookup
m2pppNextSecretsDataEntryPtrAgentLookup
m2pppNextInterfaceStackObjGet
m2pppLinkStatusEntryLookup
m2pppLinkGroupUnregister
m2pppLinkGroupRegister
m2pppLinkConfigEntryLookup
m2pppLibInit
m2pppLibClear
m2pppIpcpGroupUnregister
m2pppIpcpGroupRegister
m2pppIpcpEntryLookup
m2pppInterfaceUnregister
m2pppInterfaceStackObjGet
m2pppInterfaceRegister
m2VariableUpdate
m2UdpTblEntryGet
m2UdpInit
m2UdpGroupInfoGet
m2UdpDelete
m2TcpInit
m2TcpGroupInfoGet
m2TcpDelete
m2TcpConnEntrySet
m2TcpConnEntryGet
m2SysInit
m2SysGroupInfoSet
m2SysGroupInfoGet
m2SysDelete
m2SetIfLastChange
m2RouteTableSize
m2RouteTableGet
m2RouteTable
m2PollStatsIfPoll
m2NumRouteEntries
m2LibInit
m2IpRouteTblEntrySet
m2IpRouteTblEntryGet
m2IpInit
m2IpGroupInfoSet
m2IpGroupInfoGet
m2IpDelete
m2IpAtransTblEntrySet
m2IpAtransTblEntryGet
m2IpAddrTblEntryGet
m2InterfaceSem
m2Init
m2IfVarUpdateRtnInstall
m2IfUsrCountersRemove
m2IfUsrCountersInstall
m2IfTblEntrySet
m2IfTblEntryGet
m2IfTableUpdate
m2IfTableLastChange
m2IfStackTblUpdate
m2IfStackLastChange
m2IfStackEntrySet
m2IfStackEntryGet
m2IfRcvAddrEntrySet
m2IfRcvAddrEntryGet
m2IfPktCountRtnInstall
m2IfMgtLibInit
m2IfInit
m2IfGroupInfoGet
m2IfFree
m2IfDelete
m2IfCtrUpdateRtnInstall
m2IfCount
m2IfCentiSecsGet
m2IfAlloc
m2If8023PacketCount
m2If64BitCounters
m2IcmpInit
m2IcmpGroupInfoGet
m2IcmpDelete
m2Delete
m2CounterUpdate
ltv_info
ltostr__FPcl
lstProtoInUse
lstPrevious
lstNth
lstNext
lstNStep
lstLibInit
lstLast
lstInsert
lstInit
lstGet
lstFree
lstFirst
lstFind
lstExtract
lstDelete
lstCount
lstConcat
lstAdd
lseek
lpc1016
lpc1015
looutput
loopattach
longjmp
long_lock_needdata
loioctl
loif
logout
loginUserVerify
loginUserShow
loginUserDelete
loginUserAdd
loginTimeOutInSecond
loginStringSet
loginPrompt
loginInit
loginEncryptInstall
loginDefaultEncrypt
loggingSem
logfile
log_in_vain
log_dump
logTaskStackSize
logTaskPriority
logTaskOptions
logTaskId
logTask
logShow
logMsg
logInit
logFdSet
logFdFromRlogin
logFdDelete
logFdAdd
log10
lock
localtime_r
localtime
localip
localeconv
local_log
localToGlobalOffset
localMGAddr
localIPNumber
localIPAddr
localGWAddr
loadSegmentsAllocate
loadRoutine
loadModuleGet
loadModuleAtSym
loadModuleAt
loadModule
loadElfInit
loadCommonMatch
loadCommonManage
lnglockopt_sel
lnglockopt_needdata
lng_lock_pwd_wrong
llinfo_arp
llAddrConvert
lkup
lkAddr
listofchar_free
listen
list_special_free
list_size
list_remove_el
list_remove
list_init
list_head
list_get
list_free
list_eol
list_add
linkedCtorsInitialized
link_ntoa
link_node
link_addr
linkSyms
linkDataSyms
lid_opened
lidOpened
lidInt
libiberty_demanglers
lexStateTable
lexNclasses
lexClass
lexActions
legal_vif_num
ledRead
ledOpen
ledId
ledControl
ledClose
ldiv_r
ldiv
ldexp
ldCommonMatchAll
lcp_packet_received
lcpStateActionTable
lcpSetSendActionFunctions
lcpSetReceiveFunctions
lcpRecvPcktCopy
lcpProxyLcpDo
lcpMpOptionsGet
lcpMIBPrint
lcpInterfacesInit
lcpComponentDelete
lcpComponentCreate
lcd_start
lcd_rs
lcd_reset
lcd_port_init
lcd_out_byte
lcd_mask
lcd_delay
lcd_data
lcd_cs
lcd_clk
lcd_all_port_high
lcdMsg
lastCceFocus
language_mode_needdata
labs
lableCallback
l2_task_id
l2_packet_set_rx_l2_hdr
l2_packet_send
l2_packet_init
l2_packet_get_own_addr
l2_packet_deinit
l2_data_sem
ksleep
kpddelay
kpd_shutdown
kpd_send
kpd_register
kpd_press_num
kpd_keySend
kpd_delay
kpdInit
klc_config
kill_all_transaction
killSIPStackForSoAndTFTP
killSIPStack
kill
keypad_char_idx
keyboardSpn
keyboardPor
keyboardIta
keyboardGer
keyboardFre
keyboardEng
keyboardBas
keyInt
kernel_sysctl
kernelVersion
kernelTimeSlice
kernelState
kernelIsIdle
kernelInit
kern_node
kernSysctlInit
keep_address_mapping
keepAliveMappingPort
kUniqueSignature
kSectorSize
kNVRamSize
kMacroRepeatNestMax
jsManglerHandler
join_mcast
jbTId
jbReadSocket
jbParamTable
jbParamInfo
jbDspPutManager
jbDspGetManager
jbCb
jbActvTmr__FP12TimerMessage
jbActvInit
itoa
isxdigit
isvallid_rtcp
isupper
ist_unload_fsm
ist_timeout_i_event
ist_timeout_h_event
ist_timeout_g_event
ist_snd_3456xx
ist_snd_2xx
ist_snd_1xx
ist_set_auto_send_100
ist_rcv_invite
ist_rcv_ack
ist_need_timer_i_event
ist_need_timer_h_event
ist_need_timer_g_event
ist_load_fsm
ist_kill_transaction
ist_invite_received
ist_init
ist_get_fsm
ist_fsm
ist_free
ist_create_resp_100
ist_ack_received
isspace
ispunct
isprint
isn_secret
isn_last_reseed
isn_ctx
islower
isgraph
isdigit
iscntrl
isatty
isalpha
isalnum
is_trace_level_activate
is_option_present
is_mcast
is_in_recv_thread_context
is_eloop_terminated
is_eloop_stop
is_eloop_running
isPowerOnState
isOntheSamePage
isMMIInPowerOff
isMMIInIdle
isDirKey
isCceFullScreen
iptime
iptMpuInit
ipstatShow
ipstat
ipport_lowlastauto
ipport_lowfirstauto
ipport_lastauto
ipport_hilastauto
ipport_hifirstauto
ipport_firstauto
ipintrq_present
ipintrq
ipforwarding
ipforward_rt
ipcp_zero_restart_counter
ipcp_this_layer_up
ipcp_this_layer_start
ipcp_this_layer_finished
ipcp_this_layer_down
ipcp_set_ppp_state
ipcp_pppStateGet
ipcp_pppPhaseGet
ipcp_periodic_timer
ipcp_null_state
ipcp_maxTerminationRequests
ipcp_maxConfigRequests
ipcp_initialize_restart_counter
ipcp_configReqSendInterval
ipcp_TerminationReqInterval
ipcpStateActionTable
ipcpSetSendActionFunctions
ipcpInterfacesInit
ipcpAddrGet
ipc_node
ip_stripoptions
ip_srcroute
ip_slowtimo
ip_savecontrol
ip_rtaddr
ip_protox
ip_phone_oper
ip_output
ip_optcopy
ip_node
ip_mcast_src
ip_input
ip_init
ip_id
ip_fw_ctl_ptr
ip_fw_chk_ptr
ip_freemoptions
ip_forward
ip_drain
ip_defttl
ip_ctloutput
ip_chksrcroute
ip_as_uint
ip_as_str
ip_as_static_str
ipTxStartup
ipRawSysctlInit
ipNptError
ipMaxUnits
ipInstInit
ipInputSysctlInit
ipDrvCtrlFieldsGet
ipDrvCtrl
ipDetach
ipAttach
iosWrite
iosShowInit
iosRead
iosOpen
iosNextDevGet
iosLibInitialized
iosIoctl
iosInit
iosFdValue
iosFdShow
iosFdSet
iosFdNewHookRtn
iosFdNew
iosFdFreeHookRtn
iosFdFree
iosFdDevFind
iosDvList
iosDrvShow
iosDrvRemove
iosDrvInstall
iosDevShow
iosDevFind
iosDevDelete
iosDevAdd
iosDelete
iosCreate
iosClose
ioctlBatchWrite
ioctlBatchRead
ioctl
ioTaskStdSet
ioTaskStdGet
ioMaxLinkLevels
ioHelp
ioGlobalStdSet
ioGlobalStdGet
ioFullFileNameGet
ioDefPathSet
ioDefPathGet
ioDefPathCat
ioDefPath
ioDefDirGet
ioDefDevGet
invite_cb
invite_accepted_cb
invite_accepted_as_1xxsdp_cb
int_2char
intVecTableWriteProtect
intVecBaseSet
intVecBaseGet
intVBRSet
intUnlock
intUninitVecSet
intRestrict
intRegsUnlock
intRegsLock
intLockLevelSet
intLockLevelGet
intLock
intLibInit
intLevelSet
intIntRtnPreempt
intIntRtnNonPreempt
intIFUnlock
intIFLock
intExit
intEnt
intEnable
intDisable
intDemuxErrorCount
intCount
intContext
intConnect
intCnt
int2str
install_ptk
insert_entry_in_list
insertAlternateOptionToList
inputtimeMsgbox
input_pwd_match
input
inm_piny_nd_dlg
inm_eng_nd_dlg
inm_ZIstr_nd_dlg
inm_ZIpiny_nd_dlg
inm_ZIeng_nd_dlg
initiateDspDownload__15CdspRootManagerUs
initialize_ipcp_mibs
initialize_ip_ncp
initialize
init_rtp
init_reboot
init_random_number
init_random
init_profile
init_hash_table
initConfigDataBuffer
initApplLogger
init
informative_cb
inform
inflate_trees_fixed
inflate_trees_dynamic
inflate_trees_bits
inflate_copyright
inflate_codes_free
inetsw
inetstatShow
inetdomain
inetctlerrmap
inet_pton
inet_ntop
inet_ntoa_b
inet_ntoa
inet_node
inet_network
inet_netof_string
inet_netof
inet_netmatch
inet_makeaddr_b
inet_makeaddr
inet_lnaof
inet_aton
inet_addr
index4_backup
index4
index3_backup
index3
index2_backup
index2
index1_backup
index1
index
increaseVolume__15CdspRootManager
increaseVolume__11CdspManager
increaseRingerAmplitude__15CdspRootManager
increaseRingerAmplitude__11CdspManager
increaseGain__15CdspRootManager7GainMap
increaseGain__11CdspManager7GainMap
inc_byte_array
in_status
in_socktrim
in_setsockaddr
in_setpeeraddr
in_rtqdrain
in_rtchange
in_pcbremlists
in_pcbrehash
in_pcbpurgeif0
in_pcbnotifyall
in_pcblookup_local
in_pcblookup_hash
in_pcbladdr
in_pcbinshash
in_pcbdisconnect
in_pcbdetach
in_pcbconnect
in_pcbbind
in_pcballoc
in_netof
in_multihead
in_losing
in_localaddr
in_inithead
in_ifscrub
in_ifrtchange
in_ifexists_ifa
in_ifadown
in_ifaddrhmask
in_ifaddrhead
in_ifaddrhashtbl
in_getaddr
in_delmulti
in_delayed_cksum
in_control
in_cksum_skip
in_cksum
in_canforward
in_broadcast
in_arpinput
in_addmulti
inSysctlInit
inStandby
inRmxSysctlInit
inPcbSysctlInit
in4ProtoSysctlInit
igmpstat
igmp_slowtimo
igmp_node
igmp_leavegroup
igmp_joingroup
igmp_input
igmp_init
igmp_fasttimo
igmpSysctlInit
igmpInstInit
ifw_total_count
ifw_start_address
ifw_section1
ifw_section0
ifw_offset1
ifw_offset0
ifw_count1
ifw_count0
ifunit
ifsInList
ifrfamily
ifqmaxlen
ifnet_addrs
ifnetToEndFieldsGet
ifnet
ifmaof_ifpforaddr
ifioctl
ifinit
ifindex2ifnet
ifconfig_intern
ifconfigInit
ifconfig
ifaof_ifpforaddr
ifafree
ifa_ifwithroute
ifa_ifwithnet
ifa_ifwithdstaddr
ifa_ifwithaddr
if_withname
if_up
if_unroute
if_simloop
if_setlladdr
if_route
if_name
if_indexlim
if_index
if_down
if_detach
if_delmulti
if_cloners_count
if_cloners
if_clone_lookup
if_clone_list
if_clone_detach
if_clone_destroy
if_clone_create
if_clone_attach
if_attach
if_allmulti
if_addmulti
ifSysctlInit
ifShowInit
ifShow
ifRouteDelete
ifMetricSet
ifMetricGet
ifMaskSet
ifMaskGet
ifLibInit
ifIndexToIfp
ifFlagSet
ifFlagGet
ifFlagChange
ifEtherSysctlInit
ifEtherSubrSysctlInit
ifDstAddrSet
ifDstAddrGet
ifBroadcastSet
ifBroadcastGet
ifAddrSet
ifAddrGet
ifAddrDelete
ifAddrAdd
idletxt
idle_static_needdatapic
idle_pick_4
idle_pick_3
idle_pick_2
idle_pick_1
idle_pick_0
idle_new_needdatapic
idle_mode_needdatapic
idle_change_needdatapic
idle_chaedit_needdatapic
idle_Save
idle2wfsetting
idle2setting
ict_unload_fsm
ict_timeout_d_event
ict_timeout_b_event
ict_timeout_a_event
ict_snd_invite
ict_set_destination
ict_retransmit_ack
ict_rcv_3456xx
ict_rcv_2xx
ict_rcv_1xx
ict_need_timer_d_event
ict_need_timer_b_event
ict_need_timer_a_event
ict_load_fsm
ict_kill_transaction
ict_init
ict_get_fsm
ict_fsm
ict_free
ict_create_ack
ict_6xx_received
ict_5xx_received
ict_4xx_received
ict_3xx_received
ict_2xx_received
ict_1xx_received
icmpv4SysctlInit
icmpstat
icmp_node
icmp_input
icmp_error
icmpInstInit
icmpErrorLen
iInputIndex
hyperterm_mode
hwaddr_aton
hwWatchdog_IRQ
hwWatchDogReset
hwWatchDogInit
hwFeedWDToff
hwFeedWDT
httpdTaskStackSize
httpd
http_version_11
http_version_10
http_session_reconnect_socket
httpWmbSessionGet
httpWmbPostConfInit
httpWmbParserConfInit
httpWmbParserConfAdd
httpWmbName
httpWmbErrorsExist
httpWmbErrorStore
httpWmbErrorIterator
httpWindMarkSetFailed
httpWindMarkGetFailed
httpUserNameDecode
httpUri
httpUploadRpmNotLast
httpUploadConfInit
httpUploadConfAdd
httpUpldConfigId
httpTimeoutSet
httpSystemRpms
httpSysRpmConfInit
httpSysRpmConfAdd
httpSysErrorTab
httpStringToUpper
httpStringPut
httpStrdup
httpStrNCaseCmp
httpStrCpy
httpStdIoStoreDefault
httpStdIoSetToSocket
httpStdIoSetToDefault
httpStatusSet
httpStatusMessages
httpStatusLine
httpStatus
httpSockTimeout
httpSockArray
httpSignificantChars
httpSetEnv
httpServerUncompress
httpServerTaskIds
httpServerStart
httpServerName
httpServerKill
httpServerIdentification
httpServerCreate
httpRpmWmbPostExec
httpRpmWmbPost
httpRpmWmbParse
httpRpmWmbBestEffortPost
httpRpmUpload
httpRpmPost
httpRpmPass
httpRpmMime
httpRpmIdentGet
httpRpmIdentAndDataSet
httpRpmFs
httpRpmDataGet
httpRpmCtrl
httpRpmConfInit
httpRpmConfAdd
httpRpmAlias
httpReqTrans
httpReqStructInit
httpReqMemPartSize
httpReqMemPartIdGet
httpReqLineParse
httpReqIdResource
httpPwdNameFind
httpPwdGroupStringGet
httpPwdGroupIterator
httpPwdGroupIndexIterator
httpPwdGroupDelete
httpPwdDecode
httpPwdConfUnlock
httpPwdConfSave
httpPwdConfLock
httpPwdConfLoad
httpPwdConfInit
httpPwdConfId
httpPwdConfGet
httpPwdConfDelete
httpPwdConfAdd
httpPwdAuthStringGet
httpPwdAuthIterator
httpPwdAuthIndexIterator
httpPwdAuthAdd
httpProtocolStrings
httpProcesses
httpPriority
httpPrintf
httpPostReply_alternate
httpPostReply
httpPostMultipartHeaderParseAll
httpPostMultipartHeaderParse
httpPostConfInit
httpPort
httpPersistentConnectionsAllowed
httpOutputEnable
httpOutputDisable
httpOsalStringToken
httpOsalStringError
httpOsalSemTake
httpOsalSemMCreate
httpOsalSemInit
httpOsalSemGive
httpOsalSemDelete
httpOsalSemCountShow
httpNullByte
httpMud
httpMimeParseFnConfInit
httpMimeParseFnConfAdd
httpMimeParse
httpMimeHost
httpMimeHdrSet
httpMimeHdrGet
httpMimeContentTypeSet
httpMimeContentTypeGet
httpMimeContentType
httpMimeContentLengthSet
httpMimeContentLengthGet
httpMimeContentLength
httpMimeContentEncodingSet
httpMimeContentEncodingGet
httpMimeConfInit
httpMimeAuthorization
httpMimeAcceptLanguage
httpMimeAcceptEncoding
httpMethods
httpMaxUrlSize
httpMaxTempBufSize
httpMaxSockQ
httpMaxSockBuff
httpMaxSendCookies
httpMaxRecCookies
httpMaxMimeLines
httpMaxErrors
httpMaxArguments
httpMacros
httpMacroInit
httpMacroExecute
httpMacroCleanup
httpLogInfoMsgFunction
httpLogInfoFunction
httpLogErrorMsgFunction
httpLogErrorFunction
httpLocationSet
httpLocationGet
httpLineUnescape
httpLineRead
httpIsMatching
httpIsMacro
httpIpConfId
httpInit
httpHeaderGenerate
httpGlobalMemPartSize
httpGlobalMemPartIdGet
httpGidSet
httpGidGet
httpGetWmbComp
httpGetFile
httpGetEnv
httpGenListUnlock
httpGenListRemove
httpGenListMemPartIdGet
httpGenListLock
httpGenListIterator
httpGenListItemsGet
httpGenListIndexIterator
httpGenListIdGet
httpGenListFuncGet
httpGenListFuncAppend
httpGenListFind
httpGenListDestroy
httpGenListDataGet
httpGenListDataAppend
httpGenListCreate
httpGenListCaseFind
httpFsConfInit
httpFsConfAdd
httpFileWrite
httpFileSize
httpFileSetDefaultFs
httpFileSeek
httpFileRegister
httpFileRegRemove
httpFileRegInit
httpFileRegHandle
httpFileRegGetFd
httpFileRead
httpFileOpen
httpFileMngrInit
httpFileGets
httpFileDelete
httpFileContentTypeGet
httpFileClose
httpErrorHeader
httpErrorFooter
httpError
httpErrStringGet
httpDispatcher
httpDefLocationString
httpDefGidString
httpCtrlUrlIterator
httpCtrlUrlIndexIterator
httpCtrlConfUnlock
httpCtrlConfLock
httpCtrlConfInit
httpCtrlConfId
httpCtrlConfGet
httpCtrlConfAdd
httpCtrlAllowIterator
httpCtrlAllowIndexIterator
httpCopy
httpConservativeAlloc
httpClientIPGet
httpChunkedEncodingOn
httpChunkedEncodingOff
httpBufferGet
httpBoundarySet
httpBoundaryGet
httpBlockRead
httpBlockPut
httpBase64encode
httpBase64decode
httpAuthorizationGet
httpAuthenticationSet
httpAuthenticationGet
httpAliasConfInit
httpAliasConfAdd
httpAcceptIP
http
htc_version
htc_ver
htc_unschedule_all
htc_snd_request
htc_snd_msg
htc_snd
htc_session_stop
htc_session_start
htc_session_renew
htc_session
htc_schedule_standard
htc_schedule_payload
htc_schedule_field
htc_schedule_blankline
htc_resolve
htc_resend_last_req
htc_rcv_rsp_hdr
htc_rcv_rsp_bdy
htc_rcv
htc_put_file
htc_parse_uri
htc_mutex
htc_init_flag
htc_init
htc_get_status_code
htc_get_path
htc_get_filelen
htc_get_file
htc_get_field
htc_free_status
htc_free_rsp_data
htc_disc
htc_delete_file
htc_conn
hstrerror
hostname
hosthash
hostentFree
hostentAlloc
hostapd_hexdump
hostapd_get_rand
hostTblSearchByName2
hostTblSearchByName
hostTblSearchByAddr2
hostTblSearchByAddr
hostTblInit
hostShowInit
hostShow
hostListSem
hostList
hostInitFlag
hostGetByName
hostGetByAddr
hostDelete
hostAdd
hmac_sha1_vector
hmac_sha1
hmac_md5_vector
hmac_md5
hexstr2bin
hermesDriverStopped
help
headsetPICState__Fv
headsetPICRegisterSet__Fv
headsetPICRegisterReset__Fv
headsetInterruptEnable__Fv
headsetEnable__Fv
header_setvalue
header_setname
header_param_def
header_init
header_getvalue
header_getname
header_free
header_clone
header_2char
hdrSizeFunction
hcf_service_nic
hcf_send_msg
hcf_rcv_msg
hcf_put_info
hcf_get_info
hcf_connect
hcf_cntl
hcf_action
hashinit
hash_find_exact_ctx
hash_find_base_ctx
hashTblTerminate
hashTblRemove
hashTblPut
hashTblInit
hashTblFind
hashTblEach
hashTblDestroy
hashTblDelete
hashTblCreate
hashLibInit
hashKeyStrCmp
hashKeyCmp
hashFuncMultiply
hashFuncModulo
hashFuncIterScale
hashClassId
hash2getsessid
handle_str
handle_socket_err
handle_send_err
handle_recvfrom_err
handle_recv_err
handle_param
handle_nums
handle_num
handle_listen_err
handle_list
handle_ips
handle_ippairs
handle_ip
handle_connect_err
handle_bool
handle_bind_err
handle_accept_err
halfDuplexSpkPhoneSwitch__15CdspRootManagerUs
halfDuplexSpkPhoneSwitch__11CdspManagerUs
h_write
h_read
h_nerr
h_errno
h_errlist
h261
gzeof
gtfUntimeout
gtfTimerStart
gtfTimerManagerRun
gtfTimerManagerDelete
gtfTimerManagerCreate
gtfTimerInit
gtfTimerDelete
gtfTimerCreate
gtfTimerCancel
gtfTimeout
gtfShow
gtfLibInit
gtfGetNbrOutstandTimer
gtfGetNbrFiredTimer
gtfErrorLog
gtfCalloutStop
gtfCalloutReset
gtfCalloutInit
gtfBookkeeping
gsmsinsert
gsmscont
gppPBDialog
gppCalDialog
gpbidx2srchidx
gp_pro_vollabel
gp_pb_picklist
gp_Idle_week
gp_Idle_time
gp_Idle_pic
gp_Idle_date
gpTrustedSession
gpPicField
gpPBLabel
gpPBField
gpCal
gmtime_r
gmtime
global_uninit
global_init
globalNet
gispreplay
gintvibthnr
ginspos
gfldwllcn
gfieldstate
gfieldpklstsel
gfieldpklstop
gfdpkpktop
gfdpkpksel
getwd
getw
gettimeofday
getsockopt
getsockname
getservbyport
getservbyname
gets
getpeername
getpassword
getopt
getntptime
getnewpassword
getnetbyname
getnameinfo
getipnodebyaddr
getifaddrs
gethostname
gethostbynameInit
gethostbyname
gethostbyaddrInit
gethostbyaddr
getenv
getcwd
getcomfirmpwd
getchar
getc
getaddrinfo
getaddrfromsockbuf
get_video_codec_list
get_value_type
get_value_string
get_timer_context
get_time_stamp
get_stun_flag_api
get_size_of_ppp_options
get_sip_sem
get_silenceSuppression__FiPi
get_sessid
get_rtpsess
get_rtp_hdr
get_rtp_fd
get_rtcpsess
get_rtcp_fd
get_rfc2833_pltype_value
get_resp
get_remote_port
get_remote_ipaddr
get_remote_addr
get_range_option_values
get_random_number
get_pointer_to_previous_entry_in_list
get_pointer_to_next_entry_in_list
get_pointer_to_last_entry_in_list
get_pointer_to_first_entry_in_list
get_packcount_sent
get_packcount_rcvd
get_option_value
get_octetcount_sent
get_octetcount_rcvd
get_mute_state
get_message
get_mappedPort_api
get_mappedIPAddr_api
get_local_port
get_local_ipaddr
get_local_addr
get_lifetime_api
get_last_rcvd_tstamp
get_keepRTPAlive_socket
get_jitter_val
get_hash_index
get_global_sip_port
get_global_sip_hostname
get_global_rtp_port
get_global_callwaiting_using_flag
get_g726_pltype_value
get_entry_from_list_using_index
get_entry_from_list
get_current_timestamp
get_current_seqno
get_avtran_delay
get_av_profile
get_audio_codec_list
get_alternate_option_values
get_NATsType_api
getWepkeylen4Config
getWepkeylen3Config
getWepkeylen2Config
getWepkeylen1Config
getWFMode4Config
getWFMode3Config
getWFMode2Config
getWFMode1Config
getWEPAuth4Config
getWEPAuth3Config
getWEPAuth2Config
getWEPAuth1Config
getVolume__15CdspRootManagerUsPUs
getVolume__11CdspManagerUsPUs
getUserPassword
getUserName
getTermNetInfo
getSyslogTaskid
getServerIPConfig
getScriptInfo
getSSIDConnectedTo
getResetToDefaultConfig
getReboot
getProvConfProtocol
getPBIsInited
getOptServ
getNumIcon
getNextTFTPPort
getNetInfo
getMACAddress
getLcpOptionName
getJbConMask
getIpcpOptionName
getIndex4Config
getIndex3Config
getIndex2Config
getIndex1Config
getIconId
getHandsetMixerGain__11CdspDecoder
getGain__15CdspRootManager7GainMapPUs
getGain__11CdspManager7GainMapPUs
getGainMap__15CdspRootManager7GainMapPUsUs
getGainMap__11CdspManager7GainMapPUsUs
getFirmwareVersion
getFileState
getDspConfiguration__15CdspRootManager
getDspConfiguration__11CdspManager
getDefaultScript
getDecoderHandsetGain__11CdspManagerUs
getDateDay
getDSPStatus__15CdspRootManager
getDSPStatus__11CdspManager
getCurrentStatus
getCurTFTPPort
getConfig
getCodecType__15CdspRootEncoder
getCodecType__15CdspRootDecoder
getCodecType__11CdspEncoder
getCodecType__11CdspDecoder
getBuffer__16CdspRootDataPortPvUlUsi
getBuffer__16CdspRootDataPortPvUlUs
getBuffer__15CdspRootEncoderPvPUs
getBuffer__11CdspEncoderPvPUsT2
getAudioSource__15CdspRootManager
getAudioSource__11CdspManager
getAudioOutput__15CdspRootManager
getAudioOutput__11CdspManager
generic_param_setvalue
generic_param_setname
generic_param_parseall
generic_param_getvalue
generic_param_getname
generic_node
generating_request_out_of_dialog
generate_xid
generate_option_list_entry
generateSilence__15CdspRootDecoderUsUc
generateSilence__11CdspDecoderUsUc
generateNewInterfaceIdentifier
generateDtmf__15CdspRootManagerUsUsUsUsUs
generateDtmf__11CdspManagerUsUsUsUsUs
gen_retransmit
gcurpos
gccetypebak
gccetype
gcannotint
gbsmsindex
gbmfieldflag
gbflashan
gbcurfront
gbType
gbTrvlDial
gbTabNum
gbStrMsgBox
gbMsgWtLngKey
gbKeyValue
gbKeyFlag
gbIsLabelClr
gbInputOn
gbColor
ganfldpkgrp
gai_strerror
g_wtd_taskbit_opt_sem
g_wd_test
g_watchdog_task_bits
g_wZiCodetoGB
g_vibrating
g_transfer_num_string
g_timer_stop
g_timer_start
g_timer_reset
g_timer_new
g_timer_elapsed
g_timer_destroy
g_test_stream
g_tagSpeedKeyInfo
g_tagPBEntryInfo
g_tagGroupInfo
g_tagCompressData
g_sys_return_cnting
g_sys_redial_interval
g_sys_redial_index
g_sys_redial_count_max
g_sys_redial_count
g_sys_pm_tmtype
g_strdup_printf
g_sta_pLabel
g_stMMIScriptInfo
g_ssid_table
g_ssidIndex
g_sip_wakeup
g_searchedRow
g_saver_yes
g_resolverMutexSem
g_remoteSupportRfc2833
g_reg_usrname
g_reg_usrgrp
g_reg_total_index
g_reg_telnum
g_reg_savename
g_reg_pwd
g_reg_pbname
g_reg_opr_topnum
g_reg_opr_index
g_reg_offset
g_reg_index
g_reg_groupid
g_reg_flash
g_reg_doid
g_reg_del_topnum
g_reg_del_index
g_reg_calllogbuf
g_reg_c
g_reg_b
g_reg_a
g_refer_to_disc
g_recreate_sys_entity
g_pscChgCurrent
g_pscBatVol
g_pscBatTemp
g_profile_type
g_profile_key
g_profile_flash
g_profile_f
g_profile_c
g_profile_b
g_profile_a
g_pre_pLabel
g_power_key
g_pb_tClass
g_pb_speedkey_toprow
g_pb_search_pinyin
g_pb_searchIdxTbl
g_pb_nActualPBSearchNum
g_pb_NumIndex
g_pSpeedKeyField_Value
g_pSpeedKeyField_Num
g_pSpeedKeyField_Name
g_pSpeedKeyField_Group
g_pField_Url
g_osip_timers
g_open_ap_only
g_nTopRow
g_nSpeedKeyIndex
g_nRecordMenuID
g_nCurrentTone
g_nCurrentPBEntryIndex
g_nCurrentGroup
g_nActualPBNum
g_nActualPBGroupNum
g_muted
g_multikey_state
g_msg_Qid
g_memoidsound
g_memocoming_an
g_melodyVolume
g_melodySem
g_melodyIndex
g_lpShortMenu
g_log_state
g_log_mode
g_list_sort_with_data
g_list_sort
g_list_reverse
g_list_remove_all
g_list_remove
g_list_prepend
g_list_position
g_list_nth_prev
g_list_nth_data
g_list_nth
g_list_length
g_list_last
g_list_insert_sorted
g_list_insert_before
g_list_insert
g_list_index
g_list_free_1
g_list_free
g_list_foreach
g_list_first
g_list_find_custom
g_list_find
g_list_copy
g_list_concat
g_list_append
g_list_alloc
g_labelfonttype
g_key_polarity
g_is_refer_ok
g_is_incomming
g_is_incalling
g_is_end_key_press
g_is_cw_reject_incall
g_is_busy
g_insleep
g_incoming_num_edit
g_incoming_name_label
g_idle_state
g_idle_rtc
g_idle_lock
g_iTftpCurPort
g_finish_hangup_sem
g_dsp_test
g_dns_name
g_dns_debug
g_debug_print
g_debug_pcate
g_cnted_time_label
g_cnted_num_edit
g_cnted_name_label
g_cnted_icon_label
g_cnted_12num_edit
g_calllog_flag
g_cDefaultScript
g_blUrlIsNull
g_bat_test
g_bTftpServerOK
g_bTFTPXferInProcess
g_bTFTPRetry
g_bTFTPNeedCancel
g_bTFTPFlag
g_bSetSuccess
g_bRightSoftKeyIsSearch
g_bPaintCannotReg
g_bIsEnterNetSearchFromIdle
g_bInAlarmEdit
g_bHasRegister_Switch
g_bFirstRgsFail
g_ate_result
g_ate_mode
g_ate_cmd_table
g_arrVonage
g_arrMacString
g_arrCntingSSID
g_ap_infos
g_UsrDataBuff
g_Timer_num
g_TftpManualUp
g_TftpIsDeinited
g_TftpFirmwareUp
g_TftpErrTime
g_TftpDhcpStatus
g_TftpConfigUp
g_TFTPLocationParams
g_TFTPBinLoct
g_SecTimer_mutex
g_SecTimer
g_PBGroupIdxTbl
g_Memo_AnOn
g_Lcd_Philips
g_Idle_sleepNum
g_Idle_pb
g_IdleInput_pb
g_FlashSetBuff
g_FlashPBReadIdx
g_FlashPBInited
g_FlashPBIndex
g_Delay_num
g_DSPpowerOnWd
g_ClockSem
g_CanDel
g_AllCallTime
gZcount
gT8307Thp
gT8307TBt
gT8300D2
gT8300D1
gStunConfig
gScrSaverType
gSaveElementCount
gResumeFlag
gPBName
gOpeType
gOpeTimeout
gNewServiceFlag
gNewSerAttrs
gNewIdleRow
gModeFlag
gMenuIDNetServ
gMenuID2
gMenuID1
gMemoStopFlag
gMacPortTbl
gMLCDRowReg
gLastRssiVal
gLabel
gIsVibrThenRing
gIpFieldFlag
gIpCursorPos
gInboxMsgOver
gIfEmpty
gIdleStaRow
gIdleSpdIdx
gIdleEditRow
gIdleChaRow
gIconIdArrayHour
gIconIdArrayDay
gIconIdArray3Hours
gIconId
gGALInfo
gFlagStaticToEdit
gFlagRepeat
gFlagOfTraveller
gFlagOfPic1ToSta
gFlagOfIntoSta
gFlagOfEdit
gFlagOfCallForward
gField
gFalgOfNewSet
gEthernetInterfaceName
gEnglishFont
gEarphnStaus
gDspDataBlock_p
gDspDataBlock
gDisplayStr
gDiscFlag
gDialNumOfRow
gDSPtoneParams
gDSPspkvolumeMap
gDSPringPattern
gDSPhstvolumeMap
gDSPerrorMsgs
gDSPdtmfParams
gDSPcurrentMelody
gDSPcoder
gDSPcadenceCount
gCursorIndex
gChineseFont
gCceExport
gCallpField
gBaseAddr
g729ab
g729a
g729Ainfo
g729ABinfo
g726info
g726PTValue
g726
g723EncodeRate
g7231
g711u
g711a
fwrite
fw_enable
ftplTransientRetryInterval
ftplTransientMaxRetryCount
ftplPasvModeDisable
ftplDebug
ftpXfer
ftpVerbose
ftpTransientFatalInstall
ftpTransientConfigSet
ftpTransientConfigGet
ftpReplyTimeout
ftpReplyGetEnhanced
ftpReplyGet
ftpLs
ftpLogin
ftpLibInit
ftpLibDebugOptionsSet
ftpHookup
ftpErrorSuppress
ftpDebug
ftpDataConnInitPassiveMode
ftpDataConnInit
ftpDataConnGet
ftpCommandEnhanced
ftpCommand
ftell
ft_Password_Error
ft_MsgBox_WriteFlashError
ft_MsgBox_Update
ft_MsgBox_Succ
ft_MsgBox_PBFull
ft_MsgBox_NoRecord
ft_MsgBox_Exist
ft_MsgBox_Confirm
ft_MsgBox_Cancel
ft_MenuClose
ft_Add_Error
fstatfs
fstat
fsm_tbl
fsm_findmethod
fsm_callmethod
fsetpos
fseek
fscanf
from_tag_new_random
from_tag_match
from_seturl
from_setdisplayname
from_parse
from_param_get
from_init
from_geturl
from_getdisplayname
from_free
from_compare2
from_compare
from_clone1
from_2char_without_params
from_2char
frexp
freopen
freeifaddrs
freehostent
freeaddrinfo
free_ppp_tx_accepted_option_list
free_ppp_option_lists
free_ppp_option_list_entry
free_ppp_option_list
free_list
free_hash_ctx_chain
free_hash_ctx
free_events
free
fread
fr_checkp
fputs
fputc
fprintf
fprint_char
fppTaskRegsShow
fppTaskRegsSet
fppTaskRegsGet
fppTaskRegsDFmt
fppTaskRegsCFmt
fppShowInit
fppSave
fppRestore
fppProbe
fppInit
fppDisplayHookRtn
fppCreateHookRtn
fppArchTaskCreateInit
fppArchInit
fp_nquery
fpTypeGet
fpRegName
fpCtlRegName
fpClassId
fpArmModules
fopen
fmod
flushroutes
floor
floatInit
flashupTestWrite
flashupReboot
flashupProgramImage
flashupProgramEx
flashupInflateAndProgramImage
flashupChecksumCompute
flashupChecksumClear
flash_hook_timer_max_count
flashSemInitialized
flashSem
flashSectorSize
flashSectorNum
flashSectorAddr
flashReadQuery
flashReadDeviceID
flashInfo
flashEraseImage
flashDeviceID
flashDevice
flags
firmwareVersion
fir_pwd
fioScanV
fioRead
fioRdString
fioLibInit
fioFormatV
fioFltInstall
find_public_subobj__C16__user_type_infoiRC9type_infoPvT3
find_next_occurence
find_next_crlfcrlf
find_next_crlf
find_matching_option_beyond
find_matching_option
find_hash_ctx
find_default_interface
findDataPort__Fv
findConnId
fill_remsrc_info
fileno
filename_null_flag
filename4_new
filename3_new
filename2_new
filename1_new
file_active
fileRename
fifo_tryget
fifo_size
fifo_insert
fifo_init
fifo_get
fifo_free
fifo_add
fieldvalue
fieldname
fieldSzIncludeSign
fgets
fgetpos
fgetc
ffsMsbTbl
ffsMsb
ffsLsbTbl
ffsLsb
fflush
ferror
feof
feed_timer
fdprintf
fdopen
fdTable
fcnTimerOorWakeup
fcnTimerOorWaitForConnection
fclose
fc_worldtime_NeedData
fc_groupring_anykey_stoptimer
fc_ViewDetail_TalkKey
fc_SubMenu_Return_g
fc_SubMenu_Return
fc_SubMenu_Modify_g
fc_SubMenu_Modify
fc_SubMenu_DelConfirm
fc_Speedkey_BackView
fc_SpeedKey_View
fc_SpeedKey_Set
fc_SpeedKey_Operate
fc_SpeedKey_Modify
fc_SpeedKeySet_Succ
fc_SpeedKeySet_NoInfo
fc_SpeedKeySetSucc_View
fc_SpeedKeyMenu_NeedData
fc_SpeedKeyCancel_Refresh
fc_SpeedKeyCancel_OK
fc_SpeedKeyCancel_Confirm
fc_Search_Remlabel
fc_Search_List
fc_RightSoftkey_Return
fc_Return_MainMenu
fc_Return_Idle1
fc_Return_Idle
fc_Pbdetail_Return
fc_Password_Error
fc_PasswordError_Return
fc_PB_RingPlay_timer
fc_PBStorageSta_NeedData
fc_PBSelectGroup_NeedData
fc_PBSearchList_NeedData
fc_PBRingSetExit
fc_PBRingSetEntry
fc_PBRecordMenu_NeedData
fc_PBListAll_NeedData
fc_PBGroupList_NeedData
fc_NotSearch
fc_NotAdd
fc_Modify_SelectGroup_g
fc_Modify_SelectGroup
fc_Modi_Result_g
fc_Modi_Result
fc_Modi_Error_g
fc_Modi_Error
fc_ModiSucc_Detail_g
fc_ModiSucc_Detail
fc_MainMenu_Storage
fc_MainMenu_SpeedKeyView
fc_MainMenu_Search
fc_MainMenu_GroupView
fc_MainMenu_GroupRingSet
fc_MainMenu_DelByOne
fc_MainMenu_DelByAll
fc_MainMenu_Add
fc_LongPressTalkkey
fc_List_Rewind
fc_List_Idle
fc_List_Detail_g
fc_List_Detail
fc_LeftSoftkey_Press
fc_GroupView_NoInfo
fc_GroupRing_Move
fc_GroupRingSet_Succ
fc_GroupRingSet_NeedData
fc_GroupRingSetSucc_Menu
fc_GPbdetail_Return
fc_Detail_SubMenu
fc_DelSucc_RefreList_g
fc_DelSucc_RefreList
fc_DelSucc_MainMenu
fc_DelSucc_Idle_g
fc_DelSucc_Idle
fc_DelConfirm_OK_g
fc_DelConfirm_OK
fc_DelByOne_NoInfo
fc_DelByOne_Confirm
fc_DelByOneSucc_RefreList
fc_DelByOneSucc_MainMenu
fc_DelByOneConfirm_OK
fc_DelAll_Succ
fc_DST_NeedData
fc_ConfirmMsgBox_Back
fc_BatchDelSucc_MainMenu
fc_Add_SelectGroup
fc_Add_Error
fc_AddSucc_List
fc_AddName_Save
fc_AddName_Idle
fc_AddName_Error
fc_ADD_Result
fatClugFac
fat16VolMount
fat16Debug
fat16ClustValueSet
fat16ClustValueGet
fastUdpInitialized
family_enqueue
failover
faillure_cb
fabs
f_UA_stop_ring
f_UA_start_ring
f_UA_registration_success
f_UA_registration_failure
f_UA_refer_in_progress
f_UA_refer_5XXreceived
f_UA_refer_4XXreceived
f_UA_refer_202received
f_UA_redireced
f_UA_one_onhold_dialog_left
f_UA_notify_received
f_UA_net_failure
f_UA_message_reached
f_UA_message_incoming
f_UA_message_delivered
f_UA_incoming_call
f_UA_incoming_another_call
f_UA_call_unregistering
f_UA_call_terminated
f_UA_call_reject
f_UA_call_registering
f_UA_call_failure
f_UA_call_canceled
f_UA_call_accepted
f_UA_UDP_listener_failure
f_UA_2xxforNotifyReceived
fRequestjbReadTaskStop
fRequestPutMgrTaskStop
fRequestGetMgrTaskStop
expm1
explicit_prefix
expand
exit_tomenucon
exit_tomenu
exit_tolnglock
exit_to_sta
exit_to_sermenu4
exit_to_change
exit
execute_ppp_state_machine
execute
exception_init
exception_handler
exception_dump
excVecSet
excVecInit
excVecGet
excTaskStackSize
excTaskPriority
excTaskOptions
excTaskId
excTask
excShowInit
excMsgQId
excJobAdd
excIntHandle
excIntConnect
excInit
excHookAdd
excExcepHook
excExcHandle
excExcContinue
excEnterUndef
excEnterSwi
excEnterPrefetchAbort
excEnterDataAbort
evt_settype_outgoing_sipmessage
evt_settype_incoming_sipmessage
evtAction
event_setelement
event_parse
event_init
event_getelement
event_free
event_destroy
event_clone
event_2char
eventTerminate
eventTaskShow
eventStart
eventSend
eventSem
eventRsrcShow
eventRsrcSend
eventReceive
eventLibInit
eventInit
eventEvtRtn
eventClear
etherbroadcastaddr
ether_status
ether_resolvemulti
ether_output
ether_node
ether_ipmulticast_min
ether_ipmulticast_max
ether_inet_node
ether_getaddr
etherMultiGet
etherMultiDel
etherMultiDebug
etherMultiAdd
errsys
errnoSet
errnoOfTaskSet
errnoOfTaskGet
errnoGet
errno
errmsg
eraseRingerDownload__15CdspRootManagerUsUsUsPUs
eraseRingBuff
erasePhoneParam
eraseMelodyToneDownload__15CdspRootManagerUsUsUsPUs
eraseMelodyToneBuff
envShow
envPrivateDestroy
envPrivateCreate
envLibInit
enter_lnglock_opt
enter_input_newpwd
enter_input_confirmpwd
enterCode
endTxSemTake
endTxSemGive
endRcvRtnCall
endPollStatsInit
endObjectUnload
endObjInit
endObjFlagSet
endMultiLstNext
endMultiLstFirst
endMultiLstCnt
endMibIfInit
endFlagsSet
endFlagsGet
endFlagsClr
endFirstUnitFind
endFindByName
endEtherPacketDataGet
endEtherPacketAddrGet
endEtherAddressForm
endDevTbl
endDevName
endConn
end8023AddressForm
encap_rtp_payload
encap_rtcp_sr
encap_rtcp_sdes
encap_rtcp_rr
encap_rtcp_pack
encap_rtcp_bye
encap_report_block
enable_dump
emiInit
eloop_user_data_get
eloop_unregister_read_sock
eloop_terminate
eloop_satus
eloop_run
eloop_register_timeout
eloop_register_signal
eloop_register_read_sock
eloop_init
eloop_destroy
eloop_cancel_timeout
elfRelocRelaEntryRd
elfRelocRelEntryRd
elfArmInit
elementBuffer2
elementBuffer
eapol_sm_step
eapol_sm_rx_eapol
eapol_sm_register_scard_ctx
eapol_sm_notify_tx_eapol_key
eapol_sm_notify_portValid
eapol_sm_notify_portEnabled
eapol_sm_notify_portControl
eapol_sm_notify_pmkid_attempt
eapol_sm_notify_logoff
eapol_sm_notify_eap_success
eapol_sm_notify_eap_fail
eapol_sm_notify_ctrl_response
eapol_sm_notify_ctrl_attached
eapol_sm_notify_config
eapol_sm_notify_cached
eapol_sm_init
eapol_sm_get_status
eapol_sm_get_mib
eapol_sm_get_key
eapol_sm_deinit
eapol_sm_configure
eap_sm_step
eap_sm_request_password
eap_sm_request_otp
eap_sm_request_identity
eap_sm_notify_ctrl_attached
eap_sm_init
eap_sm_get_status
eap_sm_get_eap_methods
eap_sm_deinit
eap_sm_buildIdentity
eap_sm_abort
eap_set_workaround
eap_set_fast_reauth
eap_register_scard_ctx
eap_notify_success
eap_method_md5
eap_key_available
eap_get_type
eap_get_phase2_types
eap_get_phase2_type
eap_get_eapRespData
eap_get_eapKeyData
eap_get_config
e_logfullflag
e_log_w_offset
e_log_fifo_write__FP15locallog_info_s
e_log
eZiTextProc
eZiTextClear
eZiText2Field
eZiTapProcTimer
eZiTapProc
eZiStrokeProc
eZiPyProc
dyncast__C16__user_type_infoiRC9type_infoPvT2T3
dynamicRingerPtrInit__Fv
dynamicMelodyTonePtrInit__Fv
dxXfer
dxLibInited
dxGetErrNo
duplicate_option_with_values
duplicate_option
dup_sockaddr
dump_test
dump_data_for_show
dump_data_for_log
dump
dummy_int
dummyPut__15CdspRootManagerPUsUlUs
dummyPut__11CdspManagerPUsUlUs
dummyGet__15CdspRootManagerPUsUlUs
dummyGet__11CdspManagerPUsUlUs
dummy
dstFlag
dsplen
dspWriteToDccRingerControl__Fv
dspWriteToDccMediaMessage__Fv
dspWriteToDccControlMessage__Fv
dspWakeup__Fv
dspVerLoc
dspUpdateCadence__Fv
dspUdpServer__Fv
dspToneDirection__FP15tDSPframeHeaderUs
dspToneAudioOutput__FP15tDSPframeHeaderUs
dspSoftVersion
dspSoftReset__Fv
dspSleep
dspReset__Fv
dspReadFromDccMediaMessage__Fv
dspReadFromDccControlMessage__Fv
dspPrepareControlWords__Fv
dspPowerSaver__15CdspRootManagerUs
dspPowerSaver__11CdspManagerUs
dspPowerOn
dspPowerOff
dspPlayRinger__Fv
dspPlayCadence__Fv
dspParamUnblock__Fv
dspParamBlock__Fv
dspMiscControlInit__Fv
dspMgr
dspMelodyToneSequence
dspMelodyCadence__Fv
dspLoopback
dspJump__Fv
dspIsr__Fv
dspIsrTask__Fv
dspIsr2Task__Fv
dspInterruptStatus__Fv
dspInterruptEnable__Fv
dspInterruptDisable__Fv
dspInterruptClear__Fv
dspInt
dspInstall__Fv
dspInit__Fv
dspInitRinger__Fv
dspInitCadences__Fv
dspGetToneRepeatCadence__Fv
dspGetToneCadence__Fv
dspGetRingerRepeatCadence__Fv
dspGetRingerCadence__Fv
dspGetMelodyTone__Fi
dspGetMelodyToneRepeatCadence__Fv
dspGetMelodyToneCadence__Fv
dspEncoderUnblock__FUs
dspEncoderBlock__FUs
dspDownloadPrepare__FPUs
dspDownloadData__Fv
dspDownloadCommand__FUs
dspDecoderUnblock__FUs
dspDecoderBlock__FUs
dspBootLoaderDownload__Fv
dspAteMgr
dspAteEncoder
dspAteDecoder
dspAsleep
dspApiMgr
dspApiEncoder
dspApiDecoder
dspACKBSem
dsmNbytes
dsmInst
drvTable
drmfTxMode
dp_test3
dp_test2
dp_test1
dp_test0
download_com_readbyte
down_if
dot1xFlags
dosVDirLibInit
dosVDirDebug
dosSetVolCaseSens
dosFsVolUnmount
dosFsVolOptionsSet
dosFsVolOptionsGet
dosFsVolIsFat12
dosFsVolFormatRtn
dosFsVolFormat
dosFsVolDescGet
dosFsShow
dosFsReadyChange
dosFsModeChange
dosFsMkfsOptionsSet
dosFsMkfs
dosFsLibInit
dosFsLastAccessDateEnable
dosFsInit
dosFsHdlrInstall
dosFsFmtLibInit
dosFsFatInit
dosFsDrvNum
dosFsDevInitOptionsSet
dosFsDevInit
dosFsDevCreate
dosFsDebug
dosFsDateTimeInstall
dosFsConfigShow
dosFsConfigInit
dosFsConfigGet
dosFsChkTree
dosFsChkRtn
dosFsChkDsk
dosFsCacheSizeDefault
dosFatHdlrsList
dosDirOldLibInit
dosDirOldDebug
dosDirHdlrsList
dosChkMinDate
dosChkLibInit
dosChkEntryMark
dosChkDsk
dosChkDebug
domains
domaininit
doalias
do_upcast__C17__class_type_infoQ216__user_type_info8sub_kindRC9type_infoPvRQ216__user_type_info13upcast_result
do_upcast__C16__user_type_infoQ216__user_type_info8sub_kindRC9type_infoPvRQ216__user_type_info13upcast_result
do_upcast__C14__si_type_infoQ216__user_type_info8sub_kindRC9type_infoPvRQ216__user_type_info13upcast_result
do_registration
do_find_public_subobj__C17__class_type_infoiRC9type_infoPvT3
do_find_public_subobj__C16__user_type_infoiRC9type_infoPvT3
do_find_public_subobj__C14__si_type_infoiRC9type_infoPvT3
do_dyncast__C17__class_type_infoiQ216__user_type_info8sub_kindRC9type_infoPvT3T4RQ216__user_type_info14dyncast_result
do_dyncast__C16__user_type_infoiQ216__user_type_info8sub_kindRC9type_infoPvT3T4RQ216__user_type_info14dyncast_result
do_dyncast__C14__si_type_infoiQ216__user_type_info8sub_kindRC9type_infoPvT3T4RQ216__user_type_info14dyncast_result
do_cmd
dns_server_ip
dns_failed
dnsQueryType
dnsIPAddressSrc
dnsIPAddress2
dnsIPAddress1
dnsDebug
dname
dllTerminate
dllRemove
dllInsert
dllInit
dllGet
dllEach
dllDelete
dllCreate
dllCount
dllAdd
div_r
displayName
diskInit
diskFormat
disable_dump
dirList
difftime
dialog_update_tag_as_uac
dialog_update_route_set_as_uas
dialog_update_route_set_as_uac
dialog_update_cseq_as_uas
dialog_set_state
dialog_replaces_inv_match_as_uas
dialog_match_as_uas_only_as_url
dialog_match_as_uas
dialog_match_as_uac
dialog_init_as_uas
dialog_init_as_uac
dialog_free
dialog_fill_route_set
dial
dhf_download_fw
dhf_download_binary
dhcpread
dhcpfilter
dhcpcVerify
dhcpcTimersShow
dhcpcTimerGet
dhcpcShutdown
dhcpcShowInit
dhcpcServerShow
dhcpcServerGet
dhcpcRelease
dhcpcReadTaskId
dhcpcRead
dhcpcPrivateCleanup
dhcpcParamsShow
dhcpcParamsGet
dhcpcParamsCopy
dhcpcOptionSet
dhcpcOptionMerge
dhcpcOptionGet
dhcpcOptionAdd
dhcpcOptFieldCreate
dhcpcOptCreate
dhcpcMutexSem
dhcpcMsgOut
dhcpcMsgIn
dhcpcMinLease
dhcpcMessageList
dhcpcMaxLeases
dhcpcLibInit
dhcpcLeaseList
dhcpcLeaseGet
dhcpcLeaseCleanup
dhcpcInitialized
dhcpcInit
dhcpcInformGet
dhcpcEventSem
dhcpcEventRing
dhcpcEventHookDelete
dhcpcEventHookAdd
dhcpcEventAdd
dhcpcDiscoverRetries
dhcpcDefaultsSet
dhcpcDataSock
dhcpcConfigSet
dhcpcCacheHookDelete
dhcpcCacheHookAdd
dhcpcBufSize
dhcpcBootLease
dhcpcBind
dhcpcArpSend
dhcp_timerid
dhcp_release
dhcp_msgtoparam
dhcp_mode
dhcp_decline
dhcp_client_setup
dhcp_client
dhcpWaitForWpaEap
dhcpWaitForWpa
dhcpTime
dhcpSend
dhcpHandle
dhcpCookie
dhcpConvert
devs
destroyEncoder__15CdspRootManagerP11CdspEncoder
destroyEncoder__11CdspManagerP11CdspEncoder
destroyDecoder__15CdspRootManagerP11CdspDecoder
destroyDecoder__11CdspManagerP11CdspDecoder
destroyCodecs__15CdspRootManager
destination
delete_entry_from_option_list
delete_entry_from_list
deleteWpaTaskForce
deleteFile
delFile4
delFile3
delFile2
delFile1
def_manager
decreaseVolume__15CdspRootManager
decreaseVolume__11CdspManager
decreaseRingerAmplitude__15CdspRootManager
decreaseRingerAmplitude__11CdspManager
decreaseGain__15CdspRootManager7GainMap
decreaseGain__11CdspManager7GainMap
decode_identifier_styled
decode_identifier
debug_udp
debug_rtp
debug_rtcp
debugRESET
debugCMD
debug
ddiv_mantissas
dcacheUpdTaskStack
dcacheUpdTaskPriority
dcacheUpdTaskOptions
dcacheUpdTaskId
dcacheUpd
dcacheShow
dcacheDevTune
dcacheDevMemResize
dcacheDevEnable
dcacheDevDisable
dcacheDevCreate
dcacheCtrl
dbgmsg
dbg_write
dbgVibOn
dbgVibOff
dbgVibDe
dbgVibAlwaysOff
dbgVib
dbgUnbreakableOld
dbgTaskStep
dbgTaskCont
dbgTaskBpTrap
dbgTaskBpTrace
dbgTaskBpHooksInstall
dbgTaskBpBreakpoint
dbgSoundMix
dbgSoundAlways
dbgSafeUnbreakable
dbgRingerOn
dbgRingerOff
dbgRingerDe
dbgRingerAlwaysOff
dbgRinger
dbgPutBuffer
dbgPrintSimd
dbgPrintFpp
dbgPrintDsp
dbgPrintCall
dbgMixModeOff
dbgMixModeInit
dbgMixMode
dbgLog
dbgLockUnbreakable
dbgInstallRinger
dbgInit
dbgHelp
dbgDspApiMgr
datetime_edit_msgbox
date
dataXferTask
dataXfer
dataPort
dOldSignal
current_demangling_style
currentStatus
currentContext
cur_script_info
ctime_r
ctime
cseq_setnumber
cseq_setmethod
cseq_parse
cseq_match
cseq_init
cseq_getnumber
cseq_getmethod
cseq_free
cseq_clone
cseq_2char
cret
creationDate
create_sip_sem
create_setting_new_ser
create_setting_idle_new
create_setting_call_set
create_satime_needdata
create_rtcp_thread
create_rtcp_msgq
createEncoder__15CdspRootManagerUsUs
createEncoder__11CdspManagerUsUs
createDecoder__15CdspRootManagerUsUs
createDecoder__11CdspManagerUsUs
createCodecs__15CdspRootManager
creat
cre_setting_inm_pinyin
cre_setting_inm_eng
cre_setting_inm_ZIstr
cre_setting_inm_ZIpiny
cre_setting_inm_ZIeng
cre_setting_idle_sta
cre_setting_idle_pic1
cre_setting_idle_pic0
cre_setting_idle_mode
cre_setting_idle_edit
cre_setting_idle_cha
cpsr
cplus_mangle_opname
cplus_demangle_set_style
cplus_demangle_opname
cplus_demangle_name_to_style
cplus_demangle
cplusXtorStrategy
cplusXtorSet
cplusUnloadFixup
cplusMatchMangled
cplusLoadFixup
cplusDtorsLink
cplusDtors
cplusDemanglerStyleSet
cplusDemanglerStyle
cplusDemanglerSet
cplusDemanglerMode
cplusDemanglerInit
cplusDemangleFunc
cplusDemangle
cplusCtorsLink
cplusCtors
cplusCallDtors
cplusCallCtors
count
cosh
core
copysign
copyright_wind_river
copy_parameter
copy_option_from_entry
copy_option
copy_data_to_option
copy_configuration_options_to_tx_accepted_options
copy_configuration_options_list
copyStreams
copy
convert2DTMF2833
content_type_parse
content_type_init
content_type_get_type
content_type_free
content_type_clone
content_type_2char
content_length_parse
content_length_init
content_length_free
content_length_clone
content_length_2char
contained_public_p__16__user_type_infoQ216__user_type_info8sub_kind
contained_p__16__user_type_infoQ216__user_type_info8sub_kind
contained_nonvirtual_p__16__user_type_infoQ216__user_type_info8sub_kind
contained_nonpublic_p__16__user_type_infoQ216__user_type_info8sub_kind
contacted
contact_parse
contact_init
contact_free
contact_clone
contact_2char
consoleFd
connectWithTimeout
connect
config_if
config_data_buffer
configStatus
conf_solar_rtn
conf_solar_2idle
conf_ringmode_timer
conf_ringmode_change
conf_reg_totaltimeok
conf_reg_totaltime_msgyes
conf_reg_timeall_msgno
conf_reg_timeall_msgclose
conf_reg_time_exit
conf_reg_telnum_saveyes
conf_reg_telnum_saveno3
conf_reg_telnum_saveno2
conf_reg_telnum2savename
conf_reg_talk
conf_reg_savegroup_ok
conf_reg_savegroup_no
conf_reg_return_missing
conf_reg_return_incoming
conf_reg_return_idle
conf_reg_return
conf_reg_pwd_ok
conf_reg_pwd_input
conf_reg_pwd_err
conf_reg_outlog_arrow
conf_reg_nametogroup
conf_reg_missinglog_arrow
conf_reg_main_totaltime
conf_reg_main_selected
conf_reg_main_recv
conf_reg_main_outall
conf_reg_main_noinfo
conf_reg_main_missing
conf_reg_main_dellog
conf_reg_in_arrow
conf_reg_group_selok
conf_reg_group_pick
conf_reg_dolog_time
conf_reg_dolog_telnum
conf_reg_dolog_preselect
conf_reg_dolog_pickdata
conf_reg_dolog_msgyes
conf_reg_dolog_msgclose3
conf_reg_dolog_msgclose2
conf_reg_dolog_msgclose1
conf_reg_dolog_dur
conf_reg_dolog_delete
conf_reg_dialog_left
conf_reg_dellog_predo
conf_reg_dellog_pickdata
conf_reg_dellog_msgyes
conf_reg_dellog_msgc2
conf_reg_dellog_msgc1
conf_reg_dellog_listsel
conf_reg_dellog_all
conf_reg_delllog_msgno
conf_reg_back_outcall
conf_reg_back_mainmenu
conf_pro_whis_pickdata
conf_pro_whis_listsel
conf_pro_warning_listsel
conf_pro_volume_timer
conf_pro_volume_pickdata
conf_pro_volume_ok
conf_pro_volume_listsel
conf_pro_volume_change
conf_pro_time_play
conf_pro_smstone_listsel
conf_pro_ring_pickdata
conf_pro_ring_listsel
conf_pro_ring_change
conf_pro_return_speed
conf_pro_return_mainmenu
conf_pro_preplay
conf_pro_mode_pickdata
conf_pro_mode_listsel
conf_pro_memotone_listsel
conf_pro_main_whisper
conf_pro_main_warning
conf_pro_main_volume
conf_pro_main_start
conf_pro_main_ringtone
conf_pro_main_ringmode
conf_pro_main_memotone
conf_pro_main_keytone
conf_pro_main_infotone
conf_pro_main_alarmtone
conf_pro_keytone_pickdata
conf_pro_keytone_listsel
conf_pro_anykey_stoptimer
conf_msgokclose
conf_msgok2speed
conf_msgerrorclose
conf_lunar_2solar
conf_lunar_2date
conf_datesel_rtn
conf_calenrtn2tool
conf_calen2solar
conf_calen2lunar
conf_calen2datesel
conf_cal_return
conf_cal_2idle
conf_WorldTime_return
conf_WorldTime_Select
conf_WorldTime_Save
conf_WorldTime_LeftRight
conf_WorldTime_ChangeSuc
conf_WorldTime_ChangeFailure
conf_TimeFormat_Select
conf_Dst_Select
conf_DST_Save
conf1_pro_return_speed
conf1_pro_return_mainmenu
conf1_pro_keytone_listsel
complete_answer_that_establish_a_dialog
communicating
commfd
codecs_config_uninit
codecs_config_init
codec_unregister_all
codec_rtpmap
codec_pt
codec_init_default
codec_config_update
cmp_time
cmds
clr_dump
closelog
closedir
close_rtp_session
close
clock_show
clock_settime
clock_setres
clock_gettime
clock_getres
clockLibInit
clock
client_port
cliSem
clearerr
clearaddr
clear_rtp_events_pack
clearPrimaryNode
clearJb
clearDataNode
cleanse_ctr
clean_param
classShowConnect
classMemPartIdSet
classLibInit
classInstrument
classInstConnect
classInit
classDestroy
classCreate
classClassId
clarinet_random_seed
cisShow
cisRegsShow
cisParse
cisGetWord
cisCORReset
cipher_val
chkdsk
checksum
checkedHandler
check_sipurl
check_req_sdes_items
check_options_from_reject_packet
check_for_registration
checkStack
checkPort__16CdspRootDataPort
checkInetAddrField
chdir
charge_timeout_process
charge_sys_pause
charge_sleep
charge_full_process
charge_draw_icon_stop
charge_draw_icon_full
charge_draw_icon
charge_ctrl
charge_adc_psc_poll
charcnt
char_present
chapRemoteUserNameGet
chapLocalUserNameSet
chapLocalUserNameGet
change_picture_sel
change_constrast
changeReg
changePhoneParam
changeOptionValueInConfiguredList
changeMacAddr
changeLogLevel
changeBootParam
cfree
cfi_sup
cfg_drv_sup_range
cfg_drv_identity
cfg_drv_act_ranges_sta
cfg_drv_act_ranges_pri
cfg_drv_act_ranges_hsi
cfg_drv_act_ranges_apf
cevent2
cevent
ceil
cce_bsearch2
cbioWrapBlkDev
cbioUnlock
cbioShow
cbioRdyChk
cbioRdyChgdSet
cbioRdyChgdGet
cbioParamsGet
cbioMutexSemOptions
cbioModeSet
cbioModeGet
cbioLock
cbioLibInit
cbioIoctl
cbioDevVerify
cbioDevCreate
cbioClassId
cbioClass
cbioBytesRW
cbioBlkRW
cbioBlkCopy
catInfo
candidatesBuffer2
candidatesBuffer
cancel
calog_Start
calogTask
calloc
callnumtxtNet
callnumtxt
callleg_match
callleg_list
callid_getcopy
call_info_seturi
call_info_parse
call_info_init
call_info_geturi
call_info_free
call_info_clone
call_info_2char
call_id_setnumber
call_id_sethost
call_id_parse
call_id_new_random
call_id_match
call_id_init
call_id_getnumber
call_id_gethost
call_id_free
call_id_clone
call_id_2char
call_err_sub
call_disconnect_timer
calg_getProductID
calgWriteNack
calgWriteAck
calgReadCmdHeader
calendar_passdate
calendar_freeglb
calendar_destool
calendar_dessolar
calendar_desidle
calendar_desdate
calen_savedate
calen_dateCallBack
calculator_destool
calculator_desidle
calculate32BitFcs
calculate16BitFcs
calNumber
cadenceOn
cacheUserFuncs
cacheUnlock
cacheTextUpdate
cachePipeFlush
cacheNullFuncs
cacheMmuAvailable
cacheLock
cacheLibInit
cacheLib
cacheInvalidate
cacheFuncsSet
cacheFlush
cacheEnable
cacheDrvVirtToPhys
cacheDrvPhysToVirt
cacheDrvInvalidate
cacheDrvFlush
cacheDmaMallocRtn
cacheDmaMalloc
cacheDmaFuncs
cacheDmaFreeRtn
cacheDmaFree
cacheDisable
cacheDataMode
cacheDataEnabled
cacheClear
cacheArm946eLibInstall
cacheArm946eIdentify
cacheArm946eIInvalidateAll
cacheArm946eIInvalidate
cacheArm946eIClearDisable
cacheArm946eDInvalidateAll
cacheArm946eDInvalidate
cacheArm946eDFlushAll
cacheArm946eDFlush
cacheArm946eDClearDisable
cacheArm946eDClearAll
cacheArm946eDClear
cacheArm946eArchPipeFlush
cacheArchState
cacheArchIntMask
cacheArchIntLock
cacheArchIndexMask
cacheArchAlignSize
c_rngmd_anykey_stptmr
c_pro_alarmtone_listsel
bzero
bypass_rx_fsm
bye_cb
byToneType
buildOnePBNumIndexTbl
bufReleaseSingle
bufPoolInit
bufFree
bufAlloc
btaCallNumberForSave
bswap
bsearch
bsdZbufSockRtn
bsdSocket
bsdSockLibInit
bsdSockFunc
bsdSock43ApiFlag
bsdShutdown
bsdSetsockopt
bsdSendto
bsdSendmsg
bsdSend
bsdRecvmsg
bsdRecvfrom
bsdRecv
bsdListen
bsdGetsockopt
bsdGetsockname
bsdGetpeername
bsdConnectWithTimeout
bsdConnect
bsdBind
bsdAccept
bplaying
bpf_validate
bpf_filter
bpfWrite
bpfWakeup
bpfTkProtoShutdown
bpfTkProtoInput
bpfTimeStamp
bpfSleep
bpfSetFilter
bpfSelectDelete
bpfSelectAdd
bpfRead
bpfProtoShutdown
bpfProtoInput
bpfProtoInitDone
bpfPacketCatch
bpfOpen
bpfLockTaskId
bpfLockSemId
bpfIoctl
bpfIfSet
bpfDrvRemove
bpfDrvNum
bpfDrvCount
bpfDrv
bpfDltTblSize
bpfDltTbl
bpfDevReset
bpfDevFree
bpfDevDelete
bpfDevCreate
bpfClose
bpfBufsAlloc
bpfBufSize
bpList
bpFreeList
bound
bootStructToString
bootStringToStruct
bootScanNum
bootParamsShow
bootParamsPrompt
bootParamsErrorPrint
bootNetmaskExtract
bootLeaseExtract
bootChange
bootBpAnchorExtract
body_setheader
body_setcontenttype
body_parse_mime
body_parse_header
body_parse
body_init
body_handler_init_with_ua
body_handler_init
body_handler_create_context
body_handler_class_init
body_gen_answer_according_localprofile
body_free
body_context_init
body_clone
body_2char
binvert
bindresvportCommon
bindresvport
bind
bfillBytes
bfill
belowIcon
before__C9type_infoRC9type_info
bdall
bcopyWords
bcopyLongs
bcopyBytes
bcopy
bcmp
bchoosempeg4
bb_speaker_volumn
batteryAniPage
bat_stop_volt_Det
bat_low_volt_Det
bat_charge_mode
bandwidths
badport_bandlim
backplaneBoot
backlight_fader
backlight_ctrl
back_light_needdata
bWflash
bTonePri
bToPuncInput
bSoWriteOn
bSmsFull
bSignDisplay
bSIPInited
bResume
bPhoneIsSleep
bOverflowFlag
bNegKeyPress
bLcdVopVol
bKeyQueLock
bIsVolumePreview
bIsUpdate
bIsPWWrong
bIsLocalUpdate
bIpEmpty
bInsKeyPress
bIdleSpeed2NetSrv
bIPField
bGotoIdle
bFilterKeyEvt
bErrorInfo
bErrorFlag
bEquKeyPress
bEnglishSingleWellField
bEnglishSingleField
bEnglishOnlyField
bDotKeyPress
bDisplayFlag
bDirKeyPress
bDelDirKey
bDeinitPuncField
bCceHasEvent
awWeekdayID
awDateIcon
avlTreeWalk
avlTreePrintErase
avlTreePrint
avlTreeErase
avlSuccessorGet
avlSearchUnsigned
avlSearch
avlRemoveInsert
avlRebalance
avlPredecessorGet
avlMinimumGet
avlMaximumGet
avlInsertUnsigned
avlInsertInform
avlInsert
avlDeleteUnsigned
avlDelete
av_profile_init
av_profile
autoscanInter
autoscanFlag
authorization_setusername
authorization_seturi
authorization_setresponse
authorization_setrealm
authorization_setopaque
authorization_setnonce_count
authorization_setnonce
authorization_setmessage_qop
authorization_setdigest
authorization_setcnonce
authorization_setauth_type
authorization_setalgorithm
authorization_parse
authorization_init
authorization_getusername
authorization_geturi
authorization_getresponse
authorization_getrealm
authorization_getopaque
authorization_getnonce_count
authorization_getnonce
authorization_getmessage_qop
authorization_getdigest
authorization_getcnonce
authorization_getauth_type
authorization_getalgorithm
authorization_free
authorization_clone
authorization_2char
audio_stream_stop
audio_stream_start_full
audio_list
audio_codec_list
attrib
atol
atoi
atof
atintrq2_present
atintrq1_present
atexit
ate_write_username
ate_write_station_num
ate_write_rx_agcclib
ate_write_rf_txcont
ate_write_rf_iqdac
ate_write_rf_agcclib
ate_write_psid
ate_write_pc_debugflag
ate_write_password
ate_write_mac
ate_write_flash
ate_word_to_str
ate_vibration_test
ate_toggle_sleepmode
ate_toggle_factorymode
ate_toggle_atetest
ate_test_isenable
ate_test_enable
ate_sram_test
ate_sram_check
ate_spk_vol_test
ate_sleep_isenable
ate_sleep_enable
ate_show_voltage
ate_set_tftp_param
ate_set_result_withdata
ate_read_sw_version
ate_read_station_num
ate_read_psid
ate_read_mac
ate_read_flash
ate_pro_tab_init
ate_pc_write_para
ate_pc_task_init
ate_pc_task
ate_pc_read_para
ate_pc_clr_usr_data
ate_pc_ack_result
ate_para_info
ate_out_title
ate_out_text
ate_out_paradisc
ate_out_keybuf
ate_open_comport
ate_mmi_tab_init
ate_mic_bias_volt
ate_link_check
ate_led_test
ate_lcd_test
ate_keypad_test
ate_key_tone_test
ate_init_cmd_parameter
ate_hardware_init
ate_hand_task_init
ate_hand_task
ate_hand_show_result
ate_getkey_withtimeout
ate_getkey
ate_get_tftp_param
ate_get_pc_command
ate_get_hand_command
ate_get_cmd_test
ate_flash_test
ate_factory_mode_isenable
ate_factory_mode_enable
ate_execute_cmd
ate_enter_testmode
ate_eeprom_rdwr
ate_eeprom_rd
ate_earphone_loop_audio
ate_earphone_insert_test
ate_dsp_init
ate_curr_detection
ate_com_writen
ate_com_readn
ate_cmd_construct
ate_clr_usr_data
ate_close_comport
ate_clib_data
ate_check_powerdown
ate_check_cmdtbl
ate_check_cmd_param
ate_charging_test
ate_bat_voltage_test
ate_audio_loop_test
ateVMicSwitch
ateSetVolume
ateSetGains
ateSetDecoderHandsetGain
atePlayKeyTone
ateIsDspOK
ateDspPowerOff
ateDspLoopback
atan2
atan
async_resolv_and_send_ack
async_resolv_and_send
astuDebugInfo
astuAnimation
asin
asctime_r
asctime
arrSaveTftpServer
arptfree
arptabShow
arpresolve
arpioctl
arpintrq
arp_reply
arp_ifinit
arp_check
arpShow
arpRxmitDelay
arpResolve
arpMaxEntries
arpLibInit
arpFlush
arpDelete
arpCmd
arpAdd
armInstrChangesPc
armInitExceptionModes
armGetNpc
answer_mode_needdata
animate_selected
animate_sel_3
animate_sel_2
animate_sel_1
animate_sel_0
analyze_ACK_4_BODY
alternate_option_value_match
alloc_hash_ctx_base
alloc_hash_ctx
align_msg
aliases9
aliases520
aliases42
alarm_switch_needdata
alarm_selecting
alarm_lazy_needdata
alarm_cycle_needdata
alarm_circle_sel
alarm_circle_needdata
alarm_bound
alarm_Swt_sel
alarm_Lazy_sel
alarm
aes_wrap
aes_unwrap
aes_128_encrypt_block
aes_128_eax_encrypt
aes_128_eax_decrypt
aes_128_ctr_encrypt
aes_128_cbc_encrypt
aes_128_cbc_decrypt
admindebug
adminPwd
addreq
add_write_msgq
add_write_fd
add_timer_event
add_remote_ppp_option
add_read_msgq
add_read_fd
add_ppp_option
add_option_to_alternate_list
add_new_ppp_option_to_list
add_entry_to_list
add_entry_to_front_of_list
add_configuration_option_range
add_configuration_option
add_char
add_alternate_to_configuration_option
addSegNames
addDomain
adc_psc_read_onetime
adc_psc_poll
adc_poll_timer_start
adc_poll_timer_cancle
activeQHead
activate_stun_result_no_reg_immed
activate_stun_result
acos
accept_video_offer
accept_encoding_setelement
accept_encoding_parse
accept_encoding_init
accept_encoding_getelement
accept_encoding_free
accept_encoding_clone
accept_encoding_2char
accept_audio_offer
accept
acc_supply_ctrl
abtWeekIconId
abtTalkingIconID
abtSearchIconID
abtPoweroffIconID
abtPowOnIconID4
abtPowOnIconID3
abtPowOnIconID2
abtPowOnIconID1
abtPowOffIconID4
abtPowOffIconID3
abtPowOffIconID2
abtPowOffIconID1
abtMtConnectingIconID
abtLowBatteryIconID
abtConnectingIconID
abtChargeIconID
abs__Fr
abs__Fl
abs__Ff
abs__Fd
aboveIcon
abort
aIconNums
aCalenFontlIcon
_zlib_tr_tally
_zlib_tr_stored_block
_zlib_tr_init
_zlib_tr_flush_block
_zlib_tr_align
_zlib_length_code
_zlib_dist_code
_wSysIPcallTimer
_vt$9type_info
_vt$9exception
_vt$9bad_alloc
_vt$8bad_cast
_vt$5CList
_vt$17__class_type_info
_vt$16__user_type_info
_vt$14__si_type_info
_vt$13bad_exception
_vt$11CdspEncoder
_vt$11CdspDecoder
_vt$10bad_typeid
_vt$10CMutexList
_speed_menus
_sigfaulttable
_sigCtxStackEnd
_sigCtxSetup
_sigCtxSave
_sigCtxRtnValSet
_sigCtxLoad
_setjmpSetup
_schedPxKernelIsTimeSlicing
_sch_toupper
_sch_tolower
_sch_istable
_rtNewAddrMsgHook
_rtMissMsgHook
_rtIfaceMsgHook
_res_resultcodes
_res_opcodes
_res
_pthread_setcanceltype
_pthreadSetCancelType
_pthreadSemStateGet
_pthreadSemOwnerGet
_pthreadLibInit
_pthreadCreate
_protoSwIndex
_protoBindStatusGet
_procNumWasSet
_presolvQuery
_presolvHostLibGetByName
_presolvHostLibGetByAddr
_presolvDNExpand
_pres_hnok
_pres_dnok
_presSearchN
_presSearch
_pingTxTmo
_pingTxLen
_pingTxInterval
_pingSockBufSize
_pfwProfileDelete
_pfwParameterAdd
_pfwObjProfileDataShow
_panicHook
_p_res
_p_getshort
_p__dn_skipname
_pUdpPcbHead
_pTcpPcbPrint
_pTcpPcbHead
_pSigQueueFreeHead
_pNetSysPool
_pNetPoolFuncTbl
_pNetDpool
_pNetBufCollect
_muxTkSendNpt
_muxTkSendEnd
_muxProtosPerEndStart
_muxProtosPerEndInc
_mmuCrValue
_mCastRouteCmdHook
_m2SetIfLastChange
_m2IfTableUpdate
_ll_uto_f
_ll_uto_d
_ll_ufrom_f_r
_ll_ufrom_f
_ll_ufrom_d_r
_ll_ufrom_d
_ll_sto_f
_ll_sto_d
_ll_sfrom_f_r
_ll_sfrom_f
_ll_sfrom_d_r
_ll_sfrom_d
_ipsecSizing
_ipsecOutput
_ipsecInput
_ipsecFilterHook
_ipFilterHook
_ipAttach
_igmpQuerierTimeUpdateHook
_igmpMessageHook
_igmpLeaveGrpHook
_igmpLeaveAlertHook
_igmpJoinGrpHook
_igmpJoinAlertHook
_icmpErrorHook
_http
_hpcopy
_hostconf
_getshort
_getnetbydnsname
_getlong
_gethostbyname
_gethostbyaddr
_func_wvNetPortFilterTest
_func_wvNetAddressFilterTest
_func_wdbIsNowExternal
_func_vxMemProbeHook
_func_valloc
_func_trgCheck
_func_trap
_func_tmrStampLock
_func_tmrStamp
_func_tmrPeriod
_func_tmrFreq
_func_tmrEnable
_func_tmrDisable
_func_tmrConnect
_func_taskRegsShowRtn
_func_taskDeleteHookAdd
_func_taskCreateHookAdd
_func_symValueGet
_func_symTypeGet
_func_symNameGet
_func_symFindSymbol
_func_symFindByValueAndType
_func_symFindByValue
_func_sseTaskRegsShow
_func_spyTask
_func_spyStop
_func_spyReport
_func_spyClkStop
_func_spyClkStart
_func_spy
_func_smObjObjShow
_func_sigprocmask
_func_sigTimeoutRecalc
_func_sigExcKill
_func_selWakeupListTerm
_func_selWakeupListInit
_func_selWakeupAll
_func_selTyDelete
_func_selTyAdd
_func_selPtyDelete
_func_selPtyAdd
_func_remCurIdSet
_func_remCurIdGet
_func_pthread_setcanceltype
_func_printErr
_func_netLsByName
_func_memalign
_func_logMsg
_func_ioTaskStdSet
_func_ftpTransientFatal
_func_ftpLs
_func_fppTaskRegsShow
_func_fileDoesNotExist
_func_fclose
_func_fastUdpPortTest
_func_fastUdpInput
_func_fastUdpErrorNotify
_func_excPanicHook
_func_excJobAdd
_func_excIntHook
_func_excInfoShow
_func_excBreakpoint
_func_excBaseHook
_func_evtLogTSched
_func_evtLogT1_noTS
_func_evtLogT1
_func_evtLogT0_noInt
_func_evtLogT0
_func_evtLogString
_func_evtLogReserveTaskName
_func_evtLogPoint
_func_evtLogOIntLock
_func_evtLogO
_func_evtLogM3
_func_evtLogM2
_func_evtLogM1
_func_evtLogM0
_func_dspTaskRegsShow
_func_dspRegsListHook
_func_dspMregsHook
_func_dbgTargetNotify
_func_dbgHostNotify
_func_bdall
_func_armPageSource
_func_armIrqHandler
_func_armIntStackSplit
_fsub
_frsb
_frdiv
_fp_trapveneer
_fp_trap
_fp_round
_fpStatus
_fneq
_fneg
_fmul
_fls
_fleq
_fgr
_fgeq
_ffltu
_fflt
_ffixu_r
_ffixu
_ffix_r
_ffix
_feq
_fdiv
_fcmple
_fcmpge
_fcmpeq
_fadd
_fabs
_f_utof
_f_ulltof
_f_sub
_f_mul
_f_lltof
_f_itof
_f_ftoull
_f_ftou
_f_ftoll
_f_ftoi
_f_ftod
_f_fne
_f_flt
_f_fle
_f_fgt
_f_fge
_f_feq
_f_div
_f_cmpe
_f_cmp
_f_add
_f2d
_dsub
_dsqrt
_drsb
_drem
_drdiv
_dneq
_dneg
_dmul
_dls
_dleq
_dhcpcStateTaskStackSize
_dhcpcStateTaskPriority
_dhcpcStateTaskOptions
_dhcpcReadTaskStackSize
_dhcpcReadTaskPriority
_dhcpcReadTaskOptions
_dhcpcBootFlag
_dgr
_dgeq
_dfltu
_dflt
_dfixu_r
_dfixu
_dfix_r
_dfix
_deq
_ddiv
_dcmple
_dcmpge
_dcmpeq
_dbgTaskPCSet
_dbgTaskPCGet
_dbgRetAdrsGet
_dbgInstSizeGet
_dbgFuncCallCheck
_dbgDsmInstRtn
_dbgArchInit
_dadd
_dabs
_d_utod
_d_ulltod
_d_sub
_d_mul
_d_lltod
_d_itod
_d_fne
_d_flt
_d_fle
_d_fgt
_d_fge
_d_feq
_d_dtoull
_d_dtou
_d_dtoll
_d_dtoi
_d_dtof
_d_div
_d_cmpe
_d_cmp
_d_add
_d2f
_cplusDemangle
_cmd_paradisc_ATE_WR_USRNAME
_cmd_paradisc_ATE_WR_STATION_NUM
_cmd_paradisc_ATE_WR_PSID
_cmd_paradisc_ATE_WR_PASSWORD
_cmd_paradisc_ATE_WR_MAC
_cmd_paradisc_ATE_TOGGLE_SLEEP
_cmd_paradisc_ATE_TOGGLE_FACTORYMODE
_cmd_paradisc_ATE_TOGGLE_ATE_TEST
_cmd_paradisc_ATE_SPK_VOL_TEST
_cmd_paradisc_ATE_SET_TFTP_PARAM
_cmd_paradisc_ATE_PC_WRITE_PARA
_cmd_paradisc_ATE_PC_READ_PARA
_cmd_paradisc_ATE_LED_TEST
_cmd_paradisc_ATE_LCD_TEST
_cmd_paradisc_ATE_EARPHONE_LOOP_AUDIO
_cmd_paradisc_ATE_CURR_DETECTION
_cmd_paradisc_ATE_CHARGING_TEST
_cmd_paradisc_ATE_BAT_VOLTAGE_TEST
_cmd_paradisc_ATE_AUDIO_LOOP_TEST
_clockRealtime
_caFlashKeyString
_bpfUnlock
_bpfUnitUnlock
_bpfUnitLock
_bpfProtoSend
_bpfProtoPromisc
_bpfProtoInit
_bpfProtoDetach
_bpfProtoAttach
_bpfPacketTap
_bpfLock
_bpfDevUnlock
_bpfDevLock
_bpfDevDetach
_archHelp_msg
_aSysBatteryMeasure
__vn__FUlRC9nothrow_t
__vn__FUlPv
__vd__FPvRC9nothrow_t
__urem64
__urem32
__unpack_f
__unpack_d
__uncatch_exception
__umodsi3
__umoddi3
__ult64
__ule64
__ugt64
__uge64
__udivsi3
__udivmoddi4
__udivdi3
__udiv_w_sdiv
__udiv64
__udiv32
__ucmpdi2
__truncdfsf2
__tix
__tiw
__tiv
__tis
__tir
__til
__tii
__tif
__tid
__tic
__tib
__tiUx
__tiUs
__tiUl
__tiUi
__tiUc
__tiSc
__ti9type_info
__ti9exception
__ti9bad_alloc
__ti8bad_cast
__ti8CdspPort
__ti7CModule
__ti5CList
__ti19__pointer_type_info
__ti19__builtin_type_info
__ti17__class_type_info
__ti17__array_type_info
__ti16__user_type_info
__ti16__ptmf_type_info
__ti16__ptmd_type_info
__ti16__func_type_info
__ti16__attr_type_info
__ti16CdspRootDataPort
__ti15CdspRootManager
__ti15CdspRootEncoder
__ti15CdspRootDecoder
__ti14__si_type_info
__ti13bad_exception
__ti12CListElement
__ti11CdspManager
__ti11CdspEncoder
__ti11CdspDecoder
__ti10bad_typeid
__ti10CMutexList
__throw_type_match_rtti_2
__throw_type_match_rtti
__throw_type_match
__throw_bad_typeid
__throw_bad_cast
__thenan_sf
__thenan_df
__tfx
__tfw
__tfv
__tfs
__tfr
__tfl
__tfi
__tff
__tfd
__tfc
__tfb
__tfUx
__tfUs
__tfUl
__tfUi
__tfUc
__tfSc
__tf9type_info
__tf9exception
__tf9bad_alloc
__tf8bad_cast
__tf5CList
__tf17__class_type_info
__tf16__user_type_info
__tf14__si_type_info
__tf13bad_exception
__tf11CdspEncoder
__tf11CdspDecoder
__tf10bad_typeid
__tf10CMutexList
__terminate_func
__terminate
__sysctl
__sym_ston
__sym_ntos
__sym_ntop
__swsetup
__swrite
__swbuf
__subsf3
__subdf3
__sub64
__strxfrm
__stdout
__stdin
__stderr
__start_cp_handler
__sseek
__srget
__srefill
__sread
__smakebuf
__sjthrow
__sjpopnthrow
__shtab
__sfvwrite
__sfpRoundMode
__sflush
__sflags
__sclose
__rtti_user
__rtti_si
__rtti_ptr
__rtti_ptmf
__rtti_ptmd
__rtti_func
__rtti_class
__rtti_attr
__rtti_array
__rtc_free_ptr
__rtc_blkinfo_ptr
__rtc_alloc_ptr
__rta_longjmp
__rt_fp_status_addr
__rem64
__rem32
__putshort
__putlong
__pack_f
__pack_d
__p_type_syms
__p_type
__p_time
__p_class_syms
__p_class
__osip_find_transaction
__nw__FUlRC9nothrow_t
__nw__FUlPv
__new_handler
__nesf2
__negsf2
__negdi2
__negdf2
__nedf2
__ne__C9type_infoRC9type_info
__ne64
__mulsf3
__muldi3
__muldf3
__mul6432
__mul64
__modsi3
__moddi3
__make_fp
__make_dp
__ltsf2
__ltdf2
__lt64
__lsr64
__lsl64
__lshrdi3
__loctime
__locale
__lesf2
__ledf2
__le64
__kernel_tan
__kernel_sin
__kernel_rem_pio2
__kernel_poly
__kernel_cos
__julday
__is_pointer__FPv
__includeGnuIntrinsics
__includeDiabIntrinsics
__ieee754_rem_pio2
__gtsf2
__gtdf2
__gt64
__get_eh_info
__get_eh_context
__get_dynamic_handler_chain
__getZoneInfo
__getTime
__getDstInfo
__gesf2
__gedf2
__ge64
__gcc_intrinsicsInit
__gcc_bcmp
__funder_d
__funder
__fpl_return_NaN
__fpl_normalise2
__fpl_fcheck_NaN2
__fpl_exception
__fpl_dcmp_InfNaN
__fpl_dcheck_NaN2
__fpl_cmpreturn
__fpcmp_parts_f
__fpcmp_parts_d
__fp_query
__floatsisf
__floatsidf
__floatdisf
__floatdidf
__fixunssfsi
__fixunssfdi
__fixunsdfsi
__fixunsdfdi
__fixsfsi
__fixsfdi
__fixdfsi
__fixdfdi
__fflt_normalise
__ff1ll
__ff1l
__ff1
__extendsfdf2
__exp10
__errno
__eqsf2
__eqdf2
__eq__C9type_infoRC9type_info
__eq64
__empty
__eh_rtime_match
__eh_free
__eh_alloc
__dynamic_cast_2
__dynamic_cast
__dunder_d
__dunder
__dummy
__dn_skipname
__dl__FPvRC9nothrow_t
__divsi3
__divsf3
__divdi3
__divdf3
__div64
__div32
__div0
__diab_unlock_semaphore
__diab_unlock_mutex
__diab_trylock_semaphore
__diab_trylock_mutex
__diab_lock_semaphore
__diab_lock_mutex
__diab_intrinsics_tornInit
__diab_intrinsics_implInit
__diab_intrinsics_impfpInit
__diab_free_semaphore
__diab_free_mutex
__diab_atomic_restore
__diab_atomic_enter
__diab_alloc_semaphore
__diab_alloc_mutex
__dflt_normalise
__default_unexpected__Fv
__default_terminate
__daysSinceEpoch
__ctype
__cplus_type_matcher
__cplusXtors_o
__cplusUsr_o
__cplusLoad_o
__cplusLoadObjFiles
__cplusLibgccObjs
__cplusDem_o
__cp_push_exception
__cp_pop_exception
__cp_exception_info
__cp_eh_info
__costate
__common_long_jmp
__common_intrinsicsInit
__cmpsf2
__cmpdi2
__cmpdf2
__clocale
__clear_cache
__check_eh_spec
__builtin_vec_new
__builtin_vec_delete
__builtin_new
__builtin_delete
__assert
__asr64
__ashrdi3
__ashldi3
__arm_call_via_o
__addsf3
__adddf3
__add64
___x_gnu_tinfo_o
___x_gnu_tinfo2_o
___x_gnu_opvnewnt_o
___x_gnu_opvnew_o
___x_gnu_opvdelnt_o
___x_gnu_opvdel_o
___x_gnu_opnewnt_o
___x_gnu_opnew_o
___x_gnu_opdelnt_o
___x_gnu_opdel_o
___x_gnu_new_o
___x_gnu_frame_o
___x_gnu_exception_o
___x_gnu_cstdlibi_o
___x_gnu_cmathi_o
___x_gnu__unpack_sf_o
___x_gnu__umodsi3_o
___x_gnu__umoddi3_o
___x_gnu__udivsi3_o
___x_gnu__udivmoddi4_o
___x_gnu__udivdi3_o
___x_gnu__udiv_w_sdiv_o
___x_gnu__ucmpdi2_o
___x_gnu__trampoline_o
___x_gnu__thenan_sf_o
___x_gnu__shtab_o
___x_gnu__sf_to_usi_o
___x_gnu__pack_sf_o
___x_gnu__negdi2_o
___x_gnu__muldi3_o
___x_gnu__modsi3_o
___x_gnu__moddi3_o
___x_gnu__make_sf_o
___x_gnu__lshrdi3_o
___x_gnu__interwork_call_via_rX_o
___x_gnu__fpcmp_parts_sf_o
___x_gnu__floatdixf_o
___x_gnu__floatditf_o
___x_gnu__fixxfdi_o
___x_gnu__fixunsxfsi_o
___x_gnu__fixunsxfdi_o
___x_gnu__fixunstfdi_o
___x_gnu__fixtfdi_o
___x_gnu__eprintf_o
___x_gnu__eh_o
___x_gnu__dvmd_tls_o
___x_gnu__dp_unpack_df_o
___x_gnu__dp_thenan_df_o
___x_gnu__dp_sf_to_usi_o
___x_gnu__dp_pack_df_o
___x_gnu__dp_make_df_o
___x_gnu__dp_fpcmp_parts_df_o
___x_gnu__dp_df_to_usi_o
___x_gnu__divsi3_o
___x_gnu__divdi3_o
___x_gnu__df_to_usi_o
___x_gnu__cmpdi2_o
___x_gnu__clear_cache_o
___x_gnu__bb_o
___x_gnu__bb_init_func_o
___x_gnu__ashrdi3_o
___x_gnu__ashldi3_o
___x_gnu___gcc_bcmp_o
___x_gnu___dummy_o
___x_diab_wr_sw_ld_o
___x_diab_wr_sw_fl_o
___x_diab_wr_sw_db_o
___x_diab_wr_pk_ld_o
___x_diab_wr_pk_fl_o
___x_diab_wr_pk_db_o
___x_diab_torn_syncsem_o
___x_diab_torn_syncmutex_o
___x_diab_torn_syncatomic_o
___x_diab_sxprem64_o
___x_diab_sxprem32_o
___x_diab_sxpmul64_o
___x_diab_sxpm6432_o
___x_diab_sxplsr64_o
___x_diab_sxplsl64_o
___x_diab_sxpdiv64_o
___x_diab_sxpcmp64_o
___x_diab_sxpasr64_o
___x_diab_sxpadd64_o
___x_diab_sfpround_o
___x_diab_sfpfsetup_o
___x_diab_sfpfnorm_o
___x_diab_sfpfcmpe_o
___x_diab_sfpfcmp_o
___x_diab_sfpdsetup_o
___x_diab_sfpdpol_o
___x_diab_sfpdnorm_o
___x_diab_sfpdcmpe_o
___x_diab_sfpdcmp_o
___x_diab_rtahooks_o
___x_diab_rd_sw_ld_o
___x_diab_rd_sw_fl_o
___x_diab_rd_sw_db_o
___x_diab_rd_pk_ld_o
___x_diab_rd_pk_fl_o
___x_diab_rd_pk_db_o
___x_diab_libg_o
___x_diab_ff1_o
___x_diab_comljmp_o
___x_diab_arm_div_o
__POL
__OSSendEvent
__InitDebugInfo
__DeleteDebugItem
__DIAB_wr_sw_ld
__DIAB_wr_sw_fl
__DIAB_wr_sw_db
__DIAB_wr_pk_ld
__DIAB_wr_pk_fl
__DIAB_wr_pk_db
__DIAB_rd_sw_ld
__DIAB_rd_sw_fl
__DIAB_rd_sw_db
__DIAB_rd_pk_ld
__DIAB_rd_pk_fl
__DIAB_rd_pk_db
__AddDebugItem
__9type_infoPCc
__9exception
__9CSyncLock
__8bad_cast
__6CError
__5CList
__17__class_type_infoPCcPCQ217__class_type_info9base_infoUl
__16__user_type_infoPCc
__16CdspRootDataPortUs
__15CdspRootManager
__15CdspRootEncoderUsUs
__15CdspRootDecoderUsUs
__14__si_type_infoPCcRC16__user_type_info
__13bad_exception
__11CdspEncoder
__11CdspDecoder
__10bad_typeid
__10CSyncEvent
__10CMutexList
_WriteUserLog
_WriteTFTPData
_WriteSmsLog
_WriteRamFsData
_WritePBRecord
_WritePBEntry
_WriteOutgoingCallsLogAll
_WriteOutgoingCallsLog
_WriteOutboxSMSLog
_WriteMissingCallsLogAll
_WriteMissingCallsLog
_WriteMMIPara
_WriteLocalLog
_WriteIncomingCallsLogAll
_WriteIncomingCallsLog
_WriteInboxSMSLog
_WriteDraftboxSMSLog
_WriteCallLog
_WriteAllCallLog
_WaitCall
_VMuteSwitch
_VMuteOnSelectChannel
_VMuteOffSelectChannel
_VHeadVolumeSet
_VHeadDSPSwitch
_VHandsetDSPSwitch
_VHandSetVolumeSet
_TlsSetLabelIcon
_TlSwitchNameOnlyByNum
_TlSwitchNameByNum
_TlStrCatWordWithSuffix
_TlStopAnimation
_TlStartAnimation
_TlSetupSpeakerVolume
_TlSetTextAttr
_TlSetSysRTC
_TlSetRTC
_TlSetLittleTxtByBuf
_TlSetLabelTxtByBuf
_TlSetLabelTxt
_TlSetEditTxtByBuf
_TlSetDateTxtByBuf
_TlResetTimer
_TlRTCAlarm2RTC
_TlIsRTCValid
_TlIsMsgboxShow
_TlInitAnimation
_TlHisOut
_TlGetWeekFromRTC
_TlGetTimeFromRTCSecond
_TlGetTimeFromRTC
_TlGetSysRTC
_TlGetLittleIconByAscii
_TlGetDateIconByAscii
_TlGetDateFromRTC
_TlGetCloseMinuteOffset
_TlEnableWarning
_TlEnableSpeaker
_TlEnableMic
_TlDisableEvent
_TlContinueBattAni
_TlContinueAnimation
_TlClearRTC
_TlCalcCntedTime
_TestHardIcon
_TemporalPageInit
_TIMuteMic
_TGetPSID
_SysVolumeStates
_SysVolumeObjIDs
_SysVolumeNumProc
_SysVolumeNumInit
_SysVolumeEntry
_SysVolumeBarProc
_SysVolumeBarInit
_SysVolume2TFCntedTimeCn
_SysVolume2TFCntedCn
_SysVolume2IPCntedTimeCn
_SysVolume2IPCntedCn
_SysVolume2ConnectedCn
_SysVolume2CntedTimeCn
_SysVolume2CWCntedTimeCn
_SysVolume2CWCntedCn
_SysVolume23WMixTimeCn
_SysVolume23WMixCn
_SysVolume23WCntedTimeCn
_SysVolume23WCntedCn
_SysUpdateFieldTestInfo
_SysUpdateBatteryInfo
_SysUpdFldTestInfoIncall
_SysTravelCallOut
_SysTransferProceedingStates
_SysTransferProceedingObjIDs
_SysTransferProceedingEntry
_SysTransferPrcdingPMCn
_SysTransferPrcding2TFDisPMCn
_SysTransferPrcding2TFDisMsgCn
_SysTransferPrcding2TFCntedMsgCn
_SysTransferPrcding2DisPMCn
_SysTransferPrcding2DisMsgCn
_SysTransferPrcding2CntedMsgCn
_SysTransferNumEditInit
_SysTransferNameLabelInit
_SysTransferEditStates
_SysTransferEditObjIDs
_SysTransferEditExit
_SysTransferEditEntry
_SysTransferEdit2TFPrcdingCn
_SysTransferEdit2TFCntingCn
_SysTransferEdit2DisPMCn
_SysTransferEdit2CntedCn
_SysTransferEdit2CWInPMCn
_SysTransferDisStates
_SysTransferDisExit
_SysTransferDisEntry
_SysTransferDis2DisPMCn
_SysTransferDis2CntedCn
_SysTransferCntingStates
_SysTransferCntingPMCn
_SysTransferCntingExit
_SysTransferCntingEntry
_SysTransferCnting2TFDisPMCn
_SysTransferCnting2TFDisCn
_SysTransferCnting2TFCntedPMCn
_SysTransferCnting2Overtime
_SysTransferCnting2DisPMCn
_SysTransferCnting2CntedMsgCn
_SysTransferCntedStates
_SysTransferCntedEntry
_SysTransferCnted2TFDisPMCn
_SysTransferCnted2TFDisCn
_SysTransfer2StandbyCn
_SysTrackLabelDraw
_SysTopCtrlLabelProc
_SysTemporalPageCn
_SysSwitchHoldStatus
_SysSubXXDis2Dis
_SysSubXXCnting2XXDis
_SysSubXXCnted2XXDis
_SysSubXCnted2Dis
_SysSubDisReturn
_SysStopCallNotice
_SysStartStates
_SysStartIPCall
_SysStartBatteryAn
_SysStartBackLight
_SysStart2PowerOnCn
_SysStandbyStates
_SysStandbyFp2StandbyCn
_SysStandbyDialogObj
_SysStandby2StandbyCn
_SysStandByExit
_SysStandByEntry
_SysSmsFullAni
_SysShowSmsIcon
_SysShowSWVersion
_SysShowRSSIValue
_SysShowRSSIVal
_SysShowIsRegister
_SysShowHardIcon
_SysShowHandOver
_SysShowFieldTestInfo
_SysShowFERVal
_SysShowCallNumber
_SysShowCallNameLabel
_SysShowCSID
_SysShowBatteryValue
_SysShowBattery
_SysSetVibration
_SysSetStatus
_SysSetState
_SysSetSignal
_SysSetRing
_SysSetRTCAlarmByRTC
_SysSetRTCAlarm
_SysSetPubChanged
_SysSetPub
_SysSetPowerKeyUpStatus
_SysSetPhone
_SysSetOpt
_SysSetNumField
_SysSetNum
_SysSetNameOnlyByNum
_SysSetNameByNum
_SysSetLongLock
_SysSetLazyPlayedCnt
_SysSetKeyLock
_SysSetIconStatus
_SysSetIconLabel
_SysSetCurCall
_SysSetCreatedIconStatus
_SysSetCallOpt
_SysSetBiosAlarm
_SysSetBatteryStatus
_SysSetBatteryLowCnt
_SysSetBattery
_SysSetBackLightOnOff
_SysSetBackLightNum
_SysSetBackLightCnt
_SysSetBackLight
_SysSetBackCallOpt
_SysSetAlarm
_SysSet12Key
_SysSendSMS
_SysSendHoldingkey
_SysSaveNum
_SysSaveMultiCallNum
_SysSaveConnectedNum
_SysReturn2Idle
_SysResetIconStatus
_SysRejectIncCall
_SysRedialWaitingInterval
_SysRedialTmProc
_SysRedialTmInit
_SysRedialStates
_SysRedialObjIDs
_SysRedialExit
_SysRedialEntry
_SysRedial2StandbyCn
_SysRedial2DisCn
_SysRedial2CntingCn
_SysReadIPInfo
_SysPubProc
_SysPoweroffStates
_SysPoweroffObjIDs
_SysPoweroffAnLabelProc
_SysPoweroffAnLabelInit
_SysPowerOnStates
_SysPowerOffEntry
_SysPlaySMSNotice
_SysPlayCallNotice
_SysPages
_SysPBListStates
_SysPBListObjIDs
_SysPBListInit
_SysPBList2TFCntedCn
_SysPBList2PBItemCn
_SysPBList2IPCntedCn
_SysPBList2ConnectedCn
_SysPBList2CWCntedCn
_SysPBList23WMixCn
_SysPBList23WCntedCn
_SysPBItemStates
_SysPBItemSoftkeyInit
_SysPBItemObjIDs
_SysPBItem2PBListCn
_SysOptMenuCreate
_SysNotStandbyDialogObj
_SysLoopTimerProc
_SysIsValidAlarm
_SysIsPoweringState
_SysIsLogin
_SysIsLimitedCallNum
_SysIsFieldTestMode
_SysIsExtCall
_SysIpCanHold
_SysInitVmailIcon
_SysInitIncCallNumInfo
_SysInitIconConst
_SysInitCallTime
_SysInitCallNumInfo
_SysInitBackLight
_SysInitAlarmInfo
_SysInitAPModules
_SysInfoInit
_SysInfo
_SysIncreaseMissedCallNum
_SysIncreaseBatteryLowCnt
_SysIncrease12Key
_SysIncomingCallStates
_SysIncomingCallObjIDs
_SysIncomingCallExit
_SysIncomingCallEntry
_SysIncomingCallEditInit
_SysIncomingCall2StandbyTMCn
_SysIncomingCall2FlipCn
_SysIncomingCall2DiscCn
_SysIncomingCall2CntedCn
_SysIncoming2StandbyPMCn
_SysIncomCallNameLabelIni
_SysIncomCall2StandbyCn
_SysInCallFlip2StandbyCn
_SysIPTalkingExit
_SysIPConnectedStates
_SysIPConnectedObjIDs
_SysIPCntedEntry
_SysIPCallOut
_SysHoldMsgHandle
_SysHideOptMenu
_SysHaveNoObjIDs
_SysGetStatus
_SysGetSignal
_SysGetSMS
_SysGetRing
_SysGetRTCAlarm
_SysGetPubChanged
_SysGetPub
_SysGetPowerKeyUpStatus
_SysGetPhone
_SysGetNumPtr
_SysGetNumField
_SysGetNewSMS
_SysGetMissedCallNum
_SysGetLongLock
_SysGetLazyPlayedCnt
_SysGetKeyLock
_SysGetIconStatus
_SysGetIPKeyParty
_SysGetIPInfo
_SysGetIPCodeCur
_SysGetFreeCallInfoIdx
_SysGetExtParty
_SysGetEntityDialog
_SysGetDialogMenu
_SysGetCallType
_SysGetCallLineNum
_SysGetCallInfoByIdx
_SysGetCallInfo
_SysGetCallIdxByLineNum
_SysGetCallCount
_SysGetCallByLineNum
_SysGetBatteryStatus
_SysGetBatteryLowCnt
_SysGetBatteryByPMMsg
_SysGetBatteryAverage
_SysGetBatteryAnimation
_SysGetBattery
_SysGetBackLightNum
_SysGetBackLightCnt
_SysGetBackCallLineNum
_SysGetBackCallInfo
_SysGetAverageBattery
_SysGetAnimation
_SysGetAlarm
_SysGet12Key
_SysFreeIPBuf
_SysFlipCloseToIdle
_SysFixIPInfo
_SysEventPreProc
_SysEraseHardIcon
_SysDropList_NeedData
_SysDropListInit
_SysDrawIcons
_SysDisplaySucMsg
_SysDisplayOptMenu
_SysDisplayFailMsg
_SysDisconnectedLableInit
_SysDisconnectStates
_SysDisconnectObjIDs
_SysDisconnectExit
_SysDisconnectEntry
_SysDisc2IdleCn
_SysDisableLazyMode
_SysDialEditInit
_SysDetectBatteryStatus
_SysDelIPCallLastChar
_SysCtrlObjs
_SysCreatePBItem
_SysConnectingStates
_SysConnectingF2StandbyCn
_SysConnectingExit
_SysConnectingEntry1
_SysConnectingEntry
_SysConnectingEditInit
_SysConnecting2StandbyCn
_SysConnecting2Redial
_SysConnecting2Overtime
_SysConnecting2DiscPMCn
_SysConnecting2DiscMsgBoxCn
_SysConnecting2DiscCn
_SysConnecting2Cnting
_SysConnectedTimeUpdate
_SysConnectedStates
_SysConnectedPMCn
_SysConnectedObjIDs
_SysConnectedMsgBoxCn
_SysConnectedFp2StandbyCn
_SysConnectedEntry
_SysConnectedEditProc
_SysConnectedEditInit
_SysConnectedAnLabelProc
_SysConnectedAnLabelInit
_SysConnected2VolumeCn
_SysConnected2StandbyCn
_SysConnected2PBListCn
_SysConnected2DiscPMCn
_SysConnected2DiscCn
_SysConnected2CWInPMCn
_SysConnected23WEditPMCn
_SysConnected12EditInit
_SysConnectAnLabelProc
_SysConnectAnLabelInit
_SysConncetingObjIDs
_SysCntingNameLabelInit
_SysCntingHandlePM
_SysCnting2ConnectedCn
_SysCntedTimeLabelUpdate
_SysCntedTimeLabelProc
_SysCntedTimeLabelInit
_SysCntedNameLabelInit
_SysCntedMenu2TFPrcdingCn
_SysCntedMenu2TFEditCn
_SysCntedMenu2CntedCn
_SysCntedMenu23WEditCn
_SysCntedIconLabelInit
_SysCntedEditKeypadProc
_SysClearMissedCall
_SysClearExtInfo
_SysCheckE
_SysCancelSMS
_SysCan12Key
_SysCallWaitingIncomingStates
_SysCallWaitingIncomingObjIDs
_SysCallWaitingIncomingExit
_SysCallWaitingIncomingEntry
_SysCallWaitingDisStates
_SysCallWaitingDisObjIDs
_SysCallWaitingDisExit
_SysCallWaitingDisEntry
_SysCallWaitingCntedStates
_SysCallWaitingCntedObjIDs
_SysCallWaitingCntedEntry
_SysCallWaiting2StandbyCn
_SysCallWaitIn2CntedTMCn
_SysCallWaitIn2CntedPMCn
_SysCallWaitIn2CWDisPMCn
_SysCallWaitIn2CWDisCn
_SysCallWaitIn2CWCntedPMCn
_SysCallWaitIn2CWCntedCn
_SysCallWaitDisPMCn
_SysCallWaitDis2IncomingCn
_SysCallWaitDis2DisPMCn
_SysCallWaitDis2CntedCn
_SysCallWaitCnted2CWDisPMCn
_SysCallWaitCnted2CWDisCn
_SysCallOutGroup
_SysCallOut
_SysCallInfo2CallLog
_SysBuildIconObjs
_SysBatteryTimerProc
_SysBatteryRSSILoopProc
_SysBatteryLabelProc
_SysBatteryAnalogProc
_SysAutoPowerOffProc
_SysAppendChar2Edit
_SysAntnaMsgboxRsltProc
_SysAntennaPMProc
_SysAntennaLabelProc
_SysAntennaIPCntedProc
_SysAntAlarmCreatePro
_SysAllCntedTmLabelProc
_SysAllCntedTmLabelInit
_SysAll2PowerOffCn
_SysAll2IncomingCallCn
_SysAPInit
_Sys3WayMixStates
_Sys3WayMixEntry
_Sys3WayMix2DisCn
_Sys3WayMix23WDropCn
_Sys3WayMix23WDisPMCn
_Sys3WayEditStates
_Sys3WayEditObjIDs
_Sys3WayEditEntry
_Sys3WayEdit2DisPMCn
_Sys3WayEdit2CntedCn
_Sys3WayEdit2CWInPMCn
_Sys3WayEdit23WCntingCn
_Sys3WayDropStates
_Sys3WayDropObjIDs
_Sys3WayDropEntry
_Sys3WayDrop2MixCn
_Sys3WayDrop2CntedCn
_Sys3WayDrop23WayDisPMCn
_Sys3WayDisStates
_Sys3WayDisPMCn
_Sys3WayDisExit
_Sys3WayDisEntry
_Sys3WayDis2DisPMCn
_Sys3WayDis2CntingCn
_Sys3WayDis2CntedCn
_Sys3WayCntingStates
_Sys3WayCntingExit
_Sys3WayCntingEntry
_Sys3WayCnting2CWInPMCn
_Sys3WayCnting23WDisPMCn
_Sys3WayCnting23WDisCn
_Sys3WayCnting23WCntedPMCn
_Sys3WayCntedStates
_Sys3WayCntedEntry
_Sys3WayCnted23WMixPMCn
_Sys3WayCnted23WDisPMCn
_Sys3WayCnted23WDisCn
_Sys3Way2StandbyCn
_SwitchTimer
_SwitchStatus
_StrCmp4Bytes
_StopWarning
_StopTone
_StopMelody
_StopAlarm
_StandbySaverResetCn
_Standby2SpdSttCn
_Standby2ProCn
_Standby2PhoneBookCn
_Standby2PBSearchCn
_Standby2OutGoingCallCn
_Standby2NetSearchCn
_Standby2MissedCallCn
_Standby2MainMenuCn
_Standby2KeyLockCn
_Standby2IncomedCallCn
_Standby2IdleVibrationST
_Standby2IdleVibrationCn
_Standby2IdleDialCn
_Spd2OthersPreCn
_Spd2Others6Cn
_Spd2Others5Cn
_Spd2Others4Cn
_Spd2Others3Cn
_Spd2Others2Cn
_Spd2Others1Cn
_Spd2IdleCn
_SoftKeys
_ShowIdleNoSignScreen
_Setdelay
_SetTotalCallTime
_SetTimeDisplayMode
_SetStandbyMenu
_SetSpeedDialIndex
_SetSpeakerVolume
_SetSaverTime
_SetSaverStyle
_SetSaverOnoff
_SetSaver
_SetRtc
_SetRTC
_SetProfileWarningTone
_SetProfileSMSTone
_SetProfileRingVolume
_SetProfileRingTone
_SetProfileRingMode
_SetProfileMode
_SetProfileMemoTone
_SetProfileLightTalk
_SetProfileKeyTone
_SetProfileAlarmTone
_SetPassword
_SetPBGroupMelody
_SetOwnNumber
_SetOpenPasswordProt
_SetNoNetworkNumber
_SetNoAnswerNumber
_SetNewSerRegInputNum
_SetNewSerCanInputNum
_SetLongCallLock
_SetLcdContrast
_SetLastInputMethod
_SetLanguage
_SetIsEnterNetSearchFromIdle
_SetIfIdleToVibration
_SetIdlepic
_SetIdleStaticText
_SetIdleStaticIconId
_SetIdleMode
_SetIdleIconId
_SetIdleDefaultMode
_SetIdleChangedText
_SetIP
_SetHighMicGain
_SetGreeting
_SetGameInfo
_SetDataOn
_SetCursorOn
_SetCursorOff
_SetCursor
_SetContrastMode
_SetCallAnswerMode
_SetBusyNumber
_SetBackLightMode
_SetBIOSAlarm
_SetAuthentKey
_SetAnimate
_SetAllNumber
_SetAllCallTime
_SetAlarmOn
_SetAlarmClockMode
_SetAlarm
_SearchNet2StandbyTr
_SaveQ9StrokeToFlash
_SaveQ9PinYinToFlash
_SaveQ9EnglishToFlash
_SavePinYinToFlash
_SaveLastSms
_SaveEnglishToFlash
_ReverseBlock
_RestoreBlock
_ResetAlarmReg
_ResWriteFlash
_RefreshTime
_RefreshLCD2
_RefreshLCD
_Recover_User_Data
_RecoverCheckDesign
_RecUint16
_ReadSmsLog
_ReadPBEntryEx
_ReadPBEntry
_ReadOutgoingCallsLogAll
_ReadOutgoingCallsLog
_ReadMissingCallsLogAll
_ReadMissingCallsLog
_ReadIncomingCallsLogAll
_ReadIncomingCallsLog
_Randseed
_PowerOff2SearchNetCn
_PowerOff2PassInputCn
_PowerOff
_PostEventMMI2PM
_PlayWarning
_PlayTone
_PlaySuccessBeep
_PlayPowerMelody
_PlayMelody
_PlayKeyMelody
_PlayErrorBeep
_PlayContinuedKeyTone
_PlayAlarm
_PhoneIdleInit
_PassInputEditProc
_PassInputEditInit
_PassInput2Timer
_PassInput2SearchNetCn
_PMMDownloadPhase
_OutStr
_OutSmallStr
_OutPrlInfo
_OutLcdSmallChnChar
_OutLcdSmallChar
_OutLcdRowLine
_OutLcdRec
_OutLcdDotj22
_OutLcdDot
_OutLcdColumnLine
_OutLcdChnChar
_OutLcdChar
_OutLcdByte
_OutLcdAdd
_OutHardIcon
_NullTextAttrs
_NullAlgorithmTest
_NormalMixDialogObj
_NormalDialogObj
_NATPTownInputIPv4
_Msgbox
_MainMenu2WFSettingCn
_MainMenu2ToolsCn
_MainMenu2StandbyCn
_MainMenu2SettingCn
_MainMenu2RegisterCn
_MainMenu2ProfileCn
_MainMenu2PbCn
_MainMenu2NetWorkService
_MainMenu2Misc
_MICSWHandset
_MICSWEarphone
_Load_MMI_Tbl
_Lists
_Labels
_LabelStandbyPhotoProc
_LabelStandbyPhotoInit
_LabelPubProc
_LabelKeyLockProc
_LabelKeyLockInit
_IsSMSNumValid
_IsFldTstMd
_IsDialNumValid
_IsBatteryCharging
_InitSysFonts
_InitHardIcon
_InitBaseAlarmRtc
_IdleWeekLabelProc
_IdleWeekLabelInit
_IdleUpdateLowBattery
_IdleTimeLabelProc
_IdleTimeLabelInit
_IdleTemporalPageCn
_IdleTelOperatorLabInit
_IdleStandbyStates
_IdleStandbyObjIDs
_IdleSpeedStates
_IdleSpeedObjIDs
_IdleSpeedExit
_IdleSpeedEntry
_IdleSetPBList
_IdleSetMainMenuSelect
_IdleSetElement
_IdleSearchNetStates
_IdleSearchNetObjIDs
_IdleSearchNetExit
_IdleSearchNetEntry
_IdleSearchNet2StandByCn
_IdleScreenSaverStates
_IdleScreenSaverObjIDs
_IdleSaverLabelInit
_IdleSaverExit
_IdleSaverEntry
_IdlePoweroffExit
_IdlePowerOffStates
_IdlePassInputStates
_IdlePassInputObjIDs
_IdlePassInputExit
_IdlePassInputEntry
_IdlePages
_IdleMyPHSLabelInit
_IdleMissedNumLabelInit
_IdleMissedCallLabelInit
_IdleMissObjIDs
_IdleMiss
_IdleMemoComingProc
_IdleMainmenuExit
_IdleMainmenuEntry
_IdleMainMenuStates
_IdleMainMenuObjIDs
_IdleLowBatteryLabelProc
_IdleLockIdlePageCn
_IdleKeyLockedStates
_IdleKeyLockedObjIDs
_IdleKeyLockedEntry
_IdleIsInPassWord
_IdleInfo
_IdleHavePassWord
_IdleGetPassWord
_IdleGetMainMenuSelect
_IdleGetElement
_IdleGetAnimation
_IdleDialStates
_IdleDialSet1Num
_IdleDialObjIDs
_IdleDialEditProc
_IdleDialEditInit
_IdleDial2StandbyCn
_IdleDial2Save2PBCn
_IdleDial2ConnectingCn
_IdleDateLabelProc
_IdleDateLabelInit
_IdleAlarmTimeLabelInit
_IdleAlarmStates
_IdleAlarmObjIDs
_IdleAlarmExit
_IdleAlarmEntry
_IdleAlarmDateLabelInit
_IdelLeftSoftInit
_HeadsetIntEnable
_HeadsetIntDisable
_HasPrmtrInit
_GrayBlock
_GetUserLog
_GetTimeDisplayMode
_GetTFTPData
_GetStr
_GetStandbyMenu
_GetSpeedDialIndex
_GetSpeakerVolume
_GetSaverTime
_GetSaverStyle
_GetSaverOnoff
_GetSaver
_GetSWVersion
_GetRtc
_GetRamFsData
_GetRTC
_GetQ9StrokeFromFlash
_GetQ9PinYinFromFlash
_GetQ9EnglishFromFlash
_GetProfileWarningTone
_GetProfileVibActiv
_GetProfileSMSTone
_GetProfileRingVolume
_GetProfileRingTone
_GetProfileRingMode
_GetProfileMode
_GetProfileMemoTone
_GetProfileLightTalk
_GetProfileKeyTone
_GetProfileIsMute
_GetProfileAlarmTone
_GetPinYinFromFlash
_GetPassword
_GetPageOff
_GetPSID
_GetPM2MMIVMailReceive
_GetPM2MMIUnHoldRes
_GetPM2MMIUnHoldInc
_GetPM2MMITransferRes
_GetPM2MMITransferLineNumRes
_GetPM2MMITimeStart
_GetPM2MMISynSuccess
_GetPM2MMISynFailure
_GetPM2MMIRgstStart
_GetPM2MMIRgstOk
_GetPM2MMIRgstFailure
_GetPM2MMIReplaceReceived
_GetPM2MMIReferReceived
_GetPM2MMIRSSIByRSSI
_GetPM2MMIRSSI
_GetPM2MMIProgress
_GetPM2MMINetServiceResponse
_GetPM2MMINetSearchResponse
_GetPM2MMIMsg
_GetPM2MMIInitEnd
_GetPM2MMIInitCall
_GetPM2MMIIncomingCall
_GetPM2MMIHoldRes
_GetPM2MMIHoldInc
_GetPM2MMIHandOverStart
_GetPM2MMIHandOverEnd
_GetPM2MMIEPROMCtrl
_GetPM2MMIDisconnect
_GetPM2MMIDataReqNum
_GetPM2MMIDataQuitType
_GetPM2MMIDataMsgType
_GetPM2MMICode
_GetPM2MMICntingSSID
_GetPM2MMICntingFail
_GetPM2MMICancelHold
_GetPM2MMICallFailure
_GetPM2MMIBtryMeasure
_GetPM2MMIBattFromRSSI
_GetPM2MMIAlert
_GetPM2MMI183
_GetPM2MMI12
_GetPCDebugFlag
_GetPBRecord
_GetPBGroupMelody
_GetOwnNumber
_GetOutboxSMSLog
_GetOperatorIndex
_GetOpenPasswordProt
_GetObj
_GetNoNetworkNumber
_GetNoAnswerNumber
_GetNewSerStr
_GetNewSerRegInputNum
_GetNewSerRegAccessNum
_GetNewSerEnable
_GetNewSerCanInputNum
_GetNewSerCanAccessNum
_GetMelodyName
_GetMMIPara
_GetLongCallLock
_GetLocalLog
_GetLastSms
_GetLastInputMethod
_GetLanguage
_GetKeyValue
_GetIsEnterNetSearchFromIdle
_GetInboxSMSLog
_GetIfIdleToVibration
_GetIdletxt
_GetIdlepic
_GetIdleStaticText
_GetIdleStaticIconId
_GetIdleMode
_GetIdleIconId
_GetIdleDefaultMode
_GetIdleChangedText
_GetIP
_GetGreeting
_GetGameInfo
_GetFlipState
_GetFieldBuf
_GetEnglishFromFlash
_GetEncode
_GetEditType
_GetEarphoneState
_GetDraftboxSMSLog
_GetDialSize
_GetCurState
_GetContrastMode
_GetCancelNumber
_GetCallLog
_GetCallAnswerMode
_GetBusyNumber
_GetBattVoltage
_GetBackLightMode
_GetBIOSAlarm
_GetAuthentKey
_GetAnimate
_GetAllNumber
_GetAllCallTime
_GetAllCallLog
_GetAlarmSwitch
_GetAlarmRTC
_GetAlarmClockMode
_GetAlarm
_GetAccessNumber
_GLOBAL_$I$dns_failed
_EraseAllFlashDataSection
_EnableVibration
_EnableKeyLED
_EnableBackLight
_Edits
_EditSearchNetProc
_EditSearchNetInit
_DrawIcon
_DelSmsLog
_DelPBEntry
_DelOutgoingCallsLog
_DelMissingCallsLog
_DelIncomingCallsLog
_DelAllSmsLog
_DelAllSMS
_DelAllPBEntry
_DelAllCallsLog
_DataConnectingEditInit
_CompareOutcallNumber
_ClrUsrDataArea
_ClrBackupArea
_ClearLcd
_ClearHeadsetInt
_ClearHardIcon
_ClearBlock
_Clarinet_MD5Update
_Clarinet_MD5Transform
_Clarinet_MD5Pad
_Clarinet_MD5Init
_Clarinet_MD5Final
_Check_User_Data
_Check_MMI_Tbl
_CallRecHead
_BuildUnMuteCall
_BuildUnHoldBackCall
_BuildUnHold
_BuildTransferResume
_BuildTransferCall
_BuildToIdle
_BuildState
_BuildSpeedMenu
_BuildSoftKeyObj
_BuildSMSSend
_BuildResponse
_BuildPowerOff
_BuildPageStates
_BuildObjs
_BuildNewCall
_BuildMuteCall
_BuildMsgboxObj
_BuildMode
_BuildMainMenu
_BuildListObj
_BuildLabelObj
_BuildHoldBackCall
_BuildHold
_BuildEndLine
_BuildEndBackCall
_BuildEndAll2Standby
_BuildEndAll2Dis
_BuildEndALL
_BuildEnd
_BuildEditObj
_BuildDialog
_BuildCallWaitSwitch
_BuildCallWaitAnswer
_BuildCall
_BuildBarObj
_Build3WaySwitch
_Build3WayMix
_Build12
_Bars
_Backup_User_Data
_BackUpBlock
_ApInitObj
_AntennaVMailReceive
_AntennaRgstTimer
_AntennaRgstStart
_AntennaRgstOk
_AntennaRgstFailure
_AntennaRSSI
_AntennaPlayShowSignal
_AntennaNetServiceInfo
_AntennaNetSearchInfo
_AntennaHandOverStart
_AntennaHandOverEnd
_AntennaDisconnect
_AntennaCntingSSID
_AntennaCntingFail
_AntennaCCHOK
_AntennaCCHFailure
_AntennaBatterySize
_AntennaBattChkVoltage
_AntennaBattCheckLight
_AntennaBattCheckAlarm
_ATEWriteFlash
_ANALOGPrcsChrg_SM
_ANALOGPrcsChrg
_6CError$TheErrorObject
_15CdspRootManager$coderPortCapabilities
_15CdspRootManager$_the_manager
_11CdspManager$_the_root_manager
_11CdspManager$_the_manager
_$_9type_info
_$_9exception
_$_9bad_alloc
_$_9CSyncLock
_$_8bad_cast
_$_6CError
_$_5CList
_$_17__class_type_info
_$_16__user_type_info
_$_14__si_type_info
_$_13bad_exception
_$_11CdspEncoder
_$_11CdspDecoder
_$_10bad_typeid
_$_10CSyncEvent
_$_10CMutexList
ZiDAWGGetSibling
ZiDAWGGetGraphInfo
ZiDAWGGetGraph
ZiDAWGGetChild
ZiDAWGGetAttribute
ZiCode2DisplayCode
Zi8getKeyLayout
Zi8WCharCount
Zi8UnicodeToGB
Zi8UnicodeToBig5
Zi8Uni2Ord
Zi8SimpToComplex
Zi8SetUWDsearchOption
Zi8SetPredictionStartAt
Zi8SetMaxWordLength
Zi8SetMaxNamesInUse
Zi8SetMaxCountValue
Zi8SetLatinSearchOrder
Zi8SetHighlightedWordW
Zi8SetCandidateBufferSize
Zi8SecMatchComp
Zi8SecMatchChar
Zi8RefUDWordW2
Zi8RefUDWordW
Zi8Punctuation
Zi8PunctTable
Zi8PriMatchNextComp
Zi8PriMatchNextChar
Zi8PrepareMatch
Zi8Ord2Uni
Zi8Ord2Ord
Zi8Memset
Zi8Memcpy
Zi8MatchWord
Zi8MatchUWDdata
Zi8MatchROMdata0
Zi8MatchROMdata
Zi8MatchPhonetic
Zi8MatchPUDdata
Zi8MatchOEMdata
Zi8MatchAltSound
Zi8MTgetKeyLayout
Zi8MTgetCount4KeyLayout
Zi8LangSupported
Zi8IsWordW2
Zi8IsWordW
Zi8IsVITone
Zi8IsUDWordW
Zi8IsMatchB
Zi8IsMatch2
Zi8IsMatch1Key
Zi8IsMatch
Zi8IsElement
Zi8IsDupWordW
Zi8IsDupWord
Zi8IsComponent
Zi8IsCharacter
Zi8InitializeDynamic
Zi8InitDupWordBuf
Zi8GetZInfo
Zi8GetZHuwdPtr
Zi8GetVisciiCombined
Zi8GetTableVersion
Zi8GetTableSize
Zi8GetTableCount
Zi8GetTableAddress
Zi8GetPyPhonetic
Zi8GetPyFinal
Zi8GetPUDfreeSpace
Zi8GetPInfo
Zi8GetPCode
Zi8GetMaxCountValue
Zi8GetLastError
Zi8GetKey2UnicodeTable
Zi8GetIntAlphaWordW
Zi8GetIntAlphaWord
Zi8GetGlobalDataSize
Zi8GetFormatVersion
Zi8GetChineseCandidates
Zi8GetCharInfo3
Zi8GetCharInfo2
Zi8GetCharInfo
Zi8GetCandidatesOrCount
Zi8GetCandidates
Zi8GetBpmfPhonetic
Zi8GetAlphaWordW
Zi8GetAlphaWord
Zi8GetActiveUWDid
Zi8Get1KeyPressSpelling
Zi8Get1KeyPressCandidates
Zi8GBToUnicode
Zi8ExactMatchNextChar
Zi8DetachUWD_ZH
Zi8DetachUWD
Zi8DetachPUD
Zi8DetachOEMdata
Zi8DeleteUDWordW
Zi8CopyWordListW
Zi8CopyWordList
Zi8CopyW
Zi8Copy
Zi8ConvertWC2UC
Zi8ConvertWC2Key
Zi8ConvertUC2WC
Zi8ConvertUC2Key
Zi8ConvertLigature2Chars
Zi8ConvertChars2Ligature
Zi8ComplexToSimp
Zi8Big5ToUnicode
Zi8AttachUWD_ZH
Zi8AttachUWD
Zi8AttachPUD
Zi8AttachOEMdata
Zi8AlphaGetCandidates
Zi8AddUsedWordW_ZH
Zi8AddUsedWordW2
Zi8AddUsedWordW
Zi8AddUsedKanji
Zi8AddUDWordW
ZeroSipCoreParam
XFER_ReferReceived
XFERLineNumNtfy
WritePBEntryEx
WriteMemEx
WriteMem
WriteMWIIndication
WriteFlashSucFlag
WriteFlashErrFlag
WriteAutoScanStatus
Write3WayCallFlag
Wifi_Strength_timer
WiFiConn
WhichStringIsMoreSimillar
WfconfigInit
WfconfigFieldSaveCallBack
Wait__10CSyncEvent
WaitUntilReady__15CdspRootManageri
WaitForZero
WaitForSignal
WaitForAvailbeAPs__Fv
WaitEvent
WSSaveFs2Flash
WPATaskId
WMB_COMPONENT_Stop
WMB_COMPONENT_Start
WLWdsPortEnable
WLWdsPortDisable
WLWakeOnLANSet
WLWakeOnLANGet
WLWPAModeSet
WLWPAAuthKeyMgmtSuiteSet
WLWMEStatusGet
WLWMENoAckEnabledSet
WLWMENoAckEnabledGet
WLWMEEnabledSet
WLWMEEnabledGet
WLWDSAddrSet
WLWDSAddrGet
WLVoiceRetryLimitSet
WLVoiceRetryLimitGet
WLVoiceContentionWindowSet
WLVoiceContentionWindowGet
WLVersion
WLUnsolicitedMsgWpaRtnSet
WLUnsolicitedMsgDot1xRtnSet
WLUnblock
WLTickTimeSet
WLTickTimeGet
WLTempTypeGet
WLTalliesGet
WLTXRateControlSet
WLTXRateControlPortSet
WLTXRateControlPortGet
WLTXRateControlGet
WLTXKeyIdSet
WLTXKeyIdGet
WLSystemScaleSet
WLSystemScaleGet
WLSupportedDataRatesBufferGet
WLSpecialVoiceSet
WLSpecialVoiceGet
WLShortRetryLimitGet
WLScanSSIDSet
WLScanSSIDGet
WLScanChannels2GhzSet
WLScan
WLScaleThresholdGet
WLReset
WLRejectAnySet
WLRejectAnyGet
WLRecvWdsRtnSet
WLRadioStatusSet
WLRTSThresholdSet
WLRTSThresholdPortSet
WLRTSThresholdPortGet
WLRTSThresholdGet
WLProtocolRspTimeGet
WLPromiscuousModeSet
WLPromiscuousModeGet
WLPrivacyOptionImplementedGet
WLPreBeaconAdjustSet
WLPreBeaconAdjustGet
WLPortTypeSet
WLPortTypeGet
WLPortStatusGet
WLPcfInfoGet
WLPMHoldoverDurationSet
WLPMHoldoverDurationGet
WLPMEnabledSet
WLPMEnabledGet
WLPHYTypeGet
WLOwnSSIDSet
WLOwnSSIDGet
WLOwnNameSet
WLOwnNameGet
WLOwnMACAddressSet
WLOwnMACAddressGet
WLOwnDTIMPeriodSet
WLOwnDTIMPeriodGet
WLOorTimesSet
WLOorTimesGet
WLNICSerialNumberGet
WLNICProfileGet
WLNICMACAddressGet
WLNICIdentityGet
WLMulticastReceiveSet
WLMulticastReceiveGet
WLMulticastRateSet
WLMulticastRateGet
WLMulticastPMBufferingSet
WLMulticastPMBufferingGet
WLModifiedScanSet
WLModifiedScanGet
WLMicrowaveRobustnessSet
WLMicrowaveRobustnessGet
WLMediumDistributionSet
WLMediumDistributionGet
WLMbxNotifyRtnSet
WLMaxTransmitLifetimeGet
WLMaxSleepDurationSet
WLMaxSleepDurationGet
WLMaxReceiveLifetimeGet
WLMaxLoadTimeGet
WLMaxDataLengthSet
WLMaxDataLengthGet
WLLongRetryLimitGet
WLLoadBalancingSet
WLLoadBalancingGet
WLLinkTestRtnSet
WLLinkTest
WLIntraBSSRelaySet
WLIntraBSSRelayGet
WLGroupAddressesSet
WLGroupAddressesGet
WLGroupAddressFilterSet
WLGroupAddressFilterGet
WLFwVersionsGet
WLFWIdentityGet
WLExcludeUnencryptedSet
WLExcludeUnencryptedGet
WLEncryptionEnabledSet
WLEncryptionEnabledGet
WLDynamicPMEnabledSet
WLDynamicPMEnabledGet
WLDownloadBufferGet
WLDisassociateAddressSet
WLDesiredSSIDSet
WLDesiredSSIDGet
WLDefaultKeysSet
WLDeauthenticateAddressSet
WLCurrentUsedRatesGet
WLCurrentTXRatePortGet
WLCurrentTXRateGet
WLCurrentSystemScaleGet
WLCurrentSSIDGet
WLCurrentRemoteRatesGet
WLCurrentPowerStateGet
WLCurrentChannelInfoGet
WLCurrentChannelGet
WLCurrentBeaconIntervalGet
WLCurrentBSSIDGet
WLCreateIBSSSet
WLCreateIBSSGet
WLCommunicationsQualityBufferGet
WLChannelSet
WLChannelInfoSet
WLChannelInfoGet
WLChannelGet
WLCFPollableGet
WLCCAModeGet
WLBlock
WLAuthenticationSet
WLAuthenticationGet
WLAuthenticationAlgorithmGet
WLApplyLight
WLApply
WLATIMWindowSet
WLATIMWindowGet
WLAPModeSet
WLAPModeGet
WLAN_CONFIG
WFsettingmenu_exit
WFconfigIdle2NetSearch
WFconfigGetAutoScanStatus
WFShortcutFlag
WFSettingMenuTable
WFSettingInit
WFSetVADState
WFSetPLCState
WFSetNSState
WFSetGJBMaxConnection
WFSetGJBBufferSize
WFSetCodecPriorityInf
WFSetCNGState
WFSetAECWorkModeState
WFSetAECTailTime
WFSearchNet
WFGetVoiceProcSubInfo
WFGetVoiceProcInfo
WFGetVersion
WFGetVendorName
WFGetVendorInfo
WFGetVADState
WFGetProductCategory
WFGetPLCState
WFGetNSState
WFGetModeName
WFGetGJBMaxConnection
WFGetGJBInfo
WFGetGJBBufferSize
WFGetEnterpriseCode
WFGetCodecPriorityInf
WFGetCNGState
WFGetAECinfo
WFGetAECWorkModeState
WFGetAECTailTime
WFConfigMsgBox
WEPKeySelect
VxQueueDestroy
VxQueueCreate
VxMessageSendQueue
VxMessageReceiveQueue
VoiceProcInf
VoiceMail
VibratorSoundDriver
VertFlipRegion_DID04
VertFlipRegion
VertData
Version
VendorInf
Vendor
ValidAuthMode__Fv
VSpeakerSwitch
VMicSwitch
VALID_String
VALID_Length
VALID_GetStringType
UsingPppoe
UsingDot1x
UsingDhcp
UpdateEeprom
Unlock__9CSyncLock
UnloadSIPStack
UnconvertEntryInfo
UncompressPhoneNumberpb
UncompressPhoneNumber
UncompressNumericDatapb
UncompressNumericData
UnchangeItemAddr
UnRegProcNtfy
UnInitRtpStat
UnCompressBitamp
UdpListenFailNtfy
UTtaskDelay
UTTimeGet
UPString
UPCASE
UILSendDiagMsg
UILPutInfo
UILGetInfo
UILAction
UA_unhold_peer
UA_transfer_peer_resume
UA_transfer_peer
UA_set_video_mode
UA_set_username
UA_set_stun_parameters
UA_set_rtpport_video
UA_set_rtpport_audio
UA_set_registrar_usage
UA_set_registrar_passwd
UA_set_registrar_addr
UA_set_proxy_addr
UA_set_primary_contact
UA_set_outgoing_CallerID_block_mode
UA_set_natuseflag
UA_set_local_packtime
UA_set_local_ipaddr
UA_set_incoming_CallerID_block_mode
UA_set_hostname
UA_set_displayname
UA_set_deviceid
UA_set_codec_video
UA_set_codec_audio
UA_set_callerid_block
UA_set_authen_username
UA_set_SIP_port
UA_set_DSP_Audio
UA_set_DSP2Mute
UA_set_DSP2Audio
UA_reject_peer
UA_register_duration_set
UA_option_peer
UA_message_peer
UA_invite_new_peer
UA_hold_cb
UA_get_video_mode
UA_get_username
UA_get_rtpport_video
UA_get_rtpport_audio
UA_get_registrar_passwd
UA_get_registrar_addr
UA_get_hostname
UA_get_codec_video
UA_get_codec_audio
UA_get_SIP_port
UA_do_unreg
UA_clear_dialog_status
UA_callwaiting_switch
UA_calltransfer_switch
UA_callhold_peer
UA_accept_peer
UA_XFER_with_consult_resume
UA_XFER_with_consult
UA_Refer_peer
UA_Invite_peer
UA_DTMF
UA_DSP_Toggle_Mute
UA_DNS_Enable
UA_Blind_XFER
UA_3_way
TryConnect2AP
Transmit
TranslateNumTops
TranslateNumToPC
TransiteNormalIdle
TransTimetoAsc
TransAlarmToAsc
TranGroupPBEntryToIndex
TranAllPBEntryToIndex
Tra_Open_Sel
Tra_Cancel_Sel
TraOpenTxt
TraCancelTxt
Tool_MainMenu_Entry
ToggleMute
Timer_SecTask
TimerStart
TimerQue
TimerInit
TimerHandler
TimerCreate
TimerCleanUp
TimerCancel
TimeTop
TimeSelRow
Time2Date
Tftp_FlashUp
TftpWriteMagicAndFileSize
TftpTxtParse
TftpTxtIsValid
TftpShowLoctParam
TftpShowDefaultValue
TftpSetRetryTime
TftpSetDefaultValue
TftpRetryRemainder
TftpParamCheck
TftpPMEnabledSet
TftpMmiSetCancel
TftpMmiSetAnswer
TftpGetRetryTime
TftpGetDefaultValue
TftpFlashupReboot
TftpDefaultValueReset
TftpCodeGet
TftpCodeCheck
TftpCleanRetryTimer
TftFlashEraseSector
TextOut_MultiLine
TextOutEx_01
TextOut
TestTableAddr
TcpLogInit__Fv
Task_pscinit_id
Task_pm_id
Task_mmi_id
Task_mmi_getrssi_id
Task_TFTP_Upgrade_ID
Task_TFTP_Main_ID
Task_TFTP_DOWNLOADFILE_ID
Task_Sec_Timer_id
Task_Main_id
Task_Charge_pause_id
TZTable
TSoAndTFTPFlag
TIME_24_Paint
TIME_12_Paint
TGetSvrPort
TGetCurLoctParams
TGetCfgFileName
TFTP_init
TFTP_Send_MMIMsg
TFTP_Main
TFTP_Connecting_Entry
TFTPWriteLog
TFTPUpgradeTask
TFTPUpgradeProc
TFTPUpgrade
TFTPRetry
TFTPResolv
TFTPGetVersion
TFTPFirmwareUpgradeProc
TFTPDownloadFileTask
TFTPDownloadFile
TFTPDhcpSetStatus
TFTPDhcpGetStatus
TFTPDeInit
TFTPCreateTask
TFTPConfigUpgradeProc
TFTPConfigSet
TFTPConfigSave
TFTPConfigGet
TFTP
SyslogUnload
SyslogTaskId
SyslogLoad
SyslogFlg
Sysctl
SysTftpUpdate
SysSetTFTPType
SysSetTFTPFlag1
SysSetTFTPFlag
SysSetRegIntervalTime
SysSetIsFromIdle2NetTFTPFlag
SysSetFwd
SysSendPowerKeyToMmi
SysIsFromIdle2NetTFTPFlag
SysGetTFTPType
SysGetTFTPFlag1
SysGetTFTPFlag
SysEntity
SysCancelOperating
SysCallTransfer
SwitchModePhase
SwitchEntry
StrAttrsDup
StorageStrBuild
Stopfeed_timer
Stop_Vibration
StopVoice
StopTone
StopTaskProcessing__15CdspRootManager
StopSounderPlayTone
StopSMSRing
StopRingTone
StopRing
StopProTimer
StopMemoRing
StopCycleRinger
StopChargeIconTimer
StopBatLow_LcdProc
StopAlarmRing
StateTbl_Init
StateTbl_GetState
StateTbl_Destroy
StateTbl_Create
StateTbl_Append
StateTbl_AddItem
StateTblItem_MatchEvt
StateTblItem_Init
StateTblItem_Destroy
StateTblItem_Create
StateFlag
Startfeed_timer
Start_Vibration
StartVoice
StartDhcpLeaseTimer
StartCharginginMMI
StartChargeinPowerOff
StackUnloadFailed
SpawnTask
SortAudioCodeOrder
SolarMonth
SolarDays
Sleep_State
Sleep
Shutdown__15CdspRootManager
ShortMenu_SetCur
ShortMenu_Paint
ShortMenu_LostFocus
ShortMenu_IndText
ShortMenu_IndPos_S
ShortMenu_IndPos_L
ShortMenu_IconPos
ShortMenu_HandleEvent
ShortMenu_GetFocus
ShortMenu_GetCur
ShortMenu_Destroy
ShortMenu_Deinit
ShortMenu_Create
ShortMenu_AddItem
ShortMenu_Add
SharedSecretResponseMsg
SharedSecretRequestMsg
SharedSecretErrorResponseMsg
Setting_ShortcutSaver
Setting_ShortcutFlag
Setting_SC_Flag2
Setting_SC_Flag1
Setting_IdleDlg
Setting_Fld_Input
Setting_AnimateDlg
SettingSecretMenu_Entry
SettingMenu_Entry
Set__10CSyncEvent
Set_LcdPageAdd
Set_LcdColAdd
Set_LcdAdd
Set_Fld_InputRes
SetWLHoldoverDuration
SetVMBoxPw
SetVMBoxNum
SetVMAccessNum
SetUnloadSIPStackFlag
SetTxCurPacketLate
SetTxCurPacketJitter
SetToolWorldTimeIndex
SetTimeZoneValueByIdx
SetTftpState
SetTFTPWorkMode
SetTFTPServerIP
SetTFTPServerDomain
SetTFTPPort
SetTFTPEncrKey
SetTFTPDirFile
SetSysTxtColor
SetSysPenColor
SetSysLanguage
SetSysFontID
SetSysCharset
SetSysBrushColor
SetSysBkColor
SetSubnetMask
SetStunServerPort
SetStunServerName
SetStringLang
SetSpeakerphone
SetSowrteState
SetSessionRemote
SetSelectParamDefault
SetSSIDAndWepKey
SetSIPUserName
SetSIPSerName
SetSIPRegSerPort
SetSIPRegSerIP
SetSIPRegSerDomain
SetSIPPw
SetSIPProxyPort
SetSIPProxyIP
SetSIPProxyDomain
SetSIPPort
SetSIPObProxy
SetSIPDnsSrv
SetSIPAuthStr
SetSIPAuthAlg
SetRxCurPacketLate
SetRxCurPacketJitter
SetRemoteTftpState
SetRTPSamplesize
SetRTPSamplesCount
SetRTPPort
SetRTPPackTime
SetRTPJitBufComp
SetRFC2833PLTypeValue
SetPixel_DID04
SetPixel
SetPBRecord
SetOutOfService
SetNATWorkMode
SetNATSerPort
SetNATSerIP
SetNATSerDomain
SetNATSTUNMode
SetNATKATime
SetNATKADest
SetNATIP
SetMMIAutoScanFlag
SetLocalLogMode
SetIdleRS2Pb
SetIdleMenu2Pb
SetIdle2NS
SetIPAddress
SetHourFormat
SetGatewayIP
SetFunctionPwm
SetFunctionOutput
SetFunctionIO
SetDhcpType
SetDSPVolume
SetDNSSecServer
SetDNSPriority
SetDNSPriServer
SetDDWakeupMode
SetDDSleepMode
SetDDSState
SetDCTextUnionColor
SetDCTextColor
SetDCPenColor
SetDCMapMode
SetDCFont
SetDCBrushColor
SetDCBkColor
SetCalenTxtByBuf
SetBAP
SetAutoScanFlag
SetAudioSource
SetAudioOutput
SetAudioDestination
SetAllCallTimeWhenPowerOff
SetAllCallTime2Buffer
Sendto
SendRtpTelephEventsPack
SendRssiAndBatMain
SendResponseInfo
SendRSSI
SendPowerKeyToMmi
SendKeyMsg
SendHeadbyByte
SendFrame
SendEventToApp__FUl
SendErrorResponse
SendBattLvl
Send
SelectFontDrvEx_01
Select
Sel_Fld_Cce_Type
SelRow
Secret_exit
SecTimerTickAnnounce
SecTimerStart
SecTimerDelete
SecTimerCreate
SecTimerCancle
SearchTimerOut
SearchNetwork
SearchAP__Fv
Screen_Time_sel
Screen_Backl_sel
Screen_Backl_needdata
ScrSv2BMP_DID04
ScrSv2BMP
Saverpick
Saver_exit_Standby
Saver_SmsComing
Saver_Onoff_NeedData
SaverTime
SaverOnFlag
Save_Fld_Cce_Type
SaveTraOpenNum
SaveTraCancelNum
SaveReceivedLog
SaveOutgoingLog
SaveMissingLog
SaveIphoneNumber
SaveElementBuff
SaveCfgParam
SaveAccessNum
STRTOK_REENTRANT
STRNICMP
STRICMP
STRICHR
SMSNeedPBListData
SIP_port
SIP_match_rtpptype2JB_type
SIP_match_JBcodec2negCodec
SIP_incoming_another_call
SIP_hook_state
SIP_get_hook_state
SIP_5XXforReferNtfy
SIP_4XXforReferNtfy
SIP_202forReferNtfy
SIPTaskInfo
SIPResetWFDrive
SHA1Update
SHA1Transform
SHA1Init
SHA1Final
SDawaAck
RtpStatHander
RingerSoundDriver
RingerPlaymelody
RingerPlayState
RingStopNtfy
RingStartNtfy
ReverseRegion_DID04
ReverseOrder
ReverseData
RestartPppoe__Fi
RestartChargingProc
Reset__10CSyncEvent
ResetWifiModule
ResetWFDrive
ResetSyslog
ResetNetParam
ResetIME
ReserveRegion
ResTextOut
ResDrawText_MultiLine
ResDrawText
ResDrawNumber
ReplaceRegionColor_DID04
ReplaceRegionColor
RepeateAnnounce
RenewDhcpLease
ReleaseDC
ReleaseCopyScreenData_DID04
ReleaseCopyScreenData
Register_Init
RegisterModule__6CErrorPcUcUcPPci
RegisterLater
RegisterErrors__FPcUcUcPPci
Reg_Offset_Set
Reg_MainMenu_Entry
RegSuccessNtfy
RegProcNtfy
RegFailNtfy
RefleshDhcpParam
RedirectNtfy
Recvfrom
Recv
Rectangle
ReceiveFrame
ReadSSIDAndWepKey
ReadPBEntryExs
ReadPBEntryEx
ReadPBDIndex
ReadMemEx
ReadMem
ReadMWIIndication
ReadAutoScanStatus
Read3WayCallFlag
RTTsrvInit__Fv
RTTsrv
RTP_port
RTC_post_event_queue
RESOLVER_DEBUG
REGISTRY_ReaderExit
REGISTRY_ReaderEnter
REGISTRY_PrivGetNumReaders
RC_Replace
RAS_setAddrPoolexptDrv
RAS_printAddrPoolInfo
RAS_pmpRemoveDriver
RAS_pmpInsertDriver
RAS_pmpGetDriver
RAS_pmpAddrPoolDrvsInit
RAS_getNumOfPools
RAS_getMaxPoolId
RAS_getAddrPoolexptDrv
RAS_getAddrPoolSize
RAS_getAddrPoolRouterId
RAS_getAddrPoolPrefix
RAS_getAddrPoolPMPmode
RAS_getAddrPoolNumFreeAddrs
RAS_getAddrPoolNumDrvs
RAS_getAddrPoolFirstIp
RAS_getAddrPool1stDrv
RAS_RelIpAddr
RAS_Ioctl
RAS_InsAddrPool
RAS_GetIpAddr
RAS_DelAddrPool
RAS_AMM_Init
QueueMaxNoMsgs
QueueInit
QueueHead
QueueDestroy
QueueCreate
PyReorder
PwrOn_Send2MainMsgQ
Put_Legal
Punctuation
PuncProc
PuncPaint
PrvDigestCalc
PrvCvtHex
ProfileMemoAdd
ProfileAlarmAdd
Profile4Add
Profile3Add
Profile2Add
Profile1Add
ProductCategory
ProcessingComplete__15CdspRootManager
Process_LeftRight
Pro_stoptimer
Pro_main_Entry
Pro_Speed_Entry
Pro_SpeedMenu_Ind
Pro_Sound_Kind
Pro_ShowTopVib
Pro_PlayMelody
Pro_Menu_Ind
Pro_ComStopVibrate
Pro_ComStopMelody
Pro_ComStartVibrate
Pro_ComEventPreProc
Pro_ComEndVibrate
Pro_ComBeginVibrate
Pro_2Menu_Ind
Print_ChgCurrent
PrintWDTCount
PrintTotalRtpStat
PppoeStatus
PppoeInProgress
PppoeCloseInProgress
PowerState
PowerOn_Poll
PortEdit
PlayWarning
PlayTone
PlaySuccessBeep
PlaySMSRing
PlayRingTone
PlayRing
PlayRegisterTone
PlayPowerTone
PlayMemoRing
PlayMelody
PlayKeyTone
PlayErrorBeep
PlayDTMF
PlayAlarmTone
PickList_setStbyLtr
PickList_Paint
PickList_Initx
PickList_HandleEvent
PickList_Destroy
PickList_DeleteRow
PickList_DeInit
PickList_Createx
PickList_Create
PickList_AddRow
PicIndex
PicFld_GetY
PicFld_GetX
PicField_PaintPunc
PicField_Paint
PicField_HandleEvent
PicField_Destroy
PicField_Create
PhoneSettingInit
Pfn_NeedData_VoiceProcPicklist
Pfn_NeedData_CodecPriorityPicklist
PfnNeedDataWfconfigPicklist
PfnCond_SuccessMsgboxExit
PfnCond_SoWriteConfirm
PfnCond_Restart
PfnCond_FailedMsgboxExit
PfnCond_Exit
PfnCond_Confirm
PfnCondWfconfigOperatingMsgbox2Menu
PfnCondWfconfigOperatingMsgbox2Idle
PfnCondWfconfigOperating2Picklist
PfnCondWfconfigOperating2Operating
PfnCondWfconfigOperating2Menu
PfnCondWfconfigOperating2Idle
PfnCondWfconfigEditMsgboxExit2Picklist
PfnCondWfconfigEditMsgboxExit2Edit
PfnCondWfconfigEdit2Picklist
PfnCondWfconfigEdit2Edit
PfnCondLocallogUpDownItem
PfnCondLocallogNextItem
PfnCondLocallog2Menu
Perror
PbTransMode
PbReadAllPhase
PbJudgeDataEmpty
PbGetValidRecordCount
PbGetPbData
PbGetParmsPhase
PbGetItemNamePhase
PbGetItemKindInfoPhase
PbFetchPhase
PbExcCommand
PbDownloadPhase
PbCheckPosition
PasswordBuffer
ParseSwapRecHead
ParseRecHead
ParsePhseRecHead
ParseMsg
ParseCalgRecHead
ParamTable
PaintScrSv
PMSendSYSLineNumMsg
PMSendRSSIMsg
PMSendAPMsg
PMM_GetVersionPhase
PMM_GetSupportModePhase
PMM_GetProtocolVerPhase
PMM_GetModelPhase
PMM_GetCurrentVersion
PMMI_StrCmp4Bytes
PMMHeadLenByVer
PMGetSYSLineNumMsg
PMGetAPMsg
PMDelSYSLineNumMsg
PHYSetChannel
PHYPower
PHYInit
PDA_Update
PDA_Traverse
PDA_Locate
PDA_GetCRC
PDA_Append
PB_SpeedkeyView_Exit
PB_RingPlay_CallBack
PB_Password_Exit
PB_Number_FieldSave
PB_Name_FieldSave
PB_MainMenu_Entry
PB_ListKeyEvent_CallBack
PB_ListInTalk_Detail
PB_DetailInTalk_List
PBSaveDialNum
PBPassWord_FieldSave
PBNumList_SearchbyNum
PBInitial
OsapiTimerInterval
OsapiEvList
Option60Len
Option60
Option43
OpenRTPSession
Old_ate_sleep_isenable
OPENSSL_cleanse
NumericProc
NoticeMsgBox
NormalEntity
NextIteration__5CList
New_Set_Sel2
New_Set_Sel
New_Service_Set
New_Service_Han
New_Service
New_Ser_Sel
New_Han_Sel
NetSrv_desidle
NetSrvInitial
NetSrvDeinitial
NetServiceMenu_exit
NetServiceMenu_Entry
NetInfo
NetFailNtfy
NAT_lifetime_test
NAT_lifetime_query
Msgbox_match
Msgbox_exit_setmenu
Msgbox_exit_set
Msgbox_exit_curnum
Msgbox_exit_access
Msgbox_exit_Menu
Msgbox_exit_Current
Msgbox_exit
Msgbox_dismatch
Msgbox_Que_No
Msgbox_Que
Msgbox_Paint
Msgbox_Init
Msgbox_HandleEvent
Msgbox_Destroy
Msgbox_DeInit
Msgbox_Create
MsgboxStr_Create
MsgQTFTP_DOWNLOADFILE
MsgQPM
MsgQMMI
MsgQMAIN
MsgQLineNum
MsgBox_Filter_KeyEvent
MsgBoxExit
MoveScreenImage
MoveDates
MonitorWifiStrength
MonitorSIP
MonitorAPRoaming__Fv
ModiRecord
ModelName
Mmi_main_getrssi
Mmi_main
Mmi_init2
Mmi_init
Mmi_Task_Reset
Mmi_Task_Destroy
MmiStart
MiscTftp_Server_FieldSave
MiscMenuEntry
MiscInit
MessageSendQueue
MessageReceiveQueue
MessageReachedNtfy
MessageIncomingNtfy
MessageDeliveredNtfy
Menu_SetToTopItem
Menu_Paint
Menu_Init
Menu_HandleEvent
Menu_Destroy
Menu_DeInit
Menu_Create
Menu_AddIndicator
MenuItem_Init
MenuItem_Destroy
MenuItem_DeInit
MenuItem_Create
MenuItem_AddChild
MelodyName_English
MelodyName_Chinese
MelodyInit
MelodyDataSuccess
MelodyDataKey
MelodyDataFail
MelodyDataAlert
MelodyData6
MelodyData5
MelodyData4
MelodyData3
MelodyData2
MelodyData1
MatchAltSound1Key
MaskLowBit
MaskHighBit
MaskBit
MallocScreenBuffer_DID04
MallocScreenBuffer
MakeRequestHeader
Main_initMsgq
Main_Start
Main_Process
MainMenu_SetCur
MainMenu_Paint
MainMenu_LostFocus
MainMenu_HandleEvent
MainMenu_GetFocus
MainMenu_GetCur
MainMenu_Destroy
MainMenu_Deinit
MainMenu_Create
MainMenu_AddItem
MainMenu_Add
MULAWinfo
MSG_Q_WUA
MQSend
MQReceive
MQInit
MQBufGet
MQBufFree
MMIMQSend
MMIMQReceive
MISCNoticeMsgBox
MD_string
MD5_PADDING
MD5Update
MD5Transform
MD5Init
MD5FinalAes256
MD5Final
MAINMsgQSend
MAC_Addr
LowString
Loop_flag
Lookup__5CListPvUl
LogHandleProc__Fv
Lock__9CSyncLock
LocalLogInit
LoadString
LoadSIPStack
LoadIcon
LoadFont
LoadEziData
LoadDeliverSet
Line_DID04
Line
Lcd_backlight_ctrl
LcdDataBuffer
LatinSearchDigitStrncmp
LanguageEntry
Lang_Mode_sel
Lang_Mode_needdata
Label_SetTextEx
Label_SetText
Label_SetIcon
Label_Paint
Label_MoveTo
Label_Init
Label_HandleEvent
Label_Destroy
Label_DeInit
Label_CreateTextLabel
Label_CreateLdigitLabel
Label_CreateIconLabel
Label_CreateDateLabel
LPC10info
Kpd_backlight_ctrl
KeypadTable_all
KeypadMonitor
Key_Send2MainMsgQ
KeyToPower
KAPI_OSTaskStart
KAPI_OSTaskPrep
KAPI_OA_TimerStart
KAPI_OA_TimerDelete
KAPI_OA_TimerCreate
KAPI_OA_TimerCancel
KAPI_OA_TicksToMillisecond
KAPI_OA_TaskWake
KAPI_OA_TaskWaitClr
KAPI_OA_TaskWait
KAPI_OA_TaskUnlock
KAPI_OA_TaskThisHandle
KAPI_OA_TaskTerminate
KAPI_OA_TaskSuspend
KAPI_OA_TaskStart
KAPI_OA_TaskSetPriority
KAPI_OA_TaskSetParameter
KAPI_OA_TaskResume
KAPI_OA_TaskLock
KAPI_OA_TaskGetPriority
KAPI_OA_TaskGetParameter
KAPI_OA_TaskFindHandle
KAPI_OA_TaskDelete
KAPI_OA_TaskDelayTick
KAPI_OA_TaskDelayMs
KAPI_OA_TaskCreate
KAPI_OA_SetMemoryHandler
KAPI_OA_SemaphoreWait
KAPI_OA_SemaphoreTryWait
KAPI_OA_SemaphoreSignal
KAPI_OA_SemaphoreFindHandle
KAPI_OA_SemaphoreDelete
KAPI_OA_SemaphoreCreateEx
KAPI_OA_SemaphoreCreate
KAPI_OA_ReallocMemory
KAPI_OA_QueueSendMsg
KAPI_OA_QueueRecvMsg
KAPI_OA_QueueQueryMsgNumber
KAPI_OA_QueuePurgeMsg
KAPI_OA_QueueFindHandle
KAPI_OA_QueueDelete
KAPI_OA_QueueCreate
KAPI_OA_PM_TimerStart
KAPI_OA_MutexUnlock
KAPI_OA_MutexLock
KAPI_OA_MutexFindHandle
KAPI_OA_MutexDelete
KAPI_OA_MutexCreate
KAPI_OA_MillisecondToTicks
KAPI_OA_GetTickCount
KAPI_OA_FreeMemory
KAPI_OA_CriticalExit
KAPI_OA_CriticalEnter
KAPI_OA_CriticalDelete
KAPI_OA_CriticalCreate
KAPI_OA_BinarySemaphoreCreateEx
KAPI_OA_BinarySemaphoreCreate
KAPI_OA_AllocZeroMemory
KAPI_OA_AllocMemory
JbUpdateJitter__FP8jbConnCb7jbEvent
JbStopTimer
JbStartTimer
JbStaReq
JbResetJitterReq
JbRemovePacket__FP8jbConnCb
JbInsertPacket__FP8jbConnCbPUcUiP9rtp_hdr_t
JbFSM
JbDiscReq
JbDatInd
JbConReq
JbConModReq
JbCntrlReq
JbCfgReq
Iskpd_num_press
IsWhisperMode
IsWarmReboot
IsWPAAP
IsUnloadSIPStack
IsTftpState
IsStringforU16Valid
IsSIPStackRuning
IsRemoteTftpState
IsPowerKeyPressed
IsOnlyRecordWhenModi_g
IsOnlyRecordWhenModi
IsOnlyRecord
IsNameAllSpace
IsMsgboxShow
IsMsgboxExist
IsMsgWtLong
IsLeapYear
IsInBlackList
IsHalfChinese
IsGWValid
IsDoingDhcp
IsDoingAutoScan
IsDifferentSubnet
IsDDWakeupMode
IsDDSleepMode
IsCurrentSpeedKeySet
IsCurrentGroupEmpty
IsAllPause
Ippwd
Ipcenter
Ipaccount
IpMsgbox_exit
IpEmpty_exit
IpDecode
IpCode
Instance__15CdspRootManager
Instance__11CdspManager
Insert__5CListPvi
Insert__10CMutexListPvi
InsertNumIndexTbl
InsertIndexTbl
InsertEntry2NumTbl
InputMatch
Inmethod_ZIstroke_sel
Inmethod_ZIenglish_sel
Inmethod_ZIPinYin_sel
Inmethod_PinYin_sel
Inmethod_English_sel
Inm_ZIstroke_NeedData
Inm_ZIeng_NeedData
Inm_ZIPinY_NeedData
Inm_PinYin_NeedData
Inm_Eng_NeedData
Initialize
Init_pscChgAveCurrent
Init_mmsgq
Init__15CdspRootManager
Init__11CdspEncoderUsP15CdspRootEncoderP15CdspRootManagerUsUs
Init__11CdspDecoderUsP15CdspRootDecoderP15CdspRootManagerUs
Init_TimerQue
Init_PMMsgQue
Init_Fld_CceTp
Init_Field
Init_DNS_Resolve
InitVonageDefault
InitSysInfo
InitSecTimer
InitRtpStat
InitResData
InitNetSearch
InitHeadInfo
InitGDI
InitFontManager
InitFontFeatureEx_01
InitFontFaceEx_01
InitEziParam
InitDeviceDriver_DID04
InitDelayTimer
InitDSP
IncreaseVolume
IncreaseTxRtpPacketCnt
IncreaseTxRtpLostCnt
IncreaseTxRtpLateCnt
IncreaseTxRtpJitterCnt
IncreaseRxRtpPacketCnt
IncreaseRxRtpLostCnt
IncreaseRxRtpLateCnt
IncreaseRxRtpJitterCnt
IncomingCallNtfy
Idlepick
Idle_have_register_switch
Idle_exit_menu
Idle_exit_Standby
Idle_Vonage_sel
Idle_Static_needdata
Idle_StaticPic1_sel
Idle_StaticPic0_sel
Idle_StaToEdit_sel
Idle_SmsComing
Idle_Pic1_sel
Idle_Pic1_KeyUp_sel
Idle_Pic1_KeyDown_sel
Idle_New_sel
Idle_New_needdata
Idle_New_Sta_sel
Idle_New_Cha_sel
Idle_Mode_sel
Idle_Mode_needdata
Idle_GetPic
Idle_Exit_New
Idle_Edit_sel
Idle_Change_sel
Idle_Change_needdata
Idle_ChToPre_sel
Idle_ChToEdit_sel
IdleRS2Pb
IdleNew_exit_menu
IdleInput2Pb
IPv6Family
IPv4Family
IP_Msgbox_show
IPMask
IPEdit
IDLE_STANDBYEXIT
IDLE_STANDBYENTRY
IDLE_SLEEPBEGIN
IDLE_OUTGOING
IDLE_MISSING
IDLE_INCOMING
ICSwitchOnlyForEnglish
ICSwitch
ICSetImeEnable
ICSetCurLang
ICLoadDefault
ICInit
ICGetLangString
ICGetImeEnable
ICGetCurIme
ICGetAllLangString
ICDestroy
ICAteSetDefaultLang
HorzData
HaveAvailableAPs
HTTPStatus_put_block
HTReader_read
HTParseInet
HTLoadHTTPBegin
HTLoadHTTP
HTGetHostByName
HTDoConnect
HTDoClose
GroupNumBuild
GetiWlanTimerValue
Get_Vibration_State
Get_Saver_TimeId
Get_Saver_On
Get_Saver_AnId
Get_PowerOnAnId
Get_Pic_Id
Get_Idle_Txt
GetWindowDC
GetVoiceMailInfo
GetVMBoxPw
GetVMBoxNum
GetVMAccessNum
GetTxtByAscii
GetTotalRtpStat
GetToolWorldTimeIndex
GetTimeZoneValueByIdx
GetTimeZoneDspnameByIdx
GetTFTPWorkMode
GetTFTPServerIP
GetTFTPServerDomain
GetTFTPPort
GetTFTPInfo
GetTFTPEncrKey
GetTFTPDirFile
GetSysTxtColor
GetSysPenColor
GetSysLanguage
GetSysFontWidth
GetSysFontID
GetSysFontHeight
GetSysCharset
GetSysBrushColor
GetSysBkColor
GetSubnetMask
GetStunServerPort
GetStunServerName
GetStringWidthEx_01
GetStringWidth
GetStringLang
GetString
GetStrDigit
GetStationFirmwareBlocks
GetSowrteState
GetSizeofTimezone
GetShortMenuItem
GetSIPUserName
GetSIPSerName
GetSIPRegSerPort
GetSIPRegSerIP
GetSIPRegSerDomain
GetSIPPw
GetSIPProxyPort
GetSIPProxyIP
GetSIPProxyDomain
GetSIPPort
GetSIPObProxy
GetSIPInfo
GetSIPDnsSrv
GetSIPAuthStr
GetSIPAuthAlg
GetRtBatteryVolume
GetResBuffer
GetRecDatabyByte
GetRecCmdHead
GetRTPPort
GetRTPPackTime
GetRTPJitBufComp
GetRTPInfo
GetRID
GetProfileMelodyName
GetPrlFlag
GetPosition__5CListPv
GetPixel_DID04
GetPixel
GetParent
GetPBName2SortCode
GetPBActualTotalNum
GetOutOfService
GetNATWorkMode
GetNATSerPort
GetNATSerIP
GetNATSerDomain
GetNATSTUNMode
GetNATKATime
GetNATKADest
GetNATInfo
GetNATIP
GetMainMenuItem
GetMainLCDWidth
GetMainLCDHeight
GetMainLCDBuffer
GetMainLCDBPP
GetMacAddrString
GetMacAddr
GetMMIAutoScanFlag
GetListLength__5CList
GetLanguageCode
GetIphoneNumber
GetIntervalRtpStat
GetIndexByIntVaule
GetImgWidth
GetImgHeight
GetIcon
GetIPInfo
GetIPAddress
GetHourFormat
GetHeadsetState
GetGatewayIP
GetFontNumber
GetFontMaxCode
GetFontInfoEx_01
GetFontDriver
GetFontCount
GetFontCharset
GetFontCharOffset
GetFontCharData
GetFontCharCode
GetFontBitCount
GetFontBeginCode
GetFirmwareExecutionAddress
GetErrorString__6CErrorUl
GetErrorMessage__FUl
GetElementAtPosition__5CListi
GetDhcpType
GetDhcpParameters__Fv
GetDNSSecServer
GetDNSPriority
GetDNSPriServer
GetDNSInfo
GetDCTextUnionColor
GetDCTextColor
GetDCPenColor
GetDCMapMode
GetDCFont
GetDCBrushColor
GetDCBkColor
GetDC
GetCurrentTimestamp
GetChild
GetCharsetEx_01
GetCharWidthEx_01
GetCharWidth
GetCharHeightEx_01
GetCharHeight
GetCharDigit
GetBatteryVolume
GetBatteryVol
GetAllCallTimeFromBuffer
GSMinfo
GJBInf
G7231info
FwStopTimer
FwSetTimer
FwSetDefaultAttrs
FwSetAttrs
FwSendEvent
FwPeakEvent
FwGetTextExtents
FwGetEvent
FreeBufferPtr
FontFace
Fld_Paint_UnderLine
Fld_Paint_Text
Fld_Paint_NoCCECursor
Fld_Cce_Switch
FlashBad
FindRecordBySpeedDialKey
FindNameOnlyByNumber
FindNameByNumber
FindFlashPBEntryByNumber
FindFirstEmptyPBFlash
FindAP
FillRectangle
FillRect_DID04
FillRecords
FillCircle_DID04
FillCircle
Field_UpLine
Field_TextBuffInsert
Field_TelnumSetCurPos
Field_TelnumPaintCursor
Field_TelnumPaint
Field_TelnumHandleDirKey
Field_ShowCursor
Field_SetType
Field_SetText
Field_SetRight
Field_SetPasswordMode
Field_SetLeftIcon
Field_SetIpCan
Field_SetCursorPos
Field_SetCCeAttr
Field_RightMove
Field_Redraw
Field_Pk_needdata
Field_PaintCursor
Field_Paint
Field_NoRgtBtn
Field_LostFocus
Field_Leftmove
Field_IpCanDel
Field_InsertAn
Field_HandleEvent
Field_GetType
Field_GetTextLength
Field_GetText
Field_GetPrevFocus
Field_GetNextFocus
Field_GetFocus
Field_GetBuf
Field_DownLine
Field_DialSetCurPos
Field_DialPaintCursor
Field_Destroy
Field_Deletechar_Ip
Field_Deletechar
Field_Deinit
Field_Cur_InitPos
Field_Create
Field_Cce_PutString
Field_Cce_PutChar
FieldCce_HandleEvent
Field2CcePre
FWTimerIsNull
FILEMGR_RetrieveResource
FILEMGR_RetrieveFile
FILEMGR_ReleaseResource
FILEMGR_ReleaseFile
FILEMGR_DeConstruct
FILEMGR_Construct
FD_PK_PUNC_LATIN
FD_PK_PUNC_CHI
Ext_Operating
Ext_AES_cbc_encrypt
Ext_AES_cbc_decrypt
Exit_To_Set
Exit_StopTimer
Exit_Sleep
ExitMonitorSIP
Execute
ExceHandle
EscapeCgiArgument
ErKeypadTableSPA
ErKeypadTablePOR
ErKeypadTableFRN
ErKeypadTableCHS
ErKeypadTable
Entity_TransitState
Entity_Init
Entity_HandleEvent
Entity_Enabled
Entity_Destroy
Entity_DeInit
Entity_Create
EnterpriseCode
Enter_Sleep
Enter_Reg_Call
Enter_Num
Enter_Msg
Enter_Can_Call
EndIteration__5CList
EndIteration__10CMutexList
Enable_Keypad
Enable
En_MsgWait
Element_GetRoot
Element_GetExternalRect
Element_DrawFrame
Element_ClearExternal
EepromWriteEx
EepromRead
EVP_md5
EVP_MD_CTX_init
EVP_MD_CTX_cleanup
EVP_DigestUpdate
EVP_DigestInit_ex
EVP_DigestFinal_ex
EVP_CipherInit_ex
EVP_CIPHER_CTX_cleanup
EVP_BytesToKey
EResearchField_SetText
EResearchField_Paint
EResearchField_LostFocus
EResearchField_HandleEvent
EResearchField_GetText
EResearchField_GetFocus
EResearchField_Destroy
EResearchField_ConfirmText
EEPROM
DtmfBurst__Fiiiii
Draw_Line
Draw_DateTimeChar
Draw_CircleCnt
Draw_Circle
DrawTransparenceIcon
DrawText
DrawSaverNumeric
DrawSaverClock
DrawRect_DID04
DrawLatticeImg_DID04
DrawLatticeImg
DrawDates
DrawCircle_DID04
DrawBitmapImg
DrawArc_DID04
Download_task
DownloadIntermediateFirmware
Dowmload_main
DomainEdit
DoCommand
DisplayCode2ZiCode
Disable_Keypad
Disable
Dis_MsgWait
DigestCalcResponse
DigestCalcHA1
Dialog_ShowRightBtn
Dialog_ShowLeftBtn
Dialog_SetRightBtnIcon
Dialog_SetMenu
Dialog_SetLeftBtnIcon
Dialog_RemoveChild
Dialog_PaintUserDialog
Dialog_Paint
Dialog_Init
Dialog_HideRightBtn
Dialog_HideLeftBtn
Dialog_HandleEvent
Dialog_GetMenu
Dialog_EnableRightBtn
Dialog_EnableLeftBtn
Dialog_DisableRightBtn
Dialog_DisableLeftBtn
Dialog_Destroy
Dialog_DeInit
Dialog_Create
Dialog_AddUrlField
Dialog_AddLable
Dialog_AddInputField
Dialog_AddField
Dialog_AddChild
Dial_Paint
Dial_HandleEvent
Dial_HandleArrowKey
DhcpPppoeProcess__Fv
DhcpInProgress
DhcpCounter
DestroyMenus
DestroyGDI
DestroyErrorObject__6CError
DemoWifiNotify__FiP4_LTV
DemoValidateData__FP8DemoMenu
DemoValidateDataAll__Fv
DemoSaveConfigData__FPc
DemoLocateData
DemoInitPhoneParam
DemoGetConfigDataSize__Fv
DemoDotUnpack__FPcUi
DemoDotPack__FPUiPc
DemoConfigInitDefaultAll
DemoConfigGet__FPv19config_data_locator
DemoConfig
DemoAddrBook
Delete__5CListi
Delete__5CListPv
Delete__10CMutexListi
Delete__10CMutexListPv
DeleteFontImgEx_01
DelayCBfunc
DelPBIdx
DelPBEntryExs
DelPBEntryEx
DelPBEntry
DelEntryInNumTbl
DelAllPBEntryEx
DecreaseVolume
DebugAssert
DbgPrintBuf
DayOfWeek
DawaAck
DateofMonth
Date_Paint
DateTime_SetCursorPos
DateTime_PutChar
DateTime_Paint
DateTime_HandleEvent
DateTime_HandleDirKey
DateDiff
Date2Time
DarkRegionColor_DID04
DarkRegionColor
DTMFRecvNtfy
DHCPType
DDSState
DDSExit
DDSEnter
DCSelectDD
DCACHE_CTRL
DATEMAX
CycleRinger__Fv
CvtHex
CurrentGWMac
CtrlFlag
Crt_Repeat_Cha
Crt_PreTo_Cha
CrtWebAuthUrlState
CrtWebAuthScriptFilesState
CrtWebAuthProcessState
CrtWebAuthInputState
CrtWebAuthDownScriptState
CrtWebAuthConnState
CrtVersionViewDlg
CrtVendorNameViewState
CrtVendorNameViewDlg
CrtVMBoxPwEditState
CrtVMBoxPwEditDlg
CrtVMBoxNumEditState
CrtVMBoxNumEditDlg
CrtVMAccessNumEditState
CrtVMAccessNumEditDlg
CrtVADPicklistState
CrtVADPicklistDlg
CrtTFTPWorkModePicklistState
CrtTFTPWorkModePicklistDlg
CrtTFTPPortEditState
CrtTFTPPortEditDlg
CrtTFTPIPEditState
CrtTFTPIPEditDlg
CrtTFTPEncrKeyEditDlg
CrtTFTPDomainEditState
CrtTFTPDomainEditDlg
CrtTFTPDirFileEditState
CrtTFTPDirFileEditDlg
CrtStunServerPortEditState
CrtStunServerPortEditDlg
CrtStunServerNameEditState
CrtStunServerNameEditDlg
CrtStunOnOffPicklistState
CrtStunOnOffPicklistDlg
CrtState_Tftp_Local
CrtState_Tftp_Downloading
CrtState_Tftp_ConnectPC_Local
CrtState_Tftp_ConnectPC
CrtState_Tftp
CrtState_Picklist
CrtState_Operating
CrtState_Menu
CrtState_InputValue
CrtState_CheckPassward
CrtSoWriteProcessingState
CrtSoWriteProcessingDlg
CrtSoWriteNotifyState
CrtSoWriteNotifyDlg
CrtSettng_TimeFormatSte
CrtSetting_TrOpSte
CrtSetting_TrCaSte
CrtSetting_TimeFormatDig
CrtSetting_ShwownSte
CrtSetting_SerSet
CrtSetting_SecretSte
CrtSetting_SecretDig
CrtSetting_SctrsmSte
CrtSetting_SctprtoptSte
CrtSetting_SctprtSte
CrtSetting_SctlngoptSte
CrtSetting_SctlngSte
CrtSetting_SctchgnewSte
CrtSetting_SctchgSte
CrtSetting_SctConfirmSte
CrtSetting_ScrwlmSte
CrtSetting_Scridl_PreSte
CrtSetting_Scridl_Pic1Ste
CrtSetting_Scridl_Pic0Ste
CrtSetting_Scridl_NewSte
CrtSetting_Scridl_MSte
CrtSetting_Scridl_EditSte
CrtSetting_Scridl_ChSte
CrtSetting_ScridlSte
CrtSetting_Scrid_StSte
CrtSetting_ScrctrSte
CrtSetting_ScrbltSte
CrtSetting_ScrTimeSte
CrtSetting_SaverTimeSte
CrtSetting_SaverTimeDlg
CrtSetting_SaverSte
CrtSetting_SaverPickSte
CrtSetting_SaverPickDlg
CrtSetting_SaverOnSte
CrtSetting_SaverOnDlg
CrtSetting_SaverDlg
CrtSetting_PicSte
CrtSetting_NewSer
CrtSetting_NewHan
CrtSetting_MenuSte
CrtSetting_MenuDig
CrtSetting_LngSetSte
CrtSetting_IpphnSte_3
CrtSetting_IpphnSte_2
CrtSetting_IpphnSte_1
CrtSetting_IpphnSte
CrtSetting_IpphnDig_3
CrtSetting_IpphnDig_2
CrtSetting_IpphnDig_1
CrtSetting_IpphnDig
CrtSetting_InmZIstrSte
CrtSetting_InmZIstrDig
CrtSetting_InmZIengSte
CrtSetting_InmZIengDig
CrtSetting_InmZIPinYSte
CrtSetting_InmZIPinYDig
CrtSetting_InmPinYSte
CrtSetting_InmPinYDig
CrtSetting_InmEngSte
CrtSetting_InmEngDig
CrtSetting_FldtstSte
CrtSetting_DatshwSte
CrtSetting_DatedtSte
CrtSetting_DatSetDig
CrtSetting_ChgnewDig
CrtSetting_ChgconfirmDig
CrtSetting_CallSetSte
CrtSetting_CallFdSte
CrtSetting_AswmodSte
CrtSetting_AnimateSte
CrtSetting_AniSelSte
CrtSetting_AlmswtSte
CrtSetting_AlmswtDig
CrtSetting_AlmsetSte
CrtSetting_AlmsetDig
CrtSetting_AlmlzySte
CrtSetting_AlmlzyDig
CrtSetting_AlmcclSte
CrtSetting_AlmcclDig
CrtSIPUserNameState
CrtSIPUserNameEditDlg
CrtSIPServiceNameEditState
CrtSIPServiceNameEditDlg
CrtSIPRegSerPortEditState
CrtSIPRegSerPortEditDlg
CrtSIPRegSerIPEditState
CrtSIPRegSerIPEditDlg
CrtSIPRegSerDomainEditState
CrtSIPRegSerDomainEditDlg
CrtSIPProxyPortEditState
CrtSIPProxyPortEditDlg
CrtSIPProxyIPEditState
CrtSIPProxyIPEditDlg
CrtSIPProxyDomainEditState
CrtSIPProxyDomainEditDlg
CrtSIPPortEditState
CrtSIPPortEditDlg
CrtSIPPasswordProtectState
CrtSIPPasswordProtectDlg
CrtSIPPasswordEditState
CrtSIPPasswordEditDlg
CrtSIPOBProxyPicklistState
CrtSIPOBProxyPicklistDlg
CrtSIPDNSSRVPicklistDlg
CrtSIPAuthStrEditState
CrtSIPAuthStrEditDlg
CrtSIPAuthAlgEditState
CrtRemoteTftpServerState
CrtRTPPortEditState
CrtRTPPortEditDlg
CrtRTPPackTimePicklistDlg
CrtRTPJitBufCompEditState
CrtRTPJitBufCompEditDlg
CrtProductCategoryViewState
CrtProductCategoryViewDlg
CrtPackTimePicklistState
CrtPLCPicklistState
CrtPLCPicklistDlg
CrtNSPicklistState
CrtNSPicklistDlg
CrtNATWorkModePicklistState
CrtNATWorkModePicklistDlg
CrtNATServerPortEditState
CrtNATSerPortEditDlg
CrtNATSerIPEditState
CrtNATSerIPEditDlg
CrtNATSerDomainEditState
CrtNATSerDomainEditDlg
CrtNATKATimeEditState
CrtNATKATimeEditDlg
CrtNATKAPackDestPicklistState
CrtNATKAPackDestPicklistDlg
CrtNATIPEditState
CrtNATIPEditDlg
CrtModeVersionViewState
CrtModeNameViewState
CrtModeNameViewDlg
CrtLocallogState
CrtIPSubnetMaskEditState
CrtIPSubnetMaskEditDlg
CrtIPGatewayIPEditState
CrtIPGatewayIPEditDlg
CrtIPDHCPInfoState
CrtIPDHCPInfoDlg
CrtIPAddressEditState
CrtIPAddrEditDlg
CrtGJBMaxConnectionEditState
CrtGJBMaxConnectionEditDlg
CrtGJBBufferSizeEditState
CrtGJBBufferSizeEditDlg
CrtEnterpriseCodeViewState
CrtEnterpriseCodeViewDlg
CrtEncrKeyEditState
CrtDNSSecIPEditState
CrtDNSSecIPEditDlg
CrtDNSSRVPicklistState
CrtDNSPriorityPicklistState
CrtDNSPriorityPicklistDlg
CrtDNSPriIPEditState
CrtDNSPriIPEditDlg
CrtDHCPPicklistState
CrtDHCPPicklistDlg
CrtCodecPriorityPicklistState
CrtCodecPriorityPicklistDlg
CrtCNGPicklistState
CrtCNGPicklistDlg
CrtAuthAlgEditDlg
CrtActiveScriptProcessState
CrtAECWorkModePicklistState
CrtAECWorkModePicklistDlg
CrtAECTailTimeEditState
CrtAECTailTimeEditDlg
Create_Tra_OpenDlg
Create_Tra_CancelDlg
Create_SCR_Pic1_Set
Create_SCR_Pic0_Set
Create_Preview_Dlg
Create_Pic_Dlg
Create_NetService_MenuDig
Create_Idle_StaticDlg
Create_Edit_Dlg
Create_EResearchField
Create_DlgTftpAskContinue_Remote
Create_DlgTftpAskContinue_Local
Create_DlgInputValue
Create_DlgFftpDownloading
Create_DlgFftpConnectPCLocal
Create_DlgFftpConnectPC
Create_CallFd_Dlg
Create_AnimateDlg
CreateWfconfigPicklistState
CreateWfconfigOperatingState
CreateWfconfigEditState
CreateWfConfigPicklistDialog
CreateWfConfigOperatingDialog
CreateWfConfigEditDialog
CreateWFSettingModStateTbl
CreateWFSettingModDialog
CreateUserDialog
CreateUIFdModStateTbl
CreateUIFdModDialog
CreateToolModStateTbl
CreateToolModDialog
CreateSysModStateTbl
CreateSysModDialog
CreateSettingModStateTbl
CreateSettingModDialog
CreateRegisterModStateTbl
CreateRegisterModDialog
CreateRegisterDurStateTbl
CreateRegTimeStateTbl
CreateRegDologStateTbl
CreateRegDispStateTbl
CreateRegDelPwdStateTbl
CreateProfileWhisTbl
CreateProfileVolTbl
CreateProfileSmsTbl
CreateProfileRingTbl
CreateProfileModeTbl
CreateProfileModStateTbl
CreateProfileModDialog
CreateProfileMemoTbl
CreateProfileMainTbl
CreateProfileAlarmTbl
CreateProSpeedTbl
CreatePMTask
CreatePBModStateTbl
CreatePBModDialog
CreateNetServiceModStateTbl
CreateNetServiceModDialog
CreateMiscModStateTbl
CreateMiscModDialog
CreateMMITask
CreateLatticeImgEx_01
CreateIdleModStateTbl
CreateIdleModDialog
CreateErrorObject__6CError
CreateCalendarSolar
CreateCalendarDate
CreateCalculatorShowMenu
CreateBitmapImgEx_01
CreToolStaTbl_WorldTime
CreToolStaTbl_DST
CrePBStaTbl_StorStatus
CrePBStaTbl_SpeedKeyView
CrePBStaTbl_SpeedKeySet
CrePBStaTbl_SpeedKeyModi
CrePBStaTbl_SpeedKeyMenu
CrePBStaTbl_Search
CrePBStaTbl_RecordMenu
CrePBStaTbl_RecMenu_g
CrePBStaTbl_NameAdd_Ret
CrePBStaTbl_NameAdd
CrePBStaTbl_ModiRecord_g
CrePBStaTbl_ModiRecord
CrePBStaTbl_ModiName_g
CrePBStaTbl_ModiName
CrePBStaTbl_ModiGroup_g
CrePBStaTbl_ModiGroup
CrePBStaTbl_Mainmenu
CrePBStaTbl_List
CrePBStaTbl_GroupRingSet
CrePBStaTbl_GroupList
CrePBStaTbl_DialSave
CrePBStaTbl_Detail_g
CrePBStaTbl_Detail
CrePBStaTbl_DelByOne
CrePBStaTbl_DelByAll
CrePBStaTbl_AddSeleGroup
CrePBStaTbl_AddName
CrePBStaTbl_Add
CopyScreen_DID04
CopyScreenImage
ConvertEntryInfo
ConvertDate2Txt
Constrast
ConnectTimerFunc
Connect2OpenAP
Connect
Conf_fldpunc2fld
Conf_fldpk2text
Conf_fldpk2smile
Conf_fldpk2self
Conf_fldpk2punc
Conf_fldpk2prase
Conf_fldpk2an
Conf_Rt2fldpk
Conf_Pk2Fld
Cond_MsgboxExit
CompressPhoneNumberpb
CompressPhoneNumber
CompressNumericDatapb
CompressNumericData
CompareDUTMem
Com_StopVibrate
Com_StartVibrate
Com_EventPreProc
CodecPriorityInf
Cnd_tftpOver2Idle
Cnd_tftp2Idle
Cnd_pwd_match
Cnd_pwd_dismatch
Cnd_TftpResultTimeoutFailed
Cnd_TftpResultDownloadingBegin
Cnd_TftpFailed
Cnd_TftpError2Idle
Cnd_TftpConnecting2AskContinue
Cnd_TftpConnecting
Cnd_TftpConnectPCRestartLocal
Cnd_TftpConnectPCRestart
Cnd_TftpAskContinue2PreDownloadRemote
Cnd_TftpAskContinue2PreDownload
Cnd_PicklistSaveflash
Cnd_PicklistOver2Menu
Cnd_Picklist2Operating
Cnd_Picklist2Menu
Cnd_Picklist2Inputvalue
Cnd_Operating2Picklist
Cnd_Operating2Menu
Cnd_Operating2Inputvalue
Cnd_OperateResult
Cnd_OperateCancel2Picklist
Cnd_OperateCancel2Menu
Cnd_OperateCancel2Inputvalue
Cnd_NetSrv_2Mainmenu
Cnd_NetSrc_2Idle
Cnd_Menu2Tftp_Local
Cnd_Menu2Tftp
Cnd_Menu2Picklist
Cnd_Menu2Operating
Cnd_Menu2Inputvalue
Cnd_InputvalueSaveOk2Menu
Cnd_InputvaluePickupSave
Cnd_InputvalueExit2Picklist
Cnd_InputvalueExit2Menu
Cnd_Inputvalue2Operating
CndMisc2RemoteTftfServer
CndMisc2Locallog
Cn_Standby2TFTPAsk
Cn_Standby2Saver
Cn_Saver_An
Cn_Missed_Missed
ClrSoftKeyExternal
CloseRTPSession
Clear_Mmi_Timer
ClearWFShortcutFlag
ClearUnloadSIPStackFlag
ClearSysIsFromIdle2NetTFTPFlag
ClearCceBuf
ClearAutoScanFlag
Circle
ChooseIcon
CheckVersion
CheckVMAccsNum
CheckUserName
CheckTimer
CheckSum
CheckSoundDevice
CheckSerName
CheckRtpPort
CheckRTPJBC
CheckPort
CheckPassword
CheckKATime
CheckIP
CheckEncrKey
CheckDomain
CheckDirFile
CheckBoxPw
CheckBoxNum
CheckAuthStr
CheckAlarmMain
Charge_Send2MainMsgQ
Charg_Stop_Proc
ChangeUnZipNumFace
ChangePortFlag
ChangeNumFace
ChangeIpFlag
Cce_getType
Cce_Repaint
Cce_Paint
Cce_Init_Type
Cce_HandleEvent
Cce_Etext_IconPaint
Cce_DirRepaint
Cce_Destroy
Cce_Deinit
Cce_Create
Cce_Cap_Conver
CceOutChnstr
CceMemInit
CceExportInit
Callback_picklist_needdata
Callback_Field_SaveUrl
Callback_Field_SaveInput
Callback_Field_SaveContent
Call_Forward
CallTerminatedNtfy
CallRejectNtfy
CallForwardMode
CallFailureNtfy
CallCancelNtfy
CallAcceptedNtfy
Calen_Paint
Calen_Init
Calen_HandleEvent
Calen_Destroy
Calen_Deinit
Calen_Create
CalculateSystemTicSpeed
CalcChkSum
Cal_Paint
Cal_HandleEvent
Cal_Destroy
Cal_Deinit
Cal_Create
CalRow
CalNewRtc
CSP_PlayMelody
CB_SIPUserName_Edit_Store
CB_SIPServiceName_Edit_Store
CB_SIPPassword_Edit_Store
CB_SIPAuthStr_Edit_Store
CB_RTPJBC_Edit_Store
CB_Port_Edit_Store
CB_PasswordProtect_Edit_Store
CB_OwnNum_Edit_Store
CB_NATTime_Edit_Store
CB_IP_Edit_Store
CB_GJB_Size_Save
CB_GJB_Max_Connection_Save
CB_EncrKey_Edit_Store
CB_Domain_Edit_Store
CB_DirFile_Edit_Store
CB_BoxPw_Edit_Store
CB_BoxNum_Edit_Store
CB_AccessNum_Edit_Store
CB_AEC_Tail_Time_Save
BufferStore
BufStatNoOfMkcontig
BufStatNoOfAllocs
BufStatMaxAllocs
BufRmTr
BufRelease
BufMkContig
BufMakeNull
BufInit
BufGetTotalSize
BufGetSize
BufDup
BufDumpStats
BufDestroy
BufCopy
BufChainTail
BufAlloc
BufAddTr
BufAddHdr
Btn_Paint
BreakDhcpProcess
BlurryMatchByName
BitBlt_DID04
BitBlt
Bios_LcdFillRec
Bios_GetLcdWidth
Bios_GetLcdHeigth
Bios_GetLcdBuffer
BiosSetTransferType
BiosSetRejectAnonyCall
BiosSetRecallBusy
BiosSetNickname
BiosSetInterval
BiosSetHideCallNum
BiosSetGroupnum
BiosSetFwd
BiosSetDigmapPattern
BiosSetDigmapMode
BiosSetCallwaitPCB
BiosSet3Way
BiosSaveNetserviceString
BiosSaveNetserviceBoolean
BiosLoadNetserviceString
BiosLoadNetserviceBoolean
BiosGetWifiMenuTbl
BiosGetTransferType
BiosGetTFTP
BiosGetRejectAnonyCall
BiosGetRecallBusy
BiosGetNickname
BiosGetNetserviceMenuTbl
BiosGetInterval
BiosGetHideCallNum
BiosGetGroupnum
BiosGetFwd
BiosGetDigmapPattern
BiosGetDigmapMode
BiosGetCallwaitPCB
BiosGet3Way
BindResponseMsg
BindRequestMsg
BindErrorResponseMsg
BeginIteration__5CList
BeginIteration__10CMutexList
Battery_low_lcd_process
Battery_Send2MainMsgQ
Bat_low_process
Bar_SetZeroFlag
Bar_SetNum
Bar_Paint
Bar_Init
Bar_HandleEvent
Bar_Destroy
Bar_Deinit
Bar_Create
BB_Power_On
BB_Power_Off
BB_Power_Keep_Low
BB_Chg_Low
AutoScan__Fv
AutoReturnToIdleMain
Ate_Send2MainMsgQ
Ate_MMI_Para_Table
AteWriteToCommPort
AteTaskInit
AteTaskId
AteTaskCleanup
AteTask
AteRestoreGlobalStdOut
AteRedirectGlobalStdOut
AteReadFromCommPortExact
AteReadFromCommPort
AtePurgeCommPort
AteOpenCommPort
AteHermesWriteWord
AteHermesWriteMultiWord
AteHermesReadWord
AteHermesReadMultiWord
AteHermesDownloadTertiary
AteGetCommPort
AteDebugPrint
AteCloseCommPort
AppShutdown
AppPreferredCodec__FP11mta_codec_t
AppPause
AppMainMMI
AppMain
AppInited
AppInit__Fv
AppGetVersion
AppBattery
ApiInit
Answer_Mode_sel
Answer_Mode_needdata
Animatepick
Analog_Draw_ChrgIcon
AmtoPm
Allocate
Alarm_Switch_NeedData
Alarm_Lazy_NeedData
AddRecord
AddCredentials
ActiveAutoScan
AccessNum
A_resolv
ATEcontrolEnterSleep
ASCTIME
ANALOG_post_event_queue
ANALOG_check_adapter
ALAWinfo
AES_set_encrypt_key
AES_set_decrypt_key
AES_encrypt
AES_decrypt
AES_cbc_encrypt
AECInf
(start of data
TX& 
( pc( 
 PZ& <[& 
\& @]& 
]& <^& 
_& D
 Xa& 
a& Xb& 
f& (g& 
o& \p& 
&  q& 
r& L
& X~( tX& 
Y& 4Y& LY& dY& 
' ds& `
Z+ ,
[+ t8+ 
`* pA+ 
* x.+ 
s& tt& 
u& L
y& \y& 
y' X
~& |Y& 
Y& (
370(
48#'159
%26*
 '+.258<?
@_B`
?D@_
`?d#
`XOpx
`XNex
`XN,x
`XNtx
v D 
cD@;
@v D
@@ @ *
wD`W
?@@*
 e`@
EEXO0
fPeRaQ
@g&E
@F p
r~q&D
 e`@
EEXO
fPeRaQ
@g&E
@F p
%F&AFc
1^\Q
EQ,X
DF@G
dD@H
eEI>d
@da@
`LaH
d@I>c
)Ea@
eLaH)D
fE'F&
D[@H@Y
d@F0`
eEI>d
eEI>c
fEeF)
*H+X
ghA$
d@J+X
@FFK<e
`AdE
+EFK&D
@F`C
*H&D
eLaH&D>e
fCdE
(g`H/X
XLdX
XLdX
`XKUx
XLdX
`XKvx
XLdX
`XKvx
XLdX
`XKUx
XLdX
ghA$
`AdE
dP:rFq
fP:rFq?
fP:rFq
dP:rFq
fP:rFq#
`AdE
 |:rdPFq
*HdD
eLaH@@
eLaH+X
!g`H,X
ghA$
`AdE
d@Pc
Hd>`
eFKeFY
d@Pc
` x'
d@ *	
 d@D0d@EAd@FD`
d@E,d@FD`
` d@A
`"d@C
DLXO
d@H,
@G@L
\%Z-
Me@ &B
\$Z-
\%Z-
Me@ *
\$Z-
\%Z-
\$Z-
\%Z-
\$Z-
\%Z-
\$Z-
\&Z-
\$Z-
\%Z-
\&Z-
\$Z-
`XNex
`XN[x
`XN,x
(G`A
`XN,x
`XN,x
`XN[x
`XN,x
`XNtx
`XNex
`XN[x
`XN,x
'G`A
`XN,x
`XN,x
`XN,x
aG`A
`XN,x
`XN[x
`XN,x
`XNtx
(^`J
a^h_'
'^`J,D2
N` z-
@LDH@G
dA FU`Uc
d`Z-
\DdA!F$
-FU`UcDE
%D F
d`Z-
%G F
d`Z-
 FU`Uc
$D!FX
N` d`Z-
eEME@ FU`Uc
 FU`Uc
ProgrammingH2
`@d@@
``d@A
`Bd@B
`bd@C?A
A_@&
dd@ &
d@D&d@E0d@F
`FdD
?@@*
e?D@&
PF`	d
\%Z-
Me@ &B
\$Z-
\%Z-
Me@ *
\$Z-
\%Z-
\$Z-
\%Z-
\$Z-
\%Z-
\$Z-
\&Z-
\$Z-
\%Z-
\&Z-
\$Z-
`XN?x
`XN5x
(G`A
`XN5x
`XNNx
(^`J
a^h_'
hD?@
\@\D\E\F\G
`ad#
`@d%
`Na>`
f:`HdX
f:`XdX
`#dZ
` dZ
`%dZ
` dZ
?@@*
d?@@&
U?@@*
?@@&K
rdP~q
rdP~q
dd@ &
wD`W
h>uD
@EXO(
fPeRaQ	
@EXO
fPeRaQ	
%F&AFc
d@Pc
?@@*e
@Pp`
T-X`CEKfE'D
DE@D
c`E$D?
j>~`
:d`RfPFd`Q
FeXO6
E@`A
fEJc
P2022200.hex
FUPU7D37dhfwci
*	+	+	
=jLZlA~
Sb?*
tX.4-6
}{R>
cB0 
fD~T
k<(y
VdNt
oJr\$8
)5)5)5)
)`/5)5)5)
35)5)5)5)5)
+5)5)5)5)5)5)5)5)5)5)5)5)5)5)5)7,5)5)5)5)5)5)5)5)5)5)5)5)5)5)
+5)5)5)5)5)5)
' *3*
*5)5)
,'/Z
,0/n)
,i.N.
q,E/
q,C/
q,(1
q,h1
q,e2
,{,~/
.$+"
,{,6=
,{,:=
,{,?=
,{,J=
,{,p
,{,t
,{,O=
.{,R.
,{,U=
,{,V=
,{,H%
,{,N%
=.{,
,{,`.
*.{,
,{,20
:J;[;[;[;d;
@ 2!2"
?h@uA
QDQDQDQDQDQDQDQDQDQDQDQDQDQD"F"F"F"F"F"F"F"F"F"F"F#F#F#F
H3HxIxIyIyIyIyIzIzIzIzI{I{I{I|I2
non-specified SSID !!           
                               
HERMES 2
                       
non-specified SSID !!           
                                
HERMES 2
                       
First WaveLAN II SSID           
                                (
 Current Service Set Identifier 
`XO/x
$`XO
DJ&F?
pahe
`E(G*_@H*G,_@J,Ge_@L
d@B(E
eEB(E
@K(G@H*G@J,G`E*^@L*D(^@J(De^@H+Dhe
`XO;x
+`,d
+`$b
aAJ@H(A
*C(E
d@H*DX
`XM-x
`XM-x
`XM-x
a)`jdX
)`&b
.`Rb
@ReC)`&b
)`Xb
6"d6
aF2E)`hb
.`Rb
)`Xb
)`\b
AR.`Rb
3` b
`dd3`
.`Rb
dd@@*
a`EeD
d cX
0`va
/`~b
/`vb
/`tb
`ddZ
 @ *
`ZdZ
`ZdZ
`~dZ
%`\a
%`Ja
%`Pa
%`na
%`ta
d@K2`XM
`XM*x
`.dZ
`XOtx
#`XN
e D$
`(d%`
 @P'
 @P'
 @@+
`%di
"`(x
`4d%`
`C)D
`Ydi
%`Pd%`
`vdZ
`(d%`
`(d%`
 @P'
`4d%`
 @@+
 `RdZ
`(d%`
!`Mx
d3`$b
 `qdi
"`(x
`4d%`
dE`C
:EI `
`(d%`
e D4
%`Pd%`
`(d%`
!`7dZ
e D$
!`XdZ
 @P'
`4d%`
e D4
`(d%`
`4d%`
`.dZ
e D4
 @Q#
"`,dZ
e D4
"`OdZ
`XOGx
3`ba
`(d%`
e D$
3`ba
`G@JdG@H#`XN
H#`XN
#`XN
e D$
3`ba
"`(x
e @ *
`E/g
@I @ *
`XNpx
CN.X
pc`@
$eAAH
$`Zx
3`hb
3`jb
%`!x
3`jb
3`pb
3`lb
3`lb
3`nb
3`nb
3`jb
3`pb
3`jb
`XNQx
`E`G
gEeP
&`XNgx
,aAH
CH.`bcCJdA(C
eELe\
6`Ee@
,^e_
eELCH*
.``b
*CeD
'`rx
&`XNgx
d_@J#`XN
H)`&b
#`XN
#`XN
`@@"
&F`E
dE`@
'`?x
@H@JZ
@L`AZ
,A*D@L(D@J
&"e)`
d_@J#`XN
H)`&b
#`XN
#`XN
`4d%`
&F/X
)`ex
)`ex
(`]c
)`ex
c%`td
)`%c
(`]c
`M?@
d@F`A
DC@M
aE-D
eAdT
a)`1x3`#x
@DDE*
DFDG?
a)`1x3`^x
a)`1xxC
a)`1x
d@Pa
?@@&
f xB
)`ex
 Dd@
@@\^
@F\A
d@K2`XM
*`=d
6DH	6DI
`PcZ
)`ex
`PcZ
)`ex
%E D
.`Fb
%E%`
BHdA
`XM-x
.`Fb
na$D
Fe4`XO
bA<`
cz`NdeFX
JedC
JedC4`XO
eAJe-`XO
`G@K
Je4`XO
eAaD
JeXO
N,`XC
` e`A
`/e%
`Xa/
ddAZ
`JdY
AKeB
.`Rb
.`Nb
)`pb
 c)`
aHdX
dA2D
dA2D@
+`$|
 aAKdC
cEfAeF
`G`E
eD)`nb
d3`&b
)`ex
eC.`
)`ex
.`Rb
b@cZ
aHd>c|
`AdD
`BaD
.`Rb
\Ad@
FK`F c
`8e"D
`\"C
.`Rb
`Je`G
fA`F`C
`CaF
Nand
g a#X
.`Rb
`Je`G
fA`F`C
`CaF
g a#X
d@AJd
FK`F c
`8e"D
`\"C
`Je`G
fA`F`C
`CaF
Nand
g a#X
`Je`G
fA`F`C
`CaF
g a#X
f\%FV
d;BJ
%`zd+
d;BJ
d;BJ
%F%D
d;BJ
d@GXO
%`td@GXO
d@GXO
)`ex
d@K2`XM
d@K2`XM
d:BJ
d:BJ
%`zd%`
d:BJ
)`ex
*dG?
)`$b
4`XO
`Je`G
fA`F`C
`CaFQ
`Je`G
fDdF
eFeC
dFbC
`CaFCK,
)`&b
%`Jd%`
%`\d%`
%`nd%`
)`ex
d3`hb
1`Nc D
1`Bb
2`nc1`Db
0D1`Fb
1D1`Hb
2D1`Jb
3D1`Lb
1`Bb
0DdC
BP@S1`Db
@R3D2B
1`Db
1`Fb
@P1`Jb
@R1`Lb
@S1A1`Hb
@Q1`Bb
`C D
1`Bb
+`"c
].`Rb
`AuD
aZH!
z)`*c
aFsBZ
`AdD
bA`U
r\gB
bA.`
aBdC
aZH!
aD.@
`CeAbE
`CbA
abE3`Tb
)`(b
]6`'x
+`"b
+` b
]DI+
@I3`
@I3` b
FC%`
d@E"
cFdC
%XdA
?D@&
`A?D '
a@@'
c:`XO}x
c:`XO}x
(`ddD
dC:`XO}x
c:`XO}x
bEd_
:`XO}x
c\eA2@
&`*c&`
`H`G
`H`G
?@ +
3`fb
dCaE
:`XO}x
3`fb
eAGe+`
:`XO}x
3`fb
:`Xx
d:`XO
d:`XO
d:`XO
d:`XO
d:`XO
(`,d:`XO
(`Hd:`XO
?@@&
3`Zb
|`H`G
CE D`
)`1d?@
&`*c&`
`H`G
`H`G
?@ +
?@ +
]CE D 
@@CE
`H`G
?@@&
3`Rb
h@(`
@@CE
`A&`
 D *
@@ D@*
@D D
$E%`
CE D 
@@dC
CE D 
@@dC
$@ '
`"d$@
W`HdD
dD`T
@F<D
'@'"
'D *
\D'D
1A<D
H`-}
\D\C\B\A\@
d@K\\
\F\I\@
`XO4x
`XOMx
`XOPx
)`ex
Bootcode !!  
STA/AP Func's
d@Pc
aAK	`
aAK	`
%`zd%`
u)`ex
?@@&>
B`	d
c3`^b
3`Vb
3`Tb
c3`\b
d3``b
3`Xb
3`^b
3`Ra
@D6`#| 
<`)|!
<`?|"
`'e[
&`*e
`(e[
a)`1x!`
e?C!`
	`*d
\A\F\G
@[\^)`pb
`'|/`~b
%`2b
=`XN
?@@&
3`Zb
.`Rb
.`Tb
`XNtx
\Q?A
@Jz`NadD
`.a<`
@`tx
`FaAK+A
.`Rb
>`wx
`WxC
`ixd
`@xC
`@xD
`)xE
8`8x
)`9x
)`hx
)`ex(
)`exD
)`exE
)`exF
)`ex
6`*xB
5`(xG
9`+x
?@@&
3`Rb
!F^b
(@@+
)@ 'f
(@H6
(@@+
)@ '
L0d:
e%D76
'D *
rR\I2v
`XOVx
`PuD
l@<F>
'ADH 
@I?@
`ik3`
<D`F
@Bd@
e`G*
@E@H
@M%^?@
@Md@
H`-}
e'D4
`ik@
*DrE$
\F%D
"FdA,
|D3`
dD@E
68d7:
!Fpc
68d7:
d@M+
d@H/
H`-}
B"F.`
`@@+
`@"&?
fC"F"
cF`@
dAdG`_ 
`G"F:
`xb`@@+$
dEdD
`AdF
e<F*
68d76
@ECM
`^e*
`C(D
H`-}
@F'D
!F`@
@G$D
`:|1@
@G<F
`U*R
\D&D
d@FA]!F
`\ d:
"idD
l_`C&
@H@'
bE#DT
@D(E
'@@&0e
(D@+
d@ +
blaz
d@FE(D@+
d@ +
bDFE!F
d`TG
PKgPi
j@@+
l@(D
@D(@
1@ *
(@P:
$D *
3`hb
@F#d:
H`-}
^&C%D
*DrE$
'@&"
H`-}
(eD`P
3`hb
!F2@
PKgP
H`-}
2t@c
j"d:
H`-}
>Tb"F
c|ADH
a(@P6
aAN(D
pb(D
(@@+
`@ +
rEeL
fD"F
(@@+
@I4d:
%`zb
FC#G
DF@E
%`zb
FC#G
@@dD
`@ +
wD`W
%`zb
FC#G
d@B"
%`td@GXO
d@GXOl
@@*@
\JFD9
$F`@
LFa:e
fPeRaQ	
fPeRaQ	
%F&AFc
aAJ|
`XNMx
`XNnx
`XNMx
`XNnx
fD%F
%DaF
`F%D	
%\`A
aF%D	
%D'C
a`F	
a(e%C
cFeD
fFE)C
DGDHDE%`
%`Jc
aD%F'
eD(EE
`F`E
eFdD
aD%F'
%`Hd
GXO!
cF'C
`F%D
%DaF
`F%D
/X@K
aD-X
%`Pb
%`Jb
 @R'
F\.`
3`hb
`\d_
fAdFo
aFdAK
~fEaFo
eeCfAdFp
fAdF
c@GP6
fCdF
'E<F
"c{`
fCdF6
`@@&
abCFC<F
F`@"&e
`EcBZ
`CdDT
`E)`bb
(E`A
fCdF
`C`G
68d76
d@""
`C`@
eD*a`@
eD2a`@
eD.a`@
,EdC
c@77
c@n;
c@77
c@n;
d`E*
3`hb
`@@'
FC`@"&	
|@C*
`XO$x
fC<F"
cF`@
dAdG
`xb`@@+$
dEdD
fAdFo
fAdF
`EaF
eD`@
fAdFo
eeCfAdFp
fAdF
aFfAdF
fAdFo
aFfAdF
fAdFo
fAdFo
fAdFp
eeCfAdFp
eD`@
fAdFo
eeCfAdFp
fAdF
`EfAdF
aF ~L
eD`@
fAdFo
aFfAdF
eeCfAdFp
fAdFo
fAdF
fAdFp
fAdFo
aFfAdF
fAdFo
eeCfAdFp
fAdF
eD`@
fAdFp
fAdFo
aFfAdF
fAdFo
fAdFp
eeCfAdFp
fAdF
aE`C(`
xcE 
%`nd%`
3`hb
`abB@
%`bd
%`hb
%`nd%`
3`hb
gEeP
)`(b
)`(b
`\.`
?@ +
d\\2
%`nd%`
`4d%`
`A%d;
>(d;
L=F*
d@@+
`Je`G
fA`F`C
`CaF
`@ +
fDd@
`XOVx
q r`S
[dG|_
`EdD
d@ +
d@ '
BBFC
bBBFC
bCFL
#F"B~:
b@~:
d@ +
-FdD:
-F`@
 d@J7
fDd@
d@K!
`@ +"
,FdGc@
cFL`
-Fa^
@C@DaF<
@@@A
DL,\
`B D
@@DAZ
DCaF
DDe_@
@I@J
`p|DME
@G@F
|DM-B
@FDGZ
`\dG
eD\a
`C`G[
`Q|r
@v@vB
`nr?
vD :
|d_`P
`"a&F
`nr`G
&F/X
a)`1x
`c`@
e@@+
d@`&
`@@:
^c`@
+dcP
&`XNgx
`Je`G
fA`F`C
`CaF
`XOhx
cEfAeF
`G`E
`E(`
`@@&(
2@@*
2@@&
7dc`@
7^c`@
7Xc`@
`Je`G
fA`F`C
`CaF
`XOhx
cEfAeF
`G`E
&FDL
,Dd@
&F`@@+
fD&F
&F,D
`C#F
`A#F
%F%D
`FFF?
&F,C*
`E(`
`E(`
d@K2`XM
Xc`G
'dca\3`"b
dEdA
:lc?
dEdA
3`"b
&FdA/X
`JedG
fDdF
eFeC
dFbC
`CaF
 |rD
$eCfAcF
`Je`G
cE`F
`JedG
fDdF
eFeC
dFbC
`CaF/
dEFCcF
e@@:
d@H&F-X
dA`@@'	
`XO;x
dD`"
&FdE#
&FdE#
&FdG
`XO3x
&Fa@
`@ *
^c`@
`XO/x
$`XO
&F%`
d@K2`XM
`@@+
dd@ +
`@/&
`XODx
D`Dd
`PdZ
e D4
e D4
e D$
`XOGx
3`ba
e D$
@@dBZ
`=dZ
`adZ
e D$
e D$
`?dZ
au`0e
e D$
e D$
d`A.``c
edA.`bc
`E`G
)`Xb
6"ed@
f\`F
)`Xb
2A`E
eF*`
aF2D
`XOTx
`/dZ
e D$
)`Xb
f\`F
`EfAeF
`G`E
fAeF
`=dZ
e D$
e D$
fEdFfC
dfAdB
)`fb
`Gd^
)`bb
)`lb
`>dZ
`cdZ
@d;BZ
D`Dd
Ad;BZ
DG)`Xb
Bd;BZ
e D4
)`Zb
%`Pd%`
Cd;BZ
&F%`
d@K2`XM
fFF @
Dd;BZ
&F@Y
&F%`
d@K2`XM
)`Xb
fAdF"d6
%`Pd%`
&F@Y
&F%`
d@K2`XM
&F@`
%`Pd%`
`(dZ
&F%`
d@K2`XM
fFF @
&F@Y
&F%`
d@K2`XM
d)`Xb
)`Xb
d)`Xb
d)`Xb
Ed;BZ
`XN/x
fFF0`
dA*`
`Ed_
3`Pb
3`Pb
/`zb
/`fd
/`jd0`
)`Xb
)`*c
)`Xb
.`j|0`
`XM8x
cA/`
%`Pd%`
Fd;BZ
)`Xb
&F@Y
&F%`
d@K2`XM
Gd;BZ
&F%`
d@K2`XM
Id;BZ
Jd;BZ
Hd;BZ
0`4c
fE&F?
0`2a
>deF
3`ra
3`>d@J
EJ|D`
*D3`@|
3`DeD
fD3`Nb
3`Nb
'E<bF
3`jcaE3`pb
|3`kd`
`XNQx
|3`hd
'E<bF
3`jcaE3`pb
|3`kd`
`XNQx
|3`hd
a3`lc
3`nd\
`C.`
3`ra
`C.`
)`Xb
6"dd@
`Je`G
fA`F`C
`CaF
`Je`G
fDdF
eFeC
dFbC
`CaFCG
e`CY
e`CY
`EfAeF
`G`E
3`Pb
)`Xb
6"dd@
F&F/
&F%`
d@K2`XM
)`db
e D$
`?dZ
3`&b
`CfAcF
`Je`G
cE`F
aF3`ha
|3`hd
`XNQx
Kd;BZ
Pd;BZ
`AdZ
Qd;BZ
@G`A
)`Xb
Sd;BZ
Td;BZ
'C.`
Ud;BZ
`?dZ
`ddZ
!`2d
`XN/x
`(dZ
)`*b
/`fd
/`jd0`
)`Xb
`XM8x
cA/`
%`Pd%`
Vd;BZ
Wd;BZ
Xd;BZ
)`Xb
Yd;BZ
&F@Y
&F%`
d@K2`XM
Zd;BZ
a)`1x
[d;BZ
0`4c0d
fE&F?
0`2a
>deF
3`ra
e`CY
e`CY
`EfAeF
`G`E
`AdG
a\`G
&F%`
d@K2`XM
\d;BZ
e D$
&F%`
d@K2`XM
&F%`
d@K2`XM
)`Zb
&F%`
d@K2`XM
&F%`
d@K2`XM
eF&F%`
d@K2`XM
fFF/X
&F/X
dA`@
)`Zb
Nd;BZ
`Je`G
fA`F`C
`CaF%
3`&b
%`Pd%`
`XM*x
`XM*x
e D4
 @K#
e D4
e D4
`Hd*
%`Pd%`
`XOGx
`<dZ
3`ba
%`Pd%`
e D4
e D$
edC4a
N4`XO
e D$
d@K2`XM
e D$
&F`C
d@ '
d@ '
&F/X
`G@L[
d@H,G
 @ *&
`@`:	
&F/X
`XM*x
`XM*x
e D$
)`&b
)`&b
e D$
 @R#
e D4
`Hd*
%`Pd%`
e D$
`KdZ
`Hd*
%`Pd%`
e D4
`*dZ
)`(b
)`(b
)`&b
%`Pd%`
)`(b
)`(b
c @R#
c @R#
%`Pd%`
e D$
e D4
`Hd*
%`Pd%`
`vdZ
)`&b
`A.`
%`Jd%`
%`\b
`&dZ
`JdZ
`kdZ
`@d%`
`@d%`
`@d%`
`xe}
dADK*`
+E`@
`xaY
cA`C
ddAZ
&F/X
c@a@
d_`C`
a\.`
`XM-x
)`Xb
1`>b
)`Vb
0`ve
gD0`
/`~b
/`vb
/`tb
gD0`
eD0`
/`zb
eD0`
/`|b
/`tb
/`|b
/`vb
AJ,@
,@ *
/`|b
/`xb
AJ,@
gD0`
`XM}x
1`>b
`XM8x
%`Pd%`
)`Vb
1`>b
`XM}x
`XM8x
%`Pd%`
fFF/X
1`@b
1`@b
1`@b
`E1`@b
1`@b
`C1`
W2@@&)
`XM*x
`Ha(DY
)`Zb
W2@@&
`XM*x
2@@&=
`XM*x
FK(`
6E `
@QjD
=`XN
)`|c
`GdA
$gLN
)`pb
`FF^1D
dD *
`XOlx
W2@@&$
`XM*x
%`nb
%`td%`
d@K2`XM
XOdX
`xeZ
XO`X
ddX@O*
%`Pd%`
fFF/X
a)`2d
d^d_Dc
)`(b
`E`@
%`\d%`
fFF/X
Rc.X
`XM-x
d3`$b
3`da
3`ba
.``c
+C`G
3`ba
3`ba
3`ba
`E3`ba
c3`$b
`$dZ
`TdZ
%`Pd%`
`{dZ
3`ba
3`ba
3`ba
`!dZ
`FdZ
d3`$b
`udZ
eG`EaD	a
EL@H @ *
eEK*E
 @ *
@KaD,
cDH(E
`CDH(E
`XM*x
dG`E
|D/`
3`Pb
3`Hb
d3`Hb
3`(d@J
3`Hb
3`Lb
3`Nb
d3`Hb
EJ|D`
3`Hb
d3`Hb
3`Lb
3`Nb
3`Jb
`F3`Jb
*D3`*|
3`4eD
3`Hb
3`Lb
3`Nb
d3`Hb
fD3`Nb
3`Nb
a\/`
|3`Pb
|3`Pb
a\/`
d@P6
3`Pb
|3`Pb
aD/`
dE/`
`AdC
|D/`
/`tb
|D/`
/`vb
|D/`
/`xb
 |/`
|D/`
|D/`
/`zb
3`Pb
)`Xb
|D/`
3`Pb
d@P:
6 ee\/`
aE3`pb
aE3`pb
3`pb
eA.X
d@`6
`8dD
`tcQ
&F1@ *
fFF/X
&F/X
.``b
eA.`bc
eaD+AE
`8e+DD
`8e+DD
` edC
decD
`C.X
`Ld%`
`Ld%`
 D@&
 @R#
e D4
`6b~c
`XOGx
`+dZ
``g,
`8dD
`xdD
%`Jd%`
`C`A
e D$
`XM-x
`@e D4
`Ld%`
e D$
HCF$Revision: 10 $
FUPU7D37dhfwci
K	 4K	 XK	 
G.722
G.723.1A 5.3kbs
G.723.1A 6.3kbs
G.729AB
AMRIETF
G.711 - mu
G.711 - A
G.726
AMRIETFwos
G.723.1 5.3kbs without silence
G.723.1 6.3kbs without silence
G.729 A without silence
 8FP 
Q 2@X
0 R@
A  RA
R[P^
bPPAPbP
0 R`;P
PPAPbP
 R`*
8E]`"
P@ RPBP
0 2T0
 RS1PBP
`P@]Q]
 rTRP
PP	&
PP	&
a!#u
 1#5
:P P@` 
a!#u
g a 
g@(P 
r&!P
r&!P
/xD_
b!S;
B.S0
:	 xG
 o" 
 o! 
0o  
0o  
bPpPp
[IPq
aM(q
 o! 
r&Pq
r&Pq
 8	i
r&Pq
r&Pq
GPq	j
/x.(
j	bPp
 o# 
j	bPpPp
0o  
8i0S
8i1S
8i0S
 LPq
8i0S
 8	(
0j4b
#5	)
/x/)
%g%g%g%g%g
%g%g%g%g%g%g%g%g%g%g%g%g
%g%g%g%g%g%g%g%g%g%g%g%g
 8	 
/8/(
%b-!
8i0S
(b%b-!
8i0Sv
8i0S
%b-!
8i0S
 x	-!
8i0S 
)j%b 
8i0S
j	bF
!j%b
Z!j%b)j%b
#5:`
q`(?
]`(?
q`(?
d@ <b  
"ibeb
	#k"
 8	D
/8/e
N@b?
 xG0
 x8Ea
}z(%Bv
pW<nj
GnjW<
0Bv(%}z
<vA<F
J9O[S0W
d-f!g
g!g-f
Z0W[S9O
J<FvA
 .`. 
 8	)
G\IlI
I~I~I~I~I~I~I~I~I~I~I~I~I~I
 ut-sip-rtp@utstar.com
,.:;?!*#"'~/%&@$()<>+-=
ram/~temp.html
Branch through zero
Undefined instruction
Software interrupt
Instruction prefetch abort
Data abort
Interrupt
Fast interrupt
Trap to uninitialized vector address 0x%x.
Exception address: 0x%08x
Current Processor Status Register: 0x%08x
Task: %#x "%s"
uninitialised interrupt vector
uninitialised interrupt vector
Exception at interrupt level:
Regs at 0x%x
Uninitialized vector %d
trcStack aborted: error in top frame
trcStack aborted: error in top frame
trcStack aborted: error in frame
%6x: %x (
<UUUUUU
?UUUUUU
/lj,D
UUUUU
?n L
v$K{
@Q0-
v<y5
=v<y5
?>UUUUU
ri7f>
?v<y5
?v<y5
UUUUU
?DR>
33333
NEJ(~
?>UUUUU
ri7f>
!	@|
!)@:F,@zj/@\G1@|
:@:F<@Z
=@zj?@L~@@\GA@l
?1cb
?LUUUUU
?IUUUUU
<cUUUUU
"mm?
?sS`
-Dt>
@ %z8
0123456789abcdef
0123456789abcdef
$CAAA==$A
'  L(  
 l'  
(  4
% TE  
% <G  
% 0H  $
% pH  4
I  l
`I  
<! |?! 
Q! ,?! 
E! <D! \G! 
FREE
DATA
HEADER
SOCKET
RTABLE
HTABLE
ATABLE
SONAME
ZOMBIE
SOOPTS
FTABLE
RIGHTS
IFADDR
CONTROL
OOBDATA
IPMOPTS
IPMADDR
IFMADDR
MRTABLE
0123456789
invalid input data were passed to avlInsertInform
ll# 
dl# 
\l# 
Tl# 
Ll# 
Dl# 
@l# 
8l# 
0l# 
$l# 
"$ 	
|"$ 
x"$ 
t"$ 
l"$ 
d"$ 
`"$ 
X"$ 
P"$ 
H"$ 
<"$ 
4"$ 
,"$ 
("$ 
$"$ 
"$  
"$ !
!$ "
!$ #
!$ $
!$ %
!$ &
!$ '
!$ (
!$ )
!$ *
!$ +
!$ ,
!$ -
!$ .
!$ /
t3$ 
K$ |K$ PK$ $K$ 
J$ tJ$ HJ$ 
	pksent
rttvar
ssthresh
sendpipe
recvpipe
expire
hopcount
GATEWAY
HOST
REJECT
DYNAMIC
MODIFIED
DONE
MASK_PRESENT	CLONING
XRESOLVE
LLINFO
STATIC
BLACKHOLE
b016
PROTO2
PROTO1
PRCLONING
WASCLONED
PROTO3
CHAINDELETE
PINNED
LOCAL
BROADCAST
MULTICAST
BROADCAST
DEBUG
LOOPBACK
RUNNING
NOARP	PPROMISC
ALLMULTI
OACTIVE
SIMPLEX
LINK0
LINK1
LINK2
MULTICAST
GATEWAY
NETMASK
GENMASK
AUTHOR
 #% 
% X#% |#% 
#% $
% 0$% 4
%% l
<4% 
HU	(
	CBIO_DEV_ID 0x%08lx is invalid per cbioDevVerify.
	CBIO_DEV_ID 0x%08lx ready changed is %d.
	BLK_DEV ptr 0x%08lx ready changed is %d.
Cached Block I/O Device, handle=%#lx
	Description: %s
Kbytes
Mbytes
Kbytes
Mbytes
Mbytes
Gbytes
	Disk size %ld %s, RAM Size %d bytes
	Block size %d, heads %d, blocks/track %d, # of blocks %ld
	partition offset %ld blocks, type %s, Media changed %s
Removable
Fixed
	Last error errno=%x, block=%ld
   Current ready changed bit for this layer and all subordinates:
CBIO to BLK_DEV Wrapper
cbioWrapBlkDev: BLK_DEV pointer 0x%08lx appears invalid.
Assertion failed: startBlock == pDev->cbioBlkNo, file cbioLib.c, line 2060
$i% tk% ,m% 
disk cache error: device %x block %d errno %x, %s
tDcacheUpd
disk removed while writing data, possible data loss
disk read failed
disk write failed, data loss may have occurred
dcacheCbio: dev=%#x cache internal error - starvation %d
CBIO Disk Data Cache - LRU
Disk Cache, %s:
Cached block numbers:
 blk %ld %c,
Total cache Blocks %d, %ld blocks (%%%ld) dirty
Tunable Params:
   Bypass Threshold %ld, Max Dirty %ld, Read Ahead %ld blocks, Sync interval %ld sec
Hit Stats: Cookie Hits %ld Miss %ld, 
Hash size %ld Hits %ld Miss %ld
   LRU Hits %ld, Misses %ld, Hit Ratio %%%ld
Write Sstats: Foreground %ld, Background %ld, Hidden %ld, Forced %ld
Subordinate Device Start:
Subordinate Device End:
	  total # of clusters:	
	   # of free clusters:	
	    # of bad clusters:	
	     total free space:	
     max contiguous free space:  
 bytes
		   # of files:	
		 # of folders:	
	 total bytes in files:	
	     # of lost chains:	
   total bytes in lost chains:  
 Entry will be deleted. 
"%s" is cross-linked on first cluster. 
Entry remains intact. 
"%s" is cross-linked on first cluster. 
Entry remains intact. 
"%s" is cross-linked on first cluster. 
"%s" directory has invalid structure.
"%s" is an illegal name. 
directory nesting limit reached, "%s" skipped
%s - Not enough room to run check disk.
%s  - disk check in progress ...
dosChkLib : 
CLOCK_REALTIME is being reset to %s
Value obtained from file system volume descriptor pointer: %p
The old setting was %s
Accepted system dates are greater than %s
 - lost chains 
%s  - Errors detected. To correct disk structure, please start check disk with a permission to repair.
Errors detected. All corrections stored to disk and lost chains recovered.
%s  - Volume is OK 
Change volume Id from %p 
to %p
"%s" too many clusters in file, adjusted.
"%s" cross-linked with another chain
"%s" has illegal cluster in chain
"%s" has illegal cluster in chain
"%s" file larger then its chain of clusters
"%s" has illegal start cluster
"%s" has illegal start cluster
"%s" has illegal start cluster
"%s" file larger then its chain of clusters
"%s" cross-linked with another chain
|||||||||||||||||||||||||||||||| !|#$%&'()|||-||0123456789||||||@ABCDEFGHIJKLMNOPQRSTUVWXYZ|||^_`ABCDEFGHIJKLMNOPQRSTUVWXYZ{|}~|
|||||||||||||||||||||||||||||||| !|#$%&'()|+,-.|0123456789|;|=||@ABCDEFGHIJKLMNOPQRSTUVWXYZ[|]^_`abcdefghijklmnopqrstuvwxyz{|}~|
NO LABEL
 - names style:			%s
8.3 STD DOS
VxLong
 - root dir start sector:		%u
 - # of sectors per root:		%u
 - max # of entries in root:		%u
 - root dir start cluster:		%u
VXEXT
VXEXT
dosDirOldLib.c : VxLong names
dosDirOldLib.c : DOS 8.3 names
dosDirOldLib.c : cluster size %d bytes is too small, min = %d
dosDirOldLib.c : Malformed volume format (FAT32: rootStartClust  = %u)
dosDirOldLib.c : Malformed volume format (FAT12/16: rootMaxEntries = 0)
dosFsFat.c : 1072 : %s : !!! DISK FULL !!!
FAT handler information:
------------------------
 - allocation group size:	%ld clusters
 - free space on volume:	
 bytes
Volume Parameters: FAT type: FAT%d, sectors per cluster %d
  %d FAT copies, %ld clusters, %ld sectors per FAT
  Sectors reserved %d, hidden %ld, FAT sectors %ld
  Root dir entries %d, sysId %-8s, serial number %lx
  Label:"%-11s" ...
VX5DOS32
VXDOS16
VXDOS12
VXEXT1.1
FAT32   
FAT16   
dosFsFmtLib: %s indicated by BPB FSTYPE string, cluster calculation was FAT12. Returning string.
FAT12   
dosFsFmtLib: %s indicated by BPB FSTYPE string, cluster calculation was FAT16. Returning string.
FAT32   
FAT12   
FAT16   
Retrieved old volume params with %%%d confidence:
Disk with %ld sectors of %d bytes will be formatted with:
dosFsVolFormat: bad format parameters, errno = %#x
dosFsVolFormat: format failed, errno=%#x
dosFsLib.c : Check disk utility not installed
dosFsLib.c : Malformed boot sector. Offset %u, value %u. %s
dosFsLib.c : cbioParams.bytesPerBlk cannot be zero.
dosFsLib.c : ERROR reading the device boot sector
dosFsLib.c : media not formatted or not present
dosFsLib.c : ERROR reading boot sector
At the end of boot sector
dosFsLib.c : bytesPerSec = 0
dosFsLib.c : cbioParams.bytesPerBlk %u != bytes-per-sec %u
dosFsLib.c : WARNING: num-sectors %u < cbioParams.nBlocks %u
dosFsLib.c : num-sectors %u > cbioParams.nBlocks %u
dosFsLib.c : secPerFat 12/16 = %u, while BPS = %u
dosFsLib.c : dosFsVolIsFat12 returned ERROR
FAT16   
WARNING: FAT16 indicated by BPB FSTYPE string, cluster calculation was FAT12. Honoring string.
FAT12   
WARNING: FAT12 indicated by BPB FSTYPE string, cluster calculation was FAT16. Honoring string.
(FAT32)
dosFsLib.c : Try to reclaim original copy of boot sector
dosFsLib.c : Problem finding volume data, trying to use the next block as boot block.
dosFsLib.c : Ensure this device is formatted and partitions are properly handled.
VXDOS4.0
VXEXT1.0
VXEXT
VXEXT
dosFsLib.c : No reading from write only device.
dosFsLib.c : Check disk utility not installed
dosFsLib.c : NULL CBIO_DEV_ID or BLK_DEV ptr
 Not A DOSFS Device
volume descriptor ptr (pVolDesc):	%p
cache block I/O descriptor ptr (cbio):	%p
auto disk check on mount:		
NOT ENABLED
%s | %s
DOS_CHK_ONLY
DOS_CHK_REPAIR
DOS_CHK_VERB_SILENT
DOS_CHK_VERB_1
DOS_CHK_VERB_2
max # of simultaneously open files:	%u
file descriptors in use:		%d
# of different files in use:		%d
# of descriptors for deleted files:	%d
# of  obsolete descriptors:		%d
can't mount volume
current volume configuration:
 - volume label:	%s ; (in boot sector:	%s)
NO LABEL
 - volume Id:		%p
 - total number of sectors:	
 - bytes per sector:		
 - # of sectors per cluster:	
 - # of reserved sectors:	
 - FAT entry size:		%s
FAT12
FAT16
FAT32
 - # of sectors per FAT copy:	
 - # of FAT table copies:	%u
 - # of hidden sectors:		
 - first cluster is in sector #	
 - Update last access date for open-read-close = %s
FALSE
TRUE
dosFsLib.c : 
 NULL handler descriptor ptr 
dosFsLib.c : 
 Unknown handler list 
dosFsLib.c : 
 Handler not installed 
|||||||||||||||||||||||||||||||| !|#$%&'()|||-||0123456789||||||@ABCDEFGHIJKLMNOPQRSTUVWXYZ|||^_`ABCDEFGHIJKLMNOPQRSTUVWXYZ{|}~|
|||||||||||||||||||||||||||||||| !|#$%&'()|+,-.|0123456789|;|=||@ABCDEFGHIJKLMNOPQRSTUVWXYZ[|]^_`abcdefghijklmnopqrstuvwxyz{|}~|
dosVDirLib.c : Bad long name structure (breached))
dosVDirLib.c : Bad long name structure (too long)
dosVDirLib.c : Malformed long name structure
dosVDirLib.c : Malformed long name structure
dosVDirLib.c : Bad long name structure
dosVDirLib.c : Erroneous long name
%c%u
dosVDirLib.c : Name is too long; use alias instead
NO LABLE
 - directory structure:		VFAT
 - root dir start sector:		%u
 - # of sectors per root:		%u
 - max # of entries in root:		%u
 - root dir start cluster:	%u
VXEXT
VXEXT
dosVDirLib.c : VxWorks proprietary long names not supported
dosVDirLib.c : cluster size %d bytes is too small, min = %d
dosVDirLib.c : Malformed volume format (FAT32: rootStartClust  = %u)
dosVDirLib.c : Malformed volume format (FAT12/16: rootMaxEntries = 0)
Radix %d  not supported
Radix %d  not supported
     
DDDDDDDDDD
AAAAAA
BBBBBB
%s: 
errno = %#x
%a %b %d %H:%M:%S %Y
TIMEZONE
TIMEZONE
(  seconds    nanosecs  freq (hz)  resolution
---------- ----------- ---------- ----------
  base ticks          base secs  base nsecs
--------------------  ---------- ----------
 %8.8ld   %9.9ld   %8.8d   %8.8d
 0x%08x%08x    %8.8ld   %9.9ld
Copyright 1984-2002 Wind River Systems, Inc.
This program contains confidential information of Wind River Systems, Inc.
and disclosure and copying are prohibited.
evnCreateHook: couldn't create private environment!
(global environment)
(private environment)
%d: %s
tExcTask
excTask: error receiving msg, status = %#x.
%d messages from interrupt level lost.
                0000000000000000
0123456789abcdef
(null)
0123456789ABCDEF
0123456789abcdef
bug in vfprintf: bad base
O8M2
(%-6.6s = %8x
%-6.6s = %8g
tLogTask
logTask: error reading log messages.
interrupt: 
%#x (): task dead
%#x (%s): 
<null "fmt" parameter>
logTask: %d log messages lost.
%3s %3s
%3s %3s
%3d %3d
(memPartAlloc: block too big - %d in partition %#x.
%s: invalid block %#x in partition %#x.
memPartRealloc
(memPartFree
No partId specified.
FREE LIST:
   num    addr       size
  ---- ---------- ----------
SUMMARY:
 status    bytes     blocks   avg block  max block
 ------ ---------- --------- ---------- ----------
current
   free %10u %9u %10u %10u
   no free blocks
  alloc %10u %9u %10u          -
   no allocated blocks
cumulative
  alloc %10u %9u %10u          -
   no allocated blocks
  invalid block at %#x deleted
  %4d 0x%08x %10u
  invalid block at %#x deleted
/\~$
selectInit: couldn't install task create hook!
selectInit: couldn't install create hook for the caller! 0x%x
selTaskDeleteHookAdd: couldn't install task delete hook!
_text
_data
_bss
_compiled.
(timerConHandler: bad timer %#x, signal %d
timerConHandler: expired %#x, signal %d
timerWdHandler: NULL timerid!
timerWdHandler: kill failed (timer=%#x, tid=%#x, errno=%#x)
task       timerid    evp        routine
---------- ---------- ---------- ----------
%#10x %#10x %#10x %#10x
dbgHelp                         Print this list
dbgInit                         Install debug facilities
b                               Display breakpoints and eventpoints
b         addr[,task[,count]]   Set breakpoint
e         addr[,eventNo[,task[,func[,arg]]]]] Set eventpoint
bd        addr[,task]           Delete breakpoint
bdall     [task]                Delete all breakpoints and eventpoints
c         [task[,addr[,addr1]]] Continue from breakpoint
cret      [task]                Continue to subroutine return
s         [task[,addr[,addr1]]] Single step
so        [task]                Single step/step over subroutine
l         [adr[,nInst]]         List disassembled memory
tt        [task]                Do stack trace on task
Task not found
Illegal Breakpoint Address: 0x%08x
Breakpoint table is full
Task not found
Illegal Eventpoint Address: 0x%08x
Eventpoint table is full
Task not found
No breakpoint at 0x%08x
 for task %#x (%s)
Task not found
Task not found
Task %#x not found
Task not found
Task %#x not found
Breakpoint table is full
Task %#x not found
Task not found
Task not found
Breakpoint table is full
Task %#x not found
Task %#x not found
   Task: %9s   Count: %2d
   Task: %#9x   Count: %2d
   (tgtsvr)
   (event)
   (temporary)
   (quiet)
No breakpoints
0x%08x: 
%-15s
+0x%-4x
%21s
Task %#x not found
Task %#x (%s) is unbreakable.
Break at 
   Task: %#x (%s)
%s restarted.
spawning new shell.
shell spawn failed!
			%s:
dbgList: no disassembler.
0x%08x
Task not found
Sorry, traces of my own stack begin at tt ().
Can't trace task %#x: invalid task id.
%6x 
%-15s+%-3x: 
                   : 
%s (
%x (
Unknown object module format 
Incorrect ELF header size: %d
Incorrect module type: %d
No program header table in executable module.
Null offset to program header table.
Incorrect program header size: %d
Incorrect section header size: %d
Null offset to section header table.
Section type SHT_DYNSYM not supported.
Section SHT_NOBITS ignored (wrong flags).
Section SHT_PROGBITS ignored (flags: %d).
Section SHT_NOBITS ignored (flags: %d).
Section of type %d ignored.
gcc2_compiled.
___gnu_compiled_c
__gnu_compiled_c
Can't add '%s' to symbol table
Undefined symbol: %s (binding %d type %d)
No relocation routine for this CPU
could not allocate text and data segments
Object module not loaded
Object module load failed
loadAoutLib error: can't add '%s' to system symbol table - error = 0x%x.
%s_text
%s_data
%s_bss
Can't add '%s' to symbol table.
VxWorks login: 
  %-15s
  User Name
  =========
Password: 
Login incorrect
Login timed out after %d seconds!
(%15s %#10x %10d %#10x %#10x %#10x
errno %#x
No free group number. Abort load operation.
Module %s, group %d added
MODULE NAME     MODULE ID  GROUP #    TEXT START DATA START  BSS START
--------------- ---------- ---------- ---------- ---------- ----------
Module not found
Can't get information about module %#x
Size of text segment:   %8d
Size of data segment:   %8d
Size of bss  segment:   %8d
Total size          :   %8d
Checksum error in segment type %d, 
module %#x (%s)
(tShell
  errno = %#x (%s)
  errno = %#x
shell restarted.
spawning new shell.
can't restart shell.
Unable to install Line EDitor interface
exit
logout
can't close output.
ambiguous output redirect.
can't create output '%s'
ambiguous input redirect.
can't open input '%s'
(%-12.12s %-10.10s %8x  %3d   %3d%% (%8d)  %3d%% (%8d)
%-12.12s %-10.10s %8s  %3s   %3d%% (%8d)  %3d%% (%8d)
spyClkInt: taskIdCurrent not ready.
Unable to add create/delete hooks.
No auxiliary clock on CPU.
NAME          ENTRY         TID   PRI   total %% (ticks)  delta %% (ticks)
--------     --------      -----  ---   ---------------  ---------------
KERNEL
INTERRUPT
IDLE
TOTAL
%d task%s created.
 was
s were
%d task%s deleted.
 was
s were
tSpyTask
Unable to spawn spyTask.
secs
millisecs
microsecs
timexHelp                      Print this list.
timex       [func,[args...]]   Time a single execution.
timexN      [func,[args...]]   Time repeated executions.
timexClear                     Clear all functions.
timexFunc   i,func,[args...]   Add timed function number i (0,1,2,3).
timexPre    i,func,[args...]   Add pre-timing function number i.
timexPost   i,func,[args...]   Add post-timing function number i.
timexShow                      Show all functions to be called.
Notes:
  1) timexN() will repeat calls enough times to get
     timing accuracy to approximately 2%.
  2) A single function can be specified with timex() and timexN();
     or, multiple functions can be pre-set with timexFunc().
  3) Up to 4 functions can be pre-set with timexFunc(),
     timexPre(), and timexPost(), i.e., i in the range 0 - 3.
  4) timexPre() and timexPost() allow locking/unlocking, or
     raising/lowering priority before/after timing.
timex: execution time too short to be measured meaningfully
       in a single execution.
       Type "timexN" to time repeated execution.
       Type "timexHelp" for more information.
timex: time of execution = %d +/- %d (%d%%) %s
timex: %d reps, time per rep = %d +/- %d (%d%%) %s
timex:
    pre-calls:
    timed calls:
    post-calls:
timex: call number must be in range 0..%d
        %d: 0x%x (
        %d: %s (
        %d: %s+%x (
0x%x
        (none)
(taskDeleteHookAdd of pthread deleteHook failed!
pthr
0123456789
  NAME        ENTRY        TID     SIZE   CUR  HIGH  MARGIN
------------ ------------ -------- ----- ----- ----- ------
????
text
data
help                           Print this list
ioHelp                         Print I/O utilities help info
dbgHelp                        Print debugger help info
nfsHelp                        Print nfs help info
netHelp                        Print network help info
spyHelp                        Print task histogrammer help info
timexHelp                      Print execution timer help info
h         [n]                  Print (or set) shell history
i         [task]               Summary of tasks' TCBs
ti        task                 Complete info on TCB for task
sp        adr,args...          Spawn a task, pri=100, opt=0x19, stk=20000
taskSpawn name,pri,opt,stk,adr,args... Spawn a task
td        task                 Delete a task
ts        task                 Suspend a task
tr        task                 Resume a task
d         [adr[,nunits[,width]]] Display memory
m         adr[,width]          Modify memory
mRegs     [reg[,task]]         Modify a task's registers interactively
pc        [task]               Return task's program counter
iam       "user"[,"passwd"]  	Set user name and passwd
whoami                         Print user name
devs                           List devices
ld        [syms[,noAbort][,"name"]] Load stdin, or file, into memory
                               (syms = add symbols to table:
                               -1 = none, 0 = globals, 1 = all)
lkup      ["substr"]         List symbols in system symbol table
lkAddr    address              List symbol table entries near address
checkStack  [task]             List task stack sizes and usage
printErrno  value              Print the name of a status value
period    secs,adr,args... Spawn task to call function periodically
repeat    n,adr,args...    Spawn task to call function n times (0=forever)
version                        Print VxWorks version info, and boot line
NOTE:  Arguments specifying 'task' can be either task ID or name.
Type <CR> to continue, Q<CR> to stop: 
hostAdd   "hostname","inetaddr"    - add a host to remote host table;
                                     "inetaddr" must be in standard
                                     Internet address format e.g. "90.0.0.4"
hostShow                           - print current remote host table
netDevCreate "devname","hostname",protocol
                                   - create an I/O device to access files
                                     on the specified host
                                     (protocol 0=rsh, 1=ftp)
routeAdd     "destaddr","gateaddr" - add route to route table
routeDelete  "destaddr","gateaddr" - delete route from route table
routeShow                          - print current route table
iam          "usr"[,"passwd"]      - specify the user name by which you
                                     will be known to remote hosts
                                     (and optional password)
whoami                             - print the current remote ID
rlogin       "host"                - log in to a remote host;
                                     "host" can be inet address or
                                     host name in remote host table
ifShow       ["ifname"]            - show info about network interfaces
inetstatShow                       - show all Internet protocol sockets
tcpstatShow                        - show statistics for TCP
udpstatShow                        - show statistics for UDP
ipstatShow                         - show statistics for IP
icmpstatShow                       - show statistics for ICMP
arptabShow                         - show a list of known ARP entries
mbufShow                           - show mbuf statistics
EXAMPLE:   -> hostAdd "wrs", "90.0.0.2"
           -> netDevCreate "wrs:", "wrs", 0
           -> iam "fred"
           -> copy <wrs:/etc/passwd   /* copy file from host "wrs" */
           -> rlogin "wrs"            /* rlogin to host "wrs" */
Type <CR> to continue, Q<CR> to stop: 
sorry, won't spawn task at PC = 0.
not able to spawn task.
task spawned: id = %#x, name = %s
Task not found.
%-12.12s %-12.12s
INTERRUPT
 %8s %5d %5d %5d %6d %s
SVC stack OVERFLOW
- SVC -
%-12.12s %-12.12s
 %8s %5d %5d %5d %6d %s
IRQ stack OVERFLOW
- IRQ -
%-12.12s
 %-12.12s
 %#-12.12x
 %-8x %5d %5d 
%5s %6s VX_NO_STACK_FILL
%5d %6d %s
OVERFLOW
Task not found.
Task not found.
Object not found.
Show routine of this object not configured into system.
Object not found.
Show routine of this object not configured into system.
Object not found.
Task not found.
sorry, the shell can't suspend itself.
Task not found.
Task not found.
sorry, the shell can't delete itself.
%s (for %s) version %s.
Kernel: %s.
Made on %s.
Boot line:
%08x:  %02x-
%08x:  %04x-
%08x:  %08lx-
%08x:  %08lx%08lx-
%08x:  %08x-
%08x:  
%*s 
  *%16s*
%08x:  
%02x
%04x
%08lx
%08lx%08lx
%02x
%*s 
  *%16s*
ld error: unable to open "%s"
ld error: too many symbols.
ld error: Module contains undefined symbol(s) and may be unusable.
ld error: error loading file (errno = %#x).
0x%08x %-25s %-8s
 (local)
mRegs: no such register %s
available registers:
%-6s: %02x - 
%-6s: %04x - 
%-6s: %08lx - 
%-6s: %08lx%08lx - 
%-6s: %02x - 
%-6s: %20g - 
%lf%1s
Error status symbol table not included (errno = %#x).
Unknown errno = %#x.
]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]
]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]
]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]
     ]]]]]]]]]]]  ]]]]     ]]]]]]]]]]       ]]              ]]]]         (R)
]     ]]]]]]]]]  ]]]]]]     ]]]]]]]]       ]]               ]]]]            
]]     ]]]]]]]  ]]]]]]]]     ]]]]]] ]     ]]                ]]]]            
]]]     ]]]]] ]    ]]]  ]     ]]]] ]]]   ]]]]]]]]]  ]]]] ]] ]]]]  ]]   ]]]]]
]]]]     ]]]  ]]    ]  ]]]     ]] ]]]]] ]]]]]]   ]] ]]]]]]] ]]]] ]]   ]]]]  
]]]]]     ]  ]]]]     ]]]]]      ]]]]]]]] ]]]]   ]] ]]]]    ]]]]]]]    ]]]] 
]]]]]]      ]]]]]     ]]]]]]    ]  ]]]]]  ]]]]   ]] ]]]]    ]]]]]]]]    ]]]]
]]]]]]]    ]]]]]  ]    ]]]]]]  ]    ]]]   ]]]]   ]] ]]]]    ]]]] ]]]]    ]]]]
]]]]]]]]  ]]]]]  ]]]    ]]]]]]]      ]     ]]]]]]]  ]]]]    ]]]]  ]]]] ]]]]]
]]]]]]]]]]]]]]]]]]]]]]]]]]]]]]
]]]]]]]]]]]]]]]]]]]]]]]]]]]]]       Development System
]]]]]]]]]]]]]]]]]]]]]]]]]]]]
 %s%s%s%s
]]]]]]]]]]]]]]]]]]]]]]]]]]]       
 version 
 %s%s
]]]]]]]]]]]]]]]]]]]]]]]]]]       KERNEL: 
]]]]]]]]]]]]]]]]]]]]]]]]]       Copyright Wind River Systems, Inc., 1984-2003
spy not configured into this system.
spy not configured into this system.
spy not configured into this system.
spy not configured into this system.
spy not configured into this system.
spy not configured into this system.
spyHelp                       Print this list
spyClkStart [ticksPerSec]     Start task activity monitor running
                                at ticksPerSec ticks per second
spyClkStop                    Stop collecting data
spyReport                     Prints display of task activity
                                statistics
spyStop                       Stop collecting data and reports
spy     [freq[,ticksPerSec]]  Start spyClkStart and do a report
                                every freq seconds
ticksPerSec defaults to 100.  freq defaults to 5 seconds.
spy not configured into this system.
cd: error = %#x.
copy: error writing file. errno %p
copy: error reading file after copying %d bytes.
Copy OK: %u bytes copied
Can't open input file "%s" errno = %p
Can't write to "%s", errno %p
---------
%c%9s
 %2d %-7d %-7d 
 %9lu 
%s %2d %02d:%02d 
%s %2d  %04d 
%s%c
Listing Directory %s:
error reading dir %s, errno: %x
error reading dir %s, errno: %x
Can't open "%s".
mv: destination "%s" not a directory
copying file %s -> %s
copying file %s -> %s
skipping directory %s
copying file %s -> %s
mv: destination "%s" not a directory
moving file %s -> %s
moving file %s -> %s
moving file %s -> %s
xcopy: error: destination "%s" is not a directory
copying file %s -> %s
copying file %s -> %s
copying dir %s -> %s
deleting file %s
deleting file %s
deleting directory %s 
Can't get stat on %s
Illegal attribute flag "%c", ignored
changing attributes on %s
changing attributes on %s
traversing directory %s to change attributes 
Couldn't open "%s".
"%s" formatting... 
Couldn't format "%s".
"%s" formatted... 
Couldn't initialize file system on "%s".
"%s" initialized.
Couldn't open file system on "%s".
Perhaps a dosFsVolFormat on the file system is needed.
Couldn't initialize file system on "%s".
"%s" initialized.
cd        "path"             Set current working path
pwd                            Print working path
ls        ["wpat"[,long]]    List contents of directory
ll        ["wpat"]           List contents of directory - long format
lsr       ["wpat"[,long]]    Recursive list of directory contents
llr       ["wpat"]           Recursive detailed list of directory
rename    "old","new"      Change name of file
copy      ["in"][,"out"]   Copy in file to out file (0 = std in/out)
cp        "wpat","dst"      Copy many files to another dir
xcopy     "wpat","dst"      Recursively copy files
mv        "wpat","dst"      Move files into another directory
xdelete   "wpat"             Delete a file, wildcard list or tree
attrib    "path","attr"    Modify file attributes
xattrib   "wpat","attr"    Recursively modify file attributes
chkdsk    "device", L, V     Consistency check of file system
diskInit  "device"           Initialize file system on disk
diskFormat "device"          Low level and file system disk format
"attr" contains one or more of: " + - A H S R" characters
"wpat" may be name of a file, directory or wildcard pattern
 in which case "dst" must be a directory name
chkdsk() params: L=0, check only, L=2, check and fix, V=0x200 verbose
Type <CR> to continue, Q<CR> to stop: 
boot device
host name
target name (tn)
file name
inet on ethernet (e)
inet on backplane (b)
host inet (h)
gateway inet (g)
user (u)
ftp password (pw)
ftp password (pw) (blank = use rsh)
unit number
processor number
flags (f)
startup script (s)
other (o)
%s(%d,%d)
%s(%d,%d)%s:%s
No boot parameter string specified.
'.' = clear field;  '-' = go to previous field;  ^D = quit
Error in boot line:
 %s=%d
 %s=0x%x
 %s=%s
%-*s: 0x%x 
%-*s: %d 
%-*s: 
%s%d
%-*s: 
invalid unit number.
%-*s: 
%-*s: 0x%x 
%-*s: %d 
invalid number.
too big - maximum field width = %d.
( PA
(SUN
SUNDAY
MONDAY
TUESDAY
WEDNESDAY
THURSDAY
FRIDAY
SATURDAY
JANUARY
FEBRUARY
MARCH
APRIL
JUNE
JULY
AUGUST
SEPTEMBER
OCTOBER
NOVEMBER
DECEMBER
%b %d %H:%M:%S:%Y
%b %d %Y
%H:%M:%S
%3s %9s  %9s  %9s  %9s  %9s  %9s  %9s
create
delete
open
close
read
write
ioctl
%3d %9x  %9x  %9x  %9x  %9x  %9x  %9x
%3s %-20s
name
%3d %-20s
%3s %-20s %3s
name
%3d %-20s %3d %s %s %s
(unknown)
%3d  %s
invalid number
invalid string
invalid char
yylex: invalid state %#x
%s: %s
invalid char
%s: ambiguous Ada identifier - Possibilities include:
char
short
long
float
double
undefined symbol: %s
undefined symbol: %s
bad assignment.
bad assignment.
not enough memory for new string.
not enough memory for new variable.
can't add '%s' to system symbol table - error = 0x%x.
new symbol "%s" added to symbol table.
%s + 0x%x
too many arguments to functions.
addArg: bad type.
funcCall: bad function type.
invalid application of 'address of' operator.
getRv: invalid rhs.
setLv: invalid lhs.
setLv: type conflict.
setRv: bad type.
0x%x
%d = 0x%x
 = '%c'
printRv: bad type.
: value = 
invalid lhs.
value = 
invalid rhs.
evalUnknown: bad evaluation.
operands have incompatible types.
operands have incompatible types.
typeConvert: bad type.
convUnknown: bad type.
yacc stack overflow
syntax error
typecast of lhs not allowed.
4* `
4* L
4* 8
5* (
* 85* 
* d5* 
5* l
* L6* X
* (7* @
8* (
* |8* 
* D9* 
* p:* 
:* l
* 4<* L
* `<* 0
Y* (;, 
P* PR* pS* ,T* TT* 
D_* 
f* 4_* \f* $_* 
^* @g* 
^* X
^*  
 + H!+ 
!+ !
(X]+ 4|+ H]+ 
|+ 4]+ 
|+ $]+ d}+ 
 n;^
Qkkbal
i]Wb
9a&g
MGiI
wn>Jj
#.zf
+o*7
(;, 
,;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
(;, 
h;, 
(;, 
(;, 
(;, 
,;, 
(;, 
(;, 
H=, 
h;, 
(;, 
(;, 
(;, 
h;, 
h;, 
h;, 
(;, 
(;, 
(;, 
h;, 
h;, 
h;, 
(;, 
(;, 
(;, 
h;, 
H=, 
h;, 
(;, 
(;, 
(;, 
h;, 
;, 	
H=, 
h;, 
(;, 
(;, 
(;, 
h;, 
H=, 
;, 	
h;, 
(;, 
(;, 
(;, 
:, 	
(;, 
(;, 
H=, 
X<, 
=, 	
:, 	
:, 	
8>, 	
:, 	
:, 	
t>, 	
S,  V, 
X, pY, 
Z, HZ, 
[, T\, p], 
^, x_, h
tRootTask
WIND version 2.6
	(Invalid message queue id: %#x
%-20s: 0x%-10x
Message Queue Id
%-20s: %-10s
Task Queuing
FIFO
%-20s: %-10s
Task Queuing
PRIORITY
%-20s: %-10d
Message Byte Len
%-20s: %-10d
Messages Max
%-20s: %-10d
Messages Queued
%-20s: %-10d
Senders Blocked
%-20s: %-10d
Receivers Blocked
%-20s: %-10d
Send timeouts
%-20s: %-10d
Receive timeouts
%-20s: 0x%x	%s
Options
MSG_Q_FIFO
MSG_Q_PRIORITY
				MSG_Q_EVENTSEND_ERR_NOTIFY
%s Blocked:
Senders
Receivers
   NAME      TID    PRI TIMEOUT
---------- -------- --- -------
%-11.11s%8x %3d %7u
Messages queued:
  #    address length value
%3d %#10x  %4d 
%02x
 ...
(BINARY
MUTEX
COUNTING
Invalid semaphore id: %#x
FIFO
PRIORITY
%-20s: 0x%-10x
Semaphore Id
%-20s: %-10s
Semaphore Type
%-20s: %-10s
Task Queuing
%-20s: %-10d
Pended Tasks
SEM_Q_FIFO
SEM_Q_PRIORITY
%-20s: %-10s
State
EMPTY
%-20s: %-10s
State
FULL
%-20s: %-10d
Count
%-20s: 0x%-10x
Owner
 Deleted!
 (%s)
%-20s: %-10s
Owner
NONE
				SEM_DELETE_SAFE
				SEM_INVERSION_SAFE
%-20s: 0x%-10x
State
				SEM_EVENTSEND_ERR_NOTIFY
%-20s: 0x%x	%s
Options
Pended Tasks
------------
   NAME      TID    PRI TIMEOUT
---------- -------- --- -------
%-11s%8x %3d %7u
0123456789
tRestart
  NAME        ENTRY       TID    PRI   STATUS      PC       SP     ERRNO  DELAY
---------- ------------ -------- --- ---------- -------- -------- ------- -----
%-6s = %8x
Task not found.
Task not found.
stack: base 0x%-6x  end 0x%-6x  size %-5d  
high %5s  margin %5s
high %-5d  margin %-5d
options: 0x%x
%-11.11s
%-12.12s
%-12x
 %8x %3d %-10.10s %8x %8x %7x %5u
taskRegsShow: invalid task id %#x
%17s
READY
DELAY
DELAY+S
PEND
PEND+T
PEND+S
PEND+S+T
SUSPEND
DEAD
0x%02x
VX_SUPERVISOR_MODE  
VX_UNBREAKABLE      
VX_DEALLOC_STACK    
VX_FP_TASK          
VX_DSP_TASK         
VX_STDIO            
VX_ADA_DEBUG        
VX_FORTRAN          
VX_PRIVATE_ENV      
VX_NO_STACK_FILL    
workQPanic: Kernel work queue overflow.
VxWorks Events
--------------
Events Pended on    : Not Pended
Received Events     : 0x%x
Options             : N/A
Events Pended on    : 0x%x
Received Events     : 0x%x
Options             : 0x%x	
EVENTS_WAIT_ALL
EVENTS_WAIT_ANY
				EVENTS_RETURN_ALL
				EVENTS_KEEP_UNWANTED
VxWorks Events
--------------
Registered Task     : NONE
Event(s) to Send    : N/A
Options             : N/A
Registered Task     : 0x%x	(%s)
Event(s) to Send    : 0x%x
Options             : 0x%x	
Deleted!
EVENTS_OPTIONS_NONE
EVENTS_SEND_ONCE
				
EVENTS_ALLOW_OVERWRITE
				
EVENTS_SEND_IF_FREE
 L-  L- 
L-  L- 
, webserver
Jun  6 2006
 M- 
(T=AL N=33 E=N
T=AL N=33 E=N
T=AL N=33 E=N
T=AL N=33 E=N
T=AL N=6 E=N
T=AL N=14 E=N
T=AL N=6 E=N
T=AL N=14 E=N
T=AL N=6 E=N
T=AL N=14 E=N
T=AL N=6 E=N
T=AL N=14 E=N
|R- 
|K/ 
hR- 
$T- 
\R- 
lI/ 
PR- 
$T- 
@R- 
$T- 
0R- 
$T- 
(R- 
$T- 
$T- 
$T- 
R- 	
$T- 
$T- 
$T- 
$T- 
$T- 
$T- 
$T- 
$T- 
$T- 
$T- 
|Q- 
$T- 
pQ- 
$T- 
dQ- 
$T- 
TQ- 
$T- 
DQ- 
$T- 
4Q- 
$T- 
$Q- 
$T- 
$T- 
"4	(
$T- 
$T- 
64	(
$T- 
$T- 
$T- 
P-  
$T- 
P- !
$T- 
P- "
$T- 
P- #
$T- 
P- $
$T- 
P- %
$T- 
P- &
$T- 
P- '
$T- 
xP- (
$T- 
lP- )
$T- 
dP- *
$T- 
XP- +
$T- 
LP- ,
$T- 
@P- -
$T- 
0P- .
$T- 
 P- /
$T- 
P- 0
$T- 
P- 1
$T- 
P- 2
$T- 
O- 3
$T- 
O- 4
$T- 
O- 5
$T- 
O- 6
$T- 
O- 7
$T- 
O- 8
$T- 
O- 9
$T- 
O- :
$T- 
pO- ;
$T- 
\O- <
$T- 
PO- =
$T- 
<O- >
$T- 
(O- ?
$T- 
O- @
$T- 
O- A
$T- 
O- B
$T- 
O- C
$T- 
N- D
$T- 
N- E
$T- 
N- F
$T- 
N- G
$T- 
N- H
$T- 
N- I
$T- 
N- J
$T- 
N- K
$T- 
N- L
$T- 
tN- M
$T- 
hN- N
$T- 
XN- O
$T- 
PN- P
$T- 
HN- Q
$T- 
<N- R
$T- 
0N- S
$T- 
$N- T
$T- 
N- U
$T- 
N- V
$T- 
N- W
$T- 
M- X
$T- 
M- Y
$T- 
M- Z
$T- 
M- [
$T- 
M- \
$T- 
M- ]
$T- 
M- ^
$T- 
M- _
$T- 
M- `
$T- 
M- a
$T- 
M- b
$T- 
xM- c
$T- 
pM- d
$T- 
hM- e
$T- 
`M- f
$T- 
XM- g
$T- 
PM- h
$T- 
HM- i
$T- 
8M- j
$T- 
(M- k
$T- 
Invalid
NEXT
COMMIT
UNDO
apple.wrs.com
System message
debug.txt
D/. 
D/. 
D/. 
D/. 
D/. 
D/. 
D/. 
D/. 
.. 	
8@. 
8C. 
\G. 
 I. 
pE. 
 I. 
hN. 
tL. 
tL. 
<|. 
4|. 
(|. 
t{. 
l{. 
`{. 
X{. 
P{. 
H{. 
@{. 
P|. 
L|. 
H|. 
D|. 
publicWMB
httpRpmWmbPost errno = %d
$f2 
 f2 
.@_,:;?!/*#"'~%&$()<>+-=.@_,:;?!/*#"'~%&$()<>+-=
20191231
(r0-r14    [task]                Display a register of a task
cpsr      [task]                Display cpsr of a task
psrShow   value                 Display meaning of psr value
nzcvift
USER32
FIQ32
IRQ32
SVC32
ABORT32
UNDEF32
SYSTEM32
------
0x%lx
,%s 
,RRX
,RRX
,%s 
#%ld
#%ld
p%d,
0x%lx
c%d,
c%d,
c%d,
p%d,
0x%lx
c%d,
c%d,
p%d,
c%d,
SDEP
SDEP
#%ld
#0.5
#0.5
CMFE
CNFE
SMLAL
UMLAL
SMULL
UMULL
cpsr
cpsr
spsr
spsr
cpsr
spsr
_%s,
Undefined Instruction
Undefined Instruction
0x%lx
EQUD    
EQUD    
0x%lx
 ; (?)
 ; (?)
0x%x
%08x  %08x  
Wrong relocation entry size.
Wrong relocation entry size.
Unknown relocation entry type.
Unsupported relocation type %d
Unsupported relocation type %d
Unknown relocation type %d
Relocation value does not fit in 26 bits.
Relocation value's lowest 2 bits not zero.
Relocation value does not fit in 23 bits.
Relocation value's lowest bit is not zero.
Relocation value does not fit in 9 bits.
Relocation value's lowest bit is not zero.
Relocation value does not fit in 12 bits.
Relocation value's lowest bit is not zero.
r11/fp
r12/ip
r13/sp
r14/lr
cpsr
: PW
: |y
: 4"
: D 
: to
: ,v4 
:  o
: 00
: l/
: (T3 
: xP3 
: ,Q3 
: XS3 
: 0V3 
: LW3 
: HX3 
: PY3 
: DU3 
: 8S
: hS
: 4R
: TQ
: D.
: $Q
: xQ
: LY
: |P
: pO
:  N
: tN
: hm
: dZ
: DU
: ls3 
: Lx3 
: px3 
:  {3 
: L9
: lb
: p@
: ,!
: 8-
: <.
: x-
: |,
: `0
: x3
: P+
: |*
: @,
: <6
: xh3 
: L[4 
: t[4 
: `[4 
: D,
: `G
: Xo
: <2
: pe
: dJ
: PF
: ,H
: df4 
: @"
: h6
: 8;
: T-
: (b
: ,Z
: dY
:  m
: dn
: lo
: 8s
: 0c
: (x
: P{
: L!
: X	
: ,d
: X'	(
:  	
: p,
: p|4 
: dt4 
: Lp4 
: $_3 
: 0A
: 4g3 
: (0
: DP4 
: `K4 
: ,/
: \,
: \n4 
: X%
: D#
: 0#
: P'
: 0v
: <(
: <1/ 
: (2/ 
: 81/ 
: x+
: @N4 
: dH4 
: @Z4 
: 4#4 
:  E4 
: T/
: `Y
: @c3 
: x`3 
: 4(
: \z
: H$	(
: xl
: h	
: 4U
: TZ
: PI7 
: Hw
: (r
: Hu
: Da
: tp
: |}
: Ln
: <n
:  U7 
: hU7 
: XU7 
:  R7 
: `f
: `	
: ht
: X!
: 0j
: 0T
: 0i
: pC
: l%	 
: ,L	 
: P*
: pj3 
: @%
: 0^
: p^
: D_
: (W
: T]
: TZ
: ,G
: 8Q
: pQ
: LU
: hT
: pE
: HH
: 0N
: \K
: (O
: XL
: ,P
: D;
: X8
~: @
~: |
~: \
t~: 8
d~: 
T~: 
<~: 
,~: 
~: \
}: ,
}: T
|}: 
h}: 
\}: H
P}: P
D}: :
4}: <8
(}: 0	
}: H
|: Pc
|: |
x|: L<
l|: 
`|: 
P|: 
<|: 
,|: 
{: P
{: 8
{: (
{: d
{: d=
|{: (A
l{: 
X{: tK7 
D{: 
({: 
 {: 
z: t:
z: \;
|z: 
hz: 
\z: 
Hz: 
4z: Lt
 z: 
y: 8
y: l
y: h
y: D
ty: 
`y: \
Hy: H^
4y: d_
 y: 
x: H
x: x=
x:  ?
xx: t0
lx: 
Xx: 
Lx: 
@x: 4!
(x: `x
w: 8
w:  
tw: d
dw: 
Tw: H
Dw: 
0w: 
$w: ,
w: `
v: t
v: 4
|v: X
hv: <
Xv: 
Tv: 
@v: tL3 
,v: 0P3 
 v: 
u: <
u: (
xu: 8
lu: 
\u: 
Du: 
4u: @U	(
$u: 
u: d"
t: T1
t: >
t: 0
t: |*
xt: 
`t: 
Pt: l1
8t: 
 t: 
s: $R
s: |t
s: L
xs: T
ls: 4
`s: 
Ps: D
Ds: X
<s: 
0s: 4
 s: 
s: `g
r: x
r: p
r: H
r: h
lr: |
Xr: X
Lr: Tf
<r: lh
(r: `d
q: $
xq: T
hq: `
Pq: l
<q: 
,q: 
 q: 
q: D
p: X
p: 8
p:  
p: L
hp: 
Hp: 
$p: p
o: T
to: X
Po: 
,o: 0
o: d
ln: <
Ln: 
8n: 
(n: ha4 
m: xb4 
m:  
pm: 8
\m: 
Hm: 
0m: 
 m: 
m: l
l: l
l: |
l: |
l: ,
l: <
xl: 
hl: H
\l: 4
Ll: x
@l: 
4l: l
(l: @V
l: P
k: L9
k: H9
k: |
|k: 
hk: dk3 
Tk: 
@k: 
,k: xl3 
k: <l3 
j: \
j: \
j: D
j: p
j: l
j: l
Xj: 
Hj: t0
<j: 
0j: 
$j: 
i: D*
i: x
i: |z4 
i: (:
i: \
pi: 
di: <
Xi: 
Hi: 
8i: 
(i: `
i: t
h: H
h: $
ph: 
Xh: 
@h: 
,h: 0
h: h
hg: L
\g: 
@g: 
(g: 
g: \
f: X
f: `
f: lT
tf: 
df: 
Tf: 0
Df: 
0f:  
 f: 
e: p\
e: d[
e: H
e: l
te: 
de: ,0
@e: 
0e: 
d: LZ
d: @
ld: 
`d: 8
Pd: 
Dd: 
4d: 
(d: 
d: |
c: P
c: 0|
c: L
c: p]
|c: (]
lc: 
Xc: 
Dc: ,P
4c: P
(c: 
c: @
c: @
c: 4
b: pw
b: @
b: 8`
b: p
tb: 
Xb: \X
<b: 
 b: 
b: 08
a: @
a: 0
a: @\
|a: 
la: \
\a: 
Ha: 
8a: 
$a: 4
`: 4
`: P
|`: 
l`: 
\`: 
L`: 
<`: 
,`: xW
_: 4
_: |i
_: x
_: @W
x_: 
d_: X
X_: d
H_: 
<_: 
(_: H<
^: @5
^: T
^:  
|^: 
l^: 
\^: D
T^: 
@^: 
0^: 
 ^: $
]: 8
]: D
t]: 
d]: 8
X]: 
H]: 
4]: 
$]: 
]: T
]: hU
\: @	
\: T
x\: 
h\: 
X\: d
L\: 
<\: 
,\: 
\: ,
[: 0
[: Lx
p[: <
X[: 
D[: 
4[: 
$[: 
Z: 0b
Z: `q
pZ: 
`Z: 
LZ: 
4Z: 
 Z: 
Z: X
Y: 0
Y: <
tY: 
dY: 
TY: @
DY: x
4Y: 
$Y: 
X: @
xX: 
`X: 
PX: 
DX: X
8X: 8
 X: 4
X: L
W: x
xW: 
hW: D
TW: 
@W: 
(W: 
V: X
V: d
tV: d
`V: 
LV:  
8V: 
 V: |
U: 4
|U: 
tU: 
hU: 
\U: D
PU: \~
<U: <
0U: 
U: T
T: l
T: (
xT: 
dT: 
LT: 8
8T: p
(T: H
S: 4
S: d
S: 09
xS: xm3 
lS: L
\S: 
PS: 
<S: (
S: p
R: D
R: \d3 
R: x
R: H
R: 8
R:  
tR: `
dR: 
TR: 
DR: $
(R: L
Q: 4
Q: H
xQ: H<
lQ: 
\Q: D<
LQ: 
DQ: 
4Q: p
$Q: 4
P: T
P: `
tP: p
dP: @
XP: 
LP: t
@P: 
0P: 
 P: 
P: H
O: H
O: 8
O: 0q4 
|O: 
lO: 
dO: X*
LO: 
<O: @
(O: 
N: @w
N: L
|N: 
lN: Hj
XN: 
DN: 
0N: 
 N: 
M: x
tM: 0
`M: 
LM: 
8M: 
 M: 
L: 0
L: D
L: $	
L: h
L: `
xL: 
hL: x
\L: X
PL: 
DL: 
4L: ,Z
(L: 
L: (b
K: X
K: H
tK: 
`K: 
LK: 4
@K: 
0K: 
$K: 
J: $k
J: tn
pJ: 
XJ: 8n
@J: (o
(J: P
J: 0r
I: (
I: Lu
I: <s
tI: 8t
dI: <v
PI: 
DI: 
0I: 8
 I: \
I: X
H: Hp
H: (e
H: Pe
lH: Ht
XH: 
DH: $
4H: Lt
 H: 
G: @}
G: P}
pG: 
\G: 
DG: 
,G:  s
F: (t
|F: 
lF: L
`F: `{
TF: 
HF: 
8F: 
0F: 
$F: 
hE: x
PE:  
<E: d
,E: 
D: 40
D: <0
D: 80
D: X|. 
D:  
D: p
D: l
xD: T0
lD: hW	(
dD: 
XD: 
HD: 
0D: xV
D: \P
D: P"	(
D: (
C: P
C: ,
C: d
C: `r
hC: 
XC: |t
HC: 
0C: $w
C: X
B: @
B: hV
B: Xi
B: $k
xB: 
hB: 
XB: 
DB: 
,B: 
 B: 
A: 8q
A: (
A: (n
A: Pj
pA: 
`A: 
LA: v~
<A: x
 A: 
@: d
x@: 
d@: 
P@:  
H@: 
8@: 
(@: 0
@: \
?: ,
?: p
l?: 
X?: 
@?: 
(?: <
>: 0
p>: 
\>: 
H>: ,
,>: p
>: t
=: h
=: 8
x=: 
h=: D
P=: L
8=: 
$=: 
<: d
<: $
x<: (
d<: 
P<: 
8<: 
 <: 
;: `
;: 0
;: 8
p;: x
\;: $
H;: 
,;: h
:: L
:: x
:: t
h:: 
X:: (
H:: 
4:: 
 :: P
9: \
9: 4
9: D
9: l
9: L
p9: 
X9: 
H9:  
89: 
(9: 
9: D
8: `
8: T
8: (
l8: ,
T8: t
<8: $
(8: 
7: |
7: x
7: h
7: H
p7: 
\7: 0
H7: 
(7: 
7: x
6: ,
6: @
x6: 
h6: 
X6: 
H6: d
<6: 
 6: 0
5: $
5: `
5: H
p5: 
`5: 
P5: 
85: 
 5: 
4: d
4: \
x4: XS- 
l4: 
\4: 
P4: `
84: L
(4: 
4: t
3: 4d
3: $0
|3: 
h3: 
T3: <T
@3: P
,3: 
3: t
2: @
2: p
t2: 
`2: (
H2: 
42: 
$2: 
2: `
1: 4R5 
1: h_5 
l1: 
\1: x[5 
T1: d
H1: 
81: 
$1: 0
1: $
0: 0
0: 8
p0: |s5 
\0: 
L0: 
80: h
$0: `
0: 0'5 
p/: 
\/: 
D/: 
4/: X
 /: 
.: 4
.: `A5 
.: LD5 
l.: 
\.: 4
P.: 
<.: 
$.: 
-: (75 
-: T
x-: 
l-: T!7 
X-: P&5 
@-: 
,-: 0+7 
-: <,7 
,: l
,: $
|,: <
p,: x
`,: h07 
L,: 
8,: 
(,: 
+: h
x+: 
d+: 
P+: 
8+: L%5 
 +: @
+:  
*: h 5 
*: 0(7 
*: |
*: p	7 
t*: 
`*: `
L*: 
<*: 
,*: P
*: H		 
): 8
): T*
): 0
t): 
d): 
T): 
D): 8
4): 
(: x
(: |
l(: 
\(: 
D(: 
,(: T
(: |
': p
t': <
\': 
D': p
,': T
': 8
&: \
&: (/
t&: 
d&: ,
P&: 
@&: 0
4&: 
&: l
%: $
%: 4
%: x
%: X
x%: X
l%: $
X%: 
H%: 
8%: 0
(%: 
$: 4
$: H
x$: 
l$: 
\$: h
H$: 
0$: 
 $: 
$: h
#: $
#: TG
#: HJ
#: 8t# 
#: $u# 
l#: 
X#: tt# 
L#: 
<#: Pe
(#: |
": ,z
x": 
d": 
L": h
@": 
4": 
(": 
": 0
": L
!: L/
!: Xx
!: \m3 
!: ,
x!: 
l!: 
X!: 
H!: 06
8!: 
(!: 
!: pD
 : <<
 : @E
 : XD
 : X1
t : 
` : 
P : 
@ : P
, : 
 : <
 : x
: <?
: T9
: d@
: LB
: P5
: ,2
: `A
: dD
: |D
: ( 
: x&
: h-
: $7
: X,
:  >
: X5
: |C
: $;
: |"
: T/
: ,2
: 0W
: |%
: (Z
: XW
: Tu
: \n
: ,`
: t4
: t7
: HF
: @?
: t?
: $f
: `p
: P4
: L>
: d5
: 45
: x8
: (?
: d?
: 4H
: @X
: (}
: Xn
: xP
: lk
: $m
: ,i
: Lj
: (2
: <&
: Tf
: 4V
: 4W
: tY
: (4
:  g
: lO
: <d
: 0A
: P=
: h>
: l-
: hD
: |<
: HE
: T7
: PD
	: d3
	: t
x	: 
d	: 
P	: |B
@	: 
0	: 
: T:
: \D
: tD
: `5
: PE
: L6
: D#
: d-
: p 
: 4C
: h;
: D4
: (0
: ,1
:  9
: <J
: @L
: Dd
: \I
: TF
: ta
: ,G
: Le
: LI
: ${
: 0o
: Tz
: pz
: `n
: p|
: Hp
: 0}
:  w
: 0z
: 4~
: x}
: @-
9 L!
9 T/
9  f
9 <f
9 P_
9 P]
9 d`
9 4,
9 ,T
9 DV
9 XW
9 t%
9 HC
9 8B
9 T[
9 8S
9 X1
9 LM
9  L
9 pR
9 \.
9 `1
9 XK
9  X
9 xs
9 hs
9 @t
9 ds
9 P1
9 Th
9 Lr
9 dt
9 8Y
9 $I
9 Te
9 tB
9 (C
9 \A
9 `@
9 $-
9  )
9 hy
9 8(
9 @4
9 `{
9 H2
9 p1
9 p,
9  '
9 t+
9 ,,
9 |,
9 D;
9 0Y
9 xY
9 LG
9 TX& 
9 \+
9 8K
9  K
9 h+
9 |?
9 $K
9 ,K
9 4K
9 8C
9 p7
9 D?
9 H?
9 4a
9 0	
9 8+
9 D!
9 $H
9 dH
9 TB
9 L=
9 (g
9 Lh
9 H<
9   
9 (o
9 Dr
9 @@# 
9 $8# 
9 $@# 
9 @o
9 p@
9 4F
9 @3
9  4
9 h2
9 d`& 
9 @r& 
9 @{& 
9 `x& 
9 x~& 
9  ~& 
9 L~& 
9 t{& 
9 8?# 
9 l*
9 @G
9 PF
9 `E
9 pD
9  :
9 @8
9 09
9 xd
9 4p
9  "	(
9 `b
9  \
9 `$	(
9 pr
9 xr
9 `r
9 Xr
9 hr
9 Hr
9 Pr
9 Dp
9 hw
9 l}
9 4I
9 tI
9 he7 
9 4e7 
9   
9   
9 T:
9 ,"	(
9 @;
9 th	(
9 \5
9 l2
9 <Y
9 $&	(
9 HL
9 Dt
9 $!	(
9 4\
9 l$	(
9 ,5
9 (H
9 \h
9 ,>
9 DL
9 DH
9 P5
9 Pt
9 0\
9 Ht
9 @$	(
9  Q
9 (\
9 |h	(
9  b
9 d.! 
9 Po" 
9 D{) 
9 D[) 
9  F
9 0:( 
9 l%
9 <%
9 @c
9 Xz
9 (r, 
9 4u, 
9 ('
9 0 ! 
9 <"! 
9  A
9 H&
9 ,w
9 8}
9 $x
9 @z
9 \y( 
9 ty
9 @t
9 |f# 
9 `d# 
9 Th# 
9 0h# 
9 tb# 
9 8d# 
9 Lg# 
9 Lj# 
9 <k# 
9 X5
9 (5
9 (Y
9 8Y
9 (#
9 <P
9 t-
9  4
9 4T
9 |?! 
9 ,?! 
9 \G! 
9 <D! 
9 tI
9 T"
9 4"
9 ("
9 L"
9 <"
9 TU
9 @B
9 ,B
9 P0
9 |z
9 lM% 
9 HU	(
9 4N% 
9 <H% 
9 ,K% 
9 lL% 
9 TK% 
9 4I% 
9 8O% 
9 tf( 
~9 x
~9 H
~9 8
~9 X
l~9 
\~9 
H~9 
0~9 x
(~9 
~9 T"
}9 ,
}9 4
t}9 |K/ 
h}9 
`}9 
T}9 
H}9 
<}9 
0}9 
$}9 
}9 T
|9 D
|9 T
p|9 
d|9 
X|9 
H|9 (1, 
@|9 \
,|9 |1, 
|9 X
{9 0
{9  z
{9 8
|{9 
h{9 H
\{9 
P{9 
D{9 
<{9 hW$ 
0{9 H
z9 8
z9 p
z9 X
hz9 
Lz9 <
0z9 T
y9 P
y9 |
y9 @
y9 l
ty9 
\y9 
Dy9 
4y9 
$y9 XB
x9 ,
x9 @
x9 l
px9 
`x9 
Dx9 
(x9 
x9 H
w9  
|w9  
hw9 $
Pw9 
8w9 D
 w9 x
tv9 
\v9 L
Dv9 
(v9 D
v9 t
u9  
u9 L
u9 x
hu9 
Pu9 
8u9 h
 u9 @0
t9 T(
t9 @)
xt9 p'
`t9 
Ht9 
0t9 `2
t9 L2
t9 L5
|s9 
ds9 
Ps9 
<s9 4;
$s9 $<
r9 P
r9 D
lr9 
Pr9 
8r9 
 r9 
r9 HJ
q9 ,J
tq9 ,A
\q9 L@
Lq9 
0q9 
q9 $6
p9 l.
lp9 0.
Tp9 
@p9 
,p9 
o9  M
o9 X
o9 L
o9 4
to9 
ho9 
 o9 
Tn9 
<n9 
$n9 l
n9 @
m9 4
|m9 
hm9 
Tm9 x
Lm9 lh( 
@m9 
 m9 8{, 
l9 \l, 
l9 p
xl9 
tl9 x
ll9 T
dl9 
`l9 Hq( 
Pl9 
@l9 
4l9 
$l9 TJ
l9 p
k9 l
k9 @c7 
|k9 
lk9 
Xk9 TN
Dk9 
4k9  b7 
 k9 `
j9 l_
j9 (_
j9 @g7 
pj9 ,
Xj9 
@j9 X
(j9 
i9 `
i9 4
ti9  R	 
Pi9 
(i9 TU	 
i9 <'	 
h9 XH
lh9 D
Th9 
Dh9 
4h9 
,h9 x
 h9 0
g9 0
g9  
tg9 
dg9 
Hg9 t
Dg9 \O( 
8g9 
,g9 
 g9 @
f9 L
f9 T
f9 D
f9 (&	(
tf9 
df9 8
Xf9 
Lf9 
<f9 dz
,f9 4=
 f9 
e9 Db
xe9 
he9 
\e9 
Pe9 
<e9 PX
4e9 
$e9 
d9 @
d9 X
d9 t_% 
d9 <r% 
xd9 Dy% 
ld9 Hx% 
\d9 
Dd9 
,d9 
c9  
pc9 
Hc9 |
 c9 x1	 
b9 h
b9 $/	 
b9 d
b9 h
b9 l
tb9 p
hb9 p
Tb9 
<b9 
b9 P>
a9 LW	 
da9 
4a9 $Z	 
,a9 
 a9 
a9 0
`9 hw! 
`9  
`9 4
p`9 8
``9 t,
P`9 
D`9 
4`9 @>
$`9  U	(
_9 `w
_9 D
_9 x
p_9 4
`_9 `!	(
P_9  8
@_9 p
4_9 
 _9 
^9 $
^9  
^9  w
^9 @K
^9 @
p^9 \
\^9 
L^9 
<^9 |
(^9 
^9 4
]9  5
]9 X
]9 <
x]9 
h]9 
X]9 l
H]9 
<]9 H
0]9 
$]9 
\9 Ha
\9 |X
d\9 
@\9 
,\9 XU
\9 <V
[9 0H
x[9 
l[9 w
h[9 
`[9 x
X[9 
L[9 
@[9 P
4[9 l
,[9 
$[9 
[9 <
Z9 |
Z9 (,
|Z9 
Z9 T
Y9 L
X9 (
`X9 P$
PX9 p
tW9 
V9 x
V9 p
V9 x
V9 t
V9 4
lV9 (
\V9 
DV9 
8V9 (
,V9 
V9 D
U9 0
U9 d#& 
U9 ,
tU9 
dU9 t
PU9 D)& 
DU9 pc( 
(U9 
T9 H
T9 @
pT9 
\T9 
LT9 D
8T9 
(T9  
T9 8U& 
T9 @0
S9 0
S9 TJ
S9 HJ
S9 4J
S9  
S9 P&	(
S9 L
tS9 
dS9 
XS9 @
LS9 
<S9 
,S9 
 S9 D
S9 4
R9 X
R9  
tR9 
\R9 
@R9 h
Q9 \
Q9 ,
Q9 8
Q9 8
pQ9 H
dQ9 
TQ9 
LQ9 
4Q9 \
Q9 H
Q9 8
P9 X
xP9 
pP9 
XP9 
DP9 
0P9 
P9 |
O9 X
O9 X 	 
lO9 l
LO9 0
<O9 
0O9 
O9 @
N9 l
pN9 h
PN9 T
0N9 D
N9 x8
M9 X
pM9 
dM9 
\M9 
HM9 
4M9 `8
(M9 
M9 D
M9 0x, 
L9 (y, 
XL9 
TL9 p
HL9 
8L9 4
,L9 t
K9 <
K9 d<
K9 `<
|K9 
hK9 (H
TK9 
<K9 
,K9 xF
K9 ,K
J9 lH
J9  :
|J9 p?
dJ9 (#
PJ9 
DJ9 
(J9 
I9 Hj
I9 4t
xI9 
hI9 
PI9 
8I9 
H9 ,s
H9 ,u
lH9 Tv
PH9 hr
4H9 
H9 $r
G9 Xp
G9 p
G9 p
hG9 
XG9 
LG9 
0G9 
F9 4
F9 x
F9 ,
F9 X
pF9 $
`F9 
PF9 
@F9 
0F9 l
F9 0)
F9 @N
E9 0L
E9 lO
E9 xQ
E9 PP
E9 dZ" 
tE9 
hE9 
\E9 
LE9 
<E9 
(E9 
E9 $L
E9 ,N
D9 8L
D9 <K
pD9 
\D9 4
PD9 
<D9 
(D9 
 D9 <
C9 Xw	 
C9 `
xC9 
lC9 
\C9 
LC9 ,
@C9 
8C9 $
(C9 d
B9 D
B9 n
B9 h
B9 |
xB9 
hB9 Ly$ 
TB9 
HB9 p
<B9 @
0B9 
 B9 
B9 T
A9 4
A9 l
xA9 
dA9 
XA9 d
LA9 
8A9 
,A9 `
A9 8
@9 |(
@9 @(
t@9 
h@9 
`@9 t
P@9 
@@9 
4@9 (
(@9 
@9 Lb
|?9  J
t?9 
X?9 
P?9 
@?9 
,?9 
 ?9 x
>9 4
>9 h<
l>9 
P>9 
<>9 `k
(>9 
>9 @F
=9  v
p=9 
X=9 
@=9  
,=9 
<9 @
<9  !	(
<9 @!	(
<9 `
l<9 
P<9 `=
@<9 `t
0<9 
(<9 X
;9 T
x;9 
h;9 
X;9 X
H;9 
8;9 
$;9 Hy
:9 $
l:9 X}
X:9 
D:9 
0:9 
 :9 
:9 T
99 D
h99 ,
P99 
<99 
(99 
89 4t
x89 `\
\89 l]
D89 H^
089 
89 ,`
79 \
79 t
79 h
x79 L
`79 
T79 
D79 P[
,79 
79 Lb
69 p
69 XK
69 tK
69 0{
|69 ,
d69 `
L69 
869 
$69  r
69 <Z
69 XZ
59 tZ
59 T`
d59 
H59 $
059 
59 L
t49 8
`49 H
L49 
849 
 49 (
39 PZ& 
39 0
39 <[& 
39  K
|39 
t39 
l39 @]& 
d39 
X39 "
P39 
D39 "
<39 
439 <^& 
,39 
39 $
29 L
29 \
29 <
29 @
29 t
t29 
d29 
T29 
@29 
829 
$29 
19 D
19 ,h, 
p19 
419 
$19 
09 m
09 0Y
09 X
p09 
`09 tY
P09 DZ
@09 
409 
 09 
09 (
|/9 
h/9 
\/9 8
T/9 D
H/9 @
@/9 
8/9 Xa& 
(/9 
/9 p
.9 ,Y
.9 DU	(
.9 <
|.9 
t.9 
h.9 
X.9 
H.9 
8.9 
(.9 
.9 ,
-9 Xb& 
-9 `
h-9 <j, 
P-9 
,-9 Dk, 
-9 ,
,9 P
t,9 h
h,9 d
X,9 
L,9 L
8,9 `
,,9 x
,9 <
+9 (g& 
+9 (
+9 @
+9 $
+9 ,z
l+9 8P
\+9 
H+9 
4+9 pM
$+9 
*9 $N
*9 <
*9 P
*9 `
|*9 
p*9 
\*9 
P*9 t
8*9 
,*9 x
 *9 
*9 <
)9 8
)9 X
|)9 
h)9 
L)9 
0)9 
$)9 \
)9 `
)9 $y
(9 `8
(9 lw
(9 $z
(9 Dw
x(9 
h(9 
T(9 
H(9 
4(9 
$(9 
(9 P
(9 L
'9 \
'9 d
'9 Hd
'9 @
'9 `
'9 H
t'9 
d'9 `4
L'9 H
<'9 (
4'9 
 '9 
'9 pz
&9 X>
p&9 
d&9 
T&9 
H&9 
<&9 
0&9 hu
 &9 
&9 0Y
%9 06
%9  
|%9 
p%9 (
`%9 
P%9 
D%9 
8%9 
0%9 
$%9 
%9 H
%9 Y~
$9 @
$9 `H
x$9  
h$9 
X$9 hi
D$9 0
4$9 0
$$9 X4
$9 Pw
#9 @I
#9 @i	(
p#9 
`#9 
L#9 
8#9 
(#9 
"9 (
"9 h
"9 0
p"9 Z~
T"9 p
@"9 
("9 
"9 u~
!9  
!9  W	(
!9 0
!9 |
l!9 @u
X!9 
D!9 `F
0!9 @8
!9 `W	(
 9 P
 9 pV
 9 (
t 9 
` 9 
T 9 
H 9 p
0 9 (
9 @b
9 h4	(
9 @d
9 hV
9 pF
9 @Y
9 xh	(
9 p>
9 |,
9 @3
9 `h	(
9 `~
9 HW
9 p$	(
9 `>
9 hz
9 pb
9 HJ
9 tJ
9 T{
9 t~
9 HF
9  R
9 T;	 
9 t+	 
9 dh	 
9 (|	 
9 ,C	 
9 L;	 
9 xH	 
9 D2	 
9 xh	 
9 $0	 
9 4b
9 x0
9 HW
9 \p& 
	9 \
	9 8
	9 ,A% 
|	9 
p	9 
`	9 p@% 
P	9 |
D	9 dC
<	9 |4% 
0	9 x
$	9  
	9  q& 
	9  
9 H"	(
9 0I
9 Xh
9 `u
9 @"	(
9 0y
9 ( $ 
9 \x
9 H3
9 8{
9 `;
9 PK
8 HT/ 
8 xQ2 
8 pS2 
8 <V2 
8 ()/ 
8 D?/ 
8 xO7 
8 TP/ 
8 8Q/ 
8 4P/ 
8 dP/ 
8 \W/ 
8 ,W/ 
8 $	/ 
8 h5/ 
8 ,f2 
8 `W2 
8 TU2 
8 $h2 
8 l'/ 
8 (_2 
8 h(/ 
8 p+/ 
8  4/ 
8 d3/ 
8 x3/ 
8 04/ 
8 ``2 
8 T`2 
8 t_/ 
8 ,`/ 
8 $\/ 
8 4\/ 
8 0[/ 
8 p`/ 
8 |[/ 
8 P[/ 
8 4?/ 
8 $?/ 
8 DZ/ 
8  s/ 
8  6/ 
8 T]2 
8 Xe2 
8 <?/ 
8 L[2 
8 l[2 
8 ,[2 
8 `F/ 
8 dH/ 
8 PH/ 
8 `h
8 L]/ 
8 L?/ 
8 X@/ 
8 ,?/ 
8 Ln
8 4g
8 (i
8 Xh
8 `m
8 0p
8 ,m
8 8i
8 T+
8 T*
8 `1
8 $!
8 t\$ 
8 ph$ 
8 d'" 
8  ;
8 , 
8 hg
8 tb
8 Lc
8 L0
8 h|
8 lj
8 P~
8 @W
8 L1	 
8 (W
8 0H
8 |@% 
8 tl# 
8 xF
8 tj
8 Tj
8 <f
8 4j
8 xe
8 |k
8 pk
8 X~( 
8 L6! 
8 \6! 
8 `3
8 X&	(
8 T{* 
8 `S
8 @l
8 tX& 
8 @Q
8  &	(
8 0&	(
8 4Y& 
8 $"
8 LY& 
8 `R
8 dY& 
8 t3
8 @p
8 T5
8 jp3 
8 !n3 
8 4y
8 hw
8 .#
8 <$
8 8#
8 l?* 
8 |b
8 qE
8 H0
8 4d
8  d
8 ,e
8 <c
8 he
8 Lc
8 @h	(
8 4q( 
8 8X
8 PS
8 (T
8  q( 
8 @;" 
8 h " 
8 D!" 
8  1" 
8  2" 
8 (4" 
8 D(" 
8 ,=" 
8 \@" 
8 |B" 
8 D', 
8 4	, 
8 05, 
8 t&
8  I
8 d'
8 tf
8 v_
8 `6
8 @)	 
8 (b	 
8 |+' 
8 D / 
8 4"/ 
8 8(' 
8 $$' 
8 d!' 
8 d_. 
8  Z. 
8 |a. 
8 TY. 
8 D,' 
8  }
8  h	(
8 pO
8 ,M
8 |L
8 `g( 
8 `*
8 T*
8 x*
8 $*
8 p*
8 h*
8 Hu
8 \u
8 di
8 Pu
8 4x
8 tW
8 LX
8 0X
8 Lt
8 d6
8 lH- 
8 pH- 
8 dY
8 l;
8 x;
8 |$
8 lO
8 lQ
8 TQ
8 `Q
8 xQ
8 P72 
8 `72 
8 x92 
8 (92 
8 \%2 
8 t72 
8 082 
8 p82 
8 p`" 
8 `G" 
8 LJ" 
8 lK" 
8 pc" 
8 db" 
8 LF" 
8 LV" 
8 pY" 
8 |N" 
8 HN" 
8 $g" 
8 Ph" 
8 Ts" 
8 |r" 
8 \T" 
8 <u" 
8 xD( 
8  !% 
8 |!% 
8  d
8 l+
8 <8
8 lu
8 \)
8 t=
8  ?
8  W
8 `<
8 $m$ 
8 (;, 
8 $3' 
8 83' 
8 x1' 
8 D0
8 h}
8 8o, 
8 Xy
8  b
8 8f
8 `O
8 dG
8 8h
8 H<
8 p"
8 HU
8 <c
8 Xw
8  x
8 8x
8 Px
8 hx
8 |v
8 tq
8 8r
8 4q
8 \z
8 t{
8 H9
8 T:
8 Hl
8 Lz
8 h{
8 H~
8 Dz
8 D|
8  u
8 `z
8 `W
8 d8
8 `'# 
8 8&# 
8 t'# 
8 db, 
8 $g, 
8 dm, 
8 0{
8 88' 
8 l3' 
8 L8' 
8 HG( 
8 @E( 
8 ds& 
~8 4
~8 l
h~8 
P~8 @
<~8 
$~8 
~8 4
}8 l
}8 $
}8 \
p}8 
P}8 
,}8 H
|8 `
|8 T
h|8 
H|8 
,|8 
|8 l
{8 `
{8 t
{8 H
{8 l
t{8 
`{8 
H{8 
0{8 l<
z8 P>
z8 $>
tz8 $
Xz8 
Dz8 H=
0z8 
y8 t=
y8 P
py8 
Ty8 8
<y8 d
$y8 
x8 0
|x8 
dx8 
Hx8 D
,x8  
x8 T
w8 (
xw8 L
`w8 x
Dw8 
(w8 p
w8 |
v8 l
v8 @
v8 |>
|v8 
dv8 
Pv8 
8v8 
u8 \
u8 (f
|u8 
hu8 Tf
Hu8 
0u8 
u8 @
t8 L
pt8 
Xt8 
@t8 ,
0t8 d$
 t8 
s8 ,
s8 x
s8 P
ls8 4
Ts8 t
<s8 
(s8 P
r8 8
r8 $w) 
r8 D%) 
lr8 p%) 
Xr8 
@r8 
(r8 ,() 
q8 T
q8 \3) 
lq8 l)) 
\q8 
<q8 8/) 
,q8 ,*) 
p8 @
|p8 
dp8 
Hp8 
,p8 
p8 x=) 
o8 \>) 
o8 x@) 
xo8 TA) 
`o8 p8) 
Lo8 
@o8 
0o8 
o8 (J) 
n8 <M) 
n8 PM) 
n8 ,N) 
xn8 $U) 
hn8 PZ) 
Xn8 0
8n8 `i) 
n8 `j) 
m8 tx) 
xm8 T
dm8 
Dm8 
,m8 H
m8 t
l8  
l8 \
l8 X|) 
l8 0x) 
l8 dx) 
tl8 
dl8 X}) 
Ll8 
4l8 
 l8 Lc) 
l8 (
k8 h
k8 \
k8 t
k8 \
|k8 tv) 
hk8 Tv) 
Pk8 
8k8 
(k8 @
k8 l
j8 8
tj8 
\j8 `
@j8 0
0j8 h
j8 4
i8 L
i8 x
i8 x
ti8 
`i8 l
Ti8 
Di8 
0i8 
$i8 8
i8 h>
i8 `
h8 d
h8 $
dh8 
Xh8 
Ph8 X
Dh8 P
8h8 
,h8 
 h8 0
h8 89' 
h8 $:' 
g8 <
g8 l
g8 \
g8 8(	 
Xg8 
Pg8 l
Dg8 `
4g8 
$g8 
f8 xc
f8 Px
f8 8u
pf8  z
Xf8 
@f8 
4f8 |n
,f8 
$f8 
e8 P
e8 ,
e8 L
xe8 
le8 <s
\e8 
Le8 
@e8 
4e8 Xr
$e8 <c
e8 l
d8  
d8  
d8 x
xd8 
td8 `
dd8 
Ld8 
4d8 
$d8 $
d8 ,
xc8 8
`c8 `
Hc8 <
0c8 
c8 t8+ 
b8 t9+ 
b8 `
b8 0-+ 
|b8 pA+ 
db8 
Pb8 
8b8 8
$b8 H
a8 L
a8 T
a8 |9
a8 x9
pa8 
Xa8 
La8 
4a8  
a8 x
a8 \-+ 
`8 L
`8 x.+ 
t`8 p/+ 
\`8 |
D`8 x
4`8 <
`8 <
_8 @ 
t_8 (4
`_8 h5
P_8 
H_8 
<_8 0W& 
0_8 
$_8 dW& 
^8 x^( 
^8 X
^8 <
^8 ,
x^8 
l^8 p
`^8 t
P^8 T
D^8 <:
8^8 
$^8 0]
^8 TZ
^8 $
]8 t
]8 -
]8  
t]8 
`]8 P
P]8 @
<]8 
$]8 
\8 $
\8 ,
\8 4
\8 87
|\8 
l\8 
X\8 ,
D\8 P.
4\8 
 \8 H6
\8  +
[8 (
[8 x-
x[8 
h[8 
X[8 
D[8 
8[8 
,[8 8
 [8 4
[8 Hg7 
Z8 T'( 
hZ8 
LZ8 h%( 
4Z8 
xY8 
\Y8 (%( 
DY8 d$( 
(Y8 
X8 $7( 
X8 p#( 
X8 D!( 
xX8 
`X8 
LX8 
0X8 4!( 
X8 $(( 
W8 T(( 
W8 D5( 
W8 D9( 
tW8 L)( 
dW8 
LW8 
,W8 x
V8 L
V8 x
tV8 L
TV8 
<V8 x
U8 d7( 
|U8 x8( 
lU8 
XU8 
LU8 
@U8 
(U8 
T8 tt& 
T8 <g( 
|T8 
dT8 $
TT8 
DT8 
4T8 
 T8  u
T8  
S8 `
S8  
S8 H
S8 |
S8 X
xS8 0
pS8 X
dS8 
\S8 @
TS8 8
HS8 4
<S8 
0S8 
$S8 
S8 L
S8 x
S8 x
R8 8
R8 @
xR8 
lR8 
XR8 
DR8 
8R8  
(R8 
Q8 0
Q8 X
Q8 D
|Q8 
lQ8 
\Q8  
PQ8 
DQ8 p
0Q8 
 Q8 
Q8  
P8 h
P8 8
P8 x
P8 T
P8 L
P8 |
|P8 tk
hP8 
dP8 
`P8 
\P8 
XP8  g7 
TP8 (g7 
PP8 0g7 
LP8 8g7 
HP8 
DP8 
@P8 
<P8 
8P8 
4P8 
0P8 
,P8 
$P8 
O8 LK
O8 0N
O8 8L
pO8 
hO8 p
XO8 (
PO8 ,
DO8 0"
8O8 
,O8 
N8 dG% 
xN8 t
lN8 @{
hN8 
\N8 
LN8 
DN8 `
4N8 
$N8 
N8 D
N8 d
M8 (
M8 @
|M8 
tM8 
hM8 
`M8 
PM8 4?' 
@M8 
4M8 `V
$M8 <7
L8 <
L8 \
L8 h
L8 X
L8 $
pL8 
`L8 
PL8 \
@L8 
,L8 
K8 d
xK8 
hK8 `Y
TK8 
<K8 
$K8 
J8 4
J8 P:
J8 PA
J8 X
tJ8 <,
`J8 d-
HJ8 D
0J8 H%
J8 D&
J8 x
I8 $
I8 |
tI8 
\I8 T
@I8 P
(I8 t
I8 X
H8 ,
xH8 
lH8 \
`H8 
PH8 
DH8 H
,H8 
 H8 4
H8 T
H8 $
G8 D
G8 `
G8 x
G8 pw, 
xG8 
lG8 
LG8 @z, 
<G8 `
,G8 0
F8 p
F8 DE# 
|F8 0I# 
hF8 
\F8 
LF8 
4F8 
E8 Xi	 
E8 pi	 
E8 8i	 
E8 4
pE8 
dE8 
TE8 
LE8 T'
<E8 t
,E8 8
D8 T2% 
D8 H7
tD8 
hD8 X&
TD8 
4D8 l
(D8 \
tC8 
\C8 
HC8 \
4C8 
C8 t
B8 8
B8 (
xB8 |
XB8 
LB8 
DB8 
8B8 
0B8 
 B8 
B8 t
A8 D
A8 tu
|A8 
lA8 
\A8 
LA8 TS
4A8 ,V
A8 hT
@8 Pu
@8 4u
t@8 
d@8 
T@8 @$  
H@8 
<@8 
0@8 
 @8 
?8 0
?8 |
?8 h
?8 x
|?8 $
p?8 
d?8 
X?8 
L?8 
@?8 
0?8 
$?8 
?8 `
>8 <
>8 P
>8 l#$ 
>8 l
|>8 (
p>8  
d>8 4
X>8 
L>8 H
@>8 
8>8 
,>8 
 >8 
|=8 
p=8 
\=8 
P=8 
D=8 |T  
4=8 
$=8 ,W  
=8 d@  
<8 @
x<8 
l<8 
`<8 `
T<8 
L<8 
D<8 XC  
<<8 
0<8 
 <8  
<8 `d
;8 <
;8 d
;8  
;8 |
x;8 4
`;8 
L;8 
0;8 ,
:8 0
p:8 P
T:8 X
D:8 x
8:8 
,:8 09
 :8 h9
:8 T4  
98 09  
98 `]  
98 `
|98 h
l98 
\98 T
L98 
<98 
098 P
$98 
98 `
88 (
88 0q
88 `
t88 
`88 P~
H88 
<88 $~
,88 
88 <
78 h
78 d
78  
78 (
78 H
78 $
t78 8
d78 
\78 
L78 ,
D78 
878 
,78 0
 78 
68 h
68 \
68 |
68 XB( 
x68 
h68 XA( 
T68 
<68 
,68 
68 PB( 
58 Lh
58 X
58 `
58 $
58 @
l58 
X58 
858 
48 D
48 `
l48 \
X48 
D48 Tt
048 
48 ,p
48 (q
38 D
38 hv
38 0v
l38 
L38 
<38 
(38 
28 d
28 Ho
28 Tx
p28 
T28 
@28 d
028 
18 d
18 (
18 t
18 @C
p18 TA
P18 \C
818 
$18 
18 dF
x08 
X08 
408 
/8 X>
/8 @m
/8 xr
/8 \s
|/8 
l/8 
\/8 \w
L/8 
</8 du
 /8 
p.8 
\.8 xl
H.8 
0.8 
.8 @n
-8 dn
-8 8
x-8 
l-8 h~
`-8 t
T-8 ,
H-8 
<-8 
(-8 
,8  r
,8 0m
,8 @q
t,8 
`,8 
P,8 
@,8 
,,8 hl
,8 Pl
,8 hr
+8 Pr
+8 (t
+8 lI/ 
+8 (E' 
p+8 
d+8 8D' 
T+8 
@+8 4F' 
,+8 \F' 
+8 XF' 
+8 dF' 
*8 pi
*8 ,
*8 8v
*8 <
t*8 
h*8 
\*8 
L*8 
@*8 t
4*8 
(*8 
*8 d
)8 d
)8 4L- 
)8 L
t)8 
h)8 
`)8 
P)8 l
@)8 
4)8 l
,)8 
)8 h
(8 @
(8 D
(8 p
(8 h
(8 8
(8 d3
|(8 
p(8 0
`(8 d
T(8 
H(8 
<(8 
,(8 
$(8 ,y
(8 0
'8 d
'8 \
t'8 
X'8 
8'8 xN, 
('8 
&8 h
&8 p
l&8 x
L&8 
@&8 H'
0&8 
%8 d
%8 T
%8 g
\%8 H-	 
0%8 hx	 
%8 8+	 
h$8 4
D$8 
 $8 
$8 0
#8 pz	 
h#8 8.	 
8#8 <|	 
(#8 `
"8 H*	 
t"8 @g	 
L"8 
 "8 
!8 `0	 
!8  1	 
`!8 
4!8 
!8 8
 8 X
 8 P
 8 H
 8 @
 8 H
| 8 P/	 
X 8 `~	 
D 8 
0 8 (
 8 ,
8 Hi	 
8 8P
8 \'
8 Xb
8 Db
8 \	
8 \y& 
8 Hl$ 
8 Lq$ 
8 `X
8 Hz
8 tz
8 ${
8 @|
8 l|
8 |{
8 P{
8 ,}
8 (y
8 |8
8 0f
8 pr# 
8 DR
8 pZ' 
8 (K' 
8 dK' 
8 $J' 
8 xR' 
8 |T' 
8 <P' 
8 4Z' 
8 hZ' 
8 @`+ 
8  L
8 tK+ 
8 xR+ 
8 8k
8 4C
8 $D
8 $	
8  2	 
8 @%% 
8 ,'% 
8 4(% 
8 0t
8 <F( 
8 @z
8 |_( 
8 l`( 
8 $e
8 ,\
8 8`( 
8 D_( 
8 86
8 `L
	8 `
|	8 0
t	8 
d	8 
T	8 4m
D	8 
4	8 
$	8 8i
8  i
8 ,|& 
8 Di
8  x	 
8 p7% 
8 T,	 
8 tv	 
8 pI
8  =
8 $"3 
8 ,93 
8 t03 
8 PE3 
8 TP
8 DU( 
8 Xh
8 <p' 
8 8p' 
8  o' 
8 Df' 
8 ts' 
8 \g' 
8 tk' 
8 `5
7 <[
7 0h
7 Ta
7 dm
7 LP
7 xl
7  H
7 @L
7 <{
7 @H
7  i	(
7 dv' 
7 $R
7 4u' 
7 (2
7 Xv' 
7 `{' 
7 <|' 
7 (b  
7 @e
7 `i
7 Ly
7 0&
7 @1
7 h5
7 0-
7 d6
7 x&- 
7 h&- 
7 l;
7 <&- 
7 @i
7 `{
7 <~' 
7 pK
7 P4
7 |Y& 
7 <l
7 8l
7 4l
7 4^( 
7 `e
7 \<
7 X<
7 @s
7 4{
7 Hc
7 ,{
7 p!
7 d#
7 XL
7 PS
7 tS
7 tL
7 HM
7  ,
7 H&
7 D1
7 ,8
7 $9
7 8;
7 @>
7 pQ
7 $C
7 pC
7  R
7 4R
7 lR
7 `R
7 |R
7 <T
7 ,S
7 ,!
7 hL( 
7 0v
7 8i
7 ti
7 Xv
7 lv
7 xy
7 x,
7 X+- 
7 l'- 
7 `+- 
7 P+- 
7 4.- 
7 @W	(
7 @k
7 05
7 PF
7 hF
7 $3- 
7 |7- 
7  ;- 
7 PC- 
7 ,0- 
7 `/- 
7  =- 
7 `4- 
7 l5- 
7 Pc. 
7  c. 
7 0c. 
7 @c. 
7 `c. 
7 tc. 
7 @j. 
7 `i. 
7 (v. 
7 Ll. 
7 hk. 
7 |y. 
7 4w. 
7 |o. 
7 hz. 
7 ,}. 
7 X'. 
7 h!. 
7 x#. 
7 @*. 
7 x.. 
7 x+. 
7 0-. 
7 T). 
7 <.. 
7 D/. 
7 ,=. 
7 tS. 
7 |R. 
7 <S. 
7 hW. 
7 xV. 
7 xU. 
7  X. 
7 DX. 
7 \1. 
7 |F- 
7 D$	(
7 ,,
7 \!
7 4 
7 dQ
7  e
7 (T
7 tR
7 hz
7 D_
7 `e
7 D4
7 t(
7 \&
7 ,%
7 D*
7 \$
7 Tm
7 H~
7 l 
7 P;
7 p1
7 ti
7 @U
7 Dy
7 `L
7 |L
7 p=
7 xi
7 `4	(
7 dO2 
7 pL2 
7 pI2 
7 4K2 
7 hK2 
7 <N2 
7 $J2 
7  u
7 pg
7 ,v
7 8~
7 lu
7 x[
7  [
7 Tb
,IMCFG
*68*
*52*
*51*
*53*
#68#
#52#
#51#
#53#
Low Battery
Please Charge
Charging!
Connecting...
Holding
No Caller ID
Hold # to 
Unlock
Hold
Unhold
End Back Call
Swap
New call
Call transfer
Blind
Consult
Transfer to:
Transfer...
Call park
Conference
Mute
Unmute
Drop
Redial...
Operating...
Invalid Operate
Empty
Busy
Monday
Tuesday
Wednesday
Thursday
Friday
Saturday
Sunday
2001--07--17
 11:01:00
Add Entry
Delete Entry
Edit
Enable
Number:
Modify
Emoji
Common Phrases
Symbols
Greetings
Expressions
Classic
Urgent
Appointment
Affection
Celebration
Animation
Punctuation
Toll Call  Locked
IP Not Set
Out Of Area
Delete?
Reset?
No Record
Update?
Exists
Error
Code Error
New Message
Failed to Send
Not Matched
Memory Full
Number Error
Enter Name
Empty
Failed
Enter:
Enter Code:
New Code:
Confirm Code:
Name:
Number:
Select Group
(0--6)
Enter Time:
Prompt Time:
Search
Group Info
Speed Dial
Memory
Edit Message
Inbox
Outbox
Draft
Clear
Memory
Missed Log
Received Log
Dialed Log
Delete Log
Duration
Standard
Meeting
Silent
Outdoor
Own Number
Alarm
Date/Time
Scheme
Answer Mode
Language
Input Method
IP Phone
Display
Set Security
Call Forwarding
Family
Friend
Colleague
Classmate
Partner
Blacklist
Others
One By One
Ring Tone
Browse
Edit
Cancel
Key 1
Key 2
Key 3
Key 4
Key 5
Key 6
Key 7
Key 8
Key 9
Unset
Used
Unused
Clear Inbox
Clear Outbox
Clear Draft
Clear All
Delete
Reply
Forward
Call Back
Save Number
Send
Sender:
Receiver:
Sent:
Received:
Save
Send Failed
Message Sent
Inbox
Outbox
Draft
Inbox Full
SMS Center
Send  Mode
Priority
Notice
PS to PS
PS to Center1
PS to Center2
PS to Center3
Activate
Set SMS Center Number
Middle
High
Full
Full
High
Pick Up Number
Missed
Received
Dialed Log
Delete All
Received:
Dialed:
Total Time:
Dialed
Set 
Time
Save
Delete
Number
Time
Edit
Whisper Mode
Ring Mode
Ring Tone
Ring Volume
Message Tone
Keypad Tone
Alert Tone
Ringing
Ascending
Ring Once
Vibration
Vibration And Ring
Ring After Vibration
Mute
Alarm Tone
User Define
Memo Alert
Volume
Key Music
Standard Keytone
On/Off
Set Time
Repeat Type
Snooze
Date/Time
Any Key
Talk Key
Flip Key
Backlight
Contrast
On/Off Animation
Screen Saver
Sim Stroke
English
eZI English
Letter
PinYin
Select Mode
Static Picture
Change Picture
User Edit
Default
User Edit
Change Preview
Picture1
Picture2
Picture3
Picture4
Picture5
Picture6
Picture7
Picture8
Picture9
Picture10
Picture11
Picture12
Picture13
Picture14
Picture15
Picture16
Picture17
Picture18
Picture19
Picture20
Picture21
Picture22
Picture23
Picture24
User-defined
Photograph1
Photograph2
Photograph3
Photograph4
Photograph5
Photograph6
Photograph7
Photograph8
Photograph9
Photograph10
Photograph11
Photograph12
Photograph13
Photograph14
Photograph15
Photograph16
Photograph17
Photograph18
Photograph19
Photograph20
Photograph21
Photograph22
Photograph23
Photograph24
Static Picture
Every Hour
Every 3 Hours
Every Day
On/Off
Select Picture
Picture 1
Picture 2
Picture 3
Picture 4
Digital Mode
Analog Mode
Animation 1
Animation 2
Animation 3
Animation 4
Startup Time
1  Minute
5  Minutes
10 Minutes
Toll Lock
Change Code
PowerOn Code
Reset All
Once
Everyday
Mon.~Fri.
Mon.~Sat.
Every Sat.
Every Sun.
Battery Saving
Normal
Access No:
Accounts:
Password:
Enable
Disable
Own Number:
Unconditional
No answer
Busy
Unreachable
Config
Cancel
Forward to:
Forward to
Listen to voice answer
Register
Cancel
Config
Service Number
Mobile:
Mobile Number
Password:
Password
Disable Number:
Disable Number
End Mark:
End Mark
Access No:
Access Number
Listen to voice answer
Input Mobile Number
Enable Service
Number:
Disable Service
Number:
New Service
Calculator
Calendar
Browse Date
Select Date
Edit
View
Delete
Today's Memo
All Memos
One By One
Modify
Memo
SSID
WEP Key
Authentication
DHCP
Signal Protocol
Auto Identify
User Define
None
64 bit Encrypt
128 bit Encrypt
Open System
Share Key
LEAP
802.1x
PPPoE
Auto 
Standard
Manual
Pls Waiting
WiFi
Network Parameter
DHCP
TFTP
Work Mode
Server Domain Name
Server IP
Port
Encryption Key
IP Address
Subnet Mask
Gateway IP Address
Network Information
Primary DNS Server IP Address
Secondary DNS Server IP Address
Priority
Signal Protocol
SIP Register Server Mode
SIP Service Name
SIP Register Server Domain Name
SIP Register Server IP Address
SIP Register Server Port
SIP Outbound Proxy Mode
SIP Outbound Server Domain Name
SIP Outbound Server IP Address
SIP Outbound Server Port
SIP User Name
SIP Password
SIP Authentication Algorithm
SIP Port
RTP Port
Packetize Time
RTP Jitter Buffer Compensation
Voice Mail
Voice Mail Access Number
Voice Mailbox Number
Voice Mailbox Password
NAT IP
NAT Server Domain Name
NAT Server IP Address
NAT Server Port
NAT keep-alive Time
NAT keep-alive Pack Dest
STUN
Directory/File Name
Disable
Enable
Disable
Standard
Auto Provision
Local First
DHCP First
20ms
30ms
40ms
NAT Server
SIP Proxy
Voice Process
Noise Suppression
Acoustics Echo Cansellation
Codec Priority
General Jitter Buffer
Per-call Jitter Buffer
Tail Time
(ms)
g.711a
g.711mu
g.729
g.729a
g.729b
Max Connection
Size
Max Latency
Max Hold Threshold
Min Buffer Size
Min Stable Event
HWM Grow Rate
HWM Shrink Rate
Silence Timer
WiFi Config
WiFi Authentication
2 Layer Authentication
SET1
SET2
SET3
SET4
SSID&WEP KEY
Auto Scan
SSIDs
SSID
SSID1
SSID2
SSID3
SSID4
WEP KEY
WEP Key1
WEP Key2
WEP Key3
WEP Key4
Shared Key
802.1x-MD5
Leap
PPPoE
Username
Service Name
Activate
Null
64bit
128bit
Vendor Information
Vendor Name
Enterprise Code
Product Category
Model Name
Version
Net Search
Tail Time:
Max Connection:
Size:
Username:
Password:
Service Name:
SSID1:
SSID2:
SSID3:
SSID4:
SSID:
WEP Key1:
WEP Key2:
WEP Key3:
WEP Key4:
WEP KEY:
SSID-A:
SSID-B:
SSID-C:
SSID-D:
SSID-E:
SSID-F:
SSID-G:
SSID-H:
SSID-I:
SSID-J:
SSID-A
SSID-B
SSID-C
SSID-D
SSID-E
SSID-F
SSID-G
SSID-H
SSID-I
SSID-J
Operating...
Vendor Name:
Enterprise:
Product Category:
Model Name:
Version:
Domain Name:
Server IP:
Port:
Name:
Encryption:
Subnet Mask:
Gateway IP:
Service Name:
OutbdDomain:
Outbd IP:
Outbd Port:
Reg Domain:
Reg IP:
Reg Port:
SIP User:
SIP Password:
SIP Auth:
SIP Port:
RTP Port:
RTP JBC:
Access Num:
Mailbox Num:
Mailbox PW:
NAT IP:
Nat Domain:
NAT Ser IP:
NAT Port:
NAT Time:
IP Address:
Subnet Mask:
Gateway IP Address:
(NULL)
MAC Address:
Connected SSID:
DNS Address:
PC Config
WEP Key Index
WEP Key Index:
Call Waiting
Register Interval Time
Caller-ID Block
Repeat Dial on Busy
Remote TFTP Update
Local TFTP Update
Erasing old software...
Call Transfer
Call Pickup
Reject Anonymous Incoming Call
Digit map 
Personal Information 
Pattern 
Pattern:
Caller ID:
Regular expression 
Blind
Consult
Network
Three Way Call
Cancel all forward
Forward number
Operating
Net service started
Net service not started
Interval:
Recall interval
Recall times
Search finished
Net service
Started
Stop
Wait time
Globel Setting
Per Call Basis
Group Num:
(Minutes)
Connecting...
Processing...
Pls Waiting
Time Zone
Current zone changed
GMT(Greenwich)
London
Paris
Cairo
Jerusalem
Jeddah
Karachi
Dacca
Bangkok
Beijing/HK
Seoul
Sydney
Noumea
Wellington
Honolulu
Anchorage
Los Angeles
Denver
Chicago
New York
Caracas
TFTP Update is a long process! Please do not cut off power!It will power off when update completion! Then you can power on and use it.
Error
Overflow
Full Charged!
Charge Done!
Charging
Low Battery!
Ring 1
Ring 2
Ring 3
Ring 4
Ring 5
Ring 6
????
English
Fran
ais 
Portugu
Espa
nh t?
Deutsch
Italiano
IP Call
You Zi Gui Jia
Multi-Color
Primitive Colors
Yellow
Blue
Green
Cyan
Purple
White
Led Color
New Record!
Game Over
Black-white Chess
Start Game
Set Level
Set First
Set Chess Manual
Game Rule
Whammy
Set Speed
High Score
Slow
Medium
Fast
Easy
Difficult
Player First
Player Second
Chess Manual 1
Chess Manual 2
Chess Manual 3
Chess Manual 4
Chess Manual 5
Chess Manual 6
Chess Manual 7
Chess Manual 8
Chess Manual 9
Chess Manual 10
You Lost
You Won!
Tie Game
Set Music
Restart
Continue
Last Score
Game Score
Game
Player with black pieces goes first. Capture rival's pieces by surrounding them horizontally, vertically or diagonally. If one has no moves, the other plays. When board is full, or both must pass, game ends. Player with most pieces is the winner.
The game is limited to 1 minute. Every time a rat is hit, one point is won. You can start/pause the game by pressing soft-left key and return by soft-right key. If your score breaks the record, it will be saved as the top score.
Press keys 'Up','Down','Left','Right','Mode' to execute the actions.The action is enabled when it is white, and disenabled when it is gray.");
   strcpy((LP_S8)textattrs.text, "The one with cards valued closer to 21 wins. If one's value exceeds 21, he'll bust and lose. Aces count as 1 or 11, face cards as 10, other cards as face value. A blackjack is an ace plus a 10-value card. Once bet is made, each one gets a upcard and a downcard. Player can HIT/DOUBLE/STAND. Then banker must hit until his value exceeds 17. If the banker's upcard is an ace, the player can buy insurance. If the banker has blackjack, the insurance pays 2 to 1; if not, the insurance is lost.
Couldn't connect to AP
Connecting to
Registering 
PC Config may take a long time. Do not unplug the battery. When computer prompt PC Config completed,restart the phone to initiate the change.
12 Hour
24 Hour
DST Setting
Time Format
SIP Authentication String
Server Name
Server Name:
Server Port
Server Port:
Auth String:
Remote TFTP Server
Local Log
Web Authentication
Set Address
TFTP Server
Processing...
Parsing config file...
Connecting to new config file...
Downloading firmware...
Tftp DNS failure.
Tftp Port Blocked failure.
Tftp network transfer failure.
Tftp unknown failure.
Tftp decryption failure.
Connecting to new port.
Tftp file not found failure.
Erasing old software...
Connecting...
Tftp update finished.
The firmware in the phone is newer. Are you sure that you want to go back to an older version?
New config file or config is available. Please press [Update] to update.
The current config file or software needs update. Please press [Update] to update.
Last update failure. Try once more?
TFTP Update is a long process! Please do not cut off power!It will power off when update completion! Then you can power on and use it.
Log In
Blind & Consult
AP Profile
Security Mode
Open AP
WPA-PSK
Auth. Method 
PSK Key: 
Open Key
Item
GMT-12:00 - Int'l Date Line
GMT-11:00 - Midway Island
GMT-10:00 - Hawaii
GMT-09:00 - Alaska
GMT-08:00 - US Pacific
GMT-07:00 - US Mountain
GMT-06:00 - US Central
GMT-05:00 - US Eastern
GMT-04:00 - Atlantic
GMT-03:30 - Newfoundland
GMT-03:00 - Buenos Aires
GMT-02:00 - Mid-Atlantic
GMT-01:00 - Azores
GMT - London
GMT+01:00 - Central Europe
GMT+02:00 - East Europe
GMT+03:00 - Moscow
GMT+04:00 - Abu Dhabi
GMT+04:30 - Kabul
GMT+05:00 - Islamabad
GMT+05:30 - Delhi
GMT+05:45 - Katmandu
GMT+06:00 - Novosibirsk
GMT+06:30 - Rangoon
GMT+07:00 - Bangkok
GMT+08:00 - Beijing
GMT+09:00 - Tokyo
GMT+09:30 - Darwin
GMT+10:00 - Sydney
GMT+11:00 - Solomon Is
GMT+12:00 - New Zealand
GMT+13:00 - Nuku'alofa
WEP Key Info
WPA-PSK Info
(1~4)
Download Script
Decompressing
Script Files
No service  try other AP
Bater
a Baja
Cargue Bat.
Cargando!
Conectando...
En Espera
Desconocido
Pulse # para
Desbloquear
Presione  
Libere
Term. Llamada en Espera
Cambiar
Nueva Llamada
Transferir
Directa
Consultar
Desviar a:
Desviar...
Estacionar Llamada
Conferencia
Silencio On
Silencio Off
Abandonar
Marque...
Operando...
Oper. Inv
lida
Ocupado
Lunes
Martes
rcoles
Jueves
Viernes
bado
Domingo
17--07--2001
 11:01:00
Nuevo 
Borrar
Activar
Desactivar
Editar
Activar
mero:
Modificar
Emoji
Frases Comunes
mbolos
Mensajes de Saludo
Expresiones
sico
Urgente
Cita
Afecto
Celebraci
Animaci
Puntuaci
Llamada Bloqueada
IP no Configurada
Fuera de 
Eliminar?
Reconfigurar?
Sin Registro
Actualizar?
Existe
Error
Error de C
digo
Mensaje Nuevo
Error al Enviar
digo Incorrecto
Directorio Lleno
mero Err
Agregue Nombre
Falla
Intro.:
digo:
Nuevo C
Confirmar:
Nombre:
mero:
Seleccione Grupo
(0--6)
Poner en Hora:
Confirmar Hora:
Buscar
Informaci
n de Grupo
Marcado R
pido
Memoria
Editar Mensaje
n de Entrada
n de Salida
Borrador
Borrar
Memoria
Perdidas
Recibidas
Enviadas
Borrar Reg. Llamadas
Duraci
ndar
Reuni
Silencio
Exterior
Nro. Propio
Alarma
Fecha/Hora
Pant. Espera
Modo de Respuesta
Idioma
Modo de Entrada
fono IP
Pantalla
Seguridad
Desv
o de Llamada
Familia
Amigo
Oficina
Compa
Negocios
ListaNegra
Otros
Uno a Uno
Todos
Tono de Timbre
Buscar
Editar
Cancelar
Tecla 1
Tecla 2
Tecla 3
Tecla 4
Tecla 5
Tecla 6
Tecla 7
Tecla 8
Tecla 9
No Asignado
Usada
Libre
Vaciar Buz
n de Entrada
Vaciar Buz
n de Salida
Vaciar Mensajes no Enviados
Vaciar Todo
Borrar
Responder
Reenviar
Devolver Llamada
Guardar N
mero
Enviar
Nuevo
Para:
Enviado:
Recibido:
Guardar
Error
Msj. Enviado
Entrada:
Salida:
Borrador:
n Lleno
Centro de mensajes
Modo Env
Prioridad
Aviso
PS a PS
PS a Centro1
Ps a Centro2
PS a Centro3
Activar
Confirme Nro. del Centro SMS
Bajo
Medio
Alto
Lleno
Lleno
Alto
Apunte Nro.
Perdidas
Recibidas
Enviadas
Borrar Todas
Recibidas:
Enviadas:
Duraci
Marcados
Configurar
Hora
Guardar
Eliminar
mero
Hora
Editar
Amplif. Voz
Modo de Timbre
Tono de Timbre
Volumen de Timbre
Tono de Mensaje
Tono Teclado
Tono Alerta
Timbre
Ascendente
Timbre Una sola Vez
Vibrar  
Vibrar y Timbre
Vibrar Despu
s Timbre
Silencio
Tono de Alarma
Def. Usuario
Alerta Memo
Volumen
Musical
ndar
Apagado
Encendido/Apagado
Ajustar Hora
Repetir
Snooze
Fecha/Hora
Cualquier Tecla
Tecla de Respuesta
Al Abrir
Luz de Pantalla
Contraste
Animaci
n Encendida/Apagada
Fondo de Pantalla
Modo Sim
Ingl
Ingl
s eZI
Carta
PinYin
Seleccionar Modo
Imagen Fija
Cambiar Fondo
Protector de Pantalla
ndar
Personalizada
Ver Cambios
Imagen1
Imagen2
Imagen3
Imagen4
Imagen5
Imagen6
Imagen7
Imagen8
Imagen9
Imagen10
Imagen11
Imagen12
Imagen13
Imagen14
Imagen15
Imagen16
Imagen17
Imagen18
Imagen19
Imagen20
Imagen21
Imagen22
Imagen23
Imagen24
Defin. Usuario
Foto1
Foto2
Foto3
Foto4
Foto5
Foto6
Foto7
Foto8
Foto9
Foto10
Foto11
Foto12
Foto13
Foto14
Foto15
Foto16
Foto17
Foto18
Foto19
Foto20
Foto21
Foto22
Foto23
Foto24
Imagen Fija
Cada Hora
Cada Tres Horas
Cada D
Encendido/Apagado
Seleccionar Imagen
Imagen 1
Imagen 2
Imagen 3
Imagen 4
Modo Digital
Modo Anal
gico
Apagado
Animaci
Animaci
Animaci
Animaci
Tiempo de Espera
1 Minuto
5 Minutos
10 Minutos
Bloqueo de Larga Distancia
Cambio C
digo de Seguridad
d. Encender
Reconfigurar Todo
Una vez
Cada d
Lunes~Viernes
Lunes~S
bado
Cada S
bado
Cada Domingo
Ahorro de Bater
Normal
Num. Acceso:
Cuentas:
Contrase
Activar
Desactivar
Nro. Propio:
Incondicional
Sin Respuesta
Ocupado
No Disponible
Configurar
Cancelar 
Desviar a:
Desviar a
Escuchar a Respuesta
Registrar
Cancelar 
Configurar
Nro. Servicio
vil:
Nro. M
Contrase
Contrase
Desactivar N
mero:
Desactivar N
mero
Marca Final:
Marca Final
Num. Acceso:
Num. Acceso
Escuchar a Respuesta
Introduzca Nro. M
Activar Servicio
mero:
Desactivar Servicio
mero:
Nuevo Servicio
Nro.
Calculadora
Calendario
Buscar Fecha
Seleccionar Fecha
Editar
Ver 
Eliminar
Nota de Hoy 
Todas las Notas
Uno a Uno
Todos
Modificar
Nota
SSID
Clave WEP
Autentificaci
DHCP
Protocolo de se
alizaci
Auto Identificar
Def. Usuario
Inexistente
Cifrado 64-Bit
Cifrado 128-Bit
Sist. Abierto
Clave Compartida
LEAP
802.1X
PPPoE
Auto  
ndar
Manual
Favor Espere
Encender
Apagar
WiFi
Red IP
DHCP
TFTP
Modo de Trabajo
Nombre de Dominio del Servidor
IP del Servidor
Puerto
Clave
IP  
Direcci
n IP:
Mascara de Subred:
Direcci
n IP Gateway:
Informaci
n de Red
Direcci
n IP Servidor DNS
Direc. IP Servidor DNS Secundario
Prioridad
Protocolo de se
alizaci
Modo del Servidor de Registro SIP
Nombre de Servicio SIP
Nombre de Dominio del Servidor de Registro SIP
Direcci
n IP del Servidor de Registro SIP
Puerto del Servidor de Registro SIP
SIP Proxy
Nombre de Dominio del SIP Proxy
Direcci
n IP del SIP Proxy
Puerto del SIP Proxy
Nombre del Usuario SIP
Contrase
a SIP 
Algoritmo Autentificaci
n SIP
Puerto SIP 
RTP  
Puerto RTP
Tiempo de Empaquetamiento
Buffer de Compensaci
n de Jitter RTP
n de Voz
Nro. Buz
n de Voz
Contrase
a para Buz
n de Voz
Contrase
a para Buz
n de Voz
NAT  
NAT IP 
Nombre de Dominio del Servidor NAT
Direcci
n IP del Servidor NAT
Puerto del Servidor NAT
Tiempo keep-alive del NAT
NAT keep-alive Pack Dest
Modo STUN
Directorio/Archivo
Desactivar
Activar
Desactivar
ndar
Auto Provisi
Local Primero
DHCP Primero
20ms
30ms
40ms
Servidor NAT
SIP Proxy
Proceso de Voz
Supresi
n de Ruido
Cancelaci
n Echo Ac
stico
Prioridad Codec
Jitter Buffer General 
Jitter Buffer por Llamada
Tail Time
(ms)
g.711a
g.711mu
g.729
g.729a
g.729b
Conexi
xima
Tama
Latencia M
xima
Umbral de M
xima Retenci
Tama
nimo de Buffer
nimo Evento Estable
Tasa de Crecimiento HWM
Tasa de Decrecimiento HWM
Contador Silencio
Config. WiFi
Autent. WiFi
Autent. en Layer2
Definir1
Definir2
Definir3 
Definir4
SSID & Clave WEP
Auto B
squeda
SSIDs
SSID 
SSID1
SSID2
SSID3
SSID4
Cualquiera
Clave WEP
Clave WEP1
Clave WEP2
Clave WEP3
Clave WEP4
Clave Compartida
802.1x-MD5
Leap
PPPoE
Nombre del Usuario
Nombre del Servicio
Activar
Nulo
64Bit
128Bit
Informaci
n del Fabricante
Fabricante
Operador:
Producto:
Modelo:
Versi
squeda de Redes
Tiempo de Tail:
xima Conexi
Tama
Nombre del Usuario:
Contrase
Nombre del Servicio:
SSID1:
SSID2:
SSID3:
SSID4:
SSID:
Clave WEP 1:
Clave WEP 2:
Clave WEP 3:
Clave WEP 4:
Clave WEP:
SSID-A:
SSID-B:
SSID-C:
SSID-D:
SSID-E:
SSID-F:
SSID-G:
SSID-H:
SSID-I:
SSID-J:
SSID-A
SSID-B
SSID-C
SSID-D
SSID-E
SSID-F
SSID-G
SSID-H
SSID-I
SSID-J
Operando...
Fabricante:
Operador:
Producto:
Modelo:
Versi
Nom.Dominio:
Servidor IP:
Puerto:
Nombre:
Cifrado:
scara:
Gateway IP:
Servicio:
Dom. Proxy:
IP Proxy:
Puerto Proxy:
Dominio Reg:
IP Reg:
Puerto Reg:
Usuario SIP:
Password SIP:
Autent. SIP:
Puerto SIP:
Puerto RTP:
RTP JBC:
Nro. Acceso:
Num. Buz
Clave Buz
IP NAT:
Dominio NAT:
Ser. NAT IP:
Puerto NAT:
Tiempo NAT:
Direcci
n IP:
Mascara de Subred:
Direcci
n IP Gateway:
(NULO)
Direcci
n MAC:
SSID Conectado:
Direcci
n DNS:
Config. PC
ndices Claves WEP
ndices Claves WEP:
Llamada en Espera
Tiempo del Interv. Registro
Id. Privado
Repetir Llamada Cuando Ocupado 
Actualizar V
a TFTP Remoto
Actualizar V
a TFTP Local 
Borrando Software...
Transferir
Contestar Llamadas
Rechazar Llamadas no Ident. 
Mapa Digital 
Informaci
n Personal
Patr
Patr
Id. Llamante:
Frases Comunes
Directa
Consultar
Llamada a tres
Cancelar Desv
o de Llamadas
Desviar a
Operando...
Servicio de Red Conectado
Servicio de Red no Conectado
Intervalo:
Intervalo entre Reconexiones
Nro. de Intentos Reconexi
squeda Terminada
Servicio de Red
Comenzado
Parada
Tiempo en Espera
Ajuste Global
Por Cada Llamada
Num. Grupo:
(Minutos)
Conectando...
Procesando...
Favor Espere
Huso Horario   
Huso Horario Cambiado
GMT(Greenwich)
Londres
Paris 
El Cairo
Jerusal
Yeddah
Karachi
Dhaka
Bangkok
n/HK
Sydney
Noumea
Wellington
Honolulu
Anchorage
Los Angeles
Denver
Chicago 
Nueva York
Caracas
Rio de Janeiro
La carga TFTP puede tardar. No apagar. Apagado autom
tico al terminar.
Error
Exceso
Lleno!
Carga completa!
Cargando...
Bater
a Baja!
Ring1
Ring2
Ring3
Ring4
Ring5
Ring6
????
English
Fran
ais 
Portugu
Espa
nh t?
Deutsch
Italiano
Llamada IP
You Zi Gui Jia
Multi-Color
Primitive Colors
Yellow
Blue
Green
Cyan
Purple
White
Led Color
Nuevo Record!
Juego Finalizado
Reversi Blanco y Negro
Comenzar Juego
Definir Nivel
Definir Primero
Definir Tablero de Inicio
Reglas del Juego
Whammy
Configurar Velocidad
Record
Lento
Medio
pido
Jugador Primero
Jugador Despu
Tablero 1
Tablero 2
Tablero 3
Tablero 4
Tablero 5
Tablero 6
Tablero 7
Tablero 8
Tablero 9
Tablero 10
Ud. Perdi
Ud. Gan
Empate
Reiniciar
Continuar
UltimoRes.
21 Black Jack!
Resultados
Juego
El jugador con las piezas negras juega primero. Captura las piezas rivales rode
ndolas horizontal, vertical o diagonalmente. Si un jugador no tiene movimientos, el otro juega. Cuando el tablero est
 lleno, o si ambos deben pasar, el juego termina. El jugador con m
s piezas es el ganador.
El juego esta limitado a un minuto. Cada vez que una rata es golpeada, un punto es ganado. El juego puede comenzar/pausarse presionando la tecla de navegaci
n izquierda y regresado con la derecha. Si el puntaje rompe el record entonces ser
 guardado como puntaje m
s alto. 
El jugador cuyas cartas sumen lo m
s cercano a 21, gana. Si excede de 21, pierde. Ases cuentan como 1 o 11, las figuras como 10, y todas las dem
s su valor nominal. Un Blackjack es un As m
s una carta de valor 10. Una vez hecha la apuesta, cada uno recibe una carta destapada y otra boca abajo. El jugador puede PEDIR/DOBLAR/PASAR. El banquero debe pedir hasta que su valor exceda 17. Si la carta destapada del banquero es un as, el jugador puede comprar un seguro. Si el banquero tiene Blackjack, el seguro paga 2 a 1, sino el seguro se pierde.
No se encontr
Conectando a.
Registrando. 
La configuraci
n puede tardar. No apagar. Apagado autom
tico al terminar.
12 Horas
24 Horas
Configuraci
n DST
Formato Hora
Clave Autencicaci
n SIP
Nombre del Servidor
Nom.Servidor:
Puerto del Servidor
Pto.Servidor:
Clave Aut.:
Servidor TFTP Remoto
Registro Local
Autenticaci
n Web
Configurar Direcci
Servidor TFTP
Procesando...
Leyendo fichero configuraci
n...
Conectando nuevo fihero de configuraci
n...
Descargando C
digo...
Fallo TFTP: DNS.
Fallo TFTP: Puerto Bloqueado.
Fallo TFTP: Fallo transferencia de red.
Fallo TFTP:  Fallo desconocido.
Fallo TFTP: Fallo desencriptaci
Conectando a un nuevo puerto.
Fallo TFTP: No se encuentra el fichero.
Borrando anterior c
digo...
Conectando...
Actualizaci
n TFTP finalizada.
El c
digo de este tel
fono es m
s nuevo.
 seguro que quiere volver a uno m
s antiguo?
 disponible un nuevo fichero de configuraci
n. Por favor pulse [Update] para actualizarlo.
El fichero de configuraci
n actual debe ser actualizado. Por favor pulse [Update] para actualizarlo.
ltima actualizaci
n fall
Quiere intertarlo de nuevo?
La carga TFTP puede tardar. No apagar. Apagado autom
tico al terminar.
Acceder
Directa & Consulta
Config. AP
Mdo.Seguridad
AP. Abierto
WPA-PSK
Mdo. Aut.
Clave PSK
Clave Abierto
culo
nea fecha Int'l
Isla Midway
Hawai
Alaska
fico E.E.U.U.
Mountain E.E.U.U.
Central E.E.U.U.
Este E.E.U.U.
ntico
Newfoundland
Buenos Aires
Centro-Atl
ntico
Azores
Londres
Madrid. Europa Central
Este Europa
Mosc
Abu Dhabi
Kabul
Islamabad
Deli
Katmandu
Novosibirsk
Rangun
Bangkok
Tokio
Darwin
Sydney
Islas Solom
New Zealand
Nuku alofa
Info Clave WEP
Informaci
n de WPA-PSK
(1~4)
Descargar la Escritura
Descompresi
Script Files
Sin servicio
***(*
(***
`````
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
    ``
``    
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
     
|DD8
hhhhi
koki
````
#$$$
8HHH
.....
/////
////oo
oo////
/////
/.../
..//oo
oo////
/////
//...
plll
|lll
lllr
?wgggw?
?scccs?
XXXXX
<||<
=}}=
ppppp
"dyr$
$SID&
3aa3
<<~~~
v~~~<<
`px|~~wwwww~~|xp`
HDDH
ppppppp0p
`co~x
`co~x
pppp
`co~x
`co~x
`co~x
`co~x
`co~x
`co~x
`co~x
`co~x
      
      
      
      
      
      
      
      
@@@@@@
@@@@@@
@@@@@@
@@@@@@
@@@@@@
@@@@@@
@@@@@@
@@@@@@
+,)n
i(,+
b#"#"?
Dh 9
pP8lT4
pP8lT4
pP8lT4
      
      
      
@@@@@
a#'~
||xxp`
||xxp`
|xxp`
?AFH?
0@CD8
0@DD;
~DDDC
@   
?DDD#
p@CLp
;DDD;
<BBB?
@   
jVBBBVj
((EE
3333333333333
aa!!/
					
DDDDD
@@@````````````````````````````````````````
@@@@@
Vj~~~jV
((EE
0Xxx8
0P `
+!#!
ABUJVj5
@  `
@@@@
X,T,T
(TLD
H4(Pa
@ ``
Q !*%+5
P0P    
(0iSbBb
@b@ P`Ph
$@ @
@@@A 
MIw2
    
FjDDD$
uj5*
*5(4
*tJDB
@@@A 
```1?
FjDDD$
uj5*
*5(4
```1?
```1?
0P `
'3!aY
!"DEI
JJI%$
0P `
I$b!(4S0
(TLD(
0P `
'3!aY
!"DEI
KKI%$
,T,T
(TLD(
0P `
#5`U
I$b!(4S0
X,T,T
(TLD(
0P `
'3!aY
!"DEI
KKI%$
W'W'V
(TLD(
#5`U
I$b!(4S0
ABUJVj5
@@@@
X,T,T
(TIC+
'3!aY
!"DEI
+!#!
ABUJVj5
@  `
@@@@
X,T,T
(TLD(
#5`U
@ ``
I$b!(4S0
 A@@@
    
$DDDjF
4(5*
*5ju
` P0
(DLT(
T,T,X
$%IKK
IED"!
@@CC@ACB
BCBBBAB
`                     ?
(DLT(
001300001210001210ppqrqpppp
03?<00 
8888888888888888xxxxxxxp
< =?< <"#<#>)?:3,0!(!" ""0""8
??> 
???8
888???88888
????????????
      
??> 
???8
888???88888
????????????
      
??> 
???8
888???88888
????????????
      
@@ ` ` P0Q
p( @A@A*
` P0
2"%9
5+%*! Q
    P0P
hP`P @b@
bBbSi0(
$CFBV<
$%IK
""%!&
@D@E
5jVJUBA
!#!+
T,T,X
@@@@
`  @
5jVJUBA
!#!+
T,T,X
@@@@
`  @
Ya!3'
$%IKK
IED"!
5jVJUBA
!#!+
(DLT(
T,T,X
@@@@
`  @
0S4(!b$I
5jVJUBA
(DLT(
T,T,X
@@@@
Ya!3'
$%IKK
IED"!
` P0
)CKW'
T,T,X
0S4(!b$I
aa!!!
1#cC
aa!!!
hh`hh
 !'-*)o
TT|TT
]kwk]
|||||
hh`hh
?@OPPQSTTWSSWWWSQPPO@?
__]]YQAAAAQY]]__
?@@OIIIIIIIIIIIIIO@@?
pppppswwwppppp
quuuuuuuuu
<fBBf|@@@|fBBf<
p00000000000000000p
l||||||||l
|||`ll
?_O=_
w?W?
7_/=_/7
0000000
0000000
#ssS#
;_?_O?
o?W?__/
6-6-6-6-6
O7_O
_O7_?O7_
6-6-6-6-6
OOG# 
[?O?_/
O?W?_
OOG# 
?O?/
?O7_7_7_7_7_?O?_?
_7_?_O?
    !
`   
q<?'
811! `
7__?
?_O?_/
?K?_
6-6-6-6-6
?O?_
?[?W
O?W?_/W?
00``c
?W_?
?W_?
?_/W_7_
.~[?/
{=?<
W_?_
;-7;
o^p `@g?
@@@pp
/_7__O?_/
?W_/7_
O?_o?o3_
CC@@@r3?
@@@`
00003s
<<?701
0``@@`
0bcCAAc?
@ABBD 0
N0oKKI
H@@ 0
@`@p\b@
@ABBD 0
N0oKKI
H@@ 0
@`@p\b@
0``@@`
0bcCAAc?
@ABBD 0
N0oKKI
H@@ 0
@`@p\b@
   8	
!"    
00/'#!
??000<03><
<<<<
????
CC@@@r3?
@@@`
00003s
<<?701
   8	
!"    
00/'#!
??000<03><
<<<<
????
CC@@@r3?
@@@`
00003s
<<?701
< !!
?  C
    @
00<<000?00008<
xxxxx
????
??#!
000000000
<<000000
000000
00<<30
@ABBD 0
N0oKKI
H@@ 0
@`@p\b@
@ABBD 0
N0oKKI
H@@ 0
@`@p\b@
~__{
|@@@CC
|@@@CC
CpH@@
oGGWo
T(T4
0``@@`
0bcCAAc?
@  P
@cG3Tco
Ye3q 
@ `P
X$2qk!
+rEmD
``dN
GA@GA
72m1
A``bN
p[wd
DCNB
2j;a]
aau?4ma
.?;]
p88888xx
ieWz
18ya
6ll+
~z>~~~<
00pp
t88<
8840880pxp8
888<<
<8xxpp
xx||??
8x800xy9
?_O=_
w?W?
3"'<
8!/8 0
8#< ?0
PPPPPPPPPPPPPP
7_/=_/7
??> 
???8
:::8???89:::
????????????
OOO@@@@GHGOO@@@@@@@@@OOHHHH@@@LOO@G@@GOHHOG@@GOHHOG@@GOHHOG@G@@@@@@@@@AANOOO@
/?O?_
/?O?
/_/_/?M?_/7_?O?[??o?
7_//7_/7
W?W?_
6-6-6-6-6
O7_O
_O7_?O7_
6-6-6-6-6
OOG# 
[?O?_/
O?W?_
OOG# 
?O?/
?O7_7_7_7_7_?O?_?
_7_?_O?
    !
`   
q<?'
811! `
7__?
?_O?_/
?K?_
6-6-6-6-6
?O?_
?[?W
O?W?_/W?
00``c
?W_?
?W_?
?_/W_7_
.~[?/
{=?<
W_?_
;-7;
o^p `@g?
@@@pp
/_7__O?_/
?W_/7_
O?_o?o3_
0x<x0
@ABBD 0
N0oKKI
H@@ 0
@`@p\b@
w{}<>
?701
???<
?????
??????
@ABBD 0
N0oKKI
H@@ 0
@`@p\b@
0x<x0
@ABBD 0
N0oKKI
H@@ 0
@`@p\b@
@ABBD 0
N0oKKI
H@@ 0
@`@p\b@
xxxxx
????
??#!
000000000
<<000000
000000
00<<30
< !!
?  C
    @
00<<000?00008<
   8	
!"    
00/'#!
??000<03><
<<<<
????
CC@@@s3?
<<?701
<<?701
v??->7
2UPTRHbE0%0
7)&!
IdBu
|*md
8aac
?x!`C?pc`z
A^PPP
8aac
?x!`C?pc`z
A^PPP
8aac
?x!`C?pc`z
A^PPP
6??+?
 :QTRHePB5 5
7)&!
B:B)
zm~w~ow}
;>?;
(${@TRhBT!4(
X}$u
(B%Q
}ot~{=7=
"8RUDqHRA5 5
8aac
og}<
("yDR`[@R("4
~~}=;
8aac
H#H%
IgQEE
Pk`U
qJF%(QX1
uz-E
Cp2(
~~}=;
8acg|w
tbuI
A^PPP
h"I"J
{{z}}|~~??>
CVL<2?8`@
A^PPP
{y}|:;;
8aac
?x!`C?pc`z
A^PPP
H0PP
8aac
?x!`C?pc`z
A^PPP
}Z~5
 A@@@
    
$DDDjF
4(5*
*5ju
` P0
(DLT(
T,T,X
$%IKK
IED"!
@@CC@ACB
BCBBBAB
`                     ?
(DLT(
001300001210001210ppqrqpppp
03?<00 
8888888888888888xxxxxxxp
< =?< <"#<#>)?:3,0!(!" ""0""8
@@ ` ` P0Q
p( @A@A*
` P0
2"%9
5+%*! Q
    P0P
hP`P @b@
bBbSi0(
$CFBV<
$%IK
""%!&
@D@E
5jVJUBA
!#!+
T,T,X
@@@@
`  @
5jVJUBA
!#!+
T,T,X
@@@@
`  @
Ya!3'
$%IKK
IED"!
5jVJUBA
!#!+
(DLT(
T,T,X
@@@@
`  @
0S4(!b$I
5jVJUBA
(DLT(
T,T,X
@@@@
Ya!3'
$%IKK
IED"!
` P0
)CKW'
T,T,X
0S4(!b$I
1 @@`U*5
HH@@
p -J
@@p?
88800000
@@p?
S'G#C%C+GG'
@qO#
 O0@
@ _ 
Gx@xC'-.
>ow{=
#LP!"
hqx~
?{3'F
@AFK@@`
>A@@ 
DDJQ
@  !
u:<:4yt
P(T(
"$IB@! 0L
33qfe
%kekg
H(0  
p~??
<8:2
$(KD
@@@@
EG[_
            
J'_OlSmTo{-
UZ/5
&-VMZ,
y2c5W;
Wo93222q
o?/>??/
7+5k
*uUUU*
'sp$
;UuU;
@ 8x
"UEU"
;1;7?
08080(0 0`0`p`p`p`P`
    0
 `@A
ZJF'?
x4 BBP
$80 @
DBA  0
  `@
@@@  @
@@@ PP
((( (
@@@@@@
b#"#"
b#"#"
"E*T8
8Ll<
b#"#"?
 @\D 
b#"#"?
b#"#"?
b#"#"?|
?111
}Ju)Q
"AKU*
(PP(
|xp`
?!!!!a
(((((
88888
(((((
==9!!  ?
   0
??0000
pp<<00<<??00p
[}o?;
`J`&0*
/__?
_6oSMC 8
,p0X(X
oPhP`P 
hTj5
4)1"
=<x8
2kQhTjUjUjT
@@@@@
QECfJFE
0b H
(X)X
@  ` 
  p 
#$DIIE$"
@@@A
rtkN7_?
H@LpfAu=)
Ww)kQ
U?p/o/o.l
/((o
h((/
d$$$
$$$d
DDDD
?0($"!!!!"$(0?
@``````````````````````````````````````````````
@``````````````````````````````````````````````````````````````````````````````````
888888888
ppppppppp
888888888888
ppppppppp
888888888888
ppppppppp
ppppppppp
888888888888
ppppppppp
888888888
ppppppppp
888888888
ppppppppp
888888888
**')=6l
TTTTTT
<   
<   
<   
?`@CFDDFGDDDGFDDFC@`
c##c
c##c
@   
   @
Xl7.
@``000
  ""
    
   @
(T,T(\
  ""
    
   @
Xl7.
@``000
  ""
    
   @
  ""
    
   @
%$''$$
PPPPPPPPpp
@   
   @
@JJJJJJJJ@
PPPPPPPPpp
@   
   @
  """""""  
HHHHHHH
PPPPPPPPpp
@   
   @
   &#97
xXxx
   @
$ &83 :
xhxh
@   
   @
   @
   @
   &#97
xXxx
   @
$ &83 :
xhxh
@   
   @
   @
   @
 !"#"#! @@@`
?!!!
   @
!!!!!!!
!!!!!!!
?!!!
   @
!!!!!!!
				
?!!!
   @
!!!!!!!
?!!!
   @
?  @
*V,X
?!!!
   @
@   
?  A
?!!!
   @
@   
pp88
8L\|
*V,X
?!!!
   @
@   
*EKV
@` 0
   ?
*EKV
   ?
*5kV
@` 0
   ?
5+VlXp`@<
 "%J5
0 `@
   ?
>Ax<
    
?   
   ?
p8X<
    
?   
   ?
,<,\
    
?   
   ?
  ` @@@
@   
@   
AAA!
@   
@   
HHH(
A@@@@@@
@   
@   
74|oiy
@ P0
  ?  
@   
0001=
?>=xxxqs
$"A@@@@!"
@@  
  @@
  ?  
@   
$"A@@@@!"
>74?
<89xxpp
  @@
  ?  
@   
>74<gi
  @@
  ?  
@   
U+V-J
    
?   
   ?
    
?   
   ?
    
?   
   ?
    
?   
   ?
""""
"""""
"""""
   0,
"""""
"""""
   0,
"""""
"""""
?`@@@!
0HHH
HHH0
@@@@@@@@@@@@@N@
JfR^V
>III:
>III:
>III:
@@DDDD@|<
@@DDD@@
2III&
2III&
DDDD8
000000000000
>III:
>AAA
&III?
000000000000
00000000000000000000
@@@?
AAA>
xxxxxx
xxy{sg
llnfgs
2III&
>III:
@@@?
&III?
>III:
   ?
>AAA>
>AAA
>AAA>
@@@?
>AAA>
>AAA"
?@@@ 
8DDD#
   @
?!!!
   @
? ? 
?   
?!!!
@   
   @
>AAA>
>III:
>AAA"
>AAA>
>AAA
?8888888
DDD@
@@@@
DDD@
DDDDD
DDDDD
@@@`X
DDDDD
DDDDD
CCCCC
CCCCC
DDD@
0HHH
HHH0
?   
?!!!
   @
   @
   ?
          
?@@@ 
DDD@
@@@@
?;;<
<;;?;;<
<;;?;;< <;;?
DDDDDDDDDD
? ? 
FFFFFFFFFF
vzzzzv
?  """ 
?  """ 
IIIIII
IIIIII
          
          
0HHH
0HDB!
  ?  
   @
?   
DDDDD
DDDDD
    
``00000``
>AAA"
@@@?
&III?
@@@?
>AAA
>III:
>AAA
H(((
(((H
((((
(((H
(((H
(((H
(((H
(((H
(((H
(((H
H(((
((((
(((H
(((H
(((H
(((H
((((
((((
(((H
(((H
H(((
H(((
(((H
(((H
(((H
((((
((((
H(((
(((H
(((H
(((H
(((H
(((H
(((H
(((H
(((H
(((H
((0`
(((H
(((H
H(((
(((H
H(((
(((H
H(((
(((H
(((H
H(((
(((H
H(((
H(((
(((H
H(((
((P0
(((H
(((H
H(((
?   
?   
! @@
@@     @@
`````````````````
Xl7.
@``000
   ?
(T,T(\
   ?
Xl7.
@``000
   ?
   ?
%$''$$
PPPPPPPPpp
@   
@JJJJJJJJ@
PPPPPPPPpp
@   
  """""""  
HHHHHHH
PPPPPPPPpp
@   
   &#97
xXxx
?""#
?@   
   @
   @
   @
   @
$ &83 :
xhxh
?""#
?@   
   @
   @
   @
   @
   &#97
xXxx
?""#
?@   
   @
   @
   @
   @
$ &83 :
xhxh
?""#
?@   
   @
   @
   @
   @
 !"#"#! @@@`
?   
   @
   @
   @
!!!!!!!
!!!!!!!
?   
   @
   @
   @
!!!!!!!
				
?   
   @
   @
   @
!!!!!!!
?   
   @
   @
   @
?  @
*V,X
?!!!
   @
   @
@   
?  A
?!!!
   @
   @
@   
pp88
8L\|
*V,X
?!!!
   @
   @
@   
*EKV
@` 0
    
@   
*EKV
    
@   
*5kV
@` 0
    
@   
5+VlXp`@<
 "%J5
0 `@
    
@   
>Ax<
?@@@ 
   ?
p8X<
?@@@ 
   ?
,<,\
?@@@ 
   ?
  ` @@@
@   
@   
AAA!
@   
@   
HHH(
A@@@@@@
@   
@   
74|oiy
@ P0
   @
0001=
?>=xxxqs
$"A@@@@!"
@@  
  @@
   @
$"A@@@@!"
>74?
<89xxpp
  @@
   @
>74<gi
  @@
   @
U+V-J
?!!!
?""" 
   @
@   
?!!!
?""" 
   @
@   
?!!!
?""" 
   @
@   
?!!!
?""" 
   @
@   
""""
"""""
"""""
   0,
"""""
"""""
   0,
"""""
"""""
?`@@@!
&III?
@@@?
>AAA"
>III:
&III?
EEE9
@@@@@@@@@@@@@N@
JfR^V
? ? 
?   
@@DDDD@|<
@@DDD@@
DDD@
@@@@
DDDD8
0HHH
xxxxxx
xxy{sg
llnfgs
?   
   ?
? ? 
?"""
   @
   @
8DDD#
?""" 
?!!!
    
   @
@@@?
>AAA>
8DDD#
>III:
>AAA
2III&
>AAA>
?8888888
>III:
>AAA>
?   
?""" 
DDDDD
DDDDD
@@@`X
@@@ 
DDDDD
DDDDD
CCCCC
CCCCC
?   
?   
   @
   @
@   
!@@@@@!
?"""
!  @
DDG8
          
?@@@ 
?@@@ 
?;;<
<;;?;;<
<;;?;;< <;;?
? ? 
DDDDDDDDDD
FFFFFFFFFF
    
   @
vzzzzv
0HHH
0HHH
EEE9
?   
   ?
?  """ 
?  """ 
IIIIII
IIIIII
!"$(0
          
          
?""" 
    
   @
0HDB!
?   
   ?
@  #
@   
DDDDD
DDDDD
``00000``
0HHH
HHH0
?""#
   @
? ? 
?   
?   
?   
?   
?   
?   
?   
?   
(((H
H(((
(((H
(((H
(((H
(((H
(((H
(((H
(((H
((((
H(((
(((H
H(((
(((H
((((
(((H
(((H
H(((
(((H
H(((
((((
((((
(((H
H(((
(((H
((((
(((H
(((H
(((H
(((H
(((H
(((H
(((H
(((H
(((H
(((H
((((
H(((
(((H
((((
(((H
(((H
(((H
H(((
(((H
((P0
(((H
H(((
? ? 
?   
9eiarntsolcdupmbhgfkvywzjqx.-'02
14/38,?!
"():
;+&%*=<>
$`@_#9?
? ?!?"?#?$?%?&?'?(?)?*?+?,?-?.?
LW]Z
h,R?
<HB?
P4C/
1B@I
c@DO
HCBt
VL6<3v
 {Uv
TFGI
<J@:
%m-r
NH6CB
@3:#zhQ
$dxw
{A2f
BEA&
>@BY
+78p
^H"g
yLt3
%3M~
p5j5j
vFAy
E>$W
@H D
GM\6	M
%<0~
Np2:$
##9r
 3j{
(~GI
"RHr
#u^Q
-"k~
RpAp
ojR1f
LAH(
z3IR
}UH2
S7ADo
"]/y
FE0Q
8MHB
+@I/
h:_r
'%	r
@3D$
~iA]
~H6+
BC@R
(~j~
MAYd
x*_	
sYF_
~cR`
HJNP
q_	r
(9rq
+Jvy
DJ `
!U%~
BCAO
e0:p
w #J
hTV\.
C'A6
'syy
*'#o
]xE"
HB3N
k!vzp
'x/y
aP'#-y
n^_	
%&H~
?	CB
g\H@U
lvAD
f TE
rvUC
c#0!
AxMd
TFC 
m$:DU
7'Gs
&5.O	
@(`oA\
W`qH
@D0QJ
idFB
^B:x
fxA~
g^Hp
hFsY
!/W#
g>`{y
wH&H
&a	y
5vCLG
:=A	
QkA'
@,u9'
f":t
e%@/
%h]~
eDL"
6sg6']Er
d	Xu
<ZD^
+!~y
#RSy
%GFB*T
RAI_
XG#q
&c$Q
HQTC
xMAD
7BCs
#p{t
!a(@
HhIX
.OGS
!H`p
HB$r.
$j=z
"FDBH
^q+O
'kSMr
Taf#
)v=D E
6FB/
p%"%V.
OqH+
Vp`c
Npk;\
o9H(
"5{I
S<-&
*X:p
XH9y
%:nAX
HpJQ
1eLHBA$
HRXt
;qIEQ
MD6T
ZPU!Z3z
OE)]*z
>SH_
D2YJ
z!-P
M)cO
E^Q)
CVS`
dkq>
3ENU
H$Hr
2<#l
7~MB$}
#OgC"
G5F\
!W~LB
K }sJ
Im@O
+?{?
,|-p
f;?LB!
EBE@j
;uA/
;\Ir
>7FI+z
j\6O
%DNB#
=fHB
)QDTw
51IC@P
HQab
HRNR
-.C@_
@YugM
?YA*
CP:t
8.6/
&qRD
M!kF
>W:T
>.:T
!ExP
<y@f
RDDY{q
	+Fg
9eKDy{
;MJCU
'].p
4TRx
^?q@
91:_
&A<O
/IA/
7LWQO
)@:#
4)DJR
0EJZ
5bH?
"`W]
0H2Dz
-v5H
P[DO
c"p=C
$f4z
-$CB
(H.MR
+uL2
$6F\
BYx"
X,huG?
'rNB
*IC^
@jQLQ
){LPz"
)>AIrz[
JL!s
R{GY
CJ^x
,kVS
-=CA
P4EAx
,ojY
*9K$
 lN^
C8RK;
6R~;d
B^1L$
Rv}N
O!B(i
CBHAVI
$#HP
%W6O	
#tLP
#*XU
ZvVX
+y_&
L"Fn
M@HR
F%7^
#{WyBTh
M@J!
%,L@Y
$y@q
!y7u
B^$~II
	++d
!+NF
IGM@
@%*CH >H
9C@B
%BqT
 ?NF
$RdO
-uiq
Y:gH
vsLp
%^,@I
=ky/
#x>@
@D+:
'N,q
I ZW+
	IG_
BN!O
'rzq
By`:
I@,q
B)+q
=E'W]
"07w
uBD*w
)rNT
+~]X
xQ3gF
i@f!
#$B.
SCBZIv
"2~@O
LR{.
)})FA
jp]X
X6&tf
4=D_
-AVYg
YqdJ
	7jj
s=C:B
RQa_
)BiW
B#sE
wMqR:
#])x
$FpS
Pc2X
4%US
#X~C2
O4]J
"Psx
+g#?
i2Dr
D'z*
'RZx
3:#2
BTiTF
	H[:F
B8Y|
	+jG
 e	x
BxGYq
Drx0
0:@y
"TAx
R{{:H
2^,^
p&(WZ
M iKDJ&
!w?x
L,v}F
&sGx
n6F2^
 vNv
p~8:$}
f}Fx
EEPQT
#UvsO
$OOQ
bHxx
oZYb
FR1op
(F*x
E6uy<7p
!L@{b
U~TK
|rWx
6S~>
4xbx
+~Vx
W~f#_
Y<7B
^~UI
STg6/
%P}G_
QzdH
F#i50_
(~[A	_
z!r;
vU|Rr
l,oEO
^'z@
|/tu
$r$_
HBQ}
I`pF
!WbCsZ
O	+p
DBzi
!*TF_
:fnAL+a=C
Yy[@
^};_
$BfO
	+x-0:p
'zDN
#}yP|
psmJH
JApq
CRt_
DR(V
hp5ERe
%y:@J
#|LO
X{ sq
.Ar|
2>	t
]a=DB
RsZ:
TY\U
vUQy
tz{;
"an}
MP5H
qAXz
{]qs
	~zt
&zi}
 Hh}
@vzg
~xg"x
X7^6%z*!\
x'4\k4
8TAO
Hht 
FI"s
Rj#N
#w]IB&[
Px~H
%xs]u?\:
_	o %	d_
-ihO
quhF
PxUAxs
x>qo
Wi*fg
`qC%r
]wBD
2ZmQO
'OS-q?}
v>Y@~w
Qw#EB
p]sM
vvE0F
-t&@
gdQv
"uHO
pf	ja,E
BNQm}
hnvO}
r!r7E
8f[d
 u7w
):1}
f:FI@
rrT^l,T
RgeA
EYS?@#J*
&hb}
E#r$
!Wut
u@7rr
w&aTm
A*_C
Cpsk:
Rr4'(Zt
"V*w
mJK}
 &qw
J(bh
Zo2 &Nt
@D:YrmZj
uROB
pGhSr8
rfiXn
qe,g^}
)Vn@
YlcO
QmC(mk_
VR)%2
FRm(p8
NZ@"p
XokT@
\CvC"O
HXe[@
HPeS! 
i>@:
]go}AO
Tl6G
p7:] 
l"oC
toN_
Rg'Nrf
Rj4A
E7fO
p_dB
[E"5
BIXo
!$p@
+k8Pn
+o=O
*d]O
"n4A
FAXn
Pl	Wj
rj&$
IPkZ
D JULO
@xm:
Qn*D
Vm}%k'}
]ia$77
0C'c
!JPl
~20AH
=V_8
qhqRh)YhR H1
rl8c*
@TkjSb
&kQ_
B&aUJQl4'
L2FPj
)Y,@
tDt/
C\'HC!1
bBhSZA$_
+ lTU
$JDs
(BYg
49DPg
qbQD
J@Rat
Qf`HQ
T SC
jZ^)
$_T}
':ls
j4dV
(\QOw
HB$M
 V\L
M@*i
#E5E
*]3t
Y^xJ
@:#F=
4=$gLw
RU|Pc
-??w
C\SH#f
+gjw
#YPyfZB
JRU%
QclHB
PfdqY
H"^7
W\cNCrKp
FPf9A*fgO
(>Ot
e'N@"d
IB}+
Gt3~
->_O
qDy(<
]+jf
(>(/
*D$Q6F
#bB[d
PJ-O
#%p}
3:#5
-<Hw
a_:K
jeqA
6%U^
j4[?
GxA$T
b9d:[(
Qe/NR`
@cB~_
]K^W=g
26>T/
RN&Pd
!`B6
RME(
J c?T\
IP_K
sbR?
RRw`F
hcuQd
Yc+^c
^`nI@J
#W)PA
ZKGO
q[ZD
qG<I!O
SPpD
V9VY@
6<FRX
 C E
dQtO
?4Nq
_HK*`
^-tp
fY}H
"O9_
%/*WV
.FgJjCC'U#
FFP`
AT]hwT%
B%T"
aYQauW`u
`"raM
fZ0|
"J%s
#&E|
"^8s
kGr`
M P`4=
QX6C
Y-`z\
R]+G
|_oA
\_&C
:|]^
"[5s
#UZs
P|T[6
EsAPAIA
T)4P
R,qpW{
2N~]{"E
HqR)"S
(XC|
r]kJ
`PKs
CADB
BD%Qg
(\fs
V72+P
\URC
"]Nv
2A"P
A4C`=n
'ST+[7|
"Fns
Y-PY
X0LEW
R>4^'mI
 DSZZ
`[BxIO'V2O
]IgWL.C'$
[`P[[Q[wX4J
=Dz',B
W6XrWL4
Mz}U
RU:7
'<]YM
.ZYy
SXq6_
%Ra Z
@DB#$
9dN/
QV?/
N'T-
J#Y"_
",QZI
fJ[v
@zRd+F
'VTI
Wd6uJ
 E\A@
#YDH
*6/|
'N:v
,GMv
WU+"
#6S|
CBI@
Xd!8
YVHB
|(+?
*-+s
F';S
QAU/
C@@Y4
!7jA^0Q
P-LXT3
J[%,
&MYL
PWM!A
$U0L@
)LpK
R7fA
Z-CO
(FWs
*HKHAB
@:fKJO
rU^.	
#QP@JArQK^LJ
rLX^L
#:1(>
CAyS
>n@9|
!>4C
Tm	:
#Tr|
;6T&
jI)T8
],}D
P"GH:
I(TFGSG.
,Oh|
QFM'Q/
RO1@
pSgjG
R][=M
.4qs
)/,s
@!UG
P*Pos
%BxL^AO
QR!=
NB%G
A#Qy
Hy0+
+*ZB
@A\E
.qHr7
QOdH(
Q)D ,
G`RP
"N<s
B<CQPw
PMVQPB]EH
BCyP!/
8TP	
RONpL
%ODs
LNJl
qLOt
(NJ@
)A{v
"H)s
yMUE
JJ 4W
ErH@
EmJ\v
WL(/
 M?s
 C-s
 3Gs
\M 3<SI
"<XAO
F-B}
D*,dM K
!@/|
L=:D
L#A,
%@8|
):{s
%K9v
A:T7
QK!]IP
+H&v
.Ifs
&Hi]H\\5
)Ij|
\*AC
+ ys
PFdw8CS.=
%IpKtHn
)<VG
-7`p
7R'|TE
EVI>|
RH6!
BI0QH
&=}v
 ,Es
$*tv
P)do
p?$jD
RDLpB
+C	|
U:-2I
pGF:
A@fFF]6
:c:os
 D:Q
!=9v
x@v(D
Y:0R+}
#7b|
BLpFC:X(8
C:@:
3(!:
PAC_
=QEQX
NP9](>=yA
A(9T
Y3O6
Y>FC
Eb6E/
>p:xLO
RBQ 1
,@<CR=
 @]v
J@F%
+Cdv
x8v@
$B/v
!3rv
pB~:
@:s=|
QB~6C'=BU
Q00}?l
-:I@3
MLHP@
T(;u_
QArX@>
P@X?
QAPXA-
(5dQ?
A2T:
2%:Ds
V?$|6
\.~3
q<3@
J*9?O
-3x8
%,Es
IR9|A
=1?Y
w'hH
B%4o@H
u69)/
]<,/
eDZ=
P,d!!7v
B\,{V
U3aK
=Ix<	
=?5/
!.wv
M-;KDT:,
;N=vO
p=Aj
*)\$
<mHBD
];RD
F&$5
X;H6,
**6s
N(7"
8_,.N
7}N@C
'8KQ;t6?
 8@v
P8(Q;
AX0~S
"6^|
Lp:_
)5uv
AB^6
q9$	s
zT3)
9m8m|
'5T|
J!8$
R8U+4
HG-5
Y.<Q+ 6
''O|
'2ov
Np7e
~6W'0
C&6<E
7Z53t
tW-z
++	F
6mj#
S1%&1"s
L\$Y
12%5
'1vs
B.0ZP5?H
#%F|
2j2VU"
)-+|
'%J|
,-i^
+x!3O
C09P4
S2"v#:
)	4|
$#(O
5FP(
S0GA
Cr)e
3o:DI
FP+>Q3z
.,EA
3AQ3],&K
W)XL
/j'ov
*-zv
q.yy.sB
6EBIX'_
 2N|
JAIR
R)"@
MBC!'?
,#~v
@DY0
$0Cv
X0K6+
%*h@@
y)U+
!#qw0NO
0#0+&
HP/<
CBA$,.D
6%+q@B
p'	:}
"%v|
IR*Yq+
V#iu
AY*/ &
.-3v
,!P-
x-"A
JBS*
Q-qL
nQ-'?
'EP,
)fV)M
-+*A9D
R,1@:
 f#E
%,4v
pK$,
BT+1
,>Q!*
*4a"
Q,-+%
K>R*
M^(G
+$!/
MB#(?
NF@O	
E!$fY*
X'b%*
V&xE
I@P) 
R%w@
JP'{G
!7'O
!$MJ
r'?$
W6\!
&!Ms
&4L/
-&R%#)
%HMr	
p&>_
! VAD
!%Qs
+&Dv
t%[D
"xt#
#"Vv
)!:s
+#Zs
Q#vX
r!Z)#F|
#.A$
C@D*
@BS"
	JA)
0Ah HM
( $T
bB54
@0B5
6:HP
4=D2_
}C0Q
C7@$
IHB!
.F@#
@BC%
TAO	
IMBD
{GH:/
\J@:M
AP	=
UCAO
'D!	Rf
=C=@T
=Q	aG
	$6/
*	eu
U<6{
f@J@
[ !"#
%&'()*+,-./0123456789:;<=>?
ABCDEFGHIJKLMNOPQRSTUVWXYZabcdefghijklmnopqrstuvwxyz
9aeirncodtslmbupgvfjhz
qy}xkw0284-1'.,`@
"()/:
;+&%*=<>
$?!_#739?
? ?!?"?#?$?%?&?'?(?)?*?+?,?-?.?
x]bU
3\-*U
}3w#f
sDE@4\
01@4\
GQI!
}`CS
"pGF	0
1E@[
FLM	B&
^?0w
@	`o8
?3	O
z~EO
i-B@
&vgp
pb	\
w@D!
h@JV
xa@	
t3_	
HA#`)
e2G"
p_AE
|zDE
vPAT
bmDG
|tsW
uR	F	
?3	p
FDE!
xDGA
:*Af
At?9p
z$4C
]|IP
-asJ 
y>4S
xqN!
G*49
UH.G
m.	|
wdJ\[
tw	|
siJA	
%:1u
16@c
 uv|
rr	p
O !B
KJ	p
)4VQ
p>	A
06@G
06@3\
Wz)[
 owu
D@4Lp
Pg)K
o.4S
>F	|
01@4\/SG6
QD+_
_-	$
j	=p
iz#T
jA	T
h7	u
#Vi|
j-	u
b|	u
WDmQ
a'#7
S9E	|
#h:|
@:4JA	"
c2YVK
^		T
`H#|
U]Q4x"
IHBz
(7]"
_<AT
rX-O
`RJA	r
TWJP{
vV7	C
Eqfc	W
`#mCu
K%I+S
W.EA
\s~_
F>	[
G0A[
*h)p
>6	J6@	
*h@p
\3G@	
%nF&f
]s9s
O_NU
%d!|
FK]h
	w o
&B*R*
X7G6p
	B	[
CF	S-
LT@\
i	4[
RJE_
9m6N
HPq!`
E@	z
T(C#
$~:C"
VBWb
r-X	u
[v7D
-u)l
N8U&
^i!#
MBJP
%M-=
,wL@/	
9YL 
q$h	
R~4sp
@|n+A(V
&U<BK
5F1R
TBW	A_
NA	@E
P,A9
	MKL
P)0f
S[8I
){~p
BlM\
0C	B
0;{R
=&pQ{
 va|
${ou
\VF%VCu
%gZ	t
Vc(Cq
'4O|
I'P	|
C$hA	
HuAT
u^C/
(*BE
0|B	[
FK,_
Dt$~8u
8CA	r
)T#u
FU4S_A
|Q$`
DNDE
BpWO
DP	16)
@V		
A'<Z
+T"}
	(zTC&P
>PEA4
=qC@U
AN4C
Bp|'	Z
<~}E
!Ddu
@.DY |
&WuG
-t4[
<F}tD
	I1R
4,"#
;`&o]
=l	F
"cDW
Q^*R
<I4[
<t	R
0WRP
9TBP
0hXh
8%&g)K
uR	u
"=Zu
,DwN
9GPGE
-XB	j
@	EU
6>Gp
VJV-
/$	/
7.B	
Cx@&A_
 _WC
%$aY
[AR#
4ZFJF
"1TC
+HBJ*
)P	)8
@cvmA	
 3<|
	KF	"
4H4I
nquwS
tSZU
 G&6O
Oo	A
8hq c
#1Au
(L=u
Ps|r
/,	|
&mou
1B0E
 ]|u
7A#I
-AA#mo
LWz+	
x#w D
DF	@/
"6	p
"ecu
lB	*
5	qZ
&e`e
-h6s
Y)mCCR
I P$C
-D(u
-"ju
-"fp
-v.u
Q6k-
*;?u
ZXet
(A4L93Y
E6-;7Qj
`~Nf
KF	@Yr1D
DH@w
&YIA
hNZ;
7B	T
qs$	CK
B	4S
I@N@
 CKp
))4S
(DBA$r
EFJ&
$oDEA
"43A
#,/E
!JIG
!mus
IAKL@
#~@O
*z'D
)9	CW
L"k(
G"deAE
%rJQ`>F+
"lGC
$f^y!y
PTwAD
BA$Z
0E@G``
ff{q
'2R-
E"NsL
Gp7;	As
!$A	
R{/z>
B	4[
`p7	
fADA
p,S	O
- )H
-jEw
 >U:
rwV\
v-6-
Nwva
'-_n
439/
"Z;O
4Ys$/
-Q C!Z#
AtdE
HQgR/
"1UVW
_5JBu
iV8R*
zv|m
&KjDGQ<
I@	r
|$BdBA$
#IUV,
`wn&1
G6@	0r
u`	_	b
	EHR
|Tt=
_q>Ap
#j5O
%w}6
aU@/
4p>$H@
/c	B	[
@	\@@
)wvDGA
eKA$+>
"#SD
Au\4/
=BE1"R~
A%YaZv
(Z/D :7F
A(q^R
Yr\S
*0~!MCXo
cfn&O
LM#L
I@	r
	"DPw
P5w\
%w)A
,(iw
JA	r
UCAE
A)JM(q
{rv+Wf%
Z%KA
C+u_?
($hJ
ir6FZ
Fuuv
S:,)z
@UzPJ@/
s	/	~
0<D#
h`{!
AD'Z
#dY\
*GA\
@D%C3
	pH5|
^~u)c
!rXO
Y	#J
&:Yq
ZmC{
Zm/v0@
Rb.H
 o>O
QNo_
/	im
(FBT
eC@)@
H@*u
Pu%&lrq
PemU
"h(w
&e#B/
wGIA*v
{t\u
A34SI
(~6D
w	M'j
#n/KP
#]0q
lK4G
A9U>$D(v
-u5B
'vy_
c2CU
#m7/	
	l$O
2FDO
C PI
AEB_
%N7O
N-}l
#u,q
VJ!(LIE
.~GF'
yFbQw
WX=_
D'J0N@|dY
.rAIp"%	N
J j	&sEw
#D'w
^o:ST
CBLB
wlQ|4[
;6s~
\x?Wz\[
sxK@	
tR^X
E@)^
r>|jB
}TK,ob$|
DE@	A
wIB`q[F	fx
	6-Z
yc&t
U{`W
&|Gq
W}:J
GB60F	
J@E(h'
4K\z<F	
x|Vzxp
\~}Uz>W|
RV&ZaBK
T~d9
~v$u
R{{1Bq=
Q{fO
	"MfBP}||w
@%{V
t3FO
}v2us
2F,x
-0ZFL
y!Q{
@LPw^
UzmG0
S|8	
G@Uz[	Rv
H0B9
AWz,	
Z|<Tx,
\|]WyW4Sz8	
y9gsF
	Q`8
|d!h
_ N E
C'{n/
AC`x
	B%mGJA
{\pH
"(=[
	[{ DP)
A	`]
6Y8U
I&R2CD
&zKIF
s@;Rw
@	zz
B	4[{EDG
w}Qw
RxbZy
T{&I
$x6?
xt4[{
\iFE!*
\pbE
t]k'f{
polr
)\xOUv"Wx
Z]#K
\x!Uu
B	zl
JUyn1
xHYii#
pTB	
K|[`S/
@|;n
l	!=
 CQv
Pvzrr
"obq
K!D|D
q(P4
UvEWM
DB@*+
UWOLRk
tGxB
PCKpnm
C@Wg
:"<g
uzvu
LA#p
[w*qf(srgF
vjQt
G@*r
-OF_
o AWv
@	\v
BQqu
SrT7D
Rv2D
E#_hGSY
yvRN
Skw	
O}D':
$ext
|s	rs
Ssf	
siZ	I
-gUA
\rgG
J6A	
	-p#S:VYt
	rt~
\qL!T
pD95DG
 CPj
&sHr
q-kg
	0Vs=
J0AD
%NBZsb
TnA#Y
(!`r
A	rp
qM\p
q<Qq8
@Lpo
Uo9(,W
qKK!)x
I0B&
B+q[FD
Q8cJ
e>$mo
'J=)Y
A#YjD
(3gJQn
I0Reh
!\XKF
p<[S
+l]O
ECAWk
TK\[a
"F^#fbGRl
'U.\]NEQm
	Ep[
\m0UmnGpY
(mP$]
IEC!-
Q?m-)T
EUm	1"Z~Zn?y
q8r	AO
SjMIE
QO^J
tO>Uo
+J"b
k4BA
$Z6J@Ulr\mHUl
Uj1Gpe:	
g:[n
Z<zF
lPSlM
C@Uk
#K$A
ADrU{A
@*L+QY
0BUjW
@'B	AG
Pkp`
ATm9#(
FCPi
Q]XDai
FK"Do
MFU)KW
)f;NA
AUezO
#ZtD)\
8BG"h
-R[[Xe
~5IA
)`]r
UhTWl
-0@{
plTUi
@%T^
YGUi}
ia1r
"HAJA
!$mDE
pk *i]IPg
i3RFE@
AWaF
(Yc&V
"/cA
#fpBVi
!/<J-
%RBB
GUfz
"Mx[a	
)"R-R
@Gq28
f6aB
@\jqUf
TjAcQ
Ph'A
p)>	BPY
ef<%
	THH=
	ji]
Whw	
Efi(+f
fp	ZhT
)^|K
#5hN
,EuJ
,fND
QBrraY
	!YrK E[
h`iMXO
G\gS[gPE
JPG9qg?
Rdn	D!Y
\xC@,f
W]nO
p+&	
Tfg@
Q1eG@
 [+F	
WgtAO
f~R]
X[rc<W[
rg/Ug
\dPWM
e5fE	
H+5"
"Rvz
F]"B/
ufF0VG
!O@z
GQbnRY
	-_?B%DT_
 b;D
\cRWL
F	^ejSa
!E\Sd
HQ^L
B	4[2
pQNC
eO#$
"c)C@
R3^)
zc:(Y
d[]g
a{Xt
A	rbJWb?/
J!ca
0qUv	.,
LI\Z7B&'
`)t	
[aSC
WY A\^
B	[cP
-;%O
Zbj+,
$ap$07
b1)[
B	[b
D0W\
!S7f^3
T@C`U
KPa^
\YkWS.[b-
__D0
@3\[|W^{[a
\^zWV
B	[a
\^\W^
[>FC
p]/	
A	r^
\a.EFK&L
:D'_RK
^/^G
WU\[`
	B0w`|
WIf[`QT`
	Kr=
pMX	D@
E@SE
#]pq_
-s^|GA
\;T-B
Y^GPDA
]8\\
W_i[K84
W]`dZ%
Jp^/	F
#\<N
#*xDFJ
WT}A
`.tB
MPW+A
0!/{y	U%I
SOsN@	A
C@E@
W~-M
E@W\
B@uW
W^%6DQPW
S]1_
=Is\
]HFT]8
SZ.	
Y_SW
z[D*EgO
93I@UX
\hiM
"kRE
`)9O
T]bK
 9]	DGR[
ZF~Qa
H#&%
\ZUW[::[]
1rQ$G
	CE@TN
G6A6
(O\QQ
tGA/
SiBG"Z
*8#I
IQ[]
*\KB
(U`O
%ZT_
		aOj
-EKr
Z;CP\)
RDW0B:
C@	q9
`S#RN
xYXV[{#R
[[t4
WU	B^Z
K"ZI
Z~V.
/	Z2
!H7{
B	[Zi
TZWy
!OZF
4[Z(TW
WTvWK	
PV:!$
(8Pt
N(NIC
A	RYB
QL|L
"Xlt
Y-WY.A
\VQWR'[Y
PX4G1PX
Aw	t
,B(-
+SZE
N&*H9H
>MSJ
)7dHP
WXe_
W'[Xd
	C!S
CGAWH
"=KAtW0
U3L-N
(WWQ:
c7%I
iU4K
(&wt
JA	rU6
vU[!T
-EtC
QWMB$&
pS|L
 Pxt
\"<UR
r8I	
HrBG
H!OG
"Hbt
#$:t
WT#J0
u.e"F
WVLQ
UYV2
H"T_
AGAu@m
zU>"F
aQ &,
';]C
zH0Q4
&,yt
 5]{
!BNt
*By{
(.,v
BU<:
B	[U
&<W6
 4=t
OCPP
EA$A
UP WH
43i4kF
#.CVP	[&
A	rQ
!D${
B	[T
=lBG
?mBO
-Hw/
.?@{
H6#;
ERO?-R
CB(C|
K 7RCB
P*Oe	
URWT@Z
UP^WR
$P'/
\PgG
Pv	t
-6=u
MJPFlRM
R?UO
N5\O
)L?q
E 9'
E@UM7+=
&|	QF
O5%'m
'Nev
ADGqNn
!>{t
\N|UN
[Q@TQ
O];|v
FTP	
2RBUP
]OJXK
*6K(P
F.O=Y-
xC@	
B	dM
9>3I
0RB$
H6PD
ZGZ	/
$OA&
ATMY	
*Nh[M
HvHR3f
P;[&
'Lpt
O5M[eN
GRD8
WLqAWO
K,'X
SNZp
%1	t
I5XHQ/
N"	C
-+qt
HB[N
^A@wK
[N|6
"8!J
L^R%
f8w{
I;[N
mF(s
UK^PM
$K<{
RBD@
\KUG
_H@c4
0rMq).+
(>js
IP\M0UJ
")tQ
@DrM&_
4\[M
J7;V
J*;m
)2	J
(H;rJ
C$@	F	
J~R<)
	NJZ9a6
9x\ImUG
JRR#
4sC&
UKtJ
	CG`I
-Cwt
))C{
!I|{
"I@v
%Gyt
E";1K
UH*wF
I0E@
D@E-+
X7WO
DQ;_E/
;[0E
Ge1HQ(
Y@]HF	PG:
#% Q4
G8AO
fA|9
\G+WH
BF)$
E}F-RG
GAUD
$EIO
A#Fk_
"=QO
D5\H
 <DTC
)8}F
.EzK
!D ;sF
$;%N@
*6\?
ADU,
\A"UEA
BGQE
	M.&^H
rCN/
K1BpB<
DGQ2
RBw(E
'?*D
P?>aC
 .-I@	B
WC.4
+CgLZ
b@LJ!D
iLQE
EAGA	
E}FAJ
GM%B
@UCF
B30UC'w
KAYD
7MDF
6pEe
B('w
NR/W@
B0AW2
FY0]DA
C+;&C
0|q#
C#!j
B5CxO
YCg/
AAEu8
BW/rD
XDBU?
8MG!>
,>T?
 !;y
A	L*C
@	LA
S@p)9<A|Cy
JUC^A
BWA'Q9
qCi	^@
&8F	
p?WU@
G@\@XG
!7#~
Y;4s;M(A
ACA7[B
	,zAV+A
U?j&
;pR.
F)?pIR?
1BACv9
Bg1k
B	[BA
?b?\s
&09~
C6GF
P?8AC
@#Q?*
?+?Qv?L
4dT<z
U?@W.
`@RR.
r>L%?
TA\Y
OS?xI
z)GA	r>
	0Q5 
C@*?
\=}GQ6
`@h6
AT@D#
F[@z6
>3/zQ@
+>Os
:F?DF
A	BE
W-b[
[=?/
?7W8
=QW<
@3\=jw/
6NR%
76L"70EBA
#4k@
74[>
AT>Qs=
Kv=1	f-
u=*U;
,TDE
W)uO
\<}W>+
G@[>
<&J`)
U<~@()f
; ;U
(:js
0AS<
s95Q*
 /C~
B	[=V4i
W;k[=L
;nQ:u
u<YU:
(dB[9m
EU:g
%#-AGR$;-
')eBQ#!D`
p<vw-
\<FU9
W<b	
C@%9
AD0'3
A#8 O
Kq:f
%1%~
,9"s
;6;Q?
p:	w#@
	-9B_
8sU5
)%es
#!r~
4s1A
7)19
W6qT3
L 3BE
C-7SI
C-33
L*1CA)1vJ)
I@*!mL
\00U4m
5wB	[8
/	'uO
 /oB6
5i#5k
8G2_	B6
U5zw2
@Y#ER7bD
Q5CB
E!30
MDR6
4*AT7
6z	)5
5QQ4XR4Yy4|
 /(F
B	[6
3BHp$
AT63
!3"s
6-#dO
O	`2MD'#
AW2Z
A\5\
	(3A/
$,LZ#u+#<~
Lp,,	"
)5U~
C.%pY0PC
q$Ms0
Er-PA
1@),bq
1g3;G
B	4[4
1c2{
0=	J 
K.4V
%-y	U)
W+HA*,
NAz2
a4M	B
#1 7_
-3^C
^3;C
p/l	N
JQ3j
`$a^
	B	O
B	z0
.3@E-2
\0qG
[384
CW3 
IA[3
4F		
2GS0
IBV0
0R%W
	^2,C
^*fO
	EBF
\,EU04
+-	G
	AT2[s
,b07Y.
S1w	
S/%	H@O
AS+2P+}D
0B@S.
$&FE
W11	O
$*+s
P* [1
6@U/
j/!E
.XQ1
'+R~
	q1"
#+C~
 ,_~
!)oZ$W	/
 /Q~
@\,6w/
 (Ks
-jG6-.
4s'R@	
%z69
R)dV/8
EF	C@[.3	
@|/=
W/ O
W+]K
*	Uy
*+Qy
[.<T*^
- %<~
JX**M
U+5G@	
,l[,Y
-j39/
"y	O
!*;R*
#	0/	-By
",nQ,T2
	BW*|_
.*+E
@u((U)
",wM
J")G
`%L_
P"rL
+i	~
A	r(
( `y
(4R(5
D'$S
p*1W*
I@S 
d	B	KF	
'%qs
KAw)
A	R%
DP"pG
U'rW&
(?"r
@U'4w
% &y
:i&ZL#
$&C~
A$)WY&
#Z(]
)&Y~
,"_y
I@u'
Z%dK
r$f#&$
&kB	[(P
&mAr%s	r!
'x\(
)&[s
%:%Ay
A#&/
#&e~
A['@
$B'!~
B@B	
&h{%@
+	N`
uCQ%s
\%DE"
)$|y
(%Wy
U$"W$
!"?y
`%I	A	r"	
U#|G
%5	s
9X#w/
U!EW%
$!vy
T#!CW!
 $t~
AK,$~
""CS$
r 7*"
 #Ks
Dr$~
f$Vs
)!8y
G& AJ@G
J@,#
A("/R
p#8W!Q
\ zW
DH@B	["
BAS!
	&!py
HBP!
_A3[!
CA	J
v!+)
A[!dY!
3>CE
9F	O
:39X
S!Zi
A10AW
#	@Q
:	A'
:F	H@
_	;~
HN0A
IEAG
zB	[
CEAW
CF	C
TB	4[
DE1F	
[IJ 
;	HP
0BI{
N@	AE
1BAs
cKN&
 	G@
iv	n	
B	d	
8J@|
"	fx
	-	z	O
439/
K-	0DH
0	BJ
&64S
CC@%
C@G0
	LB6
UB	[
DA	G
BLB*
43	N
VH@1
B		[
A	BG
H@DG
[ !"#
%&'()*+,-./0123456789:;<=>?
ABCDEFGHIJKLMNOPQRSTUVWXYZabcdefghijklmnopqrstuvwxyz
@@SHANGHAISAILONGFMCBUBUBU$$
MIC:2d69567ca5520c783b76005bd61f2058
Model:F1000
Version:4.50st
